(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 809)
    (zones 0)
    (modules 172)
    (nets 205)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.35)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.9)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.4 0.9)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 165.735 86.995)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(C802-Pad1)")
  (net 2 "Net-(C702-Pad1)")
  (net 3 "Net-(C602-Pad1)")
  (net 4 "Net-(C502-Pad1)")
  (net 5 "Net-(C402-Pad1)")
  (net 6 "Net-(C302-Pad1)")
  (net 7 VCC)
  (net 8 "Net-(R811-Pad1)")
  (net 9 "Net-(R810-Pad1)")
  (net 10 GND)
  (net 11 +2V5)
  (net 12 "Net-(R710-Pad1)")
  (net 13 "Net-(R711-Pad1)")
  (net 14 "Net-(R611-Pad1)")
  (net 15 "Net-(R610-Pad1)")
  (net 16 "Net-(R510-Pad1)")
  (net 17 "Net-(R511-Pad1)")
  (net 18 "Net-(R411-Pad1)")
  (net 19 "Net-(R410-Pad1)")
  (net 20 "Net-(R310-Pad1)")
  (net 21 "Net-(R311-Pad1)")
  (net 22 "Net-(R808-Pad2)")
  (net 23 "Net-(R807-Pad2)")
  (net 24 "Net-(R806-Pad2)")
  (net 25 "Net-(R805-Pad2)")
  (net 26 Clk)
  (net 27 Reset)
  (net 28 ~enable_Shiftregister)
  (net 29 "Net-(R804-Pad2)")
  (net 30 "Net-(R803-Pad2)")
  (net 31 "Net-(R802-Pad2)")
  (net 32 "Net-(R801-Pad2)")
  (net 33 Data)
  (net 34 "Net-(R701-Pad2)")
  (net 35 "Net-(R702-Pad2)")
  (net 36 "Net-(R703-Pad2)")
  (net 37 "Net-(R704-Pad2)")
  (net 38 "Net-(R705-Pad2)")
  (net 39 "Net-(R706-Pad2)")
  (net 40 "Net-(R707-Pad2)")
  (net 41 "Net-(R708-Pad2)")
  (net 42 "Net-(R608-Pad2)")
  (net 43 "Net-(R607-Pad2)")
  (net 44 "Net-(R606-Pad2)")
  (net 45 "Net-(R605-Pad2)")
  (net 46 "Net-(R604-Pad2)")
  (net 47 "Net-(R603-Pad2)")
  (net 48 "Net-(R602-Pad2)")
  (net 49 "Net-(R601-Pad2)")
  (net 50 "Net-(R501-Pad2)")
  (net 51 "Net-(R502-Pad2)")
  (net 52 "Net-(R503-Pad2)")
  (net 53 "Net-(R504-Pad2)")
  (net 54 "Net-(R505-Pad2)")
  (net 55 "Net-(R506-Pad2)")
  (net 56 "Net-(R507-Pad2)")
  (net 57 "Net-(R508-Pad2)")
  (net 58 "Net-(R408-Pad2)")
  (net 59 "Net-(R407-Pad2)")
  (net 60 "Net-(R406-Pad2)")
  (net 61 "Net-(R405-Pad2)")
  (net 62 "Net-(R404-Pad2)")
  (net 63 "Net-(R403-Pad2)")
  (net 64 "Net-(R402-Pad2)")
  (net 65 "Net-(R401-Pad2)")
  (net 66 "Net-(R301-Pad2)")
  (net 67 "Net-(R302-Pad2)")
  (net 68 "Net-(R303-Pad2)")
  (net 69 "Net-(R304-Pad2)")
  (net 70 "Net-(R305-Pad2)")
  (net 71 "Net-(R306-Pad2)")
  (net 72 "Net-(R307-Pad2)")
  (net 73 "Net-(R308-Pad2)")
  (net 74 "Net-(C704-Pad1)")
  (net 75 "Net-(C804-Pad1)")
  (net 76 "Net-(C304-Pad1)")
  (net 77 "Net-(C404-Pad1)")
  (net 78 "Net-(C504-Pad1)")
  (net 79 "Net-(C604-Pad1)")
  (net 80 /Tubes/sheet5BB3E86D/e)
  (net 81 /Tubes/sheet5BB3E86D/d)
  (net 82 /Tubes/sheet5BB3E86D/g)
  (net 83 /Tubes/sheet5BB3E86D/f)
  (net 84 /Tubes/sheet5BB3E86D/a)
  (net 85 /Tubes/sheet5BB3E86D/c)
  (net 86 /Tubes/sheet5BB3E86D/b)
  (net 87 /Tubes/sheet5BB3E86D/Dot)
  (net 88 /Tubes/sheet5BB3E86C/Dot)
  (net 89 /Tubes/sheet5BB3E86C/b)
  (net 90 /Tubes/sheet5BB3E86C/c)
  (net 91 /Tubes/sheet5BB3E86C/a)
  (net 92 /Tubes/sheet5BB3E86C/f)
  (net 93 /Tubes/sheet5BB3E86C/g)
  (net 94 /Tubes/sheet5BB3E86C/d)
  (net 95 /Tubes/sheet5BB3E86C/e)
  (net 96 /Tubes/sheet5BB3BB93/e)
  (net 97 /Tubes/sheet5BB3BB93/d)
  (net 98 /Tubes/sheet5BB3BB93/g)
  (net 99 /Tubes/sheet5BB3BB93/f)
  (net 100 /Tubes/sheet5BB3BB93/a)
  (net 101 /Tubes/sheet5BB3BB93/c)
  (net 102 /Tubes/sheet5BB3BB93/b)
  (net 103 /Tubes/sheet5BB3BB93/Dot)
  (net 104 /Tubes/sheet5BB36ADE/Dot)
  (net 105 /Tubes/sheet5BB36ADE/b)
  (net 106 /Tubes/sheet5BB36ADE/c)
  (net 107 /Tubes/sheet5BB36ADE/a)
  (net 108 /Tubes/sheet5BB36ADE/f)
  (net 109 /Tubes/sheet5BB36ADE/g)
  (net 110 /Tubes/sheet5BB36ADE/d)
  (net 111 /Tubes/sheet5BB36ADE/e)
  (net 112 /Tubes/sheet5BB32DC8/e)
  (net 113 /Tubes/sheet5BB32DC8/d)
  (net 114 /Tubes/sheet5BB32DC8/g)
  (net 115 /Tubes/sheet5BB32DC8/f)
  (net 116 /Tubes/sheet5BB32DC8/a)
  (net 117 /Tubes/sheet5BB32DC8/c)
  (net 118 /Tubes/sheet5BB32DC8/b)
  (net 119 /Tubes/sheet5BB32DC8/Dot)
  (net 120 /Tubes/IV-9_Tube/Dot)
  (net 121 /Tubes/IV-9_Tube/b)
  (net 122 /Tubes/IV-9_Tube/c)
  (net 123 /Tubes/IV-9_Tube/a)
  (net 124 /Tubes/IV-9_Tube/f)
  (net 125 /Tubes/IV-9_Tube/g)
  (net 126 /Tubes/IV-9_Tube/d)
  (net 127 /Tubes/IV-9_Tube/e)
  (net 128 ~latch)
  (net 129 /Tubes/sheet5BB3E86C/Data_in)
  (net 130 /Tubes/sheet5BB3E86D/Data_in)
  (net 131 /Tubes/sheet5BB36ADE/Data_in)
  (net 132 /Tubes/sheet5BB3BB93/Data_in)
  (net 133 /Tubes/sheet5BB32DC8/Data_in)
  (net 134 /Tubes/IV-9_Tube/Data_in)
  (net 135 "Net-(R902-Pad2)")
  (net 136 "Net-(R902-Pad1)")
  (net 137 /uC/INT0)
  (net 138 "Net-(R914-Pad2)")
  (net 139 ~Reset)
  (net 140 CS_ADC)
  (net 141 "Net-(R916-Pad2)")
  (net 142 "Net-(R915-Pad2)")
  (net 143 /uC/INT1)
  (net 144 "Net-(R901-Pad1)")
  (net 145 "Net-(R901-Pad2)")
  (net 146 "Net-(R913-Pad2)")
  (net 147 "Net-(R912-Pad1)")
  (net 148 "Net-(R912-Pad2)")
  (net 149 "Net-(R911-Pad2)")
  (net 150 "Net-(R911-Pad1)")
  (net 151 "Net-(R910-Pad1)")
  (net 152 "Net-(R910-Pad2)")
  (net 153 "Net-(R909-Pad2)")
  (net 154 "Net-(R909-Pad1)")
  (net 155 "Net-(R908-Pad1)")
  (net 156 "Net-(R908-Pad2)")
  (net 157 "Net-(R907-Pad2)")
  (net 158 "Net-(R907-Pad1)")
  (net 159 clk)
  (net 160 "Net-(R906-Pad2)")
  (net 161 "Net-(R905-Pad2)")
  (net 162 MISO)
  (net 163 MOSI)
  (net 164 "Net-(R904-Pad2)")
  (net 165 "Net-(R903-Pad2)")
  (net 166 "Net-(R903-Pad1)")
  (net 167 "Net-(U1001-Pad8)")
  (net 168 "Net-(U1001-Pad7)")
  (net 169 /Tube_current_monitoring/V_ref:4.096V)
  (net 170 "Net-(U1001-Pad5)")
  (net 171 "Net-(U1001-Pad3)")
  (net 172 "Net-(U1001-Pad1)")
  (net 173 ~CS_ADC)
  (net 174 "Net-(U1002-Pad8)")
  (net 175 "Net-(U1002-Pad7)")
  (net 176 Currentsensing_Tube_6)
  (net 177 Currentsensing_Tube_5)
  (net 178 Currentsensing_Tube_4)
  (net 179 Currentsensing_Tube_3)
  (net 180 Currentsensing_Tube_2)
  (net 181 Currentsensing_Tube_1)
  (net 182 /uC/XTAL2)
  (net 183 /uC/XTAL1)
  (net 184 "Net-(C901-Pad1)")
  (net 185 PSU_2.7V_feedback)
  (net 186 "Net-(R921-Pad2)")
  (net 187 "Net-(R921-Pad1)")
  (net 188 "Net-(R918-Pad1)")
  (net 189 "Net-(R918-Pad2)")
  (net 190 "Net-(R924-Pad2)")
  (net 191 "Net-(R924-Pad1)")
  (net 192 "Net-(R923-Pad1)")
  (net 193 "Net-(R923-Pad2)")
  (net 194 "Net-(R922-Pad2)")
  (net 195 "Net-(R922-Pad1)")
  (net 196 "Net-(R920-Pad1)")
  (net 197 "Net-(R920-Pad2)")
  (net 198 "Net-(R919-Pad2)")
  (net 199 SCL)
  (net 200 SDA)
  (net 201 /RTC/Bat)
  (net 202 "Net-(U1101-Pad4)")
  (net 203 "Net-(U1101-Pad3)")
  (net 204 "Net-(U1101-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V5)
    (add_net /RTC/Bat)
    (add_net /Tube_current_monitoring/V_ref:4.096V)
    (add_net /Tubes/IV-9_Tube/Data_in)
    (add_net /Tubes/IV-9_Tube/Dot)
    (add_net /Tubes/IV-9_Tube/a)
    (add_net /Tubes/IV-9_Tube/b)
    (add_net /Tubes/IV-9_Tube/c)
    (add_net /Tubes/IV-9_Tube/d)
    (add_net /Tubes/IV-9_Tube/e)
    (add_net /Tubes/IV-9_Tube/f)
    (add_net /Tubes/IV-9_Tube/g)
    (add_net /Tubes/sheet5BB32DC8/Data_in)
    (add_net /Tubes/sheet5BB32DC8/Dot)
    (add_net /Tubes/sheet5BB32DC8/a)
    (add_net /Tubes/sheet5BB32DC8/b)
    (add_net /Tubes/sheet5BB32DC8/c)
    (add_net /Tubes/sheet5BB32DC8/d)
    (add_net /Tubes/sheet5BB32DC8/e)
    (add_net /Tubes/sheet5BB32DC8/f)
    (add_net /Tubes/sheet5BB32DC8/g)
    (add_net /Tubes/sheet5BB36ADE/Data_in)
    (add_net /Tubes/sheet5BB36ADE/Dot)
    (add_net /Tubes/sheet5BB36ADE/a)
    (add_net /Tubes/sheet5BB36ADE/b)
    (add_net /Tubes/sheet5BB36ADE/c)
    (add_net /Tubes/sheet5BB36ADE/d)
    (add_net /Tubes/sheet5BB36ADE/e)
    (add_net /Tubes/sheet5BB36ADE/f)
    (add_net /Tubes/sheet5BB36ADE/g)
    (add_net /Tubes/sheet5BB3BB93/Data_in)
    (add_net /Tubes/sheet5BB3BB93/Dot)
    (add_net /Tubes/sheet5BB3BB93/a)
    (add_net /Tubes/sheet5BB3BB93/b)
    (add_net /Tubes/sheet5BB3BB93/c)
    (add_net /Tubes/sheet5BB3BB93/d)
    (add_net /Tubes/sheet5BB3BB93/e)
    (add_net /Tubes/sheet5BB3BB93/f)
    (add_net /Tubes/sheet5BB3BB93/g)
    (add_net /Tubes/sheet5BB3E86C/Data_in)
    (add_net /Tubes/sheet5BB3E86C/Dot)
    (add_net /Tubes/sheet5BB3E86C/a)
    (add_net /Tubes/sheet5BB3E86C/b)
    (add_net /Tubes/sheet5BB3E86C/c)
    (add_net /Tubes/sheet5BB3E86C/d)
    (add_net /Tubes/sheet5BB3E86C/e)
    (add_net /Tubes/sheet5BB3E86C/f)
    (add_net /Tubes/sheet5BB3E86C/g)
    (add_net /Tubes/sheet5BB3E86D/Data_in)
    (add_net /Tubes/sheet5BB3E86D/Dot)
    (add_net /Tubes/sheet5BB3E86D/a)
    (add_net /Tubes/sheet5BB3E86D/b)
    (add_net /Tubes/sheet5BB3E86D/c)
    (add_net /Tubes/sheet5BB3E86D/d)
    (add_net /Tubes/sheet5BB3E86D/e)
    (add_net /Tubes/sheet5BB3E86D/f)
    (add_net /Tubes/sheet5BB3E86D/g)
    (add_net /uC/INT0)
    (add_net /uC/INT1)
    (add_net /uC/XTAL1)
    (add_net /uC/XTAL2)
    (add_net CS_ADC)
    (add_net Clk)
    (add_net Currentsensing_Tube_1)
    (add_net Currentsensing_Tube_2)
    (add_net Currentsensing_Tube_3)
    (add_net Currentsensing_Tube_4)
    (add_net Currentsensing_Tube_5)
    (add_net Currentsensing_Tube_6)
    (add_net Data)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C304-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C404-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C504-Pad1)")
    (add_net "Net-(C602-Pad1)")
    (add_net "Net-(C604-Pad1)")
    (add_net "Net-(C702-Pad1)")
    (add_net "Net-(C704-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C804-Pad1)")
    (add_net "Net-(C901-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad2)")
    (add_net "Net-(R306-Pad2)")
    (add_net "Net-(R307-Pad2)")
    (add_net "Net-(R308-Pad2)")
    (add_net "Net-(R310-Pad1)")
    (add_net "Net-(R311-Pad1)")
    (add_net "Net-(R401-Pad2)")
    (add_net "Net-(R402-Pad2)")
    (add_net "Net-(R403-Pad2)")
    (add_net "Net-(R404-Pad2)")
    (add_net "Net-(R405-Pad2)")
    (add_net "Net-(R406-Pad2)")
    (add_net "Net-(R407-Pad2)")
    (add_net "Net-(R408-Pad2)")
    (add_net "Net-(R410-Pad1)")
    (add_net "Net-(R411-Pad1)")
    (add_net "Net-(R501-Pad2)")
    (add_net "Net-(R502-Pad2)")
    (add_net "Net-(R503-Pad2)")
    (add_net "Net-(R504-Pad2)")
    (add_net "Net-(R505-Pad2)")
    (add_net "Net-(R506-Pad2)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R508-Pad2)")
    (add_net "Net-(R510-Pad1)")
    (add_net "Net-(R511-Pad1)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad2)")
    (add_net "Net-(R605-Pad2)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R607-Pad2)")
    (add_net "Net-(R608-Pad2)")
    (add_net "Net-(R610-Pad1)")
    (add_net "Net-(R611-Pad1)")
    (add_net "Net-(R701-Pad2)")
    (add_net "Net-(R702-Pad2)")
    (add_net "Net-(R703-Pad2)")
    (add_net "Net-(R704-Pad2)")
    (add_net "Net-(R705-Pad2)")
    (add_net "Net-(R706-Pad2)")
    (add_net "Net-(R707-Pad2)")
    (add_net "Net-(R708-Pad2)")
    (add_net "Net-(R710-Pad1)")
    (add_net "Net-(R711-Pad1)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad2)")
    (add_net "Net-(R805-Pad2)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R807-Pad2)")
    (add_net "Net-(R808-Pad2)")
    (add_net "Net-(R810-Pad1)")
    (add_net "Net-(R811-Pad1)")
    (add_net "Net-(R901-Pad1)")
    (add_net "Net-(R901-Pad2)")
    (add_net "Net-(R902-Pad1)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad1)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R904-Pad2)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(R907-Pad1)")
    (add_net "Net-(R907-Pad2)")
    (add_net "Net-(R908-Pad1)")
    (add_net "Net-(R908-Pad2)")
    (add_net "Net-(R909-Pad1)")
    (add_net "Net-(R909-Pad2)")
    (add_net "Net-(R910-Pad1)")
    (add_net "Net-(R910-Pad2)")
    (add_net "Net-(R911-Pad1)")
    (add_net "Net-(R911-Pad2)")
    (add_net "Net-(R912-Pad1)")
    (add_net "Net-(R912-Pad2)")
    (add_net "Net-(R913-Pad2)")
    (add_net "Net-(R914-Pad2)")
    (add_net "Net-(R915-Pad2)")
    (add_net "Net-(R916-Pad2)")
    (add_net "Net-(R918-Pad1)")
    (add_net "Net-(R918-Pad2)")
    (add_net "Net-(R919-Pad2)")
    (add_net "Net-(R920-Pad1)")
    (add_net "Net-(R920-Pad2)")
    (add_net "Net-(R921-Pad1)")
    (add_net "Net-(R921-Pad2)")
    (add_net "Net-(R922-Pad1)")
    (add_net "Net-(R922-Pad2)")
    (add_net "Net-(R923-Pad1)")
    (add_net "Net-(R923-Pad2)")
    (add_net "Net-(R924-Pad1)")
    (add_net "Net-(R924-Pad2)")
    (add_net "Net-(U1001-Pad1)")
    (add_net "Net-(U1001-Pad3)")
    (add_net "Net-(U1001-Pad5)")
    (add_net "Net-(U1001-Pad7)")
    (add_net "Net-(U1001-Pad8)")
    (add_net "Net-(U1002-Pad7)")
    (add_net "Net-(U1002-Pad8)")
    (add_net "Net-(U1101-Pad1)")
    (add_net "Net-(U1101-Pad3)")
    (add_net "Net-(U1101-Pad4)")
    (add_net PSU_2.7V_feedback)
    (add_net Reset)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
    (add_net clk)
    (add_net ~CS_ADC)
    (add_net ~Reset)
    (add_net ~enable_Shiftregister)
    (add_net ~latch)
  )

  (module Battery_Holders:BatteryHolder_CoinCell_Keystone_3000 (layer F.Cu) (tedit 0) (tstamp 5BB5E8BB)
    (at 47.75 43.18)
    (descr "Keystone type 3000 coin cell retainer")
    (path /5BB6494F/5BB6519B)
    (fp_text reference BT1101 (at 0 -8.1) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_text value Battery_Cell (at 0 6.9) (layer F.Fab)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_line (start 0.6096 2.921) (end 1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start 1.8542 3.1496) (end 3.0988 3.6576) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.0988 3.6576) (end 4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.064 4.5212) (end 4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.7244 5.1816) (end 5.2832 5.4356) (layer F.SilkS) (width 0.381))
    (fp_line (start 0 2.8956) (end 0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.064 4.5212) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -5.2832 5.4356) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start -1.8542 3.1496) (end -0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -0.6096 2.921) (end 0 2.8956) (layer F.SilkS) (width 0.381))
    (fp_arc (start 5.2832 4.1148) (end 6.604 4.1148) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_arc (start -5.2832 4.1148) (end -5.2832 5.4356) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_line (start 6.604 -3.429) (end 6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start -6.604 -3.429) (end -6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.0005 -5.969) (end 6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -5.969) (end -6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.9995 -6.731) (end 3.9995 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end -4.0005 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end 4.0005 -6.731) (layer F.SilkS) (width 0.381))
    (pad 1 smd rect (at -7.9 0) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 201 /RTC/Bat))
    (pad 1 smd rect (at 7.9 0) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 201 /RTC/Bat))
    (pad 2 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Battery_Holders.3dshapes/BatteryHolder_CoinCell_Keystone_3000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB5E42D)
    (at 55.245 57.265 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB6494F/5BB64C0D)
    (attr smd)
    (fp_text reference C1101 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB5D616)
    (at 60.325 57.15)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB6494F/5BB64ADA)
    (attr smd)
    (fp_text reference U1101 (at 0 -3.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS3231MZ (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 SCL))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 200 SDA))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 201 /RTC/Bat))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(U1101-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(U1101-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(U1101-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB395DC)
    (at 80.645 44.45 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB48A1C/5BB494B1)
    (attr smd)
    (fp_text reference U1001 (at 0 -3.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ADR292 (at 0 3.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U1001-Pad8)"))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U1001-Pad7)"))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 /Tube_current_monitoring/V_ref:4.096V))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U1001-Pad5)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U1001-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U1001-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532) (tstamp 5BB4D8DD)
    (at 135.89 36.195)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (path /5BB48B05/5BB4F230)
    (attr smd)
    (fp_text reference J901 (at 0 -4.87) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AVR-ISP-6 (at 0 4.87) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.9 -4.35) (end -5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.9 4.35) (end 5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 4.35) (end 5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 -4.35) (end -5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 0.76) (end 2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 0.76) (end -2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -1.78) (end 2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.78) (end -2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 3.3) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.3) (end -2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -3.87) (end 2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.04 -3.3) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.87) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end 2.6 -3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.6 2.86) (end 2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 2.22) (end 3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 2.22) (end 3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.86) (end -2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.22) (end -3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 2.22) (end -3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 0.32) (end 2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -0.32) (end 3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -0.32) (end 3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 0.32) (end -2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -0.32) (end -3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -0.32) (end -3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.22) (end 2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.86) (end 3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -2.86) (end 3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.22) (end -2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.86) (end -3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -3.81) (end 2.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -1.59 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 3.81) (end -2.54 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -1.59 -3.81) (end 2.54 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end -2.54 3.81) (layer F.Fab) (width 0.1))
    (pad 6 smd rect (at 2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 5 smd rect (at -2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 139 ~Reset))
    (pad 4 smd rect (at 2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 163 MOSI))
    (pad 3 smd rect (at -2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 159 clk))
    (pad 2 smd rect (at 2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 162 MISO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB4253B)
    (at 115.05 30.988 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60B72)
    (attr smd)
    (fp_text reference R919 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R919-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 PSU_2.7V_feedback))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB4252A)
    (at 104.521 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63D55)
    (attr smd)
    (fp_text reference R920 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R920-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R920-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB424F9)
    (at 101.854 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DF5)
    (attr smd)
    (fp_text reference R922 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R922-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R922-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB44180)
    (at 103.251 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DFC)
    (attr smd)
    (fp_text reference R923 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R923-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R923-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB424D7)
    (at 104.648 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CA3)
    (attr smd)
    (fp_text reference R924 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R924-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R924-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB424A6)
    (at 115.05 35.179 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60C0B)
    (attr smd)
    (fp_text reference R918 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R918-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R918-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB43A55)
    (at 103.124 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CF7)
    (attr smd)
    (fp_text reference R921 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R921-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R921-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48) (tstamp 5BB44C3A)
    (at 106.68 33.02)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5BB48B05/5BB3F13B)
    (attr smd)
    (fp_text reference U901 (at 0 -6.05) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega328-AU (at 0 6.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.625 -3.4) (end -5.05 -3.4) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 -3.625) (end 3.3 -3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 3.625) (end 3.3 3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 3.625) (end -3.3 3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 -3.625) (end -3.3 -3.625) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 3.625) (end -3.625 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 3.625) (end 3.625 3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.625 -3.625) (end 3.625 -3.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.625 -3.625) (end -3.625 -3.4) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.3 5.3) (end 5.3 5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -5.3) (end 5.3 -5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 -5.3) (end 5.3 5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -5.3) (end -5.3 5.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.15))
    (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R914-Pad2)"))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R921-Pad2)"))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R920-Pad2)"))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R913-Pad2)"))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R912-Pad2)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R911-Pad2)"))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R910-Pad2)"))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R909-Pad2)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R908-Pad2)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R907-Pad2)"))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R919-Pad2)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(C901-Pad1)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R918-Pad2)"))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R906-Pad2)"))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R905-Pad2)"))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(R904-Pad2)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R903-Pad2)"))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R902-Pad2)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R901-Pad2)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R924-Pad2)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R923-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R922-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 182 /uC/XTAL2))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 183 /uC/XTAL1))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R916-Pad2)"))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R915-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BB3A69F)
    (at 67.100001 30.980001)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BB48B05/5BB3C67E)
    (attr smd)
    (fp_text reference SW901 (at 0 -4.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 2.875 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at 2.875 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 139 ~Reset))
    (pad 1 smd rect (at -2.875 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 139 ~Reset))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A385)
    (at 115.177 33.782)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A35B)
    (attr smd)
    (fp_text reference C901 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(C901-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A374)
    (at 99.187 31.6745 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A26C)
    (attr smd)
    (fp_text reference C902 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A363)
    (at 99.187 34.4805 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB39CC9)
    (attr smd)
    (fp_text reference C903 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A352)
    (at 99.187 37.58 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A69F)
    (attr smd)
    (fp_text reference C904 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 183 /uC/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A341)
    (at 99.187 41.414 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A72A)
    (attr smd)
    (fp_text reference C905 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 182 /uC/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A330)
    (at 86.995 44.335 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48A1C/5BB4970E)
    (attr smd)
    (fp_text reference C1001 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A31F)
    (at 85.471 44.335 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48A1C/5BB49846)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A30E)
    (at 86.995 50.915 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48A1C/5BB4AD4E)
    (attr smd)
    (fp_text reference C1003 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 169 /Tube_current_monitoring/V_ref:4.096V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A2FD)
    (at 85.471 50.915 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48A1C/5BB49155)
    (attr smd)
    (fp_text reference C1004 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 169 /Tube_current_monitoring/V_ref:4.096V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A2EC)
    (at 85.471 48.145 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48A1C/5BB48CDB)
    (attr smd)
    (fp_text reference C1005 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystals:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 58CD2E9D) (tstamp 5BB455F6)
    (at 95.504 37.905 270)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (path /5BB48B05/5BB3A603)
    (attr smd)
    (fp_text reference Y901 (at 0 -3.55 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 0 3.55 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.015 0) (end 3.015 -2.115) (angle 180) (layer F.Fab) (width 0.1))
    (fp_arc (start -3.015 0) (end -3.015 -2.115) (angle -180) (layer F.Fab) (width 0.1))
    (fp_line (start 6.8 -2.6) (end -6.8 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.8 2.6) (end 6.8 -2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.8 2.6) (end 6.8 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.8 -2.6) (end -6.8 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 2.55) (end 5.9 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.7 -2.55) (end -6.7 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.9 -2.55) (end -6.7 -2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.015 2.115) (end 3.015 2.115) (layer F.Fab) (width 0.1))
    (fp_line (start -3.015 -2.115) (end 3.015 -2.115) (layer F.Fab) (width 0.1))
    (fp_line (start 5.7 -2.35) (end -5.7 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start 5.7 2.35) (end 5.7 -2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -5.7 2.35) (end 5.7 2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -5.7 -2.35) (end -5.7 2.35) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 182 /uC/XTAL2))
    (pad 1 smd rect (at -4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 183 /uC/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB3982C)
    (at 144.117 11.938)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54DD6)
    (attr smd)
    (fp_text reference D903 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 159 clk))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB39813)
    (at 149.606 25.372 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E24)
    (attr smd)
    (fp_text reference D902 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 163 MOSI))
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB397FA)
    (at 151.892 25.372 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E76)
    (attr smd)
    (fp_text reference D901 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 162 MISO))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB397E1)
    (at 80.645 53.34)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB48A1C/5BB48A66)
    (attr smd)
    (fp_text reference U1002 (at 0 -6) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MCP3208 (at 0 6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -5.05) (end -3.45 -5.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 5.075) (end 2.075 5.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -5.075) (end 2.075 -5.075) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 5.075) (end -2.075 4.97) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 5.075) (end 2.075 4.97) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -5.075) (end 2.075 -4.97) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -5.075) (end -2.075 -5.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.7 5.25) (end 3.7 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -5.25) (end 3.7 -5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -5.25) (end 3.7 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -5.25) (end -3.7 5.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -3.95) (end -0.95 -4.95) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.95) (end -1.95 -3.95) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.95) (end -1.95 4.95) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.95) (end 1.95 4.95) (layer F.Fab) (width 0.15))
    (fp_line (start -0.95 -4.95) (end 1.95 -4.95) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.9 0.9) (thickness 0.135)))
    )
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 /Tube_current_monitoring/V_ref:4.096V))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 clk))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 162 MISO))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 MOSI))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 ~CS_ADC))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U1002-Pad8)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U1002-Pad7)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 176 Currentsensing_Tube_6))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 177 Currentsensing_Tube_5))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 178 Currentsensing_Tube_4))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 Currentsensing_Tube_3))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 180 Currentsensing_Tube_2))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 Currentsensing_Tube_1))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39576)
    (at 108.839 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F7)
    (attr smd)
    (fp_text reference R903 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R903-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(R903-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39565)
    (at 110.236 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F0)
    (attr smd)
    (fp_text reference R904 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 MOSI))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39554)
    (at 111.633 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E9)
    (attr smd)
    (fp_text reference R905 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB44CE7)
    (at 115.05 37.973 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E2)
    (attr smd)
    (fp_text reference R906 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 clk))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R906-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39532)
    (at 115.05 29.591 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D849)
    (attr smd)
    (fp_text reference R907 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R907-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R907-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39521)
    (at 115.05 28.194 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D7AF)
    (attr smd)
    (fp_text reference R908 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R908-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R908-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39510)
    (at 111.506 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D785)
    (attr smd)
    (fp_text reference R909 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R909-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R909-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394FF)
    (at 110.109 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D75D)
    (attr smd)
    (fp_text reference R910 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R910-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R910-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394EE)
    (at 108.712 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D737)
    (attr smd)
    (fp_text reference R911 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R911-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R911-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394DD)
    (at 107.315 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D711)
    (attr smd)
    (fp_text reference R912 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R912-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R912-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394CC)
    (at 105.918 24.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BA78)
    (attr smd)
    (fp_text reference R913 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R913-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 ~Reset))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394BB)
    (at 106.045 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB43320)
    (attr smd)
    (fp_text reference R901 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R901-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R901-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB394AA)
    (at 98.564 28.194)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E7E0)
    (attr smd)
    (fp_text reference R915 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R915-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 /uC/INT1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39499)
    (at 98.564 29.591)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB4E3C2)
    (attr smd)
    (fp_text reference R916 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 CS_ADC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R916-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB4D9D2)
    (at 116.84 24.765 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BE4C)
    (attr smd)
    (fp_text reference R917 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 ~Reset))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39477)
    (at 101.727 24.638 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E361)
    (attr smd)
    (fp_text reference R914 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/INT0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R914-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB39466)
    (at 107.442 41.39 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6FE)
    (attr smd)
    (fp_text reference R902 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R902-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(R902-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24F28)
    (at 174.37 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BB249C1)
    (attr smd)
    (fp_text reference U801 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 /Tubes/sheet5BB3E86C/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R808-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R807-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R806-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R805-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R804-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R803-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R802-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 /Tubes/sheet5BB3E86D/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB43BBE)
    (at 157.310001 129.660001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB26FB6)
    (attr smd)
    (fp_text reference C602 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB437AD)
    (at 154.460001 131.010001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2A8D5)
    (attr smd)
    (fp_text reference R614 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C604-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 178 Currentsensing_Tube_4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB4377C)
    (at 157.310001 128.310001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2A02D)
    (attr smd)
    (fp_text reference R612 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C604-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R611-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB4376B)
    (at 154.460001 129.660001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB24A28)
    (attr smd)
    (fp_text reference R611 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R610-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R611-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB4375A)
    (at 154.460001 128.310001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB24A35)
    (attr smd)
    (fp_text reference R610 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R610-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB44064)
    (at 161.67 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BB249C1)
    (attr smd)
    (fp_text reference U701 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 /Tubes/sheet5BB3E86C/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R701-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R702-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R703-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R704-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R705-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R706-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R707-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R708-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 /Tubes/sheet5BB3BB93/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A496)
    (at 78.465001 92.615001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB26FB6)
    (attr smd)
    (fp_text reference C302 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A486)
    (at 74.915001 92.615001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2E9BF)
    (attr smd)
    (fp_text reference C303 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A476)
    (at 71.365001 92.565001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB29F6A)
    (attr smd)
    (fp_text reference C304 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C304-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB40D60)
    (at 119.9 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2618D)
    (attr smd)
    (fp_text reference C401 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3FCCD)
    (at 118.86 87.63)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB26FB6)
    (attr smd)
    (fp_text reference C402 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3F680)
    (at 118.86 89.535 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2E9BF)
    (attr smd)
    (fp_text reference C403 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A436)
    (at 115.685 93.345 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB29F6A)
    (attr smd)
    (fp_text reference C404 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C404-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB41A2A)
    (at 139.585 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2618D)
    (attr smd)
    (fp_text reference C501 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A416)
    (at 132.940001 113.570001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB26FB6)
    (attr smd)
    (fp_text reference C502 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A406)
    (at 129.390001 113.520001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2E9BF)
    (attr smd)
    (fp_text reference C503 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A3F6)
    (at 136.490001 113.570001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB29F6A)
    (attr smd)
    (fp_text reference C504 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C504-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A3E6)
    (at 149.11 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2618D)
    (attr smd)
    (fp_text reference C601 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A3C6)
    (at 151.615001 97.185001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2E9BF)
    (attr smd)
    (fp_text reference C603 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A3B6)
    (at 155.165001 97.235001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB29F6A)
    (attr smd)
    (fp_text reference C604 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C604-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A3A6)
    (at 168.795 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2618D)
    (attr smd)
    (fp_text reference C701 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A396)
    (at 163.865001 96.795001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB26FB6)
    (attr smd)
    (fp_text reference C702 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A2E6)
    (at 165.565001 110.395001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2E9BF)
    (attr smd)
    (fp_text reference C703 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB3A136)
    (at 169.115001 110.395001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB29F6A)
    (attr smd)
    (fp_text reference C704 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C704-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39F86)
    (at 178.32 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2618D)
    (attr smd)
    (fp_text reference C801 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39E36)
    (at 110.375 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2618D)
    (attr smd)
    (fp_text reference C301 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39DE6)
    (at 185.510001 98.455001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB26FB6)
    (attr smd)
    (fp_text reference C802 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39C36)
    (at 203.870001 84.905001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2E9BF)
    (attr smd)
    (fp_text reference C803 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39A86)
    (at 181.960001 98.455001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB29F6A)
    (attr smd)
    (fp_text reference C804 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C804-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25721)
    (at 134.065001 100.285001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2A02D)
    (attr smd)
    (fp_text reference R512 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R511-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C504-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25710)
    (at 108.585 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249DD)
    (attr smd)
    (fp_text reference R301 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 120 /Tubes/IV-9_Tube/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R301-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256FF)
    (at 107.315 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249D6)
    (attr smd)
    (fp_text reference R302 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R302-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 121 /Tubes/IV-9_Tube/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256EE)
    (at 106.045 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249CF)
    (attr smd)
    (fp_text reference R303 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 122 /Tubes/IV-9_Tube/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R303-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256DD)
    (at 104.775 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249C8)
    (attr smd)
    (fp_text reference R304 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R304-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 123 /Tubes/IV-9_Tube/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256CC)
    (at 103.505 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F9)
    (attr smd)
    (fp_text reference R305 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 124 /Tubes/IV-9_Tube/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R305-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256BB)
    (at 102.235 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F2)
    (attr smd)
    (fp_text reference R306 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R306-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 125 /Tubes/IV-9_Tube/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256AA)
    (at 100.965 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249EB)
    (attr smd)
    (fp_text reference R307 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 126 /Tubes/IV-9_Tube/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R307-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25699)
    (at 99.695 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249E4)
    (attr smd)
    (fp_text reference R308 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R308-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 127 /Tubes/IV-9_Tube/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25688)
    (at 89.375001 84.650001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB24A35)
    (attr smd)
    (fp_text reference R310 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R310-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25677)
    (at 86.115001 88.730001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB24A28)
    (attr smd)
    (fp_text reference R311 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R310-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R311-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25666)
    (at 89.375001 86.000001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2A02D)
    (attr smd)
    (fp_text reference R312 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C304-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R311-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25655)
    (at 84.515001 91.430001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2A864)
    (attr smd)
    (fp_text reference R313 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C304-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25644)
    (at 89.375001 87.350001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2A8D5)
    (attr smd)
    (fp_text reference R314 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 181 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C304-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25633)
    (at 119.38 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249DD)
    (attr smd)
    (fp_text reference R401 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R401-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 119 /Tubes/sheet5BB32DC8/Dot))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25622)
    (at 118.11 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249D6)
    (attr smd)
    (fp_text reference R402 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 118 /Tubes/sheet5BB32DC8/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R402-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25611)
    (at 116.84 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249CF)
    (attr smd)
    (fp_text reference R403 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R403-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 117 /Tubes/sheet5BB32DC8/c))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25600)
    (at 115.57 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249C8)
    (attr smd)
    (fp_text reference R404 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 116 /Tubes/sheet5BB32DC8/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R404-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB255EF)
    (at 197.410001 94.620001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2A8D5)
    (attr smd)
    (fp_text reference R814 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C804-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 176 Currentsensing_Tube_6))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB255DE)
    (at 203.520001 87.840001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2A864)
    (attr smd)
    (fp_text reference R813 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C804-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB255CD)
    (at 203.520001 86.490001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2A02D)
    (attr smd)
    (fp_text reference R812 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R811-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C804-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB255BC)
    (at 195.810001 98.270001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB24A28)
    (attr smd)
    (fp_text reference R811 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R811-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R810-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB255AB)
    (at 197.410001 95.970001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB24A35)
    (attr smd)
    (fp_text reference R810 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R810-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2559A)
    (at 114.3 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F9)
    (attr smd)
    (fp_text reference R405 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 115 /Tubes/sheet5BB32DC8/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R405-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25589)
    (at 168.91 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249E4)
    (attr smd)
    (fp_text reference R808 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R808-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 80 /Tubes/sheet5BB3E86D/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25578)
    (at 170.065 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249EB)
    (attr smd)
    (fp_text reference R807 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 81 /Tubes/sheet5BB3E86D/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R807-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25567)
    (at 171.335 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F2)
    (attr smd)
    (fp_text reference R806 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R806-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 82 /Tubes/sheet5BB3E86D/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25556)
    (at 172.72 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F9)
    (attr smd)
    (fp_text reference R805 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 83 /Tubes/sheet5BB3E86D/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R805-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25545)
    (at 173.99 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249C8)
    (attr smd)
    (fp_text reference R804 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R804-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 84 /Tubes/sheet5BB3E86D/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25534)
    (at 175.26 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249CF)
    (attr smd)
    (fp_text reference R803 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 85 /Tubes/sheet5BB3E86D/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R803-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25523)
    (at 176.53 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249D6)
    (attr smd)
    (fp_text reference R802 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R802-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 /Tubes/sheet5BB3E86D/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25512)
    (at 177.8 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249DD)
    (attr smd)
    (fp_text reference R801 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 /Tubes/sheet5BB3E86D/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R801-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25501)
    (at 161.525001 107.145001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2A8D5)
    (attr smd)
    (fp_text reference R714 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C704-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 177 Currentsensing_Tube_5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254F0)
    (at 164.785001 103.065001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2A864)
    (attr smd)
    (fp_text reference R713 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C704-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254DF)
    (at 167.635001 100.365001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2A02D)
    (attr smd)
    (fp_text reference R712 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R711-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C704-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254CE)
    (at 167.635001 99.015001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB24A28)
    (attr smd)
    (fp_text reference R711 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R711-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R710-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254BD)
    (at 164.785001 101.715001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB24A35)
    (attr smd)
    (fp_text reference R710 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R710-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254AC)
    (at 113.03 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F2)
    (attr smd)
    (fp_text reference R406 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 114 /Tubes/sheet5BB32DC8/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R406-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2549B)
    (at 158.115 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249E4)
    (attr smd)
    (fp_text reference R708 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R708-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 95 /Tubes/sheet5BB3E86C/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2548A)
    (at 159.385 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249EB)
    (attr smd)
    (fp_text reference R707 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 94 /Tubes/sheet5BB3E86C/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R707-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25479)
    (at 160.655 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F2)
    (attr smd)
    (fp_text reference R706 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R706-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 93 /Tubes/sheet5BB3E86C/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25468)
    (at 161.925 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F9)
    (attr smd)
    (fp_text reference R705 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 92 /Tubes/sheet5BB3E86C/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R705-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25457)
    (at 163.195 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249C8)
    (attr smd)
    (fp_text reference R704 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R704-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 91 /Tubes/sheet5BB3E86C/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25446)
    (at 164.465 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249CF)
    (attr smd)
    (fp_text reference R703 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 90 /Tubes/sheet5BB3E86C/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R703-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25435)
    (at 165.735 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249D6)
    (attr smd)
    (fp_text reference R702 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R702-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 89 /Tubes/sheet5BB3E86C/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25424)
    (at 167.005 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249DD)
    (attr smd)
    (fp_text reference R701 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 88 /Tubes/sheet5BB3E86C/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R701-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25402)
    (at 155.240001 103.670001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2A864)
    (attr smd)
    (fp_text reference R613 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C604-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB253BE)
    (at 111.76 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249EB)
    (attr smd)
    (fp_text reference R407 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 113 /Tubes/sheet5BB32DC8/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R407-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB253AD)
    (at 139.7 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249E4)
    (attr smd)
    (fp_text reference R608 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R608-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 /Tubes/sheet5BB3BB93/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2539C)
    (at 140.97 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249EB)
    (attr smd)
    (fp_text reference R607 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 97 /Tubes/sheet5BB3BB93/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R607-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2538B)
    (at 142.24 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F2)
    (attr smd)
    (fp_text reference R606 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R606-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 98 /Tubes/sheet5BB3BB93/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2537A)
    (at 143.51 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F9)
    (attr smd)
    (fp_text reference R605 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 99 /Tubes/sheet5BB3BB93/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R605-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25369)
    (at 144.78 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249C8)
    (attr smd)
    (fp_text reference R604 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 100 /Tubes/sheet5BB3BB93/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25358)
    (at 146.05 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249CF)
    (attr smd)
    (fp_text reference R603 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 101 /Tubes/sheet5BB3BB93/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R603-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25347)
    (at 147.32 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249D6)
    (attr smd)
    (fp_text reference R602 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 102 /Tubes/sheet5BB3BB93/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25336)
    (at 148.59 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249DD)
    (attr smd)
    (fp_text reference R601 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 103 /Tubes/sheet5BB3BB93/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R601-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25325)
    (at 134.065001 101.635001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2A8D5)
    (attr smd)
    (fp_text reference R514 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C504-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 179 Currentsensing_Tube_3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25314)
    (at 141.290001 109.685001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2A864)
    (attr smd)
    (fp_text reference R513 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C504-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25303)
    (at 110.49 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249E4)
    (attr smd)
    (fp_text reference R408 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R408-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 112 /Tubes/sheet5BB32DC8/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252F2)
    (at 134.065001 107.035001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB24A28)
    (attr smd)
    (fp_text reference R511 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R511-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R510-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252E1)
    (at 142.540001 112.385001)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB24A35)
    (attr smd)
    (fp_text reference R510 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R510-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB595FD)
    (at 114.935 87.11 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB24A35)
    (attr smd)
    (fp_text reference R410 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R410-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252BF)
    (at 128.905 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249E4)
    (attr smd)
    (fp_text reference R508 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R508-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 111 /Tubes/sheet5BB36ADE/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252AE)
    (at 130.175 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249EB)
    (attr smd)
    (fp_text reference R507 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/sheet5BB36ADE/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R507-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2529D)
    (at 131.445 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F2)
    (attr smd)
    (fp_text reference R506 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R506-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB36ADE/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2528C)
    (at 132.715 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F9)
    (attr smd)
    (fp_text reference R505 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB36ADE/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R505-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2527B)
    (at 133.985 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249C8)
    (attr smd)
    (fp_text reference R504 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R504-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2526A)
    (at 135.255 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249CF)
    (attr smd)
    (fp_text reference R503 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB36ADE/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R503-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25259)
    (at 136.525 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249D6)
    (attr smd)
    (fp_text reference R502 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R502-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 105 /Tubes/sheet5BB36ADE/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25248)
    (at 137.795 73.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249DD)
    (attr smd)
    (fp_text reference R501 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 104 /Tubes/sheet5BB36ADE/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R501-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25237)
    (at 118.86 91.44 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2A8D5)
    (attr smd)
    (fp_text reference R414 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C404-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 180 Currentsensing_Tube_2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25226)
    (at 118.86 93.345)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2A864)
    (attr smd)
    (fp_text reference R413 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C404-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25215)
    (at 115.685 91.44 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2A02D)
    (attr smd)
    (fp_text reference R412 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R411-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C404-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB23325) (tstamp 5BB25204)
    (at 111.875 93.345 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB24A28)
    (attr smd)
    (fp_text reference R411 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R411-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R410-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB251F3)
    (at 134.415001 98.700001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB36AE9/5BB24A0E)
    (attr smd)
    (fp_text reference R509 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB251E2)
    (at 112.125 86.36)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB32DD3/5BB24A0E)
    (attr smd)
    (fp_text reference R409 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB251C0)
    (at 149.190001 104.855001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB3BB9E/5BB24A0E)
    (attr smd)
    (fp_text reference R609 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB251AF)
    (at 158.465001 110.345001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB3E878/5BB24A0E)
    (attr smd)
    (fp_text reference R709 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB2519E)
    (at 192.610001 98.505001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB3E89F/5BB24A0E)
    (attr smd)
    (fp_text reference R809 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BB250F4)
    (at 89.725001 79.015001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB1F5A4/5BB247DF/5BB24A0E)
    (attr smd)
    (fp_text reference R309 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FF5)
    (at 103.25 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BB249C1)
    (attr smd)
    (fp_text reference U301 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 /Tubes/IV-9_Tube/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R301-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R302-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R303-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R304-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R305-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R306-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R307-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R308-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 Data))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FCC)
    (at 115.825 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BB249C1)
    (attr smd)
    (fp_text reference U401 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 /Tubes/IV-9_Tube/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R408-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R407-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R406-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R405-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R404-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R403-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R402-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R401-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 /Tubes/sheet5BB32DC8/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FA3)
    (at 132.46 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BB249C1)
    (attr smd)
    (fp_text reference U501 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 /Tubes/sheet5BB36ADE/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R501-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R502-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R503-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R504-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R505-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R506-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R507-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R508-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 /Tubes/sheet5BB32DC8/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24F7A)
    (at 145.16 60.96 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BB249C1)
    (attr smd)
    (fp_text reference U601 (at 0 -7.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 /Tubes/sheet5BB36ADE/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R608-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R607-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R606-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R605-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 ~latch))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 Clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 Reset))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R604-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R603-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R602-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 /Tubes/sheet5BB3BB93/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB24EFF)
    (at 79.915001 89.880001)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB247DF/5BB24A15)
    (attr smd)
    (fp_text reference U303 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R310-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R311-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB594C3)
    (at 112.225 90.485)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB32DD3/5BB24A15)
    (attr smd)
    (fp_text reference U403 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R411-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R410-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB24ED5)
    (at 137.940001 110.835001)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB36AE9/5BB24A15)
    (attr smd)
    (fp_text reference U503 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R510-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R511-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB24EC0)
    (at 150.640001 102.120001)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB3BB9E/5BB24A15)
    (attr smd)
    (fp_text reference U603 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R611-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R610-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB24EAB)
    (at 170.565001 107.660001)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB3E878/5BB24A15)
    (attr smd)
    (fp_text reference U703 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R710-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R711-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BB24E96)
    (at 194.060001 95.770001)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (path /5BB1F5A4/5BB3E89F/5BB24A15)
    (attr smd)
    (fp_text reference U803 (at 0 -2.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM321 (at 0 2.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -1.9 1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R811-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R810-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +2V5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E81)
    (at 104.14 83.945 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB247DF/5BB249BA)
    (fp_text reference U302 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 120 /Tubes/IV-9_Tube/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 121 /Tubes/IV-9_Tube/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 122 /Tubes/IV-9_Tube/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 123 /Tubes/IV-9_Tube/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 124 /Tubes/IV-9_Tube/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 125 /Tubes/IV-9_Tube/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 126 /Tubes/IV-9_Tube/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 127 /Tubes/IV-9_Tube/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB29692)
    (at 114.935 83.945 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB32DD3/5BB249BA)
    (fp_text reference U402 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 112 /Tubes/sheet5BB32DC8/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 113 /Tubes/sheet5BB32DC8/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 114 /Tubes/sheet5BB32DC8/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 115 /Tubes/sheet5BB32DC8/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 116 /Tubes/sheet5BB32DC8/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 117 /Tubes/sheet5BB32DC8/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 118 /Tubes/sheet5BB32DC8/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 119 /Tubes/sheet5BB32DC8/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E57)
    (at 133.35 83.945 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB36AE9/5BB249BA)
    (fp_text reference U502 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /Tubes/sheet5BB36ADE/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 /Tubes/sheet5BB36ADE/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 106 /Tubes/sheet5BB36ADE/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 107 /Tubes/sheet5BB36ADE/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 108 /Tubes/sheet5BB36ADE/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 109 /Tubes/sheet5BB36ADE/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 110 /Tubes/sheet5BB36ADE/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 111 /Tubes/sheet5BB36ADE/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB40647)
    (at 144.145 83.945 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3BB9E/5BB249BA)
    (fp_text reference U602 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /Tubes/sheet5BB3BB93/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /Tubes/sheet5BB3BB93/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /Tubes/sheet5BB3BB93/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /Tubes/sheet5BB3BB93/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /Tubes/sheet5BB3BB93/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /Tubes/sheet5BB3BB93/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /Tubes/sheet5BB3BB93/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /Tubes/sheet5BB3BB93/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E2D)
    (at 162.56 83.93267 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E878/5BB249BA)
    (fp_text reference U702 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /Tubes/sheet5BB3E86C/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /Tubes/sheet5BB3E86C/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /Tubes/sheet5BB3E86C/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /Tubes/sheet5BB3E86C/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 /Tubes/sheet5BB3E86C/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /Tubes/sheet5BB3E86C/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /Tubes/sheet5BB3E86C/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /Tubes/sheet5BB3E86C/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E18)
    (at 173.355 83.945 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E89F/5BB249BA)
    (fp_text reference U802 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 /Tubes/sheet5BB3E86D/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 /Tubes/sheet5BB3E86D/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 /Tubes/sheet5BB3E86D/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 /Tubes/sheet5BB3E86D/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 /Tubes/sheet5BB3E86D/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 85 /Tubes/sheet5BB3E86D/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 /Tubes/sheet5BB3E86D/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 87 /Tubes/sheet5BB3E86D/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 114.935 83.945) (end 114.935 86.36) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 114.935 86.36) (end 113.125 86.36) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 115.57 86.36) (end 114.935 86.36) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 116.84 87.63) (end 115.57 86.36) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 118.11 87.63) (end 116.84 87.63) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 118.745 68.175) (end 119.15 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 118.745 65.86) (end 118.745 68.175) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 119.2 65.405) (end 118.745 65.86) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.525 65.405) (end 119.2 65.405) (width 0.35) (layer F.Cu) (net 7))
  (via (at 120.015 70.485) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 119.15 69.62) (end 120.015 70.485) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 119.15 68.58) (end 119.15 69.62) (width 0.35) (layer F.Cu) (net 7))
  (via (at 137.16 68.834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 137.16 68.834) (end 136.02863 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 135.89 65.405) (end 135.255 66.04) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 135.89 65.405) (end 137.16 65.405) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 135.255 66.04) (end 135.255 68.06037) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.02863 68.834) (end 135.255 68.06037) (width 0.35) (layer F.Cu) (net 7))
  (via (at 107.696 68.834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 106.625 65.405) (end 106.045 65.985) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.95 65.405) (end 106.625 65.405) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.045 67.183) (end 107.696 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.045 65.985) (end 106.045 67.183) (width 0.35) (layer F.Cu) (net 7))
  (via (at 166.116 68.834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 166.37 68.58) (end 166.116 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.045 68.58) (end 166.37 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.37 65.405) (end 165.045 65.405) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.116 68.834) (end 165.354 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 164.465 65.985) (end 165.045 65.405) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 164.465 67.945) (end 164.465 65.985) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 165.354 68.834) (end 164.465 67.945) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.015 70.485) (end 120.015 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 120.015 68.834) (end 137.16 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 107.696 68.834) (end 120.015 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 107.95 68.58) (end 107.696 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 109.625 68.58) (end 107.95 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.414 68.58) (end 137.16 68.834) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 138.835 68.58) (end 137.414 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 147.955 65.985) (end 147.955 68.175) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.535 65.405) (end 147.955 65.985) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 147.955 68.175) (end 148.36 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.86 65.405) (end 148.535 65.405) (width 0.35) (layer F.Cu) (net 7))
  (via (at 149.225 70.485) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 148.36 69.62) (end 149.225 70.485) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.36 68.58) (end 148.36 69.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.225 70.485) (end 149.225 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 149.225 68.834) (end 166.116 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 137.16 68.834) (end 149.225 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 177.165 65.985) (end 177.165 68.175) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 177.745 65.405) (end 177.165 65.985) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 177.165 68.175) (end 177.57 68.58) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 179.07 65.405) (end 177.745 65.405) (width 0.35) (layer F.Cu) (net 7))
  (via (at 178.435 70.485) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 177.57 69.62) (end 178.435 70.485) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 177.57 68.58) (end 177.57 69.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 176.784 68.834) (end 178.435 70.485) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 166.116 68.834) (end 176.784 68.834) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 102.43 34.22) (end 105.975 34.22) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.775 35.02) (end 110.93 35.02) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.045 34.29) (end 106.775 35.02) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 105.975 34.22) (end 106.045 34.29) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 105.975 34.22) (end 105.975 32.95) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 105.645 32.62) (end 103.505 32.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 105.975 32.95) (end 105.645 32.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 102.43 32.62) (end 103.505 32.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.33 32.62) (end 102.43 32.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.095 32.385) (end 100.33 32.62) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.187 32.385) (end 100.095 32.385) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 101.035 34.22) (end 102.43 34.22) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.187 35.2305) (end 100.0245 35.2305) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.0245 35.2305) (end 100.965 34.29) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.965 34.29) (end 101.035 34.22) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.08 35.02) (end 110.93 35.02) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 113.411 36.351) (end 112.08 35.02) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 81.915 48.895) (end 81.28 48.26) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 83.345 48.895) (end 81.915 48.895) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 83.345 45.085) (end 85.471 45.085) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 85.471 45.085) (end 86.995 45.085) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 81.28 46.355) (end 81.28 45.72) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 81.28 48.26) (end 81.28 46.355) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 81.915 45.085) (end 83.345 45.085) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 81.28 45.72) (end 81.915 45.085) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 83.345 48.895) (end 85.471 48.895) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 114.935 89.535) (end 113.325 89.535) (width 0.35) (layer F.Cu) (net 7))
  (via (at 115.57 89.535) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 118.11 89.535) (end 115.57 89.535) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 115.57 89.535) (end 114.935 89.535) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 55.245 56.515) (end 57.625 56.515) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 111.125 65.405) (end 111.125 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 107.95 66.675) (end 111.125 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 68.58) (end 111.125 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 120.65 66.8) (end 120.525 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 120.65 68.58) (end 120.65 66.8) (width 0.35) (layer F.Cu) (net 10))
  (via (at 138.684 70.358) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 10))
  (segment (start 140.335 68.326) (end 140.335 68.707) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 137.16 66.675) (end 140.335 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 68.326) (end 140.335 67.31) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 67.31) (end 140.335 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 66.675) (end 140.335 66.04) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 66.04) (end 140.335 65.405) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 68.326) (end 111.125 66.675) (width 0.35) (layer F.Cu) (net 10))
  (via (at 109.728 70.358) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 10))
  (segment (start 111.125 68.326) (end 111.125 68.961) (width 0.35) (layer F.Cu) (net 10))
  (via (at 168.148 70.358) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 10))
  (segment (start 169.545 68.961) (end 168.148 70.358) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 169.545 68.58) (end 169.545 68.961) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 166.37 66.675) (end 169.545 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 169.545 68.58) (end 169.545 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 169.545 66.675) (end 169.545 65.405) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 156.97 66.675) (end 156.97 65.405) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 149.735 66.675) (end 156.97 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 137.16 55.245) (end 140.335 55.245) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 55.245) (end 107.95 55.245) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 166.37 55.245) (end 169.545 55.245) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 149.735 55.245) (end 156.97 55.245) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 120.525 55.245) (end 127.76 55.245) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 127.76 65.405) (end 127.76 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 68.961) (end 109.728 70.358) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 68.58) (end 111.125 68.961) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 68.707) (end 138.684 70.358) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 140.335 68.58) (end 140.335 68.707) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 149.86 68.58) (end 149.86 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 179.07 68.58) (end 179.07 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 120.525 66.675) (end 127.76 66.675) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 85.471 51.665) (end 86.995 51.665) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 84.685 51.665) (end 84.455 51.435) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 85.471 51.665) (end 84.685 51.665) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 83.345 51.435) (end 84.455 51.435) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 84.431 42.545) (end 85.471 43.585) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 83.345 42.545) (end 84.431 42.545) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 85.471 43.585) (end 86.995 43.585) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 119.61 89.535) (end 119.61 87.63) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 111.125 86.36) (end 111.125 89.535) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 113.325 92.645) (end 112.625 93.345) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 113.325 91.435) (end 113.325 92.645) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 114.295 91.435) (end 114.3 91.44) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 114.3 91.44) (end 114.935 91.44) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 113.325 91.435) (end 114.295 91.435) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 111.125 93.345) (end 111.125 91.435) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 112.8 87.86) (end 114.3 87.86) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 112.268 90.932) (end 112.268 88.392) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 112.268 88.392) (end 112.8 87.86) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 111.765 91.435) (end 112.268 90.932) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 111.125 91.435) (end 111.765 91.435) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 114.3 87.86) (end 114.935 87.86) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 172.085 63.5) (end 172.085 68.465) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 168.91 71.64) (end 168.91 72.39) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 171.45 62.865) (end 172.085 63.5) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 172.085 68.465) (end 168.91 71.64) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 169.545 62.865) (end 171.45 62.865) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 170.065 71.64) (end 170.065 72.39) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 172.72 68.985) (end 170.065 71.64) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 172.72 62.23) (end 172.72 68.985) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 172.085 61.595) (end 172.72 62.23) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 169.545 61.595) (end 172.085 61.595) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 171.335 71.755) (end 171.335 72.39) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 173.355 69.735) (end 171.335 71.755) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 173.355 60.96) (end 173.355 69.735) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 172.72 60.325) (end 173.355 60.96) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 169.545 60.325) (end 172.72 60.325) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 172.72 71.64) (end 172.72 72.39) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 173.99 70.37) (end 172.72 71.64) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 173.99 59.69) (end 173.99 70.37) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 173.355 59.055) (end 173.99 59.69) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 169.545 59.055) (end 173.355 59.055) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 148.41 56.515) (end 147.955 56.06) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 149.735 56.515) (end 148.41 56.515) (width 0.35) (layer F.Cu) (net 26))
  (via (at 147.955 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 147.955 56.06) (end 147.955 49.53) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 135.835 56.515) (end 135.255 55.935) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 137.16 56.515) (end 135.835 56.515) (width 0.35) (layer F.Cu) (net 26))
  (via (at 135.255 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 135.255 55.935) (end 135.255 49.53) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 135.255 49.53) (end 147.955 49.53) (width 0.35) (layer B.Cu) (net 26))
  (segment (start 119.2 56.515) (end 118.745 56.06) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 120.525 56.515) (end 119.2 56.515) (width 0.35) (layer F.Cu) (net 26))
  (via (at 118.745 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 118.745 56.06) (end 118.745 49.53) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 118.745 49.53) (end 135.255 49.53) (width 0.35) (layer B.Cu) (net 26))
  (segment (start 106.625 56.515) (end 106.045 55.935) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 107.95 56.515) (end 106.625 56.515) (width 0.35) (layer F.Cu) (net 26))
  (via (at 106.045 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 106.045 55.935) (end 106.045 49.53) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 106.045 49.53) (end 118.745 49.53) (width 0.35) (layer B.Cu) (net 26))
  (via (at 164.465 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 147.955 49.53) (end 164.465 49.53) (width 0.35) (layer B.Cu) (net 26))
  (segment (start 165.045 56.515) (end 166.37 56.515) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 164.465 55.935) (end 165.045 56.515) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 164.465 49.53) (end 164.465 55.935) (width 0.35) (layer F.Cu) (net 26))
  (via (at 177.165 49.53) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 26))
  (segment (start 164.465 49.53) (end 177.165 49.53) (width 0.35) (layer B.Cu) (net 26))
  (segment (start 177.165 56.06) (end 177.62 56.515) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 177.62 56.515) (end 178.945 56.515) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 177.165 49.53) (end 177.165 56.06) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 149.735 57.785) (end 146.685 57.785) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 146.05 57.15) (end 146.05 50.8) (width 0.35) (layer F.Cu) (net 27))
  (via (at 146.05 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 146.685 57.785) (end 146.05 57.15) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 137.16 57.785) (end 133.985 57.785) (width 0.35) (layer F.Cu) (net 27))
  (via (at 133.35 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 133.35 57.15) (end 133.35 50.8) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 133.985 57.785) (end 133.35 57.15) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 146.05 50.8) (end 133.35 50.8) (width 0.35) (layer B.Cu) (net 27))
  (segment (start 120.525 57.785) (end 117.475 57.785) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 117.475 57.785) (end 116.84 57.15) (width 0.35) (layer F.Cu) (net 27))
  (via (at 116.84 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 116.84 57.15) (end 116.84 50.8) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 116.84 50.8) (end 133.35 50.8) (width 0.35) (layer B.Cu) (net 27))
  (segment (start 107.95 57.785) (end 104.775 57.785) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 104.14 57.15) (end 104.14 50.8) (width 0.35) (layer F.Cu) (net 27))
  (via (at 104.14 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 104.775 57.785) (end 104.14 57.15) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 104.14 50.8) (end 116.84 50.8) (width 0.35) (layer B.Cu) (net 27))
  (segment (start 166.37 57.785) (end 163.195 57.785) (width 0.35) (layer F.Cu) (net 27))
  (via (at 162.56 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 162.56 57.15) (end 162.56 50.8) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 163.195 57.785) (end 162.56 57.15) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 162.56 50.8) (end 146.05 50.8) (width 0.35) (layer B.Cu) (net 27))
  (via (at 175.26 50.8) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 27))
  (segment (start 175.26 50.8) (end 162.56 50.8) (width 0.35) (layer B.Cu) (net 27))
  (segment (start 175.895 57.785) (end 175.26 57.15) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 175.26 57.15) (end 175.26 50.8) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 178.945 57.785) (end 175.895 57.785) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 140.335 57.785) (end 142.24 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 142.24 57.785) (end 142.875 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 142.875 57.785) (end 143.51 57.785) (width 0.35) (layer F.Cu) (net 28))
  (via (at 144.145 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 144.145 57.15) (end 144.145 52.07) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.51 57.785) (end 144.145 57.15) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 127.76 57.785) (end 130.175 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 130.175 57.785) (end 130.81 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 130.81 57.785) (end 131.445 57.15) (width 0.35) (layer F.Cu) (net 28))
  (via (at 131.445 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 131.445 57.15) (end 131.445 52.07) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 131.445 52.07) (end 144.145 52.07) (width 0.35) (layer B.Cu) (net 28))
  (segment (start 111.125 57.785) (end 112.45 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 111.125 57.785) (end 114.3 57.785) (width 0.35) (layer F.Cu) (net 28))
  (via (at 114.935 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 114.935 57.15) (end 114.935 52.07) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 114.3 57.785) (end 114.935 57.15) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 114.935 52.07) (end 131.445 52.07) (width 0.35) (layer B.Cu) (net 28))
  (segment (start 98.55 57.785) (end 100.965 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 100.965 57.785) (end 101.6 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 101.6 57.785) (end 102.235 57.15) (width 0.35) (layer F.Cu) (net 28))
  (via (at 102.235 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 102.235 57.15) (end 102.235 52.07) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 102.235 52.07) (end 114.935 52.07) (width 0.35) (layer B.Cu) (net 28))
  (via (at 160.655 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 144.145 52.07) (end 160.655 52.07) (width 0.35) (layer B.Cu) (net 28))
  (segment (start 160.655 52.07) (end 160.655 57.15) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 160.02 57.785) (end 156.97 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 160.655 57.15) (end 160.02 57.785) (width 0.35) (layer F.Cu) (net 28))
  (via (at 173.355 52.07) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 28))
  (segment (start 160.655 52.07) (end 173.355 52.07) (width 0.35) (layer B.Cu) (net 28))
  (segment (start 173.355 52.07) (end 173.355 57.15) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 172.72 57.785) (end 169.545 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 173.355 57.15) (end 172.72 57.785) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 173.99 71.64) (end 174.625 71.005) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 173.99 72.39) (end 173.99 71.64) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 174.625 59.69) (end 175.26 59.055) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 174.625 71.005) (end 174.625 59.69) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 175.26 59.055) (end 179.07 59.055) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 175.895 60.325) (end 178.945 60.325) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 175.26 60.96) (end 175.895 60.325) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 175.26 72.39) (end 175.26 60.96) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 176.53 72.39) (end 176.53 71.64) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 175.895 71.005) (end 175.895 62.23) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 175.895 62.23) (end 176.53 61.595) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 176.53 71.64) (end 175.895 71.005) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 176.53 61.595) (end 178.945 61.595) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 177.8 71.64) (end 177.8 72.39) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 176.53 63.5) (end 177.165 62.865) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 176.53 70.37) (end 176.53 63.5) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 178.945 62.865) (end 177.165 62.865) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 176.53 70.37) (end 177.8 71.64) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 163.195 63.5) (end 163.83 62.865) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 163.83 62.865) (end 166.37 62.865) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 167.005 72.39) (end 167.005 71.64) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 167.005 71.64) (end 163.195 67.83) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 163.195 67.83) (end 163.195 63.5) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 162.56 68.465) (end 165.735 71.64) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 163.195 61.595) (end 162.56 62.23) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 165.735 71.64) (end 165.735 72.39) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 162.56 62.23) (end 162.56 68.465) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 166.37 61.595) (end 163.195 61.595) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 164.465 71.64) (end 161.925 69.1) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 164.465 72.39) (end 164.465 71.64) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 161.925 69.1) (end 161.925 60.96) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 162.56 60.325) (end 166.37 60.325) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 161.925 60.96) (end 162.56 60.325) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 163.195 71.755) (end 163.195 72.39) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 161.29 69.85) (end 163.195 71.755) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 161.29 59.69) (end 161.29 69.85) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 161.925 59.055) (end 161.29 59.69) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 166.37 59.055) (end 161.925 59.055) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 160.02 59.055) (end 156.97 59.055) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 160.655 59.69) (end 160.02 59.055) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 160.655 70.37) (end 160.655 59.69) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 161.925 71.64) (end 160.655 70.37) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 161.925 72.39) (end 161.925 71.64) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 160.655 71.64) (end 160.655 72.39) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 160.054989 71.039989) (end 160.655 71.64) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 160.054989 60.994989) (end 160.054989 71.039989) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 159.385 60.325) (end 160.054989 60.994989) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 156.97 60.325) (end 159.385 60.325) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 159.385 72.39) (end 159.385 62.23) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 158.75 61.595) (end 156.97 61.595) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 159.385 62.23) (end 158.75 61.595) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 158.115 71.64) (end 158.115 72.39) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 158.635 71.12) (end 158.115 71.64) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 158.295 62.865) (end 158.635 63.205) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 158.635 63.205) (end 158.635 71.12) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 156.97 62.865) (end 158.295 62.865) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 139.7 71.64) (end 142.875 68.465) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 139.7 72.39) (end 139.7 71.64) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 142.875 68.465) (end 142.875 63.5) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 142.24 62.865) (end 140.335 62.865) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 142.875 63.5) (end 142.24 62.865) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 140.335 61.595) (end 142.875 61.595) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 142.875 61.595) (end 143.51 62.23) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 140.97 71.64) (end 140.97 72.39) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 143.51 69.1) (end 140.97 71.64) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 143.51 62.23) (end 143.51 69.1) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 140.335 60.325) (end 141.66 60.325) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 142.24 71.64) (end 144.145 69.735) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 142.24 72.39) (end 142.24 71.64) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 144.145 69.735) (end 144.145 60.96) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 143.51 60.325) (end 140.335 60.325) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 144.145 60.96) (end 143.51 60.325) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 143.51 71.64) (end 143.51 72.39) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 144.78 70.37) (end 143.51 71.64) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 144.78 59.69) (end 144.78 70.37) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 144.145 59.055) (end 144.78 59.69) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 140.335 59.055) (end 144.145 59.055) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 144.78 71.64) (end 145.415 71.005) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 144.78 72.39) (end 144.78 71.64) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 145.415 71.005) (end 145.415 59.69) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 146.05 59.055) (end 149.735 59.055) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 145.415 59.69) (end 146.05 59.055) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 146.05 72.39) (end 146.05 60.96) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 146.685 60.325) (end 149.735 60.325) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 146.05 60.96) (end 146.685 60.325) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 147.32 71.64) (end 146.685 71.005) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 147.32 72.39) (end 147.32 71.64) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 146.685 71.005) (end 146.685 62.23) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 147.32 61.595) (end 149.735 61.595) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 146.685 62.23) (end 147.32 61.595) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 148.59 71.64) (end 147.32 70.37) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 148.59 72.39) (end 148.59 71.64) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 147.32 70.37) (end 147.32 63.5) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 147.955 62.865) (end 149.735 62.865) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 147.32 63.5) (end 147.955 62.865) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 137.795 71.64) (end 133.985 67.83) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 137.795 72.39) (end 137.795 71.64) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 133.985 67.83) (end 133.985 63.5) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 134.62 62.865) (end 137.16 62.865) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 133.985 63.5) (end 134.62 62.865) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 136.525 71.64) (end 133.35 68.465) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 136.525 72.39) (end 136.525 71.64) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 133.35 68.465) (end 133.35 62.23) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 133.985 61.595) (end 137.16 61.595) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 133.35 62.23) (end 133.985 61.595) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 133.35 60.325) (end 137.16 60.325) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 132.715 60.96) (end 133.35 60.325) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 132.715 69.1) (end 132.715 60.96) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 135.255 71.64) (end 132.715 69.1) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 135.255 72.39) (end 135.255 71.64) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 133.985 71.64) (end 132.08 69.735) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 133.985 72.39) (end 133.985 71.64) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 132.08 69.735) (end 132.08 59.69) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 132.715 59.055) (end 137.16 59.055) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 132.08 59.69) (end 132.715 59.055) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 132.715 71.64) (end 131.445 70.37) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 132.715 72.39) (end 132.715 71.64) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 131.445 70.37) (end 131.445 59.69) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 130.81 59.055) (end 127.76 59.055) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 131.445 59.69) (end 130.81 59.055) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 131.445 71.64) (end 131.445 72.39) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 130.81 71.005) (end 131.445 71.64) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 130.81 60.96) (end 130.81 71.005) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 130.175 60.325) (end 130.81 60.96) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 127.76 60.325) (end 130.175 60.325) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 130.175 62.23) (end 129.54 61.595) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 129.54 61.595) (end 127.76 61.595) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 130.175 72.39) (end 130.175 62.23) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 128.905 71.64) (end 129.524989 71.020011) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 128.905 72.39) (end 128.905 71.64) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 129.524989 71.020011) (end 129.524989 63.304989) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 129.524989 63.304989) (end 129.085 62.865) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 129.085 62.865) (end 127.76 62.865) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 110.49 71.64) (end 110.49 72.39) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 113.665 63.5) (end 113.665 68.465) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 113.665 68.465) (end 110.49 71.64) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 113.03 62.865) (end 113.665 63.5) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 111.125 62.865) (end 113.03 62.865) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 114.3 69.1) (end 111.76 71.64) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 113.665 61.595) (end 114.3 62.23) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 111.76 71.64) (end 111.76 72.39) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 114.3 62.23) (end 114.3 69.1) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 111.125 61.595) (end 113.665 61.595) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 113.03 71.64) (end 113.03 72.39) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 114.935 60.96) (end 114.935 69.735) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 114.3 60.325) (end 114.935 60.96) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 114.935 69.735) (end 113.03 71.64) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 111.125 60.325) (end 114.3 60.325) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 114.3 71.64) (end 114.3 72.39) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 115.57 59.69) (end 115.57 70.37) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 114.935 59.055) (end 115.57 59.69) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 115.57 70.37) (end 114.3 71.64) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 111.125 59.055) (end 114.935 59.055) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 115.57 71.64) (end 116.205 71.005) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 115.57 72.39) (end 115.57 71.64) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 116.205 59.69) (end 116.84 59.055) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 116.205 71.005) (end 116.205 59.69) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 116.84 59.055) (end 120.525 59.055) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 116.84 60.96) (end 117.475 60.325) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 116.84 72.39) (end 116.84 60.96) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 117.475 60.325) (end 120.525 60.325) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 118.11 71.755) (end 118.11 72.39) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 117.475 62.23) (end 118.11 61.595) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 117.475 71.12) (end 117.475 62.23) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 120.525 61.595) (end 118.11 61.595) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 117.475 71.12) (end 118.11 71.755) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 119.38 72.39) (end 119.38 71.64) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 120.525 62.865) (end 119.38 62.865) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 118.11 63.5) (end 118.745 62.865) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 118.11 70.37) (end 118.11 63.5) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 118.745 62.865) (end 119.38 62.865) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 119.38 71.64) (end 118.11 70.37) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 104.775 63.5) (end 105.41 62.865) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 105.41 62.865) (end 107.95 62.865) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 108.585 71.64) (end 104.775 67.83) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 104.775 67.83) (end 104.775 63.5) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 108.585 72.39) (end 108.585 71.64) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 106.045 61.595) (end 107.95 61.595) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 104.14 62.23) (end 104.775 61.595) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 104.775 61.595) (end 106.045 61.595) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 104.14 68.465) (end 104.14 62.23) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 107.315 71.64) (end 104.14 68.465) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 107.315 72.39) (end 107.315 71.64) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 104.14 60.325) (end 107.95 60.325) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 106.045 71.64) (end 103.505 69.1) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 103.505 60.96) (end 104.14 60.325) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 103.505 69.1) (end 103.505 60.96) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 106.045 72.39) (end 106.045 71.64) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 106.68 59.055) (end 107.95 59.055) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 103.505 59.055) (end 106.68 59.055) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 102.87 59.69) (end 103.505 59.055) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 102.87 69.735) (end 102.87 59.69) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 104.775 71.64) (end 102.87 69.735) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 104.775 72.39) (end 104.775 71.64) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 103.505 72.39) (end 103.505 71.64) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 102.235 70.37) (end 102.235 59.69) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 100.33 59.055) (end 98.55 59.055) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 102.235 59.69) (end 101.6 59.055) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 103.505 71.64) (end 102.235 70.37) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 101.6 59.055) (end 100.33 59.055) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 102.235 72.39) (end 102.235 71.64) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 101.6 71.005) (end 101.6 60.96) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 100.965 60.325) (end 99.695 60.325) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 102.235 71.64) (end 101.6 71.005) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 99.695 60.325) (end 98.55 60.325) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 101.6 60.96) (end 100.965 60.325) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 100.33 61.595) (end 98.55 61.595) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 100.965 62.23) (end 100.33 61.595) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 100.965 72.39) (end 100.965 62.23) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 99.695 62.865) (end 98.55 62.865) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 100.33 63.5) (end 99.695 62.865) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 100.33 71.005) (end 100.33 63.5) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 99.695 71.64) (end 100.33 71.005) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 99.695 72.39) (end 99.695 71.64) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 116.84 93.345) (end 116.435 93.345) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 118.11 93.345) (end 116.84 93.345) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 116.435 93.345) (end 116.435 91.44) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 118.11 91.44) (end 116.435 91.44) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 170.577915 81.92733) (end 169.55733 81.92733) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 168.91 81.28) (end 168.91 80.01) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 169.55733 81.92733) (end 168.91 81.28) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 168.91 80.01) (end 168.91 73.89) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 170.065 79.609755) (end 170.577915 80.12267) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 170.065 73.89) (end 170.065 79.609755) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 171.335 78.359003) (end 171.638667 78.66267) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 171.335 73.89) (end 171.335 78.359003) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 172.72 73.89) (end 172.72 75.565) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 173.355 76.2) (end 173.355 78.105) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 172.72 75.565) (end 173.355 76.2) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 173.99 73.89) (end 173.99 74.93) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 175.071333 76.011333) (end 175.071333 78.66267) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 173.99 74.93) (end 175.071333 76.011333) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 176.775828 79.478927) (end 176.132085 80.12267) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 176.775828 76.155828) (end 176.775828 79.478927) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 175.26 74.64) (end 176.775828 76.155828) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 175.26 73.89) (end 175.26 74.64) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 177.8 75.91) (end 176.53 74.64) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 177.8 81.28) (end 177.8 75.91) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 177.15267 81.92733) (end 177.8 81.28) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 176.53 74.64) (end 176.53 73.89) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 176.132085 81.92733) (end 177.15267 81.92733) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 177.8 74.64) (end 177.8 73.89) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 178.435 75.275) (end 177.8 74.64) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 176.96267 83.38733) (end 178.435 81.915) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 178.435 81.915) (end 178.435 75.275) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 175.071333 83.38733) (end 176.96267 83.38733) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 166.37 83.375) (end 164.276333 83.375) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 167.73 82.015) (end 166.37 83.375) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 167.73 75.365) (end 167.73 82.015) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 167.005 74.64) (end 167.73 75.365) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 167.005 73.89) (end 167.005 74.64) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 165.735 74.64) (end 165.735 73.89) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 167.005 75.91) (end 165.735 74.64) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 167.005 81.28) (end 167.005 75.91) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 166.37 81.915) (end 167.005 81.28) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 165.337085 81.915) (end 166.37 81.915) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 164.465 73.89) (end 164.465 74.93) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 165.980828 79.466597) (end 165.337085 80.11034) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 165.980828 76.445828) (end 165.980828 79.466597) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 164.465 74.93) (end 165.980828 76.445828) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 163.195 73.89) (end 163.195 75.565) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 164.276333 76.646333) (end 164.276333 78.65034) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 163.195 75.565) (end 164.276333 76.646333) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 161.925 74.64) (end 161.925 73.89) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 161.925 76.25767) (end 161.925 74.64) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 162.56 76.89267) (end 161.925 76.25767) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 162.56 78.09267) (end 162.56 76.89267) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 160.655 78.461673) (end 160.843667 78.65034) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 160.655 73.89) (end 160.655 78.461673) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 159.385 74.64) (end 159.385 73.89) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 159.385 78.981548) (end 159.385 74.64) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 159.782915 79.379463) (end 159.385 78.981548) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 159.782915 80.11034) (end 159.782915 79.379463) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 158.115 80.247085) (end 158.115 74.295) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 159.782915 81.915) (end 158.115 80.247085) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 158.115 74.295) (end 158.115 73.89) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 139.7 80.259415) (end 139.7 73.89) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 141.367915 81.92733) (end 139.7 80.259415) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 140.97 74.64) (end 140.97 73.89) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 140.97 78.993878) (end 140.97 74.64) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 141.367915 79.391793) (end 140.97 78.993878) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 141.367915 80.12267) (end 141.367915 79.391793) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 142.24 78.474003) (end 142.428667 78.66267) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 142.24 73.89) (end 142.24 78.474003) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 144.145 76.905) (end 143.51 76.27) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 144.145 78.105) (end 144.145 76.905) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 143.51 76.27) (end 143.51 73.89) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 144.78 74.93) (end 144.78 73.89) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 145.861333 76.011333) (end 144.78 74.93) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 145.861333 78.66267) (end 145.861333 76.011333) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 146.05 74.93) (end 146.05 73.89) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 147.32 76.2) (end 146.05 74.93) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 147.32 78.993878) (end 147.32 76.2) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 146.922085 79.391793) (end 147.32 78.993878) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 146.922085 80.12267) (end 146.922085 79.391793) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 147.94267 81.92733) (end 146.922085 81.92733) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 148.59 81.28) (end 147.94267 81.92733) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 148.59 76.2) (end 148.59 81.28) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 147.32 74.93) (end 148.59 76.2) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 147.32 73.89) (end 147.32 74.93) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 148.59 74.93) (end 149.225 75.565) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 147.75267 83.38733) (end 145.861333 83.38733) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 149.225 81.915) (end 147.75267 83.38733) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 149.225 75.565) (end 149.225 81.915) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 148.59 73.89) (end 148.59 74.93) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 135.875882 83.38733) (end 135.066333 83.38733) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 137.16 83.38733) (end 135.875882 83.38733) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 138.52 82.02733) (end 137.16 83.38733) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 138.52 75.565) (end 138.52 82.02733) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 137.795 74.84) (end 138.52 75.565) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 137.795 73.89) (end 137.795 74.84) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 137.14767 81.92733) (end 136.127085 81.92733) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 137.795 76.2) (end 137.795 81.28) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 137.795 81.28) (end 137.14767 81.92733) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 136.525 74.93) (end 137.795 76.2) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 136.525 73.89) (end 136.525 74.93) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 136.525 76.2) (end 136.525 79.375) (width 0.35) (layer F.Cu) (net 106))
  (segment (start 135.255 74.93) (end 136.525 76.2) (width 0.35) (layer F.Cu) (net 106))
  (segment (start 135.255 73.89) (end 135.255 74.93) (width 0.35) (layer F.Cu) (net 106))
  (segment (start 133.985 75.118667) (end 135.066333 76.2) (width 0.35) (layer F.Cu) (net 107))
  (segment (start 133.985 73.89) (end 133.985 75.118667) (width 0.35) (layer F.Cu) (net 107))
  (segment (start 135.066333 78.66267) (end 135.066333 76.2) (width 0.35) (layer F.Cu) (net 107))
  (segment (start 132.715 73.89) (end 132.715 75.565) (width 0.35) (layer F.Cu) (net 108))
  (segment (start 133.35 76.2) (end 133.35 78.105) (width 0.35) (layer F.Cu) (net 108))
  (segment (start 132.715 75.565) (end 133.35 76.2) (width 0.35) (layer F.Cu) (net 108))
  (segment (start 131.445 78.474003) (end 131.633667 78.66267) (width 0.35) (layer F.Cu) (net 109))
  (segment (start 131.445 73.89) (end 131.445 78.474003) (width 0.35) (layer F.Cu) (net 109))
  (segment (start 130.175 79.724755) (end 130.572915 80.12267) (width 0.35) (layer F.Cu) (net 110))
  (segment (start 130.175 73.89) (end 130.175 79.724755) (width 0.35) (layer F.Cu) (net 110))
  (segment (start 128.905 73.89) (end 128.905 81.28) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 129.55233 81.92733) (end 128.905 81.28) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 130.572915 81.92733) (end 129.55233 81.92733) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 110.88333 81.92733) (end 112.157915 81.92733) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BB2973C))
  (segment (start 110.49 81.534) (end 110.88333 81.92733) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BB29739))
  (segment (start 110.49 81.534) (end 110.49 80.01) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 110.49 80.01) (end 110.49 80.264) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 110.49 73.89) (end 110.49 80.01) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 111.76 78.993878) (end 111.76 78.105) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BB29757))
  (segment (start 111.76 78.993878) (end 112.157915 79.391793) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 111.76 76.2) (end 111.76 78.993878) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 112.157915 79.391793) (end 112.157915 80.12267) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 111.76 73.89) (end 111.76 76.2) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 111.76 76.2) (end 111.76 76.835) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 113.03 76.2) (end 113.03 77.204003) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.03 73.89) (end 113.03 75.565) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.03 75.565) (end 113.03 76.2) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.03 78.474003) (end 113.218667 78.66267) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.03 73.89) (end 113.03 78.474003) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 114.3 75.565) (end 114.935 76.2) (width 0.35) (layer F.Cu) (net 115))
  (segment (start 114.935 76.2) (end 114.935 78.105) (width 0.35) (layer F.Cu) (net 115))
  (segment (start 114.3 75.565) (end 114.3 73.89) (width 0.35) (layer F.Cu) (net 115))
  (segment (start 116.651333 78.66267) (end 116.15107 78.162407) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.15107 78.162407) (end 116.15107 76.835) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.15107 76.892407) (end 116.15107 76.835) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.15107 75.51107) (end 115.57 74.93) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 115.57 74.93) (end 115.57 73.89) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.15107 76.835) (end 116.15107 75.51107) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 117.712085 80.12267) (end 118.355828 79.478927) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BB29745))
  (segment (start 118.355828 79.478927) (end 118.355828 78.74) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 116.84 74.93) (end 116.84 73.89) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 118.355828 76.445828) (end 116.84 74.93) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 118.355828 78.105) (end 118.355828 76.445828) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 118.355828 78.74) (end 118.355828 78.105) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 118.355828 78.105) (end 118.355828 77.85866) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 118.11 74.93) (end 118.11 73.89) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 119.253 76.073) (end 118.11 74.93) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 119.253 81.407) (end 119.253 76.073) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 118.73267 81.92733) (end 119.253 81.407) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 117.712085 81.92733) (end 118.73267 81.92733) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 120.015 82.55) (end 119.17767 83.38733) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 120.015 75.565) (end 120.015 82.55) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 119.38 74.93) (end 120.015 75.565) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 119.17767 83.38733) (end 116.651333 83.38733) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 119.38 73.89) (end 119.38 74.93) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 108.585 74.64) (end 108.585 73.89) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 109.22 82.55) (end 109.22 75.565) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 108.585 74.93) (end 108.585 74.64) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 109.22 75.565) (end 108.585 74.93) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 108.38267 83.38733) (end 109.22 82.55) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 105.856333 83.38733) (end 108.38267 83.38733) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 107.315 74.93) (end 107.315 73.89) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 107.95 75.565) (end 107.315 74.93) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 108.204 75.819) (end 107.315 74.93) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 108.458 76.073) (end 108.204 75.819) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 108.458 81.407) (end 108.458 76.073) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 107.93767 81.92733) (end 108.458 81.407) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 106.917085 81.92733) (end 107.93767 81.92733) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 107.560828 79.478927) (end 106.917085 80.12267) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 107.560828 76.445828) (end 107.560828 79.478927) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 106.045 74.93) (end 107.560828 76.445828) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 106.045 73.89) (end 106.045 74.93) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 105.856333 78.66267) (end 105.856333 76.646333) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 104.775 75.565) (end 104.775 74.64) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 104.775 74.64) (end 104.775 73.89) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 105.856333 76.646333) (end 104.775 75.565) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 103.505 74.64) (end 103.505 73.89) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 104.14 76.905) (end 103.505 76.27) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 103.505 76.27) (end 103.505 74.64) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 104.14 78.105) (end 104.14 76.905) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 102.235 78.474003) (end 102.423667 78.66267) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 102.235 73.89) (end 102.235 78.474003) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 100.965 79.724755) (end 101.362915 80.12267) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 100.965 73.89) (end 100.965 79.724755) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 100.34233 81.92733) (end 101.362915 81.92733) (width 0.35) (layer F.Cu) (net 127))
  (segment (start 99.695 81.28) (end 100.34233 81.92733) (width 0.35) (layer F.Cu) (net 127))
  (segment (start 99.695 73.89) (end 99.695 81.28) (width 0.35) (layer F.Cu) (net 127))
  (segment (start 140.335 56.515) (end 141.605 56.515) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 141.605 56.515) (end 142.24 55.88) (width 0.35) (layer F.Cu) (net 128))
  (via (at 142.24 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 142.24 55.88) (end 142.24 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 127.76 56.515) (end 128.905 56.515) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 128.905 56.515) (end 129.54 55.88) (width 0.35) (layer F.Cu) (net 128))
  (via (at 129.54 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 129.54 55.88) (end 129.54 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 142.24 53.34) (end 129.54 53.34) (width 0.35) (layer B.Cu) (net 128))
  (segment (start 111.125 56.515) (end 111.8 56.515) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 111.8 56.515) (end 112.395 56.515) (width 0.35) (layer F.Cu) (net 128))
  (via (at 113.03 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 113.03 55.88) (end 113.03 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 112.395 56.515) (end 113.03 55.88) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 113.03 53.34) (end 129.54 53.34) (width 0.35) (layer B.Cu) (net 128))
  (segment (start 98.55 56.515) (end 99.695 56.515) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 99.695 56.515) (end 100.33 55.88) (width 0.35) (layer F.Cu) (net 128))
  (via (at 100.33 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 100.33 55.88) (end 100.33 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 100.33 53.34) (end 113.03 53.34) (width 0.35) (layer B.Cu) (net 128))
  (segment (start 158.295 56.515) (end 158.75 56.06) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 156.97 56.515) (end 158.295 56.515) (width 0.35) (layer F.Cu) (net 128))
  (via (at 158.75 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 158.75 56.06) (end 158.75 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 158.75 53.34) (end 142.24 53.34) (width 0.35) (layer B.Cu) (net 128))
  (segment (start 170.87 56.515) (end 171.45 55.935) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 169.545 56.515) (end 170.87 56.515) (width 0.35) (layer F.Cu) (net 128))
  (via (at 171.45 53.34) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 128))
  (segment (start 171.45 55.935) (end 171.45 53.34) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 171.45 53.34) (end 158.75 53.34) (width 0.35) (layer B.Cu) (net 128))
  (segment (start 169.545 64.135) (end 166.37 64.135) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 166.37 64.135) (end 165.695 64.135) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 140.335 64.135) (end 137.16 64.135) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 149.735 64.135) (end 156.97 64.135) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 120.525 64.135) (end 127.76 64.135) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 107.95 64.135) (end 111.125 64.135) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 107.08 38.42) (end 107.08 37.27) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 107.08 39.678) (end 107.08 38.42) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 107.442 40.04) (end 107.08 39.678) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 107.442 40.64) (end 107.442 40.04) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 101.727 25.388) (end 101.727 25.988) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 103.88 28.245) (end 101.727 26.092) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 101.727 26.092) (end 101.727 25.988) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 103.88 28.77) (end 103.88 28.245) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 101.343 31.02) (end 102.43 31.02) (width 0.35) (layer F.Cu) (net 141))
  (segment (start 99.914 29.591) (end 101.343 31.02) (width 0.35) (layer F.Cu) (net 141))
  (segment (start 99.314 29.591) (end 99.914 29.591) (width 0.35) (layer F.Cu) (net 141))
  (segment (start 99.879 28.194) (end 99.314 28.194) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 101.905 30.22) (end 99.879 28.194) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 102.43 30.22) (end 101.905 30.22) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 106.045 40.005) (end 106.045 40.64) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 106.28 39.77) (end 106.045 40.005) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 106.28 37.27) (end 106.28 39.77) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 106.28 27.62) (end 106.28 28.77) (width 0.35) (layer F.Cu) (net 146))
  (segment (start 106.28 26.67) (end 106.28 27.62) (width 0.35) (layer F.Cu) (net 146))
  (segment (start 105.918 26.308) (end 106.28 26.67) (width 0.35) (layer F.Cu) (net 146))
  (segment (start 105.918 25.4) (end 105.918 26.308) (width 0.35) (layer F.Cu) (net 146))
  (segment (start 107.08 26.67) (end 107.08 28.77) (width 0.35) (layer F.Cu) (net 148))
  (segment (start 107.315 26.435) (end 107.08 26.67) (width 0.35) (layer F.Cu) (net 148))
  (segment (start 107.315 25.4) (end 107.315 26.435) (width 0.35) (layer F.Cu) (net 148))
  (segment (start 108.712 26) (end 108.712 25.4) (width 0.35) (layer F.Cu) (net 149))
  (segment (start 107.88 26.832) (end 108.712 26) (width 0.35) (layer F.Cu) (net 149))
  (segment (start 107.88 28.77) (end 107.88 26.832) (width 0.35) (layer F.Cu) (net 149))
  (segment (start 110.109 26) (end 110.109 25.4) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 108.68 27.429) (end 110.109 26) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 108.68 28.77) (end 108.68 27.429) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 111.506 26) (end 111.506 25.4) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 111.506 26.219) (end 111.506 26) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 109.48 28.245) (end 111.506 26.219) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 109.48 28.77) (end 109.48 28.245) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 113.7 28.194) (end 114.3 28.194) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 113.481 28.194) (end 113.7 28.194) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 111.455 30.22) (end 113.481 28.194) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 110.93 30.22) (end 111.455 30.22) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 113.7 29.591) (end 112.271 31.02) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 112.08 31.02) (end 110.93 31.02) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 112.271 31.02) (end 112.08 31.02) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 114.3 29.591) (end 113.7 29.591) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 113.7 37.973) (end 113.665 37.938) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 114.3 37.973) (end 113.7 37.973) (width 0.35) (layer F.Cu) (net 160) (tstamp 5BB44D2A))
  (segment (start 111.455 35.82) (end 110.93 35.82) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 113.573 37.938) (end 111.455 35.82) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 113.665 37.938) (end 113.573 37.938) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 109.48 37.795) (end 109.48 37.27) (width 0.35) (layer F.Cu) (net 161))
  (segment (start 111.633 39.948) (end 109.48 37.795) (width 0.35) (layer F.Cu) (net 161))
  (segment (start 111.633 40.64) (end 111.633 39.948) (width 0.35) (layer F.Cu) (net 161))
  (segment (start 110.236 40.04) (end 108.68 38.484) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 108.68 38.42) (end 108.68 37.27) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 108.68 38.484) (end 108.68 38.42) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 110.236 40.64) (end 110.236 40.04) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 107.88 39.081) (end 107.88 38.42) (width 0.35) (layer F.Cu) (net 165))
  (segment (start 108.839 40.04) (end 107.88 39.081) (width 0.35) (layer F.Cu) (net 165))
  (segment (start 107.88 38.42) (end 107.88 37.27) (width 0.35) (layer F.Cu) (net 165))
  (segment (start 108.839 40.64) (end 108.839 40.04) (width 0.35) (layer F.Cu) (net 165))
  (segment (start 80.01 49.53) (end 80.01 44.45) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 80.645 50.165) (end 80.01 49.53) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 83.345 50.165) (end 80.645 50.165) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 79.375 43.815) (end 80.01 44.45) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 77.945 43.815) (end 79.375 43.815) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 83.345 50.165) (end 85.725 50.165) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 85.725 50.165) (end 85.471 50.165) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 86.995 50.165) (end 85.471 50.165) (width 0.35) (layer F.Cu) (net 169))
  (segment (start 99.051 42.155) (end 95.504 42.155) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 99.06 42.164) (end 99.051 42.155) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 100.33 41.91) (end 100.076 42.164) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 101.34 35.82) (end 100.33 36.83) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 100.076 42.164) (end 99.06 42.164) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 100.33 36.83) (end 100.33 41.91) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 102.43 35.82) (end 101.34 35.82) (width 0.35) (layer F.Cu) (net 182))
  (segment (start 95.504 34.905) (end 97.429 36.83) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 98.335 36.83) (end 99.06 36.83) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 97.429 36.83) (end 98.335 36.83) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 95.504 33.655) (end 95.504 34.905) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 99.187 36.83) (end 99.187 36.703) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 99.4664 36.83) (end 99.187 36.83) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 100.2164 36.08) (end 99.4664 36.83) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 101.28 35.02) (end 100.22 36.08) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 100.22 36.08) (end 100.2164 36.08) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 102.43 35.02) (end 101.28 35.02) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 110.949 33.401) (end 110.93 33.42) (width 0.35) (layer F.Cu) (net 184))
  (segment (start 113.296 33.401) (end 110.949 33.401) (width 0.35) (layer F.Cu) (net 184))
  (segment (start 113.677 33.782) (end 113.296 33.401) (width 0.35) (layer F.Cu) (net 184))
  (segment (start 114.427 33.782) (end 113.677 33.782) (width 0.35) (layer F.Cu) (net 184))
  (segment (start 103.124 26) (end 104.68 27.556) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 104.68 27.556) (end 104.68 28.77) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 103.124 25.4) (end 103.124 26) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 112.08 34.22) (end 110.93 34.22) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 112.741 34.22) (end 112.08 34.22) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 113.7 35.179) (end 112.741 34.22) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 114.3 35.179) (end 113.7 35.179) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 105.48 39.208) (end 105.48 37.27) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 104.648 40.04) (end 105.48 39.208) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 104.648 40.64) (end 104.648 40.04) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 103.251 40.04) (end 103.251 40.64) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 104.68 38.611) (end 104.68 38.1) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 103.251 40.04) (end 104.68 38.611) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 104.68 37.27) (end 104.68 38.1) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 103.88 37.795) (end 103.88 37.27) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 101.854 39.821) (end 103.88 37.795) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 101.854 40.64) (end 101.854 39.821) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 104.521 26) (end 104.521 25.4) (width 0.35) (layer F.Cu) (net 197))
  (segment (start 105.48 26.959) (end 104.521 26) (width 0.35) (layer F.Cu) (net 197))
  (segment (start 105.48 28.77) (end 105.48 26.959) (width 0.35) (layer F.Cu) (net 197))
  (segment (start 112.868 31.82) (end 110.93 31.82) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 113.7 30.988) (end 112.868 31.82) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 114.3 30.988) (end 113.7 30.988) (width 0.35) (layer F.Cu) (net 198))

  (zone (net 10) (net_name GND) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 27.94) (xy 186.055 27.94) (xy 186.055 97.79) (xy 89.535 97.79)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (tstamp 5BB44136) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 27.94) (xy 186.055 27.94) (xy 186.055 97.79) (xy 89.535 97.79)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.14 30.48) (xy 109.22 30.48) (xy 109.22 35.56) (xy 104.14 35.56)
      )
    )
  )
)
