(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")

  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 1363)
    (zones 0)
    (modules 284)
    (nets 287)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.9)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (user_via 1.4 0.9)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_fffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "../../../Desktop/"))
  )

  (net 0 "")
  (net 1 "Net-(C802-Pad1)")
  (net 2 "Net-(C702-Pad1)")
  (net 3 "Net-(C602-Pad1)")
  (net 4 "Net-(C502-Pad1)")
  (net 5 "Net-(C402-Pad1)")
  (net 6 "Net-(C302-Pad1)")
  (net 7 VCC)
  (net 8 GND)
  (net 9 "Net-(R808-Pad2)")
  (net 10 "Net-(R807-Pad2)")
  (net 11 "Net-(R806-Pad2)")
  (net 12 "Net-(R805-Pad2)")
  (net 13 ~enable_Shiftregister)
  (net 14 "Net-(R804-Pad2)")
  (net 15 "Net-(R803-Pad2)")
  (net 16 "Net-(R802-Pad2)")
  (net 17 "Net-(R801-Pad2)")
  (net 18 "Net-(R701-Pad2)")
  (net 19 "Net-(R702-Pad2)")
  (net 20 "Net-(R703-Pad2)")
  (net 21 "Net-(R704-Pad2)")
  (net 22 "Net-(R705-Pad2)")
  (net 23 "Net-(R706-Pad2)")
  (net 24 "Net-(R707-Pad2)")
  (net 25 "Net-(R708-Pad2)")
  (net 26 "Net-(R608-Pad2)")
  (net 27 "Net-(R607-Pad2)")
  (net 28 "Net-(R606-Pad2)")
  (net 29 "Net-(R605-Pad2)")
  (net 30 "Net-(R604-Pad2)")
  (net 31 "Net-(R603-Pad2)")
  (net 32 "Net-(R602-Pad2)")
  (net 33 "Net-(R601-Pad2)")
  (net 34 "Net-(R501-Pad2)")
  (net 35 "Net-(R502-Pad2)")
  (net 36 "Net-(R503-Pad2)")
  (net 37 "Net-(R504-Pad2)")
  (net 38 "Net-(R505-Pad2)")
  (net 39 "Net-(R506-Pad2)")
  (net 40 "Net-(R507-Pad2)")
  (net 41 "Net-(R508-Pad2)")
  (net 42 "Net-(R408-Pad2)")
  (net 43 "Net-(R407-Pad2)")
  (net 44 "Net-(R406-Pad2)")
  (net 45 "Net-(R405-Pad2)")
  (net 46 "Net-(R404-Pad2)")
  (net 47 "Net-(R403-Pad2)")
  (net 48 "Net-(R402-Pad2)")
  (net 49 "Net-(R401-Pad2)")
  (net 50 "Net-(R301-Pad2)")
  (net 51 "Net-(R302-Pad2)")
  (net 52 "Net-(R303-Pad2)")
  (net 53 "Net-(R304-Pad2)")
  (net 54 "Net-(R305-Pad2)")
  (net 55 "Net-(R306-Pad2)")
  (net 56 "Net-(R307-Pad2)")
  (net 57 "Net-(R308-Pad2)")
  (net 58 /Tubes/sheet5BB3E86D/e)
  (net 59 /Tubes/sheet5BB3E86D/d)
  (net 60 /Tubes/sheet5BB3E86D/g)
  (net 61 /Tubes/sheet5BB3E86D/f)
  (net 62 /Tubes/sheet5BB3E86D/a)
  (net 63 /Tubes/sheet5BB3E86D/c)
  (net 64 /Tubes/sheet5BB3E86D/b)
  (net 65 /Tubes/sheet5BB3E86D/Dot)
  (net 66 /Tubes/sheet5BB3E86C/Dot)
  (net 67 /Tubes/sheet5BB3E86C/b)
  (net 68 /Tubes/sheet5BB3E86C/c)
  (net 69 /Tubes/sheet5BB3E86C/a)
  (net 70 /Tubes/sheet5BB3E86C/f)
  (net 71 /Tubes/sheet5BB3E86C/g)
  (net 72 /Tubes/sheet5BB3E86C/d)
  (net 73 /Tubes/sheet5BB3E86C/e)
  (net 74 /Tubes/sheet5BB3BB93/e)
  (net 75 /Tubes/sheet5BB3BB93/d)
  (net 76 /Tubes/sheet5BB3BB93/g)
  (net 77 /Tubes/sheet5BB3BB93/f)
  (net 78 /Tubes/sheet5BB3BB93/a)
  (net 79 /Tubes/sheet5BB3BB93/c)
  (net 80 /Tubes/sheet5BB3BB93/b)
  (net 81 /Tubes/sheet5BB3BB93/Dot)
  (net 82 /Tubes/sheet5BB36ADE/Dot)
  (net 83 /Tubes/sheet5BB36ADE/b)
  (net 84 /Tubes/sheet5BB36ADE/c)
  (net 85 /Tubes/sheet5BB36ADE/a)
  (net 86 /Tubes/sheet5BB36ADE/f)
  (net 87 /Tubes/sheet5BB36ADE/g)
  (net 88 /Tubes/sheet5BB36ADE/d)
  (net 89 /Tubes/sheet5BB36ADE/e)
  (net 90 /Tubes/sheet5BB32DC8/e)
  (net 91 /Tubes/sheet5BB32DC8/d)
  (net 92 /Tubes/sheet5BB32DC8/g)
  (net 93 /Tubes/sheet5BB32DC8/f)
  (net 94 /Tubes/sheet5BB32DC8/a)
  (net 95 /Tubes/sheet5BB32DC8/c)
  (net 96 /Tubes/sheet5BB32DC8/b)
  (net 97 /Tubes/sheet5BB32DC8/Dot)
  (net 98 /Tubes/IV-9_Tube/Dot)
  (net 99 /Tubes/IV-9_Tube/b)
  (net 100 /Tubes/IV-9_Tube/c)
  (net 101 /Tubes/IV-9_Tube/a)
  (net 102 /Tubes/IV-9_Tube/f)
  (net 103 /Tubes/IV-9_Tube/g)
  (net 104 /Tubes/IV-9_Tube/d)
  (net 105 /Tubes/IV-9_Tube/e)
  (net 106 /Tubes/sheet5BB3E86C/Data_in)
  (net 107 /Tubes/sheet5BB36ADE/Data_in)
  (net 108 /Tubes/sheet5BB3BB93/Data_in)
  (net 109 /Tubes/sheet5BB32DC8/Data_in)
  (net 110 /Tubes/IV-9_Tube/Data_in)
  (net 111 "Net-(R902-Pad2)")
  (net 112 "Net-(R914-Pad2)")
  (net 113 "Net-(R916-Pad2)")
  (net 114 "Net-(R915-Pad2)")
  (net 115 "Net-(R901-Pad2)")
  (net 116 "Net-(R913-Pad2)")
  (net 117 "Net-(R912-Pad2)")
  (net 118 "Net-(R911-Pad2)")
  (net 119 "Net-(R910-Pad2)")
  (net 120 "Net-(R909-Pad2)")
  (net 121 "Net-(R908-Pad2)")
  (net 122 "Net-(R907-Pad2)")
  (net 123 clk)
  (net 124 "Net-(R906-Pad2)")
  (net 125 "Net-(R905-Pad2)")
  (net 126 MISO)
  (net 127 MOSI)
  (net 128 "Net-(R904-Pad2)")
  (net 129 "Net-(R903-Pad2)")
  (net 130 Currentsensing_Tube_6)
  (net 131 Currentsensing_Tube_5)
  (net 132 Currentsensing_Tube_4)
  (net 133 Currentsensing_Tube_3)
  (net 134 Currentsensing_Tube_2)
  (net 135 Currentsensing_Tube_1)
  (net 136 /uC/XTAL2)
  (net 137 /uC/XTAL1)
  (net 138 "Net-(C901-Pad1)")
  (net 139 "Net-(R921-Pad2)")
  (net 140 "Net-(R918-Pad2)")
  (net 141 "Net-(R924-Pad2)")
  (net 142 "Net-(R923-Pad2)")
  (net 143 "Net-(R922-Pad2)")
  (net 144 "Net-(R920-Pad2)")
  (net 145 "Net-(R919-Pad2)")
  (net 146 SCL)
  (net 147 SDA)
  (net 148 "Net-(U1101-Pad4)")
  (net 149 "Net-(U1101-Pad3)")
  (net 150 "Net-(U1101-Pad1)")
  (net 151 +12V)
  (net 152 "Net-(R1201-Pad1)")
  (net 153 "Net-(C1203-Pad1)")
  (net 154 "Net-(R1202-Pad2)")
  (net 155 "Net-(R1203-Pad1)")
  (net 156 "Net-(R1302-Pad2)")
  (net 157 "Net-(R1303-Pad1)")
  (net 158 "Net-(C1303-Pad1)")
  (net 159 "Net-(RV1201-Pad2)")
  (net 160 "/5V PSU /SwE")
  (net 161 "Net-(D1303-Pad1)")
  (net 162 "Net-(Q1301-Pad3)")
  (net 163 "Net-(Q1302-Pad3)")
  (net 164 "Net-(C1306-Pad1)")
  (net 165 "Net-(D1303-Pad2)")
  (net 166 enable_2.5V_PSU)
  (net 167 "Net-(SW1401-Pad1)")
  (net 168 "Net-(D1401-Pad1)")
  (net 169 "Net-(F1401-Pad2)")
  (net 170 /Tubes/IV-9_Tube/Data_out)
  (net 171 reset_Shiftregister)
  (net 172 ~latch_Shiftregister)
  (net 173 "Net-(U503-Pad4)")
  (net 174 "Net-(U803-Pad4)")
  (net 175 "Net-(U703-Pad4)")
  (net 176 "Net-(U303-Pad4)")
  (net 177 "Net-(U603-Pad4)")
  (net 178 "Net-(U403-Pad4)")
  (net 179 Encoder_B)
  (net 180 "Net-(R1501-Pad1)")
  (net 181 "Net-(R1502-Pad1)")
  (net 182 Encoder_A)
  (net 183 Encoder_push)
  (net 184 "Net-(D202-Pad1)")
  (net 185 Dot)
  (net 186 "Net-(D201-Pad1)")
  (net 187 "Net-(D202-Pad2)")
  (net 188 "Net-(D201-Pad2)")
  (net 189 Dip_3)
  (net 190 Dip_2)
  (net 191 Dip_1)
  (net 192 "Net-(D301-Pad1)")
  (net 193 Tube_LED)
  (net 194 "Net-(D401-Pad1)")
  (net 195 "Net-(D501-Pad1)")
  (net 196 "Net-(D601-Pad1)")
  (net 197 "Net-(D701-Pad1)")
  (net 198 "Net-(D801-Pad1)")
  (net 199 "Net-(D601-Pad2)")
  (net 200 "Net-(D501-Pad2)")
  (net 201 "Net-(D701-Pad2)")
  (net 202 "Net-(D801-Pad2)")
  (net 203 "Net-(D401-Pad2)")
  (net 204 "Net-(D301-Pad2)")
  (net 205 "Net-(D904-Pad1)")
  (net 206 LED_Error)
  (net 207 "Net-(D905-Pad1)")
  (net 208 "Net-(D904-Pad2)")
  (net 209 Rx)
  (net 210 +3V3)
  (net 211 "Net-(U1601-Pad2)")
  (net 212 "Net-(U1601-Pad4)")
  (net 213 "Net-(U1601-Pad5)")
  (net 214 "Net-(U1601-Pad6)")
  (net 215 "Net-(U1601-Pad14)")
  (net 216 "Net-(U1601-Pad16)")
  (net 217 "Net-(U1601-Pad17)")
  (net 218 Tx)
  (net 219 "/3_3V PSU/MC34063_Feedback")
  (net 220 "Net-(D1601-Pad2)")
  (net 221 "Net-(R1601-Pad1)")
  (net 222 "Net-(R1603-Pad2)")
  (net 223 PSU_3.3V_feedback)
  (net 224 enable_3.3V_PSU)
  (net 225 "Net-(U1601-Pad1)")
  (net 226 "Net-(U1601-Pad15)")
  (net 227 "Net-(U1601-Pad20)")
  (net 228 "Net-(U1601-Pad21)")
  (net 229 "/3_3V PSU/SwE")
  (net 230 "Net-(R1603-Pad1)")
  (net 231 "Net-(R1604-Pad2)")
  (net 232 "Net-(R1606-Pad1)")
  (net 233 "Net-(L1601-Pad2)")
  (net 234 "Net-(R1607-Pad1)")
  (net 235 V_Bat)
  (net 236 "Net-(J1602-Pad2)")
  (net 237 "Net-(L1601-Pad1)")
  (net 238 "Net-(R1604-Pad1)")
  (net 239 "Net-(C1601-Pad2)")
  (net 240 "Net-(D1602-Pad1)")
  (net 241 "/3_3V PSU/MC34063_HC_A")
  (net 242 "Net-(R1608-Pad1)")
  (net 243 /uC/MOSI_ISP)
  (net 244 /uC/MISO_ISP)
  (net 245 /uC/clk_ISP)
  (net 246 /uC/~Reset_ISP)
  (net 247 "Net-(R411-Pad2)")
  (net 248 "Net-(R933-Pad2)")
  (net 249 "Net-(R711-Pad2)")
  (net 250 "Net-(R811-Pad2)")
  (net 251 "Net-(R934-Pad2)")
  (net 252 "Net-(R935-Pad2)")
  (net 253 "Net-(R311-Pad2)")
  (net 254 "Net-(R936-Pad2)")
  (net 255 "Net-(R611-Pad2)")
  (net 256 "Net-(R511-Pad2)")
  (net 257 "Net-(R937-Pad2)")
  (net 258 "Net-(U901-Pad8)")
  (net 259 "Net-(U901-Pad7)")
  (net 260 "Net-(U901-Pad6)")
  (net 261 "Net-(U901-Pad5)")
  (net 262 "Net-(U901-Pad4)")
  (net 263 "Net-(U901-Pad3)")
  (net 264 "Net-(U901-Pad2)")
  (net 265 "Net-(U901-Pad1)")
  (net 266 "Net-(Q1201-Pad4)")
  (net 267 "/3_3V PSU/HC_Plain")
  (net 268 "/3_3V PSU/HC_Plain_b")
  (net 269 "Net-(R946-Pad2)")
  (net 270 "Net-(R946-Pad1)")
  (net 271 "Net-(R945-Pad1)")
  (net 272 "Net-(R945-Pad2)")
  (net 273 "Net-(R944-Pad2)")
  (net 274 "Net-(R944-Pad1)")
  (net 275 "Net-(R943-Pad1)")
  (net 276 "Net-(R943-Pad2)")
  (net 277 "Net-(R942-Pad2)")
  (net 278 "Net-(R942-Pad1)")
  (net 279 "Net-(R941-Pad2)")
  (net 280 "Net-(R940-Pad2)")
  (net 281 "Net-(R940-Pad1)")
  (net 282 "Net-(R939-Pad2)")
  (net 283 "Net-(R938-Pad2)")
  (net 284 "Net-(R908-Pad1)")
  (net 285 "Net-(R909-Pad1)")
  (net 286 "Net-(R910-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net "/3_3V PSU/HC_Plain")
    (add_net "/3_3V PSU/HC_Plain_b")
    (add_net "/3_3V PSU/MC34063_Feedback")
    (add_net "/3_3V PSU/MC34063_HC_A")
    (add_net "/3_3V PSU/SwE")
    (add_net "/5V PSU /SwE")
    (add_net /Tubes/IV-9_Tube/Data_in)
    (add_net /Tubes/IV-9_Tube/Data_out)
    (add_net /Tubes/IV-9_Tube/Dot)
    (add_net /Tubes/IV-9_Tube/a)
    (add_net /Tubes/IV-9_Tube/b)
    (add_net /Tubes/IV-9_Tube/c)
    (add_net /Tubes/IV-9_Tube/d)
    (add_net /Tubes/IV-9_Tube/e)
    (add_net /Tubes/IV-9_Tube/f)
    (add_net /Tubes/IV-9_Tube/g)
    (add_net /Tubes/sheet5BB32DC8/Data_in)
    (add_net /Tubes/sheet5BB32DC8/Dot)
    (add_net /Tubes/sheet5BB32DC8/a)
    (add_net /Tubes/sheet5BB32DC8/b)
    (add_net /Tubes/sheet5BB32DC8/c)
    (add_net /Tubes/sheet5BB32DC8/d)
    (add_net /Tubes/sheet5BB32DC8/e)
    (add_net /Tubes/sheet5BB32DC8/f)
    (add_net /Tubes/sheet5BB32DC8/g)
    (add_net /Tubes/sheet5BB36ADE/Data_in)
    (add_net /Tubes/sheet5BB36ADE/Dot)
    (add_net /Tubes/sheet5BB36ADE/a)
    (add_net /Tubes/sheet5BB36ADE/b)
    (add_net /Tubes/sheet5BB36ADE/c)
    (add_net /Tubes/sheet5BB36ADE/d)
    (add_net /Tubes/sheet5BB36ADE/e)
    (add_net /Tubes/sheet5BB36ADE/f)
    (add_net /Tubes/sheet5BB36ADE/g)
    (add_net /Tubes/sheet5BB3BB93/Data_in)
    (add_net /Tubes/sheet5BB3BB93/Dot)
    (add_net /Tubes/sheet5BB3BB93/a)
    (add_net /Tubes/sheet5BB3BB93/b)
    (add_net /Tubes/sheet5BB3BB93/c)
    (add_net /Tubes/sheet5BB3BB93/d)
    (add_net /Tubes/sheet5BB3BB93/e)
    (add_net /Tubes/sheet5BB3BB93/f)
    (add_net /Tubes/sheet5BB3BB93/g)
    (add_net /Tubes/sheet5BB3E86C/Data_in)
    (add_net /Tubes/sheet5BB3E86C/Dot)
    (add_net /Tubes/sheet5BB3E86C/a)
    (add_net /Tubes/sheet5BB3E86C/b)
    (add_net /Tubes/sheet5BB3E86C/c)
    (add_net /Tubes/sheet5BB3E86C/d)
    (add_net /Tubes/sheet5BB3E86C/e)
    (add_net /Tubes/sheet5BB3E86C/f)
    (add_net /Tubes/sheet5BB3E86C/g)
    (add_net /Tubes/sheet5BB3E86D/Dot)
    (add_net /Tubes/sheet5BB3E86D/a)
    (add_net /Tubes/sheet5BB3E86D/b)
    (add_net /Tubes/sheet5BB3E86D/c)
    (add_net /Tubes/sheet5BB3E86D/d)
    (add_net /Tubes/sheet5BB3E86D/e)
    (add_net /Tubes/sheet5BB3E86D/f)
    (add_net /Tubes/sheet5BB3E86D/g)
    (add_net /uC/MISO_ISP)
    (add_net /uC/MOSI_ISP)
    (add_net /uC/XTAL1)
    (add_net /uC/XTAL2)
    (add_net /uC/clk_ISP)
    (add_net /uC/~Reset_ISP)
    (add_net Currentsensing_Tube_1)
    (add_net Currentsensing_Tube_2)
    (add_net Currentsensing_Tube_3)
    (add_net Currentsensing_Tube_4)
    (add_net Currentsensing_Tube_5)
    (add_net Currentsensing_Tube_6)
    (add_net Dip_1)
    (add_net Dip_2)
    (add_net Dip_3)
    (add_net Dot)
    (add_net Encoder_A)
    (add_net Encoder_B)
    (add_net Encoder_push)
    (add_net GND)
    (add_net LED_Error)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1203-Pad1)")
    (add_net "Net-(C1303-Pad1)")
    (add_net "Net-(C1306-Pad1)")
    (add_net "Net-(C1601-Pad2)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C602-Pad1)")
    (add_net "Net-(C702-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C901-Pad1)")
    (add_net "Net-(D1303-Pad1)")
    (add_net "Net-(D1303-Pad2)")
    (add_net "Net-(D1401-Pad1)")
    (add_net "Net-(D1601-Pad2)")
    (add_net "Net-(D1602-Pad1)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad1)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D301-Pad1)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D401-Pad1)")
    (add_net "Net-(D401-Pad2)")
    (add_net "Net-(D501-Pad1)")
    (add_net "Net-(D501-Pad2)")
    (add_net "Net-(D601-Pad1)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D701-Pad1)")
    (add_net "Net-(D701-Pad2)")
    (add_net "Net-(D801-Pad1)")
    (add_net "Net-(D801-Pad2)")
    (add_net "Net-(D904-Pad1)")
    (add_net "Net-(D904-Pad2)")
    (add_net "Net-(D905-Pad1)")
    (add_net "Net-(F1401-Pad2)")
    (add_net "Net-(J1602-Pad2)")
    (add_net "Net-(L1601-Pad1)")
    (add_net "Net-(L1601-Pad2)")
    (add_net "Net-(Q1201-Pad4)")
    (add_net "Net-(Q1301-Pad3)")
    (add_net "Net-(Q1302-Pad3)")
    (add_net "Net-(R1201-Pad1)")
    (add_net "Net-(R1202-Pad2)")
    (add_net "Net-(R1203-Pad1)")
    (add_net "Net-(R1302-Pad2)")
    (add_net "Net-(R1303-Pad1)")
    (add_net "Net-(R1501-Pad1)")
    (add_net "Net-(R1502-Pad1)")
    (add_net "Net-(R1601-Pad1)")
    (add_net "Net-(R1603-Pad1)")
    (add_net "Net-(R1603-Pad2)")
    (add_net "Net-(R1604-Pad1)")
    (add_net "Net-(R1604-Pad2)")
    (add_net "Net-(R1606-Pad1)")
    (add_net "Net-(R1607-Pad1)")
    (add_net "Net-(R1608-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad2)")
    (add_net "Net-(R306-Pad2)")
    (add_net "Net-(R307-Pad2)")
    (add_net "Net-(R308-Pad2)")
    (add_net "Net-(R311-Pad2)")
    (add_net "Net-(R401-Pad2)")
    (add_net "Net-(R402-Pad2)")
    (add_net "Net-(R403-Pad2)")
    (add_net "Net-(R404-Pad2)")
    (add_net "Net-(R405-Pad2)")
    (add_net "Net-(R406-Pad2)")
    (add_net "Net-(R407-Pad2)")
    (add_net "Net-(R408-Pad2)")
    (add_net "Net-(R411-Pad2)")
    (add_net "Net-(R501-Pad2)")
    (add_net "Net-(R502-Pad2)")
    (add_net "Net-(R503-Pad2)")
    (add_net "Net-(R504-Pad2)")
    (add_net "Net-(R505-Pad2)")
    (add_net "Net-(R506-Pad2)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R508-Pad2)")
    (add_net "Net-(R511-Pad2)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad2)")
    (add_net "Net-(R605-Pad2)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R607-Pad2)")
    (add_net "Net-(R608-Pad2)")
    (add_net "Net-(R611-Pad2)")
    (add_net "Net-(R701-Pad2)")
    (add_net "Net-(R702-Pad2)")
    (add_net "Net-(R703-Pad2)")
    (add_net "Net-(R704-Pad2)")
    (add_net "Net-(R705-Pad2)")
    (add_net "Net-(R706-Pad2)")
    (add_net "Net-(R707-Pad2)")
    (add_net "Net-(R708-Pad2)")
    (add_net "Net-(R711-Pad2)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad2)")
    (add_net "Net-(R805-Pad2)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R807-Pad2)")
    (add_net "Net-(R808-Pad2)")
    (add_net "Net-(R811-Pad2)")
    (add_net "Net-(R901-Pad2)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R904-Pad2)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(R907-Pad2)")
    (add_net "Net-(R908-Pad1)")
    (add_net "Net-(R908-Pad2)")
    (add_net "Net-(R909-Pad1)")
    (add_net "Net-(R909-Pad2)")
    (add_net "Net-(R910-Pad1)")
    (add_net "Net-(R910-Pad2)")
    (add_net "Net-(R911-Pad2)")
    (add_net "Net-(R912-Pad2)")
    (add_net "Net-(R913-Pad2)")
    (add_net "Net-(R914-Pad2)")
    (add_net "Net-(R915-Pad2)")
    (add_net "Net-(R916-Pad2)")
    (add_net "Net-(R918-Pad2)")
    (add_net "Net-(R919-Pad2)")
    (add_net "Net-(R920-Pad2)")
    (add_net "Net-(R921-Pad2)")
    (add_net "Net-(R922-Pad2)")
    (add_net "Net-(R923-Pad2)")
    (add_net "Net-(R924-Pad2)")
    (add_net "Net-(R933-Pad2)")
    (add_net "Net-(R934-Pad2)")
    (add_net "Net-(R935-Pad2)")
    (add_net "Net-(R936-Pad2)")
    (add_net "Net-(R937-Pad2)")
    (add_net "Net-(R938-Pad2)")
    (add_net "Net-(R939-Pad2)")
    (add_net "Net-(R940-Pad1)")
    (add_net "Net-(R940-Pad2)")
    (add_net "Net-(R941-Pad2)")
    (add_net "Net-(R942-Pad1)")
    (add_net "Net-(R942-Pad2)")
    (add_net "Net-(R943-Pad1)")
    (add_net "Net-(R943-Pad2)")
    (add_net "Net-(R944-Pad1)")
    (add_net "Net-(R944-Pad2)")
    (add_net "Net-(R945-Pad1)")
    (add_net "Net-(R945-Pad2)")
    (add_net "Net-(R946-Pad1)")
    (add_net "Net-(R946-Pad2)")
    (add_net "Net-(RV1201-Pad2)")
    (add_net "Net-(SW1401-Pad1)")
    (add_net "Net-(U1101-Pad1)")
    (add_net "Net-(U1101-Pad3)")
    (add_net "Net-(U1101-Pad4)")
    (add_net "Net-(U1601-Pad1)")
    (add_net "Net-(U1601-Pad14)")
    (add_net "Net-(U1601-Pad15)")
    (add_net "Net-(U1601-Pad16)")
    (add_net "Net-(U1601-Pad17)")
    (add_net "Net-(U1601-Pad2)")
    (add_net "Net-(U1601-Pad20)")
    (add_net "Net-(U1601-Pad21)")
    (add_net "Net-(U1601-Pad4)")
    (add_net "Net-(U1601-Pad5)")
    (add_net "Net-(U1601-Pad6)")
    (add_net "Net-(U303-Pad4)")
    (add_net "Net-(U403-Pad4)")
    (add_net "Net-(U503-Pad4)")
    (add_net "Net-(U603-Pad4)")
    (add_net "Net-(U703-Pad4)")
    (add_net "Net-(U803-Pad4)")
    (add_net "Net-(U901-Pad1)")
    (add_net "Net-(U901-Pad2)")
    (add_net "Net-(U901-Pad3)")
    (add_net "Net-(U901-Pad4)")
    (add_net "Net-(U901-Pad5)")
    (add_net "Net-(U901-Pad6)")
    (add_net "Net-(U901-Pad7)")
    (add_net "Net-(U901-Pad8)")
    (add_net PSU_3.3V_feedback)
    (add_net Rx)
    (add_net SCL)
    (add_net SDA)
    (add_net Tube_LED)
    (add_net Tx)
    (add_net VCC)
    (add_net V_Bat)
    (add_net clk)
    (add_net enable_2.5V_PSU)
    (add_net enable_3.3V_PSU)
    (add_net reset_Shiftregister)
    (add_net ~enable_Shiftregister)
    (add_net ~latch_Shiftregister)
  )

  (module Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C) (tstamp 5BC80D5F)
    (at 120.65 40.441 270)
    (descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (path /5BB48B05/5BB3A603)
    (attr smd)
    (fp_text reference Y901 (at 0 -2.8 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 0 2.8 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.093333 0) (layer F.Adhes) (width 0.186667))
    (fp_circle (center 0 0) (end 0.213333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.333333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.4 0) (layer F.Adhes) (width 0.1))
    (fp_line (start 3.1 -1.9) (end -3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 1.9) (end 3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.9) (end 3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.9) (end -3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.05 1.8) (end 2.7 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.05 -1.8) (end -3.05 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -1.8) (end -3.05 -1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 0.6) (end -1.5 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -1.4) (end -2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 1.4) (end -2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 1.6) (end -2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 1.6) (end -2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.4) (end 2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -1.4) (end 2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -1.6) (end 2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 -1.6) (end 2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (pad 1 smd rect (at -1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_5032-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F39)
    (at 103.251 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC662F3)
    (attr smd)
    (fp_text reference R943 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 275 "Net-(R943-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(R943-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC79BE2)
    (at 108.204 34.798 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B3DE)
    (attr smd)
    (fp_text reference C906 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC1B200) (tstamp 5BC7B6C2)
    (at 108.089 53.975)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B34B)
    (attr smd)
    (fp_text reference C907 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48) (tstamp 5BC7BD1A)
    (at 108.648 44.465 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5BB48B05/5BC060C8)
    (attr smd)
    (fp_text reference U902 (at 0 -7.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega32-16AU (at 0 7.45 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.175 -4.6) (end -6.45 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -5.175 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 -4) (end -4 -5) (layer F.Fab) (width 0.15))
    (fp_line (start -5 5) (end -5 -4) (layer F.Fab) (width 0.15))
    (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.15))
    (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.15))
    (fp_line (start -4 -5) (end 5 -5) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(R942-Pad2)"))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(R941-Pad2)"))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(R940-Pad2)"))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(R939-Pad2)"))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(R938-Pad2)"))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R919-Pad2)"))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R907-Pad2)"))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R933-Pad2)"))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R934-Pad2)"))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(R935-Pad2)"))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(R936-Pad2)"))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(R937-Pad2)"))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(C901-Pad1)"))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(R946-Pad2)"))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(R945-Pad2)"))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(R944-Pad2)"))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R903-Pad2)"))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 276 "Net-(R943-Pad2)"))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R911-Pad2)"))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R912-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R910-Pad2)"))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R909-Pad2)"))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R908-Pad2)"))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R918-Pad2)"))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R921-Pad2)"))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R920-Pad2)"))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R913-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R906-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7200E)
    (at 110.236 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5FA00)
    (attr smd)
    (fp_text reference R938 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 283 "Net-(R938-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F7D)
    (at 111.633 54.864 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F9F9)
    (attr smd)
    (fp_text reference R939 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 282 "Net-(R939-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F6C)
    (at 113.03 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D25)
    (attr smd)
    (fp_text reference R940 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 280 "Net-(R940-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 281 "Net-(R940-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F5B)
    (at 114.427 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D1E)
    (attr smd)
    (fp_text reference R941 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 279 "Net-(R941-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F4A)
    (at 115.824 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC64046)
    (attr smd)
    (fp_text reference R942 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 277 "Net-(R942-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 278 "Net-(R942-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B019)
    (at 98.056 39.116)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC685A2)
    (attr smd)
    (fp_text reference R944 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 273 "Net-(R944-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 274 "Net-(R944-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B049)
    (at 98.056 40.513)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D766)
    (attr smd)
    (fp_text reference R945 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 271 "Net-(R945-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 272 "Net-(R945-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AFE9)
    (at 98.056 41.91)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D75F)
    (attr smd)
    (fp_text reference R946 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 269 "Net-(R946-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 270 "Net-(R946-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC649EC)
    (at 184.978 17.145 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D469D9)
    (attr smd)
    (fp_text reference R1203 (at 0.828 3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R1203-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BC64797)
    (at 166.227 20.066)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB8D2EE/5BC34D02)
    (attr smd)
    (fp_text reference C1206 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-669_LFPAK_ThermalVias-2 (layer F.Cu) (tedit 59217BD0) (tstamp 5BC64C4A)
    (at 131.15 33.66 180)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT669 Thermical Vias Power-SO8")
    (path /5BB8D2EE/5BC31987)
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference Q1201 (at 1.085 -5.26 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PHPT60406NY (at 1.085 5.58 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.66 4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.66 4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.855 2.5) (end 1.855 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 2.5) (end 1.855 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -2.5) (end -2.245 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.855 -2.5) (end -2.245 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 1.855 -2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 2.2) (end 1.855 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 3.155 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -1.65) (end -2.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -2.245 -2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -3.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.4) (end -2.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.85) (end -3.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -0.85) (end -3.245 -0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.85) (end -2.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.4) (end -3.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 0.4) (end -3.245 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 2.15) (end -2.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 1.7) (end -3.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 1.7) (end -3.245 1.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.345 -2.6) (end -2.345 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.345 2.4) (end -2.345 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 2.6) (end -1.155 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 -2.6) (end -1.205 -2.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 thru_hole rect (at 4.745 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 4 smd rect (at -2.835 1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(Q1201-Pad4)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 0.445 0 90) (size 4.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 2.645 0 90) (size 4.7 1.55) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.835 0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 267 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.835 -1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 267 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at -2.835 -0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 267 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.895 -0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 -1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 -1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers B.Cu B.Paste B.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC39110)
    (at 143.518001 47.952001)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E24)
    (attr smd)
    (fp_text reference D902 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 243 /uC/MOSI_ISP))
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC390F7)
    (at 143.518001 45.702001)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54DD6)
    (attr smd)
    (fp_text reference D903 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 245 /uC/clk_ISP))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_6.3x6.3_H3 (layer F.Cu) (tedit 5990349C) (tstamp 5BC64847)
    (at 179.07 33.655)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (path /5BB73C46/5BB49522)
    (attr smd)
    (fp_text reference L1201 (at 0 -4.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 4.45) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0 0) (end 1.91 1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end -1.91 -1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end -3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end -3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end 3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -3.4) (end -3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.4) (end 3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.4) (end 3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.4) (end -3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.3 -3.2) (end 3.3 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -3.2) (end 3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -1.5) (end -3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 3.2) (end -3.3 1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.2) (end -3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 1.5) (end 3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.75 0) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (pad 1 smd rect (at -2.75 0) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_Vishay_IHLP-6767 (layer F.Cu) (tedit 5990349D) (tstamp 5BC64900)
    (at 155.575 30.48 180)
    (descr "Inductor, Vishay, IHLP series, 17.0mmx17.0mm")
    (tags "inductor vishay ihlp smd")
    (path /5BB8D2EE/59D4542E)
    (attr smd)
    (fp_text reference L1301 (at 0 -9.509 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 10.009 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.3 -8.8) (end -10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.3 8.8) (end 10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 8.8) (end 10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 -8.8) (end -10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.609 8.609) (end 8.609 6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 8.609) (end 8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 6.46) (end -8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.609 -8.609) (end 8.609 -6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -8.609) (end 8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -6.46) (end -8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.509 -8.509) (end -8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start 8.509 8.509) (end 8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 8.509) (end 8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 -8.509) (end -8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 267 "/3_3V PSU/HC_Plain"))
    (pad 1 smd rect (at -8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 241 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Vishay_IHLP-6767.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC648CC)
    (at 139.815 29.21)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/59D455EA)
    (attr smd)
    (fp_text reference C1303 (at 3.81 1.016) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1303-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMC (layer F.Cu) (tedit 5864295D) (tstamp 5BC6488E)
    (at 139.7 36.42 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (path /5BB8D2EE/5BB49523)
    (attr smd)
    (fp_text reference D1301 (at 0 -4.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VSSC8L45-M3/9AT (at 0 4.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.8 -3.25) (end 3.6 -3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.8 3.25) (end 3.6 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -4.9 3.35) (end -4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 3.35) (end -4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -3.35) (end 4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -3.35) (end 4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 -3.1) (end 3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 3.1) (end -3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -4.8 3.25) (end -4.8 -3.25) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 267 "/3_3V PSU/HC_Plain"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBA573E)
    (at 85.09 63.615 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB967B8)
    (attr smd)
    (fp_text reference R1309 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC64591)
    (at 184.785 22.225 90)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB73C46/5BB49537)
    (attr smd)
    (fp_text reference RV1201 (at 0 3.4925 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 155 "Net-(R1203-Pad1)"))
    (pad 2 smd rect (at -2.75 0 90) (size 2 1.3) (layers F.Cu F.Mask)
      (net 159 "Net-(RV1201-Pad2)"))
    (pad 1 smd rect (at 2.75 -1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 154 "Net-(R1202-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC3324A)
    (at 80.01 61.976 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB48B05/5BBEE4A1)
    (attr smd)
    (fp_text reference Q901 (at -0.381 -2.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(D904-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 206 LED_Error))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC3216F)
    (at 77.47 53.975)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA0467)
    (attr smd)
    (fp_text reference C1603 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34523)
    (at 25.666 42.2656)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC06246)
    (attr smd)
    (fp_text reference R1506 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 Dip_1))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34512)
    (at 25.666 40.7416)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC0636F)
    (attr smd)
    (fp_text reference R1507 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 Dip_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34501)
    (at 25.666 39.2176)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC0639A)
    (attr smd)
    (fp_text reference R1508 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 Dip_3))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AEF9)
    (at 98.056 37.719)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F7)
    (attr smd)
    (fp_text reference R903 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R903-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B90F)
    (at 118.9235 51.181 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F0)
    (attr smd)
    (fp_text reference R904 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 /uC/MOSI_ISP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B93F)
    (at 118.9235 49.784 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E9)
    (attr smd)
    (fp_text reference R905 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88E45)
    (at 101.854 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6FE)
    (attr smd)
    (fp_text reference R902 (at 0 9.853 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC645F2)
    (at 165.227 13.81 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BC3EDF8)
    (attr smd)
    (fp_text reference C1307 (at 0 4.43 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21F8E)
    (at 91.579 50.419 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC237F5)
    (attr smd)
    (fp_text reference C504 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21FBE)
    (at 91.567 51.816 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC237F5)
    (attr smd)
    (fp_text reference C604 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21FEE)
    (at 88.637401 69.310601)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC237F5)
    (attr smd)
    (fp_text reference C704 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC220AE)
    (at 76.927401 77.370601)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BC237F5)
    (attr smd)
    (fp_text reference C804 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC220DE)
    (at 91.579 49.022 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC237F5)
    (attr smd)
    (fp_text reference C404 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC8616A)
    (at 91.579 47.625 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BC237F5)
    (attr smd)
    (fp_text reference C304 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC1DC98)
    (at 48.5394 38.3794 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB48B05/5BC39713)
    (attr smd)
    (fp_text reference U901 (at 0 -3.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ADR292 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 258 "Net-(U901-Pad8)"))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U901-Pad7)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U901-Pad6)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(U901-Pad5)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 262 "Net-(U901-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(U901-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(U901-Pad2)"))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(U901-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_1206 (layer F.Cu) (tedit 58307BE8) (tstamp 5BC6454E)
    (at 161.597 20.066)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BC1CECA)
    (attr smd)
    (fp_text reference L1202 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BLM31KN601SN1L (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.07) (end 1 -1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 1.07) (end -1 1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 241 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC827E3)
    (at 98.056 47.625)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F151)
    (attr smd)
    (fp_text reference R937 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(R937-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC221CE)
    (at 94.234 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC2388D)
    (attr smd)
    (fp_text reference R511 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 256 "Net-(R511-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 133 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC221FE)
    (at 95.631 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC2388D)
    (attr smd)
    (fp_text reference R611 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 132 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 255 "Net-(R611-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82873)
    (at 98.056 49.022)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5CD4F)
    (attr smd)
    (fp_text reference R936 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(R936-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2225E)
    (at 91.44 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC2388D)
    (attr smd)
    (fp_text reference R311 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 253 "Net-(R311-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82843)
    (at 98.056 50.419)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5AA8D)
    (attr smd)
    (fp_text reference R935 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(R935-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82813)
    (at 98.044 51.828)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC58906)
    (attr smd)
    (fp_text reference R934 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R934-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC222EE)
    (at 97.028 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC2388D)
    (attr smd)
    (fp_text reference R811 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 250 "Net-(R811-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 131 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2231E)
    (at 98.425 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC2388D)
    (attr smd)
    (fp_text reference R711 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 130 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 249 "Net-(R711-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA0D)
    (at 101.727 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC568B6)
    (attr smd)
    (fp_text reference R933 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R933-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC223AE)
    (at 120.015 55.36 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC14A1B)
    (attr smd)
    (fp_text reference R931 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 /uC/MOSI_ISP))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC223DE)
    (at 132.207 49.899 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC12BB4)
    (attr smd)
    (fp_text reference R930 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 MISO))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2201E)
    (at 92.837 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC2388D)
    (attr smd)
    (fp_text reference R411 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 247 "Net-(R411-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 134 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64767)
    (at 136.845 29.53)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC25F71)
    (attr smd)
    (fp_text reference R1311 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(Q1201-Pad4)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 229 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64737)
    (at 142.24 24.765 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC1FD35)
    (attr smd)
    (fp_text reference R1310 (at 0 -1.65 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 229 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BB8C7C3)
    (at 43.18 27.305 180)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BB48B05/5BB3C67E)
    (attr smd)
    (fp_text reference SW901 (at -5.034 1.175 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 246 /uC/~Reset_ISP))
    (pad 1 smd rect (at -2.875 -2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 246 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC52CD1)
    (at 218.5924 40.9194 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BC191B1)
    (attr smd)
    (fp_text reference R1608 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(D1602-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R1608-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Axial Connector SMD:Ceramic_GPS_Antenna_SMD" (layer B.Cu) (tedit 5BB8BE91) (tstamp 5BC3EE0C)
    (at 219.2162 3.8212 180)
    (path /5BC18D95/5BC0A07F)
    (fp_text reference J1601 (at 11.75 -15.75 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x01_Female (at -8.5 -16 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -8.75 12.25) (end 8.75 12.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.25 9.75) (end 12.25 -9.75) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.75 -12.25) (end -8.5 -12.25) (layer B.SilkS) (width 0.15))
    (fp_line (start -12.5 -9.75) (end -12.5 9.75) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -12 12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 12 -12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -12 -12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 12 12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
  )

  (module NEO-6M_24P-16X12.2MM_:GPS24P-SMD-1.1-16X12.2MM (layer B.Cu) (tedit 0) (tstamp 5BB8D36C)
    (at 182.245 -27.305 90)
    (path /5BC18D95/5BB887E8)
    (attr smd)
    (fp_text reference U1601 (at -8.3915 -5.631 180) (layer B.SilkS)
      (effects (font (size 1.00332 1.00332) (thickness 0.05)) (justify mirror))
    )
    (fp_text value "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)" (at -10.233 -7.0026 180) (layer B.SilkS)
      (effects (font (size 1.00302 1.00302) (thickness 0.05)) (justify mirror))
    )
    (fp_poly (pts (xy -4.45094 8.255) (xy 4.445 8.255) (xy 4.445 -8.26603) (xy -4.45094 -8.26603)) (layer B.SilkS) (width 0))
    (fp_circle (center -6.985 8.255) (end -6.731 8.255) (layer B.SilkS) (width 0.508))
    (fp_line (start -5.334 8.636) (end -6.096 7.874) (layer B.SilkS) (width 0.127))
    (fp_line (start 6.096 8.636) (end -5.334 8.636) (layer B.SilkS) (width 0.127))
    (fp_line (start 6.096 7.874) (end 6.096 8.636) (layer B.SilkS) (width 0.127))
    (fp_line (start -6.096 -8.636) (end -6.096 -8.001) (layer B.SilkS) (width 0.127))
    (fp_line (start 6.096 -8.636) (end -6.096 -8.636) (layer B.SilkS) (width 0.127))
    (fp_line (start 6.096 -8.001) (end 6.096 -8.636) (layer B.SilkS) (width 0.127))
    (pad 24 smd rect (at 5.896 6.888 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 23 smd rect (at 5.896 5.788 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (pad 22 smd rect (at 5.896 4.688 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 240 "Net-(D1602-Pad1)"))
    (pad 21 smd rect (at 5.896 3.588 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 228 "Net-(U1601-Pad21)"))
    (pad 20 smd rect (at 5.896 2.488 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 227 "Net-(U1601-Pad20)"))
    (pad 19 smd rect (at 5.896 1.388 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 231 "Net-(R1604-Pad2)"))
    (pad 18 smd rect (at 5.896 0.288 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 222 "Net-(R1603-Pad2)"))
    (pad 17 smd rect (at 5.896 -2.712 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 217 "Net-(U1601-Pad17)"))
    (pad 16 smd rect (at 5.896 -3.812 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 216 "Net-(U1601-Pad16)"))
    (pad 15 smd rect (at 5.896 -4.912 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 226 "Net-(U1601-Pad15)"))
    (pad 14 smd rect (at 5.896 -6.012 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 215 "Net-(U1601-Pad14)"))
    (pad 13 smd rect (at 5.896 -7.112 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 12 smd rect (at -5.904 -7.112 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 11 smd rect (at -5.904 -6.012 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 237 "Net-(L1601-Pad1)"))
    (pad 10 smd rect (at -5.904 -4.912 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -5.904 -3.812 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 234 "Net-(R1607-Pad1)"))
    (pad 8 smd rect (at -5.904 -2.712 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 234 "Net-(R1607-Pad1)"))
    (pad 7 smd rect (at -5.904 0.288 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -5.904 1.388 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 214 "Net-(U1601-Pad6)"))
    (pad 5 smd rect (at -5.904 2.488 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 213 "Net-(U1601-Pad5)"))
    (pad 4 smd rect (at -5.904 3.588 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 212 "Net-(U1601-Pad4)"))
    (pad 3 smd rect (at -5.904 4.688 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 221 "Net-(R1601-Pad1)"))
    (pad 2 smd rect (at -5.904 5.788 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 211 "Net-(U1601-Pad2)"))
    (pad 1 smd rect (at -5.904 6.888 270) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 225 "Net-(U1601-Pad1)"))
  )

  (module Resistors_SMD:R_2512 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC30021)
    (at 220.6486 35.4584)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BC18D95/5BBF012F)
    (attr smd)
    (fp_text reference R1605 (at 4.7256 -0.3302 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0R (at 0 -2.75) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 3.85 -1.85) (end -3.85 -1.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.85 -1.85) (end 3.85 1.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.85 1.85) (end -3.85 -1.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.85 1.85) (end 3.85 1.85) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.6 1.82) (end 2.6 1.82) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.6 -1.82) (end -2.6 -1.82) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.15 1.6) (end 3.15 1.6) (layer B.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end 3.15 -1.6) (layer B.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end -3.15 -1.6) (layer B.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end -3.15 1.6) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 3.1 0) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 239 "Net-(C1601-Pad2)"))
    (pad 1 smd rect (at -3.1 0) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FC6) (tstamp 5BB8D6F4)
    (at 121.285 46.24 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BE4C)
    (attr smd)
    (fp_text reference R917 (at 0.9405 -2.159) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 246 /uC/~Reset_ISP))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77) (tstamp 5BBFD60B)
    (at 220.6534 39.116 180)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /5BC18D95/5BBF235B)
    (attr smd)
    (fp_text reference U1603 (at -0.6314 -2.5908) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 24AA32A (at 0 -2.55 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.325 1.525) (end -3.675 1.525) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.325 -1.625) (end 2.325 -1.625) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.325 1.625) (end 2.325 1.625) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.325 -1.625) (end -2.325 -1.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.325 -1.625) (end 2.325 -1.425) (layer B.SilkS) (width 0.15))
    (fp_line (start 2.325 1.625) (end 2.325 1.425) (layer B.SilkS) (width 0.15))
    (fp_line (start -2.325 1.625) (end -2.325 1.525) (layer B.SilkS) (width 0.15))
    (fp_line (start -3.95 -1.8) (end 3.95 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 1.8) (end 3.95 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 3.95 1.8) (end 3.95 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.95 1.8) (end -3.95 -1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.2 0.5) (end -1.2 1.5) (layer B.Fab) (width 0.15))
    (fp_line (start -2.2 -1.5) (end -2.2 0.5) (layer B.Fab) (width 0.15))
    (fp_line (start 2.2 -1.5) (end -2.2 -1.5) (layer B.Fab) (width 0.15))
    (fp_line (start 2.2 1.5) (end 2.2 -1.5) (layer B.Fab) (width 0.15))
    (fp_line (start -1.2 1.5) (end 2.2 1.5) (layer B.Fab) (width 0.15))
    (pad 8 smd rect (at 2.95 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 238 "Net-(R1604-Pad1)"))
    (pad 7 smd rect (at 2.95 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 230 "Net-(R1603-Pad1)"))
    (pad 6 smd rect (at 2.95 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.95 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.95 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.95 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.95 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 239 "Net-(C1601-Pad2)"))
    (pad 1 smd rect (at -2.95 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BBF40DB)
    (at 225.171 33.655 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBE487C)
    (attr smd)
    (fp_text reference C1601 (at 0.2032 -1.2954 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 239 "Net-(C1601-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BBF2828)
    (at 72.1106 35.2044 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBDEE86)
    (attr smd)
    (fp_text reference R1603 (at -1.5494 -5.4864) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0R (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 230 "Net-(R1603-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 222 "Net-(R1603-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BBF2817)
    (at 72.1106 33.782 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBDFF6A)
    (attr smd)
    (fp_text reference R1604 (at -1.524 -5.5372 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0R (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 231 "Net-(R1604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 238 "Net-(R1604-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Axial Connector SMD:U.FL Coaxial Connector" (layer B.Cu) (tedit 5BB8ACB6) (tstamp 5BBD2D4F)
    (at 60.9092 31.62 270)
    (path /5BC18D95/5BBCE948)
    (fp_text reference J1602 (at 3 0 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Antenna_Conc (at 0 -3.25 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.75 1.75) (end 1.75 1.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.75 -1.75) (end 0.75 -1.75) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.75 1.75) (end -1.75 1.25) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -0.75 -1.75) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.75 -1.75) (end 1.75 -1.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 1.75 1.75) (end -1.75 1.75) (layer B.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.25) (end -1.75 -1.75) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.4 0 180) (size 2.25 1.1) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 1.4 0 180) (size 2.25 1.1) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0 -1.55 270) (size 1.1 1.1) (layers B.Cu B.Paste B.Mask)
      (net 236 "Net-(J1602-Pad2)"))
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC22664)
    (at 58.7375 29.2227 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BC4266E)
    (attr smd)
    (fp_text reference R1602 (at -0.0635 4.7625 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 0R (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 237 "Net-(L1601-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 236 "Net-(J1602-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7BA2F)
    (at 118.9235 46.99 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BA78)
    (attr smd)
    (fp_text reference R913 (at -3.06 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R913-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 246 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 5BB890DB) (tstamp 5BBC5F2A)
    (at 71.7686 41.2496)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BC18D95/5BBAE28A)
    (attr smd)
    (fp_text reference D1602 (at 1.6755 -1.397) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value D (at 0 -1.4) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.3 0.57) (end 0.8 0.57) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.57) (end 0.8 -0.57) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.45) (end 0.8 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.45) (end 0.8 -0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.45) (end -0.8 -0.45) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.45) (end -0.8 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end -0.1 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end 0.2 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0.2) (end -0.1 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer B.Fab) (width 0.1))
    (fp_line (start 1.4 0.67) (end -1.4 0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.67) (end -1.4 -0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.67) (end 1.4 -0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.67) (end 1.4 0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.57) (end -1.3 -0.57) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 1.4) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 240 "Net-(D1602-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BBACEA1)
    (at 72.136 26.416 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BB9A675)
    (attr smd)
    (fp_text reference R1606 (at 3.6068 0.0254 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value "10k (wenns nicht läuft anpassen! siehe datenblatt)" (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 232 "Net-(R1606-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BBA9425)
    (at 72.8606 36.6776)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA317C)
    (attr smd)
    (fp_text reference C1604 (at 0.901 6.5786) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BBA9414)
    (at 216.027 33.528 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA3100)
    (attr smd)
    (fp_text reference C1605 (at 0.7366 2.9972 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 58AA84B8) (tstamp 5BBA8E72)
    (at 64.159 40.259 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /5BC18D95/5BB9F9F1)
    (attr smd)
    (fp_text reference C1602 (at 0 1.75 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10uF (at 0 -2 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.25 -1.05) (end -2.25 -1.05) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.05) (end 2.25 1.05) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.25 1.05) (end -2.25 -1.05) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.25 1.05) (end 2.25 1.05) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 -1.02) (end 1 -1.02) (layer B.SilkS) (width 0.12))
    (fp_line (start 1 1.02) (end -1 1.02) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_0603 (layer B.Cu) (tedit 58307A47) (tstamp 5BC226C4)
    (at 58.7375 27.6987 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBA9401)
    (attr smd)
    (fp_text reference L1601 (at -0.127 4.5085 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 27uH (at 0 -1.9 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.3 0.8) (end 1.3 -0.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end -1.3 -0.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 233 "Net-(L1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 237 "Net-(L1601-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BBA84E2)
    (at 240.919 42.545)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BC18D95/5BB8AC9C)
    (attr smd)
    (fp_text reference D1601 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.55) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D1601-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC22694)
    (at 58.7375 26.1747 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBA78F0)
    (attr smd)
    (fp_text reference R1607 (at 0 4.2545 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 22R (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 233 "Net-(L1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 234 "Net-(R1607-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SSOP:VSSOP-8_2.3x2mm_Pitch0.5mm (layer B.Cu) (tedit 589DBB26) (tstamp 5BC37DF2)
    (at 72.378 30.353 90)
    (descr "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (tags "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (path /5BC18D95/5BB99F1D)
    (attr smd)
    (fp_text reference U1602 (at 3.1496 2.9076 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value TXB0102DCT (at 0 -2.2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.1)) (justify mirror))
    )
    (fp_line (start 1.15 1) (end 1.15 -1) (layer B.Fab) (width 0.1))
    (fp_line (start 1.15 -1) (end -1.15 -1) (layer B.Fab) (width 0.1))
    (fp_line (start -1.15 -1) (end -1.15 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start -0.6 1) (end 1.15 1) (layer B.Fab) (width 0.1))
    (fp_line (start -0.6 1) (end -1.15 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 1.1 1.1) (end -1.9 1.1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.1 -1.1) (end -1.1 -1.1) (layer B.SilkS) (width 0.12))
    (fp_line (start 2.25 1.25) (end 2.25 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.25 -1.25) (end -2.25 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.25) (end -2.25 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.25 1.25) (end 2.25 1.25) (layer B.CrtYd) (width 0.05))
    (pad 8 smd rect (at 1.55 0.75 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 218 Tx))
    (pad 7 smd rect (at 1.55 0.25 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 6 smd rect (at 1.55 -0.25 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 232 "Net-(R1606-Pad1)"))
    (pad 5 smd rect (at 1.55 -0.75 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 228 "Net-(U1601-Pad21)"))
    (pad 4 smd rect (at -1.55 -0.75 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 227 "Net-(U1601-Pad20)"))
    (pad 3 smd rect (at -1.55 -0.25 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (pad 2 smd rect (at -1.55 0.25 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.55 0.75 180) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 209 Rx))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/VSSOP-8_2.3x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBA44BD)
    (at 78.6765 43.93 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BB8A952)
    (attr smd)
    (fp_text reference R1601 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R1601-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5BB758EB) (tstamp 5BB9BB58)
    (at 76.807 68.834)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BBF0332)
    (attr smd)
    (fp_text reference D905 (at 1.933 1.651) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(D905-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BB9B3A5)
    (at 75.057 65.87 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB48B05/5BBEE58A)
    (attr smd)
    (fp_text reference D904 (at -3.005 0.127) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(D904-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D904-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB9AD5A)
    (at 73.025 68.326 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BBF0215)
    (attr smd)
    (fp_text reference R929 (at 0 -1.27 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(D905-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB9AD49)
    (at 73.025 65.52 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BBEE970)
    (attr smd)
    (fp_text reference R928 (at -1.385 1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(D905-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB9ACD8)
    (at 83.935 54.61)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BBF7914)
    (attr smd)
    (fp_text reference R927 (at 0 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 LED_Error))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Encoder:STEC11B01 (layer F.Cu) (tedit 5BB61B4C) (tstamp 5BBFC26E)
    (at 57.15 68.58 90)
    (path /5BBCA088/5BBCA305)
    (fp_text reference SW1501 (at 1.048 11.564999 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Rotary_Encoder_Switch (at 0 7.119999 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -18) (end 1 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -18) (end 1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -29) (end -1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3 -29) (end 3 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -29) (end 3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -28) (end -3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -11) (end -3 -28) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3.5 -11) (end -3.5 -4) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -11) (end -3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -4) (end 3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -6 -4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 4) (end 6 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4) (end -6 4) (layer F.SilkS) (width 0.15))
    (pad B thru_hole circle (at -2.54 -1.27 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 181 "Net-(R1502-Pad1)"))
    (pad C thru_hole circle (at 0 -1.27 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad A thru_hole circle (at 2.54 -1.27 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 180 "Net-(R1501-Pad1)"))
    (pad S2 thru_hole circle (at 2.54 1.27 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 183 Encoder_push))
    (pad S1 thru_hole circle (at -2.54 1.27 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad "" thru_hole circle (at -5.842 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.842 0 90) (size 4 4) (drill 2) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB8AD77)
    (at 174.105 102.2985)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE22E8)
    (attr smd)
    (fp_text reference R205 (at 0 1.45) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB7535A) (tstamp 5BB85CA8)
    (at 174.244 91.186)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E878/5BB7D8C2)
    (attr smd)
    (fp_text reference D801 (at 0 1.016) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(D801-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(D801-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB75351) (tstamp 5BB8D34E)
    (at 163.3855 91.2495)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E89F/5BB7D8C2)
    (attr smd)
    (fp_text reference D701 (at 0 1.0795) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(D701-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(D701-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB7533D) (tstamp 5BB85C80)
    (at 145.034 91.186)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3BB9E/5BB7D8C2)
    (attr smd)
    (fp_text reference D601 (at 0 1.016) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(D601-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB75332) (tstamp 5BB85C6C)
    (at 134.239 91.186)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB36AE9/5BB7D8C2)
    (attr smd)
    (fp_text reference D501 (at 0 1.016) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(D501-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D501-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB75368) (tstamp 5BB85C58)
    (at 115.824 91.186)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB32DD3/5BB7D8C2)
    (attr smd)
    (fp_text reference D401 (at 0 1.016) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(D401-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0402 (layer F.Cu) (tedit 5BB75372) (tstamp 5BB85C44)
    (at 104.902 91.186)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB247DF/5BB7D8C2)
    (attr smd)
    (fp_text reference D301 (at 0 1.016) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -0.45) (end 0.5 -0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 0.45) (end 0.5 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -0.2) (end -0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -0.45) (end -0.95 0.45) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(D301-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(D301-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB8C91E)
    (at 97.155 102.235 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB7D968)
    (attr smd)
    (fp_text reference R310 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 204 "Net-(D301-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BCD6)
    (at 109.474 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249DD)
    (attr smd)
    (fp_text reference R301 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BC35)
    (at 120.269 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249DD)
    (attr smd)
    (fp_text reference R401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7BB54)
    (at 107.95 102.235 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB7D968)
    (attr smd)
    (fp_text reference R410 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 203 "Net-(D401-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BB23)
    (at 138.684 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249DD)
    (attr smd)
    (fp_text reference R501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7BB02)
    (at 166.37 102.2985 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB7D968)
    (attr smd)
    (fp_text reference R810 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 202 "Net-(D801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BAC2)
    (at 178.689 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249DD)
    (attr smd)
    (fp_text reference R801 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7BA70)
    (at 155.575 102.2985 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB7D968)
    (attr smd)
    (fp_text reference R710 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 201 "Net-(D701-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7B9FF)
    (at 126.8095 102.223 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB7D968)
    (attr smd)
    (fp_text reference R510 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 200 "Net-(D501-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B9CE)
    (at 149.479 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249DD)
    (attr smd)
    (fp_text reference R601 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7B8ED)
    (at 137.16 102.235 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB7D968)
    (attr smd)
    (fp_text reference R610 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 47R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 199 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B8BC)
    (at 167.894 83.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249DD)
    (attr smd)
    (fp_text reference R701 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B4E8)
    (at 170.307 99.838 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB3E878/5BB7E97A)
    (attr smd)
    (fp_text reference Q801 (at -2.302 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 198 "Net-(D801-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B459)
    (at 159.258 99.838 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB3E89F/5BB7E97A)
    (attr smd)
    (fp_text reference Q701 (at -2.302 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(D701-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B444)
    (at 140.335 99.965 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB3BB9E/5BB7E97A)
    (attr smd)
    (fp_text reference Q601 (at -2.429 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 196 "Net-(D601-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B42F)
    (at 130.1115 100.0285 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB36AE9/5BB7E97A)
    (attr smd)
    (fp_text reference Q501 (at -2.3655 0.0635) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(D501-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B41A)
    (at 111.252 99.965 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB32DD3/5BB7E97A)
    (attr smd)
    (fp_text reference Q401 (at -2.429 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 194 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BB7B405)
    (at 100.5205 100.0285 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BB247DF/5BB7E97A)
    (attr smd)
    (fp_text reference Q301 (at -2.4925 0.0635 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 192 "Net-(D301-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 193 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BC64946)
    (at 173.355 14.48 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB73C46/5BB49533)
    (attr smd)
    (fp_text reference C1202 (at 6.0325 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Buttons_Switches_SMD:SW_DIP_x3_W5.9mm_Slide_Copal_CVS (layer F.Cu) (tedit 5BB63070) (tstamp 5BC2F72F)
    (at 36.9062 39.3192 270)
    (descr "3x-dip-switch, Slide, row spacing 5.9 mm (232 mils), Copal_CVS")
    (tags "DIP Switch Slide 5.9mm 232mil Copal_CVS")
    (path /5BBCA088/5BC054E9)
    (attr smd)
    (fp_text reference SW1503 (at 0 -3.41 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_DIP_x03 (at 0 3.41 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.675 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (fp_line (start 3.8 -2.7) (end -3.8 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.8 2.7) (end 3.8 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.8 2.7) (end 3.8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.8 -2.7) (end -3.8 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 2.41) (end 2.35 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 -2.41) (end 2.35 -2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 0.75) (end 0 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.75) (end -1 0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 1 1.25) (end 1 0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.25) (end 1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.75) (end -1 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -0.25) (end 0 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.25) (end -1 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.25) (end 1 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.25) (end 1 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.25) (end -1 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.25) (end 0 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -1.25) (end -1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.75) (end 1 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.75) (end 1 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.25) (end -1 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.35 -1) (end -1.35 -2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.35 2) (end -2.35 -1) (layer F.Fab) (width 0.1))
    (fp_line (start 2.35 2) (end -2.35 2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.35 -2) (end 2.35 2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.35 -2) (end 2.35 -2) (layer F.Fab) (width 0.1))
    (pad 7 smd rect (at 2.15 2 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.15 2 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.15 -2 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.15 -2 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.95 -1 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 189 Dip_3))
    (pad 3 smd rect (at -2.95 1 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.95 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 190 Dip_2))
    (pad 2 smd rect (at -2.95 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at 2.95 1 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 191 Dip_1))
    (pad 1 smd rect (at -2.95 -1 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_DIP_x3_W5.9mm_Slide_Copal_CVS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC24E31)
    (at 155.321 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBD4644)
    (fp_text reference D201 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 186 "Net-(D201-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 188 "Net-(D201-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC23268)
    (at 126.365 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBEEFA5)
    (fp_text reference D202 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 187 "Net-(D202-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 184 "Net-(D202-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC230E9)
    (at 126.504 84.328 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE40CE)
    (attr smd)
    (fp_text reference R201 (at 0.012 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 Dot))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC23018)
    (at 152.654 87.63 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBD471C)
    (attr smd)
    (fp_text reference R202 (at 0 1.397 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D201-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC22FE7)
    (at 155.46 84.455 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBEEFC9)
    (attr smd)
    (fp_text reference R203 (at 0 1.397 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 Dot))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC22FD6)
    (at 123.825 87.63 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBEEFB2)
    (attr smd)
    (fp_text reference R204 (at 0 1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D202-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC22B05)
    (at 155.321 87.265 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBDEA3D)
    (attr smd)
    (fp_text reference Q201 (at 0 -2.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 185 Dot))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D201-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC22AF0)
    (at 126.365 87.315 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBEEFBB)
    (attr smd)
    (fp_text reference Q202 (at 0 -2.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D202-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 185 Dot))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BB7543D) (tstamp 5BC19A8A)
    (at 79.26 88.9 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BBCA088/5A0B4628)
    (attr smd)
    (fp_text reference R1502 (at 0.647 2.921 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R1502-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 182 Encoder_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC19A7A)
    (at 79.26 90.805 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BBCA088/5A0B465E)
    (attr smd)
    (fp_text reference R1501 (at 0.647 3.556 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 179 Encoder_B))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R1501-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB75445) (tstamp 5BC33049)
    (at 77.458 92.71)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46FC)
    (attr smd)
    (fp_text reference C1501 (at -0.115 3.302) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 179 Encoder_B))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB7544A) (tstamp 5BC33019)
    (at 76.2 101.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46B9)
    (attr smd)
    (fp_text reference C1502 (at -0.115 2.921) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 182 Encoder_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC1566E)
    (at 64.377 85.725)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0DEE19)
    (attr smd)
    (fp_text reference C1503 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 183 Encoder_push))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC14474)
    (at 64.401 91.44 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3FA)
    (attr smd)
    (fp_text reference R1503 (at 0.647 -4.826 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R1502-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC14464)
    (at 64.401 93.345 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3C9)
    (attr smd)
    (fp_text reference R1504 (at 0.647 -4.318 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R1501-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC14454)
    (at 64.401 89.535 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F47F)
    (attr smd)
    (fp_text reference R1505 (at 0.647 -5.334 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 Encoder_push))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89025)
    (at 111.76 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D785)
    (attr smd)
    (fp_text reference R909 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R909-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(R909-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC647FF)
    (at 169.291 26.162 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB73C46/5BB4952F)
    (attr smd)
    (fp_text reference D1202 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BBE7DB5)
    (at 104.9573 94.119204 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB247DF/5BB249BA)
    (fp_text reference U302 (at 7.124204 -4.3733 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Battery_Holders:BatteryHolder_CoinCell_Keystone_3000 (layer F.Cu) (tedit 0) (tstamp 5BBE2D03)
    (at 219.71 21.59 90)
    (descr "Keystone type 3000 coin cell retainer")
    (path /5BB6494F/5BB6519B)
    (fp_text reference BT1101 (at 0 -8.1 90) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_text value Battery_Cell (at 0 6.9 90) (layer F.Fab)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_line (start 0.6096 2.921) (end 1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start 1.8542 3.1496) (end 3.0988 3.6576) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.0988 3.6576) (end 4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.064 4.5212) (end 4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.7244 5.1816) (end 5.2832 5.4356) (layer F.SilkS) (width 0.381))
    (fp_line (start 0 2.8956) (end 0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.064 4.5212) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -5.2832 5.4356) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start -1.8542 3.1496) (end -0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -0.6096 2.921) (end 0 2.8956) (layer F.SilkS) (width 0.381))
    (fp_arc (start 5.2832 4.1148) (end 6.604 4.1148) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_arc (start -5.2832 4.1148) (end -5.2832 5.4356) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_line (start 6.604 -3.429) (end 6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start -6.604 -3.429) (end -6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.0005 -5.969) (end 6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -5.969) (end -6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.9995 -6.731) (end 3.9995 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end -4.0005 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end 4.0005 -6.731) (layer F.SilkS) (width 0.381))
    (pad 1 smd rect (at -7.9 0 90) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 235 V_Bat))
    (pad 1 smd rect (at 7.9 0 90) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 235 V_Bat))
    (pad 2 smd rect (at 0 0 90) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Battery_Holders.3dshapes/BatteryHolder_CoinCell_Keystone_3000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EAE)
    (at 107.95 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB247DF/5BB24A0E)
    (attr smd)
    (fp_text reference R309 (at -4.6355 -0.0635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E8E)
    (at 137.16 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB36AE9/5BB24A0E)
    (attr smd)
    (fp_text reference R509 (at -4.7105 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EEE)
    (at 148.03 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3BB9E/5BB24A0E)
    (attr smd)
    (fp_text reference R609 (at -4.6355 -0.0115 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EDE)
    (at 177.165 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E89F/5BB24A0E)
    (attr smd)
    (fp_text reference R809 (at -4.6355 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6ECE)
    (at 118.745 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB32DD3/5BB24A0E)
    (attr smd)
    (fp_text reference R409 (at -4.647 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E9E)
    (at 166.37 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E878/5BB24A0E)
    (attr smd)
    (fp_text reference R709 (at -4.6355 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.025R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD3416)
    (at 112.28 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BBBEA7E)
    (attr smd)
    (fp_text reference C403 (at -0.012 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD33E5)
    (at 113.55 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB26FB6)
    (attr smd)
    (fp_text reference C402 (at 2.044 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF88)
    (at 113.665 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BBB5EFE)
    (attr smd)
    (fp_text reference U403 (at 0 3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U403-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R411-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF6C)
    (at 142.875 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BBB5EFE)
    (attr smd)
    (fp_text reference U603 (at 0 3.2385 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(R611-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U603-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB97560)
    (at 102.87 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BBB5EFE)
    (attr smd)
    (fp_text reference U303 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U303-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(R311-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEC4)
    (at 172.085 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BBB5EFE)
    (attr smd)
    (fp_text reference U703 (at -0.0635 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(R711-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U703-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEA8)
    (at 161.29 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BBB5EFE)
    (attr smd)
    (fp_text reference U803 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U803-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R811-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEE1C)
    (at 132.08 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BBB5EFE)
    (attr smd)
    (fp_text reference U503 (at 0 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(R511-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U503-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532) (tstamp 5BC970B3)
    (at 126.365 48.753 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (path /5BB48B05/5BB4F230)
    (attr smd)
    (fp_text reference J901 (at 5.207 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.9 -4.35) (end -5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.9 4.35) (end 5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 4.35) (end 5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 -4.35) (end -5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 0.76) (end 2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 0.76) (end -2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -1.78) (end 2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.78) (end -2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 3.3) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.3) (end -2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -3.87) (end 2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.04 -3.3) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.87) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end 2.6 -3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.6 2.86) (end 2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 2.22) (end 3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 2.22) (end 3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.86) (end -2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.22) (end -3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 2.22) (end -3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 0.32) (end 2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -0.32) (end 3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -0.32) (end 3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 0.32) (end -2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -0.32) (end -3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -0.32) (end -3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.22) (end 2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.86) (end 3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -2.86) (end 3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.22) (end -2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.86) (end -3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -3.81) (end 2.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -1.59 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 3.81) (end -2.54 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -1.59 -3.81) (end 2.54 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end -2.54 3.81) (layer F.Fab) (width 0.1))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 246 /uC/~Reset_ISP))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 243 /uC/MOSI_ISP))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 245 /uC/clk_ISP))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 244 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC6429E)
    (at 171.45 33.942 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49527)
    (attr smd)
    (fp_text reference C1204 (at 5.4915 1.143) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Kippschalter:B12AV (layer F.Cu) (tedit 5BB5DE12) (tstamp 5BBAFE9F)
    (at 101.6 28.575)
    (path /5BB7D616/5BB7EDAF)
    (fp_text reference SW1401 (at -7.8105 -4.826) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_SPDT (at -9.5 5.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7 -4) (end 7 1) (layer F.SilkS) (width 0.15))
    (fp_line (start 7 -4) (end -11.75 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -4) (end -11.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 4) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -1.25) (end -21.75 -1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 -1.25) (end -21.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 1.25) (end -11.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start 7 1) (end -0.75 1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.75 1) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (pad "" thru_hole rect (at -5.08 1.27) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" thru_hole rect (at -5.08 -1.27) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 151 +12V))
    (pad 2 thru_hole circle (at 2.53 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 168 "Net-(D1401-Pad1)"))
    (pad 1 thru_hole circle (at 5.08 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 167 "Net-(SW1401-Pad1)"))
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB983B0)
    (at 237.49 43.97 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5BB9689B)
    (attr smd)
    (fp_text reference D1304 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 223 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Fuse Holder:Nano Fuse Holder" (layer F.Cu) (tedit 5BB4B4A4) (tstamp 5BB8397E)
    (at 96.33 20.32)
    (path /5BB7D616/5BB7D87A)
    (fp_text reference F1401 (at -3.25 -3.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 0.5 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.5 -2.5) (end 5.5 -2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 -2.5) (end 5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 2.5) (end -5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.5 2.5) (end -5.5 -2.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4 0 90) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(D1401-Pad1)"))
    (pad 2 smd rect (at 4 0 90) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(F1401-Pad2)"))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E14) (tstamp 5BB763E2)
    (at 93.345 12.065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB8682A)
    (fp_text reference MH1401 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E06) (tstamp 5BB7BA9E)
    (at 186.055 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB86916)
    (fp_text reference MH1402 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60F0C) (tstamp 5BC63C85)
    (at 93.472 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868BC)
    (fp_text reference MH1403 (at 0 -3.048 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E19) (tstamp 5BB763CA)
    (at 185.42 12.065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868ED)
    (fp_text reference MH1404 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BB66FA0)
    (at 123.952 24.386 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB7D616/5BB7DD24)
    (attr smd)
    (fp_text reference C1402 (at 0 5.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (fp_text user + (at -2.27 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BB66F84)
    (at 123.952 14.734 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB7D616/5BB7F33C)
    (attr smd)
    (fp_text reference C1401 (at -0.002 3.175 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB669BC)
    (at 52.07 47.625)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB7D616/5BB7DDC7)
    (attr smd)
    (fp_text reference C1403 (at 0 1.397) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5BB5DBAF) (tstamp 5BB853D5)
    (at 109.855 22.86 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5BB7D616/5BB7D6F8)
    (fp_text reference J1401 (at 2.794 -0.507 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.8 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 169 "Net-(F1401-Pad2)"))
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BB85027)
    (at 101.6 14.36)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB7D616/5BB7D945)
    (attr smd)
    (fp_text reference D1401 (at 0 -3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(D1401-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB6128D) (tstamp 5BC6451E)
    (at 141.744 13.5128 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB5DF23)
    (attr smd)
    (fp_text reference C1306 (at -1.131 -1.3462 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4) (tstamp 5BC644E0)
    (at 145.6985 16.256 180)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BB8D2EE/5BB6A6ED)
    (attr smd)
    (fp_text reference D1303 (at -1.3675 1.397) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_2.5VPSU_off_red (at 0 1.7 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -0.8) (end 1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1 0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.65) (end 1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.65) (end 1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.65) (end -1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.65) (end -1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end -0.1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end 0.2 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 -0.2) (end -0.1 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.88) (end 1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -0.88) (end 1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 0.88) (end -1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 0.88) (end -1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D1303-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB61283) (tstamp 5BC644A9)
    (at 144.2052 12.7628 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5CFDD)
    (attr smd)
    (fp_text reference R1304 (at 2.4758 -1.2032 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 enable_3.3V_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB612A8) (tstamp 5BC64479)
    (at 141.744 11.938 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5D0B6)
    (attr smd)
    (fp_text reference R1305 (at 2.171 1.651 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64449)
    (at 139.815 19.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5A81D)
    (attr smd)
    (fp_text reference R1306 (at -2.401 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64419)
    (at 139.815 15.24)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB71DFD)
    (attr smd)
    (fp_text reference R1308 (at -2.401 -3.7465) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643E9)
    (at 140.015 17.272)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB57E62)
    (attr smd)
    (fp_text reference R1307 (at -2.601 -4.572) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(Q1302-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC643B1)
    (at 146.746 12.446 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB59C86)
    (attr smd)
    (fp_text reference Q1301 (at 2.286 0.447 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB610FE) (tstamp 5BC64375)
    (at 143.195 19.05 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB57D85)
    (attr smd)
    (fp_text reference Q1302 (at -2.286 -0.066 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BC850 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 219 "/3_3V PSU/MC34063_Feedback"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(Q1302-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB61104) (tstamp 5BC64339)
    (at 146.7485 19.05 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB6719E)
    (attr smd)
    (fp_text reference Q1303 (at -2.286 0.127 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D1303-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC642EF)
    (at 158.115 13.81 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/59D46505)
    (attr smd)
    (fp_text reference C1304 (at 5.6185 0 -180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 241 "/3_3V PSU/MC34063_HC_A"))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BC646BB)
    (at 132.715 14.73 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB8D2EE/5BB80A8D)
    (attr smd)
    (fp_text reference C1302 (at 0.887 -3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC647C7)
    (at 137.795 18.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB81889)
    (attr smd)
    (fp_text reference C1301 (at 1.0915 -1.7145 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64680)
    (at 155.829 20.066 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB49531)
    (attr smd)
    (fp_text reference C1305 (at 1.9805 -1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 241 "/3_3V PSU/MC34063_HC_A"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC64640)
    (at 163.957 6.858 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5AAD3380)
    (attr smd)
    (fp_text reference D1302 (at 1.425 -1.778 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_2.7V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC64BC7)
    (at 151.765 16.935 90)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB8D2EE/5BB85821)
    (attr smd)
    (fp_text reference RV1301 (at -4.87 1.016 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 156 "Net-(R1302-Pad2)"))
    (pad 2 smd rect (at -2.75 0 90) (size 2 1.3) (layers F.Cu F.Mask)
      (net 219 "/3_3V PSU/MC34063_Feedback"))
    (pad 1 smd rect (at 2.75 -1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 157 "Net-(R1303-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC649BC)
    (at 150.495 11.115 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB4952A)
    (attr smd)
    (fp_text reference R1303 (at 3.6855 -7.8105 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BB6113F) (tstamp 5BC6498C)
    (at 153.035 11.115 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB49529)
    (attr smd)
    (fp_text reference R1302 (at -3.1115 0.6985 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 27k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R1302-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 210 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BB611A5) (tstamp 5BC64707)
    (at 132.715 24.205 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB8D2EE/59D44D00)
    (attr smd)
    (fp_text reference R1301 (at 3.3135 -2.667 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64B84)
    (at 181.61 29.6545)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49524)
    (attr smd)
    (fp_text reference C1203 (at 0.8255 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 83pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1203-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BC64CDE)
    (at 185.665 30.48 90)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB73C46/59D454FD)
    (attr smd)
    (fp_text reference D1201 (at -1.397 2.9845 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SB350 (at 0 3.1 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64B24)
    (at 173.355 24.5745 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB73C46/5BB49521)
    (attr smd)
    (fp_text reference R1201 (at 0 -2.413 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC64ADC)
    (at 179.07 24.5745 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB73C46/5BB74814)
    (attr smd)
    (fp_text reference U1201 (at 0 -3.302 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1203-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(RV1201-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC64A88)
    (at 138.43 24.605 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB8D2EE/5BB49532)
    (attr smd)
    (fp_text reference U1301 (at 0 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 219 "/3_3V PSU/MC34063_Feedback"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1303-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 229 "/3_3V PSU/SwE"))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 268 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64A4C)
    (at 180.455 17.5895)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49534)
    (attr smd)
    (fp_text reference C1201 (at -0.496 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64A1C)
    (at 175.26 37.9095 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB47F9D)
    (attr smd)
    (fp_text reference C1205 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64B54)
    (at 179.705 19.4945)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D46945)
    (attr smd)
    (fp_text reference R1202 (at 0.254 -3.3655) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R1202-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB8D7D8)
    (at 225.298 35.548 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CF46)
    (attr smd)
    (fp_text reference R925 (at 3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FBD) (tstamp 5BB8D7A8)
    (at 218.186 35.56 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CFEE)
    (attr smd)
    (fp_text reference R926 (at 2.667 -0.254 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB8D778)
    (at 225.2726 32.8034 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB6494F/5BB64C0D)
    (attr smd)
    (fp_text reference C1101 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB8D730)
    (at 221.742 35.814 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB6494F/5BB64ADA)
    (attr smd)
    (fp_text reference U1101 (at -4.445 -0.0635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS3231MZ (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 235 V_Bat))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U1101-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U1101-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U1101-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA9D)
    (at 105.918 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60B72)
    (attr smd)
    (fp_text reference R919 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R919-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D64)
    (at 120.142 34.1884 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63D55)
    (attr smd)
    (fp_text reference R920 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 209 Rx))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R920-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89406)
    (at 87.515 40.259)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DF5)
    (attr smd)
    (fp_text reference R922 (at -3.1235 -0.0635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R922-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 Dip_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB893D6)
    (at 87.515 41.656)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DFC)
    (attr smd)
    (fp_text reference R923 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 Dip_2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R923-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB893A6)
    (at 87.515 43.053)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CA3)
    (attr smd)
    (fp_text reference R924 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R924-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 Dip_1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7BBCC)
    (at 114.554 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60C0B)
    (attr smd)
    (fp_text reference R918 (at -3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 179 Encoder_B))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R918-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D34)
    (at 118.745 34.1884 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CF7)
    (attr smd)
    (fp_text reference R921 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R921-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 Tx))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC7AFB9)
    (at 97.282 45.478 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A35B)
    (attr smd)
    (fp_text reference C901 (at 3.187 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(C901-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19AE4) (tstamp 5BB89244)
    (at 118.3005 44.8945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A26C)
    (attr smd)
    (fp_text reference C902 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB89214)
    (at 98.679 44.069 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB39CC9)
    (attr smd)
    (fp_text reference C903 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB891E4)
    (at 123.2662 38.7484 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A69F)
    (attr smd)
    (fp_text reference C904 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19B2A) (tstamp 5BB891B4)
    (at 123.2662 42.1506 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A72A)
    (attr smd)
    (fp_text reference C905 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB397FA)
    (at 132.207 45.72 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E76)
    (attr smd)
    (fp_text reference D901 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 244 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B99F)
    (at 118.9235 48.387 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E2)
    (attr smd)
    (fp_text reference R906 (at -3.2505 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 245 /uC/clk_ISP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R906-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA6D)
    (at 103.124 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC50B36)
    (attr smd)
    (fp_text reference R907 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R907-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89055)
    (at 113.157 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D7AF)
    (attr smd)
    (fp_text reference R908 (at -3.1235 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 284 "Net-(R908-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R908-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88FF5)
    (at 110.363 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D75D)
    (attr smd)
    (fp_text reference R910 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(R910-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R910-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88FC5)
    (at 104.66 34.163 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D737)
    (attr smd)
    (fp_text reference R911 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R911-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F95)
    (at 106.045 34.163 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D711)
    (attr smd)
    (fp_text reference R912 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R912-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F35)
    (at 87.515 44.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB43320)
    (attr smd)
    (fp_text reference R901 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 LED_Error))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R901-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F05)
    (at 115.951 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E7E0)
    (attr smd)
    (fp_text reference R915 (at 0.0254 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 Encoder_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC1B239) (tstamp 5BC7AA3D)
    (at 104.521 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB4E3C2)
    (attr smd)
    (fp_text reference R916 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 enable_2.5V_PSU))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D04)
    (at 117.348 34.1764 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E361)
    (attr smd)
    (fp_text reference R914 (at -3.048 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 183 Encoder_push))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24F28)
    (at 175.259 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BB249C1)
    (attr smd)
    (fp_text reference U801 (at -0.001 7.62 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 127 MOSI))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B5BB)
    (at 142.99 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB26FB6)
    (attr smd)
    (fp_text reference C602 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BBE33C9)
    (at 162.559 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BB249C1)
    (attr smd)
    (fp_text reference U701 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B4CB)
    (at 102.87 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB26FB6)
    (attr smd)
    (fp_text reference C302 (at 2.159 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B49B)
    (at 101.485 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BBBEA7E)
    (attr smd)
    (fp_text reference C303 (at -0.012 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608EF) (tstamp 5BB40D60)
    (at 120.789 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2618D)
    (attr smd)
    (fp_text reference C401 (at -0.242 -1.3335 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60CBD) (tstamp 5BB41A2A)
    (at 140.474 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2618D)
    (attr smd)
    (fp_text reference C501 (at -0.242 -1.2065 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B3DB)
    (at 132.195 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB26FB6)
    (attr smd)
    (fp_text reference C502 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA2D)
    (at 130.695 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BBBEA7E)
    (attr smd)
    (fp_text reference C503 (at 0.0515 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60E26) (tstamp 5BB3A3E6)
    (at 149.999 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2618D)
    (attr smd)
    (fp_text reference C601 (at -0.3055 -1.2065 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABB6)
    (at 141.49 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BBBEA7E)
    (attr smd)
    (fp_text reference C603 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DA1) (tstamp 5BB3A3A6)
    (at 169.684 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2618D)
    (attr smd)
    (fp_text reference C701 (at -0.242 -1.27 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD8FE6)
    (at 161.29 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB26FB6)
    (attr smd)
    (fp_text reference C702 (at 2.159 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA96)
    (at 159.905 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BBBEA7E)
    (attr smd)
    (fp_text reference C703 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DE8) (tstamp 5BB39F86)
    (at 179.209 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2618D)
    (attr smd)
    (fp_text reference C801 (at -0.3055 -1.27 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608D4) (tstamp 5BB39E36)
    (at 111.264 78.74 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2618D)
    (attr smd)
    (fp_text reference C301 (at -0.369 -1.27) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABE6)
    (at 171.97 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB26FB6)
    (attr smd)
    (fp_text reference C802 (at 2.044 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39C36)
    (at 170.7 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BBBEA7E)
    (attr smd)
    (fp_text reference C803 (at 0 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256FF)
    (at 108.204 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249D6)
    (attr smd)
    (fp_text reference R302 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256EE)
    (at 106.934 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249CF)
    (attr smd)
    (fp_text reference R303 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256DD)
    (at 105.664 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249C8)
    (attr smd)
    (fp_text reference R304 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256CC)
    (at 104.394 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F9)
    (attr smd)
    (fp_text reference R305 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256BB)
    (at 103.124 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F2)
    (attr smd)
    (fp_text reference R306 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB256AA)
    (at 101.854 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249EB)
    (attr smd)
    (fp_text reference R307 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25699)
    (at 100.584 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249E4)
    (attr smd)
    (fp_text reference R308 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25622)
    (at 118.999 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249D6)
    (attr smd)
    (fp_text reference R402 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25611)
    (at 117.729 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249CF)
    (attr smd)
    (fp_text reference R403 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25600)
    (at 116.459 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249C8)
    (attr smd)
    (fp_text reference R404 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2559A)
    (at 115.189 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F9)
    (attr smd)
    (fp_text reference R405 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25589)
    (at 169.6085 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249E4)
    (attr smd)
    (fp_text reference R808 (at -3.314 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25578)
    (at 170.954 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249EB)
    (attr smd)
    (fp_text reference R807 (at -3.314 -0.012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25567)
    (at 172.224 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F2)
    (attr smd)
    (fp_text reference R806 (at 3.2265 -0.012 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25556)
    (at 173.609 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F9)
    (attr smd)
    (fp_text reference R805 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25545)
    (at 174.879 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249C8)
    (attr smd)
    (fp_text reference R804 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25534)
    (at 176.149 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249CF)
    (attr smd)
    (fp_text reference R803 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25523)
    (at 177.419 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249D6)
    (attr smd)
    (fp_text reference R802 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB254AC)
    (at 113.919 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F2)
    (attr smd)
    (fp_text reference R406 (at 3.29 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2549B)
    (at 159.004 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249E4)
    (attr smd)
    (fp_text reference R708 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2548A)
    (at 160.274 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249EB)
    (attr smd)
    (fp_text reference R707 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25479)
    (at 161.544 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F2)
    (attr smd)
    (fp_text reference R706 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25468)
    (at 162.814 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F9)
    (attr smd)
    (fp_text reference R705 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25457)
    (at 164.084 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249C8)
    (attr smd)
    (fp_text reference R704 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25446)
    (at 165.354 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249CF)
    (attr smd)
    (fp_text reference R703 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25435)
    (at 166.624 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249D6)
    (attr smd)
    (fp_text reference R702 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB253BE)
    (at 112.649 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249EB)
    (attr smd)
    (fp_text reference R407 (at -3.314 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB253AD)
    (at 140.589 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249E4)
    (attr smd)
    (fp_text reference R608 (at -3.314 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2539C)
    (at 141.859 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249EB)
    (attr smd)
    (fp_text reference R607 (at -3.314 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2538B)
    (at 143.129 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F2)
    (attr smd)
    (fp_text reference R606 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2537A)
    (at 144.399 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F9)
    (attr smd)
    (fp_text reference R605 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25369)
    (at 145.669 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249C8)
    (attr smd)
    (fp_text reference R604 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25358)
    (at 146.939 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249CF)
    (attr smd)
    (fp_text reference R603 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25347)
    (at 148.209 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249D6)
    (attr smd)
    (fp_text reference R602 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25303)
    (at 111.379 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249E4)
    (attr smd)
    (fp_text reference R408 (at -3.314 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252BF)
    (at 129.794 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249E4)
    (attr smd)
    (fp_text reference R508 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB252AE)
    (at 131.064 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249EB)
    (attr smd)
    (fp_text reference R507 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2529D)
    (at 132.334 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F2)
    (attr smd)
    (fp_text reference R506 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2528C)
    (at 133.604 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F9)
    (attr smd)
    (fp_text reference R505 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2527B)
    (at 134.874 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249C8)
    (attr smd)
    (fp_text reference R504 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB2526A)
    (at 136.144 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249CF)
    (attr smd)
    (fp_text reference R503 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB25259)
    (at 137.414 83.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249D6)
    (attr smd)
    (fp_text reference R502 (at 3.2265 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FF5)
    (at 104.139 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BB249C1)
    (attr smd)
    (fp_text reference U301 (at 0 7.366 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 /Tubes/IV-9_Tube/Data_out))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FCC)
    (at 116.714 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BB249C1)
    (attr smd)
    (fp_text reference U401 (at 0.763 7.493 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24FA3)
    (at 133.349 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BB249C1)
    (attr smd)
    (fp_text reference U501 (at -0.0645 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BB24F7A)
    (at 146.049 71.12 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BB249C1)
    (attr smd)
    (fp_text reference U601 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB29692)
    (at 115.824 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB32DD3/5BB249BA)
    (fp_text reference U402 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E57)
    (at 134.239 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB36AE9/5BB249BA)
    (fp_text reference U502 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB40647)
    (at 145.034 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3BB9E/5BB249BA)
    (fp_text reference U602 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E2D)
    (at 163.449 94.09267 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E878/5BB249BA)
    (fp_text reference U702 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E18)
    (at 174.244 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E89F/5BB249BA)
    (fp_text reference U802 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text 9-24VDC (at 100.838 10.16 180) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "IV-9 Clock  Max Nowka  10.2018 V1.0 " (at 114.173 108.331) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )

  (segment (start 173.99 94.359) (end 174.244 94.105) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 172.72 95.25) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 173.99 95.25) (end 173.99 94.359) (width 0.35) (layer F.Cu) (net 1) (status 20))
  (segment (start 173.99 97.63) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 176.765 97.63) (end 177.165 97.23) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 173.99 97.63) (end 176.765 97.63) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 165.97 97.63) (end 166.37 97.23) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 163.195 97.63) (end 165.97 97.63) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 163.195 94.34667) (end 163.449 94.09267) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 162.04 95.25) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 163.195 95.25) (end 163.195 94.34667) (width 0.35) (layer F.Cu) (net 2) (status 20))
  (segment (start 163.195 97.63) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 144.94 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 143.74 95.25) (end 144.78 95.25) (width 0.35) (layer F.Cu) (net 3) (status 10))
  (segment (start 144.78 95.25) (end 144.78 97.63) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 147.63 97.63) (end 148.03 97.23) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 94.359) (end 145.034 94.105) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 95.25) (end 144.78 94.359) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 133.985 97.63) (end 136.365 97.63) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.84 97.155) (end 137.16 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.365 97.63) (end 136.84 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 133.985 94.359) (end 134.239 94.105) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 132.945 95.25) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 133.985 95.25) (end 133.985 94.359) (width 0.35) (layer F.Cu) (net 4) (status 20))
  (segment (start 133.985 97.63) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 118.27 97.63) (end 118.745 97.155) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 115.57 97.63) (end 118.27 97.63) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 115.57 94.359) (end 115.824 94.105) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 114.3 95.25) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 95.25) (end 115.57 94.359) (width 0.35) (layer F.Cu) (net 5) (status 20))
  (segment (start 115.57 97.63) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 107.55 97.63) (end 107.95 97.23) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 97.63) (end 107.55 97.63) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 94.359) (end 105.029 94.105) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 103.62 95.25) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 104.775 95.25) (end 104.775 94.359) (width 0.35) (layer F.Cu) (net 6) (status 20))
  (segment (start 104.775 97.63) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 119.634 78.335) (end 120.039 78.74) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 119.634 76.02) (end 119.634 78.335) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.089 75.565) (end 119.634 76.02) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 121.414 75.565) (end 120.089 75.565) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (via (at 120.904 80.645) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 120.039 79.78) (end 120.904 80.645) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.039 78.74) (end 120.039 79.78) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (via (at 138.049 78.994) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 138.049 78.994) (end 136.91763 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.779 75.565) (end 136.144 76.2) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.779 75.565) (end 138.049 75.565) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 136.144 76.2) (end 136.144 78.22037) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.91763 78.994) (end 136.144 78.22037) (width 0.35) (layer F.Cu) (net 7))
  (via (at 108.585 78.994) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 107.514 75.565) (end 106.934 76.145) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.839 75.565) (end 107.514 75.565) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 106.934 77.343) (end 108.585 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.934 76.145) (end 106.934 77.343) (width 0.35) (layer F.Cu) (net 7))
  (via (at 167.005 78.994) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 167.259 78.74) (end 167.005 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.934 78.74) (end 167.259 78.74) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 167.259 75.565) (end 165.934 75.565) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 167.005 78.994) (end 166.243 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 165.354 76.145) (end 165.934 75.565) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 165.354 78.105) (end 165.354 76.145) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.243 78.994) (end 165.354 78.105) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.904 80.645) (end 120.904 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 108.585 78.994) (end 120.904 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 108.839 78.74) (end 108.585 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 110.514 78.74) (end 108.839 78.74) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 138.303 78.74) (end 138.049 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.724 78.74) (end 138.303 78.74) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 148.844 76.145) (end 148.844 78.335) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.424 75.565) (end 148.844 76.145) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.844 78.335) (end 149.249 78.74) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 150.749 75.565) (end 149.424 75.565) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (via (at 150.114 80.645) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 149.249 79.78) (end 150.114 80.645) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.249 78.74) (end 149.249 79.78) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 150.114 80.645) (end 150.114 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 138.049 78.994) (end 150.114 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 178.054 76.145) (end 178.054 78.335) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 178.634 75.565) (end 178.054 76.145) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 178.054 78.335) (end 178.459 78.74) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 179.959 75.565) (end 178.634 75.565) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (via (at 179.324 80.645) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 178.459 79.78) (end 179.324 80.645) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 178.459 78.74) (end 178.459 79.78) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 177.673 78.994) (end 179.324 80.645) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 167.005 78.994) (end 177.673 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 172.255 30.9245) (end 170.815 30.9245) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64DFA) (status 20))
  (segment (start 103.505 103.03) (end 102.235 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 114.3 103.03) (end 113.03 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 102.235 104.775) (end 102.235 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 113.03 104.775) (end 113.03 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 131.445 104.775) (end 131.445 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 131.445 103.03) (end 132.715 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 142.24 104.775) (end 142.24 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 142.24 103.03) (end 143.51 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 160.655 104.775) (end 160.655 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 160.655 103.03) (end 161.925 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 171.45 103.03) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 172.72 103.03) (end 171.45 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (via (at 113.03 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 106.045 106.68) (end 113.03 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 113.03 106.68) (end 113.03 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 102.235 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 102.235 106.68) (end 102.235 105.41) (width 0.35) (layer F.Cu) (net 7))
  (via (at 131.445 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 113.03 106.68) (end 131.445 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 131.445 106.68) (end 131.445 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 142.24 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 131.445 106.68) (end 142.24 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 142.24 106.68) (end 142.24 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 160.655 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 160.655 106.68) (end 160.655 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 160.655 106.68) (end 171.45 106.68) (width 0.35) (layer B.Cu) (net 7))
  (via (at 171.45 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 171.45 106.68) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 153.035 97.79) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 153.035 101.6) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 153.035 97.79) (end 153.035 101.6) (width 0.35) (layer B.Cu) (net 7))
  (via (at 153.035 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 153.035 101.6) (end 153.035 106.68) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 153.035 106.68) (end 160.655 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 142.24 106.68) (end 153.035 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 153.035 97.79) (end 153.035 96.65863) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 153.035 96.65863) (end 150.99137 94.615) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 150.99137 81.52237) (end 150.114 80.645) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 152.454 86.88) (end 152.442 86.868) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 152.654 86.88) (end 152.454 86.88) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 152.442 86.868) (end 150.99137 86.868) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 150.99137 86.868) (end 150.99137 81.52237) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 150.99137 94.615) (end 150.99137 86.868) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 122.555 78.994) (end 122.174 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 120.904 78.994) (end 122.555 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 122.555 78.994) (end 126.365 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 84.455) (end 126.365 81.915) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 123.825 86.88) (end 123.825 84.455) (width 0.35) (layer F.Cu) (net 7) (status 10))
  (segment (start 170.491 27.404) (end 170.773 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E09))
  (segment (start 169.291 27.404) (end 170.491 27.404) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E0C) (status 10))
  (segment (start 170.773 27.686) (end 170.815 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64DFD))
  (segment (start 170.815 30.9245) (end 170.815 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E00) (status 10))
  (segment (start 176.53 19.4945) (end 178.755 19.4945) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E03) (status 20))
  (segment (start 175.895 20.1295) (end 176.53 19.4945) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E06))
  (segment (start 175.895 25.4) (end 175.895 20.1295) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E18))
  (segment (start 172.085 26.035) (end 175.26 26.035) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E1B))
  (segment (start 170.815 27.305) (end 172.085 26.035) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E0F))
  (segment (start 175.26 26.035) (end 175.895 25.4) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E12))
  (segment (start 170.815 27.686) (end 170.815 27.305) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E15))
  (via (at 128.27 78.994) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 128.27 78.994) (end 138.049 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 128.27 80.01) (end 128.27 78.994) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 24.916 39.2176) (end 24.916 40.7416) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 24.916 42.2656) (end 24.916 40.7416) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 179.324 80.645) (end 180.086 81.407) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 180.086 81.407) (end 180.086 86.106) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 126.365 81.915) (end 128.27 80.01) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 126.365 78.994) (end 128.27 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 102.235 105.41) (end 102.235 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 106.045 106.68) (end 102.235 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 180.086 86.106) (end 180.086 83.82) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 180.086 86.106) (end 180.086 84.545) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.823 50.19) (end 107.848 50.165) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 51.265) (end 107.848 50.165) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 52.741) (end 107.848 51.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.339 53.25) (end 107.848 52.741) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.339 53.975) (end 107.339 53.25) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC7AD3F))
  (segment (start 108.648 37.665) (end 108.648 38.765) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.648 35.944) (end 108.648 37.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.954 35.638) (end 108.648 35.944) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.954 34.798) (end 108.954 35.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 117.196 45.265) (end 115.448 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 115.448 45.265) (end 114.348 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 117.5755 45.6445) (end 117.196 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 118.3005 45.6445) (end 117.5755 45.6445) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 114.348 45.265) (end 110.617 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.922 45.265) (end 107.848 45.339) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 110.617 45.265) (end 107.922 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 102.948 43.665) (end 107.719 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 43.794) (end 107.719 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 50.165) (end 107.848 45.847) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 45.847) (end 107.848 45.339) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.719 43.665) (end 107.782 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.648 38.765) (end 108.648 42.799) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 43.599) (end 108.14 43.307) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.14 43.307) (end 108.648 42.799) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 44.323) (end 107.848 43.599) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.782 43.665) (end 108.14 43.307) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 45.847) (end 107.848 44.323) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 44.323) (end 107.848 43.794) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 102.948 43.665) (end 100.053 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.707 43.319) (end 98.679 43.319) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.053 43.665) (end 99.707 43.319) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.015 45.49) (end 121.285 45.49) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 119.8605 45.6445) (end 120.015 45.49) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 118.3005 45.6445) (end 119.8605 45.6445) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.014 75.565) (end 112.014 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 108.839 76.835) (end 112.014 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 112.014 78.74) (end 112.014 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 121.539 76.96) (end 121.414 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 121.539 78.74) (end 121.539 76.96) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 141.224 78.486) (end 141.224 78.867) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 138.049 76.835) (end 141.224 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 141.224 78.486) (end 141.224 77.47) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 141.224 76.835) (end 141.224 76.2) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 112.014 78.486) (end 112.014 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 112.014 78.486) (end 112.014 79.121) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 167.259 76.835) (end 170.434 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 170.434 78.74) (end 170.434 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 170.434 76.835) (end 170.434 75.565) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 157.859 76.835) (end 157.859 75.565) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 128.649 75.565) (end 128.649 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 141.224 78.74) (end 141.224 78.867) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 150.749 78.74) (end 150.749 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 179.959 78.74) (end 179.959 76.835) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 179.959 78.74) (end 179.984 78.74) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 114.3 97.63) (end 113.03 97.63) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 150.749 78.74) (end 151.13 78.74) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 154.71 85.386) (end 154.371 85.725) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 154.71 84.455) (end 154.71 85.386) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 154.371 86.265) (end 154.371 85.725) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 169.54 23.655) (end 169.291 23.904) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E21) (status 30))
  (segment (start 147.6985 20.05) (end 147.6985 20.1) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E1E) (status 30))
  (segment (start 125.415 86.315) (end 125.415 85.405) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 125.477 85.405) (end 125.754 85.128) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 125.754 85.128) (end 125.754 84.328) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (segment (start 125.415 85.405) (end 125.477 85.405) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 128.2573 87.3506) (end 126.4056 87.3506) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 125.415 86.315) (end 125.415 86.365) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 126.4056 87.3506) (end 126.4031 87.3531) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 128.27 87.3633) (end 128.2573 87.3506) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 125.415 86.365) (end 126.4031 87.3531) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (via (at 139.7 64.77) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 8))
  (segment (start 139.573 64.77) (end 139.7 64.643) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 139.573 65.405) (end 139.573 64.77) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 138.049 65.405) (end 139.573 65.405) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 139.573 65.405) (end 141.224 65.405) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (via (at 168.91 64.897) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 168.783 65.024) (end 168.91 64.897) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 167.259 65.405) (end 168.783 65.405) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 168.783 65.405) (end 168.783 65.024) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 168.783 65.405) (end 170.434 65.405) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (segment (start 112.014 65.405) (end 110.49 65.405) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 110.49 65.405) (end 108.839 65.405) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (segment (start 112.014 78.74) (end 112.014 79.121) (width 0.35) (layer F.Cu) (net 8) (status 10))
  (segment (start 141.224 76.2) (end 141.224 75.565) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (segment (start 141.224 77.47) (end 141.224 76.835) (width 0.35) (layer F.Cu) (net 8) (status 20))
  (segment (start 140.565 27.535) (end 140.335 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E6F))
  (segment (start 140.565 29.21) (end 140.565 27.535) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E63))
  (via (at 142.24 27.305) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC64E87))
  (segment (start 140.335 27.305) (end 142.24 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E7E))
  (segment (start 142.24 25.715) (end 142.24 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D31))
  (segment (start 147.696 20.0475) (end 147.6985 20.05) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D1C))
  (segment (start 147.696 13.446) (end 147.696 20.0475) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D3A))
  (segment (start 140.994 11.938) (end 140.994 13.5128) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E75))
  (segment (start 182.8495 27.2745) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D58))
  (via (at 182.88 27.305) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC64E27))
  (segment (start 180.975 27.2745) (end 182.8495 27.2745) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D52))
  (segment (start 182.36 27.825) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D3D))
  (segment (start 182.36 29.6545) (end 182.36 27.825) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D37))
  (segment (start 183.905 28.33) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D43))
  (segment (start 185.665 28.33) (end 183.905 28.33) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D64))
  (via (at 169.291 20.066) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 169.291 24.412) (end 169.291 20.066) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 169.291 20.066) (end 167.227 20.066) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 53.9) (end 108.573 53.975) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.839 52.959) (end 108.839 53.975) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 52.768) (end 108.839 52.959) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 50.165) (end 108.648 52.768) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.848 35.802) (end 107.848 37.665) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.848 37.665) (end 107.848 38.765) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.569 35.523) (end 107.848 35.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.569 34.798) (end 107.569 35.523) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 118.3005 44.1445) (end 117.463 44.1445) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 117.1425 44.465) (end 114.348 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 117.463 44.1445) (end 117.1425 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 123.2662 41.4006) (end 123.2662 39.4984) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.948 44.465) (end 100.188 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 99.834 44.819) (end 98.679 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 100.188 44.465) (end 99.834 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 97.373 44.819) (end 97.282 44.728) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 98.679 44.819) (end 97.373 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 47.625) (end 90.829 49.022) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 49.022) (end 90.829 50.419) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 51.804) (end 90.817 51.816) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 50.419) (end 90.829 51.804) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 172.974 73.66) (end 172.974 78.625) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 169.799 81.8) (end 169.799 82.55) (width 0.35) (layer F.Cu) (net 9) (status 20))
  (segment (start 172.339 73.025) (end 172.974 73.66) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 78.625) (end 169.799 81.8) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.434 73.025) (end 172.339 73.025) (width 0.35) (layer F.Cu) (net 9) (status 10))
  (segment (start 170.954 81.8) (end 170.954 82.55) (width 0.35) (layer F.Cu) (net 10) (status 20))
  (segment (start 173.609 79.145) (end 170.954 81.8) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 72.39) (end 173.609 79.145) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.974 71.755) (end 173.609 72.39) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 170.434 71.755) (end 172.974 71.755) (width 0.35) (layer F.Cu) (net 10) (status 10))
  (segment (start 172.224 81.915) (end 172.224 82.55) (width 0.35) (layer F.Cu) (net 11) (status 20))
  (segment (start 174.244 79.895) (end 172.224 81.915) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 71.12) (end 174.244 79.895) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 173.609 70.485) (end 174.244 71.12) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 170.434 70.485) (end 173.609 70.485) (width 0.35) (layer F.Cu) (net 11) (status 10))
  (segment (start 173.609 81.8) (end 173.609 82.55) (width 0.35) (layer F.Cu) (net 12) (status 20))
  (segment (start 174.879 80.53) (end 173.609 81.8) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.879 69.85) (end 174.879 80.53) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.244 69.215) (end 174.879 69.85) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 170.434 69.215) (end 174.244 69.215) (width 0.35) (layer F.Cu) (net 12) (status 10))
  (via (at 145.034 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 128.649 67.945) (end 131.064 67.945) (width 0.35) (layer F.Cu) (net 13) (status 10))
  (segment (start 131.699 67.945) (end 132.334 67.31) (width 0.35) (layer F.Cu) (net 13))
  (via (at 132.334 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 132.334 67.31) (end 132.334 62.23) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 132.334 62.23) (end 145.034 62.23) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 112.014 67.945) (end 113.339 67.945) (width 0.35) (layer F.Cu) (net 13) (status 10))
  (segment (start 112.014 67.945) (end 115.189 67.945) (width 0.35) (layer F.Cu) (net 13) (status 10))
  (via (at 115.824 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 115.824 67.31) (end 115.824 62.23) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 115.189 67.945) (end 115.824 67.31) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 115.824 62.23) (end 132.334 62.23) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 99.439 67.945) (end 101.854 67.945) (width 0.35) (layer F.Cu) (net 13) (status 10))
  (segment (start 102.489 67.945) (end 103.124 67.31) (width 0.35) (layer F.Cu) (net 13))
  (via (at 103.124 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 103.124 67.31) (end 103.124 62.23) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 103.124 62.23) (end 115.824 62.23) (width 0.35) (layer B.Cu) (net 13))
  (via (at 161.544 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 145.034 62.23) (end 161.544 62.23) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 161.544 62.23) (end 161.544 67.31) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 160.909 67.945) (end 157.859 67.945) (width 0.35) (layer F.Cu) (net 13) (status 20))
  (segment (start 161.544 67.31) (end 160.909 67.945) (width 0.35) (layer F.Cu) (net 13))
  (via (at 174.244 62.23) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 161.544 62.23) (end 174.244 62.23) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 174.244 62.23) (end 174.244 67.31) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 173.609 67.945) (end 170.434 67.945) (width 0.35) (layer F.Cu) (net 13) (status 20))
  (segment (start 174.244 67.31) (end 173.609 67.945) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 101.854 67.945) (end 102.489 67.945) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 131.064 67.945) (end 131.699 67.945) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 145.034 62.23) (end 145.034 67.31) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 144.399 67.945) (end 141.349 67.945) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 145.034 67.31) (end 144.399 67.945) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 111.633 58.039) (end 115.824 62.23) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 111.633 55.614) (end 111.633 58.039) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 174.879 81.8) (end 175.514 81.165) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 174.879 82.55) (end 174.879 81.8) (width 0.35) (layer F.Cu) (net 14) (status 10))
  (segment (start 175.514 69.85) (end 176.149 69.215) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.514 81.165) (end 175.514 69.85) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 176.149 69.215) (end 179.959 69.215) (width 0.35) (layer F.Cu) (net 14) (status 20))
  (segment (start 176.784 70.485) (end 179.834 70.485) (width 0.35) (layer F.Cu) (net 15) (status 20))
  (segment (start 176.149 71.12) (end 176.784 70.485) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 82.55) (end 176.149 71.12) (width 0.35) (layer F.Cu) (net 15) (status 10))
  (segment (start 177.419 82.55) (end 177.419 81.8) (width 0.35) (layer F.Cu) (net 16) (status 10))
  (segment (start 176.784 81.165) (end 176.784 72.39) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 72.39) (end 177.419 71.755) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 177.419 81.8) (end 176.784 81.165) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 177.419 71.755) (end 179.834 71.755) (width 0.35) (layer F.Cu) (net 16) (status 20))
  (segment (start 178.689 81.8) (end 178.689 82.55) (width 0.35) (layer F.Cu) (net 17) (status 20))
  (segment (start 177.419 73.66) (end 178.054 73.025) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 80.53) (end 177.419 73.66) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.834 73.025) (end 178.054 73.025) (width 0.35) (layer F.Cu) (net 17) (status 10))
  (segment (start 177.419 80.53) (end 178.689 81.8) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 164.084 73.66) (end 164.719 73.025) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.719 73.025) (end 167.259 73.025) (width 0.35) (layer F.Cu) (net 18) (status 20))
  (segment (start 167.894 82.55) (end 167.894 81.8) (width 0.35) (layer F.Cu) (net 18) (status 10))
  (segment (start 167.894 81.8) (end 164.084 77.99) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 77.99) (end 164.084 73.66) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 163.449 78.625) (end 166.624 81.8) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 164.084 71.755) (end 163.449 72.39) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 166.624 81.8) (end 166.624 82.55) (width 0.35) (layer F.Cu) (net 19) (status 20))
  (segment (start 163.449 72.39) (end 163.449 78.625) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 167.259 71.755) (end 164.084 71.755) (width 0.35) (layer F.Cu) (net 19) (status 10))
  (segment (start 165.354 81.8) (end 162.814 79.26) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 165.354 82.55) (end 165.354 81.8) (width 0.35) (layer F.Cu) (net 20) (status 10))
  (segment (start 162.814 79.26) (end 162.814 71.12) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 163.449 70.485) (end 167.259 70.485) (width 0.35) (layer F.Cu) (net 20) (status 20))
  (segment (start 162.814 71.12) (end 163.449 70.485) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.084 81.915) (end 164.084 82.55) (width 0.35) (layer F.Cu) (net 21) (status 20))
  (segment (start 162.179 80.01) (end 164.084 81.915) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 69.85) (end 162.179 80.01) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.814 69.215) (end 162.179 69.85) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 167.259 69.215) (end 162.814 69.215) (width 0.35) (layer F.Cu) (net 21) (status 10))
  (segment (start 160.909 69.215) (end 157.859 69.215) (width 0.35) (layer F.Cu) (net 22) (status 20))
  (segment (start 161.544 69.85) (end 160.909 69.215) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 80.53) (end 161.544 69.85) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 162.814 81.8) (end 161.544 80.53) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 162.814 82.55) (end 162.814 81.8) (width 0.35) (layer F.Cu) (net 22) (status 10))
  (segment (start 161.544 81.8) (end 161.544 82.55) (width 0.35) (layer F.Cu) (net 23) (status 20))
  (segment (start 160.943989 81.199989) (end 161.544 81.8) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 71.154989) (end 160.943989 81.199989) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.274 70.485) (end 160.943989 71.154989) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 157.859 70.485) (end 160.274 70.485) (width 0.35) (layer F.Cu) (net 23) (status 10))
  (segment (start 160.274 82.55) (end 160.274 72.39) (width 0.35) (layer F.Cu) (net 24) (status 10))
  (segment (start 159.639 71.755) (end 157.859 71.755) (width 0.35) (layer F.Cu) (net 24) (status 20))
  (segment (start 160.274 72.39) (end 159.639 71.755) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.004 81.8) (end 159.004 82.55) (width 0.35) (layer F.Cu) (net 25) (status 20))
  (segment (start 159.524 81.28) (end 159.004 81.8) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.184 73.025) (end 159.524 73.365) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 73.365) (end 159.524 81.28) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 157.859 73.025) (end 159.184 73.025) (width 0.35) (layer F.Cu) (net 25) (status 10))
  (segment (start 140.589 81.8) (end 143.764 78.625) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.589 82.55) (end 140.589 81.8) (width 0.35) (layer F.Cu) (net 26) (status 10))
  (segment (start 143.764 78.625) (end 143.764 73.66) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 143.129 73.025) (end 141.224 73.025) (width 0.35) (layer F.Cu) (net 26) (status 20))
  (segment (start 143.764 73.66) (end 143.129 73.025) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 141.224 71.755) (end 143.764 71.755) (width 0.35) (layer F.Cu) (net 27) (status 10))
  (segment (start 143.764 71.755) (end 144.399 72.39) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 141.859 81.8) (end 141.859 82.55) (width 0.35) (layer F.Cu) (net 27) (status 20))
  (segment (start 144.399 79.26) (end 141.859 81.8) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 144.399 72.39) (end 144.399 79.26) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 141.224 70.485) (end 142.549 70.485) (width 0.35) (layer F.Cu) (net 28) (status 10))
  (segment (start 143.129 81.8) (end 145.034 79.895) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.129 82.55) (end 143.129 81.8) (width 0.35) (layer F.Cu) (net 28) (status 10))
  (segment (start 145.034 79.895) (end 145.034 71.12) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 144.399 70.485) (end 141.224 70.485) (width 0.35) (layer F.Cu) (net 28) (status 20))
  (segment (start 145.034 71.12) (end 144.399 70.485) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 144.399 81.8) (end 144.399 82.55) (width 0.35) (layer F.Cu) (net 29) (status 20))
  (segment (start 145.669 80.53) (end 144.399 81.8) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 69.85) (end 145.669 80.53) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.034 69.215) (end 145.669 69.85) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 141.224 69.215) (end 145.034 69.215) (width 0.35) (layer F.Cu) (net 29) (status 10))
  (segment (start 145.669 81.8) (end 146.304 81.165) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 145.669 82.55) (end 145.669 81.8) (width 0.35) (layer F.Cu) (net 30) (status 10))
  (segment (start 146.304 81.165) (end 146.304 69.85) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.939 69.215) (end 150.624 69.215) (width 0.35) (layer F.Cu) (net 30) (status 20))
  (segment (start 146.304 69.85) (end 146.939 69.215) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.939 82.55) (end 146.939 71.12) (width 0.35) (layer F.Cu) (net 31) (status 10))
  (segment (start 147.574 70.485) (end 150.624 70.485) (width 0.35) (layer F.Cu) (net 31) (status 20))
  (segment (start 146.939 71.12) (end 147.574 70.485) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 148.209 81.8) (end 147.574 81.165) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 148.209 82.55) (end 148.209 81.8) (width 0.35) (layer F.Cu) (net 32) (status 10))
  (segment (start 147.574 81.165) (end 147.574 72.39) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 148.209 71.755) (end 150.624 71.755) (width 0.35) (layer F.Cu) (net 32) (status 20))
  (segment (start 147.574 72.39) (end 148.209 71.755) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.479 81.8) (end 148.209 80.53) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 149.479 82.55) (end 149.479 81.8) (width 0.35) (layer F.Cu) (net 33) (status 10))
  (segment (start 148.209 80.53) (end 148.209 73.66) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.844 73.025) (end 150.624 73.025) (width 0.35) (layer F.Cu) (net 33) (status 20))
  (segment (start 148.209 73.66) (end 148.844 73.025) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 138.684 81.8) (end 134.874 77.99) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 138.684 82.55) (end 138.684 81.8) (width 0.35) (layer F.Cu) (net 34) (status 10))
  (segment (start 134.874 77.99) (end 134.874 73.66) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 135.509 73.025) (end 138.049 73.025) (width 0.35) (layer F.Cu) (net 34) (status 20))
  (segment (start 134.874 73.66) (end 135.509 73.025) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 137.414 81.8) (end 134.239 78.625) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 137.414 82.55) (end 137.414 81.8) (width 0.35) (layer F.Cu) (net 35) (status 10))
  (segment (start 134.239 78.625) (end 134.239 72.39) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.874 71.755) (end 138.049 71.755) (width 0.35) (layer F.Cu) (net 35) (status 20))
  (segment (start 134.239 72.39) (end 134.874 71.755) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 70.485) (end 138.049 70.485) (width 0.35) (layer F.Cu) (net 36) (status 20))
  (segment (start 133.604 71.12) (end 134.239 70.485) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 79.26) (end 133.604 71.12) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.144 81.8) (end 133.604 79.26) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.144 82.55) (end 136.144 81.8) (width 0.35) (layer F.Cu) (net 36) (status 10))
  (segment (start 134.874 81.8) (end 132.969 79.895) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 134.874 82.55) (end 134.874 81.8) (width 0.35) (layer F.Cu) (net 37) (status 10))
  (segment (start 132.969 79.895) (end 132.969 69.85) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 133.604 69.215) (end 138.049 69.215) (width 0.35) (layer F.Cu) (net 37) (status 20))
  (segment (start 132.969 69.85) (end 133.604 69.215) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 133.604 81.8) (end 132.334 80.53) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 133.604 82.55) (end 133.604 81.8) (width 0.35) (layer F.Cu) (net 38) (status 10))
  (segment (start 132.334 80.53) (end 132.334 69.85) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 131.699 69.215) (end 128.649 69.215) (width 0.35) (layer F.Cu) (net 38) (status 20))
  (segment (start 132.334 69.85) (end 131.699 69.215) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 81.8) (end 132.334 82.55) (width 0.35) (layer F.Cu) (net 39) (status 20))
  (segment (start 131.699 81.165) (end 132.334 81.8) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 71.12) (end 131.699 81.165) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.064 70.485) (end 131.699 71.12) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 128.649 70.485) (end 131.064 70.485) (width 0.35) (layer F.Cu) (net 39) (status 10))
  (segment (start 131.064 72.39) (end 130.429 71.755) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 130.429 71.755) (end 128.649 71.755) (width 0.35) (layer F.Cu) (net 40) (status 20))
  (segment (start 131.064 82.55) (end 131.064 72.39) (width 0.35) (layer F.Cu) (net 40) (status 10))
  (segment (start 129.794 81.8) (end 130.413989 81.180011) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 129.794 82.55) (end 129.794 81.8) (width 0.35) (layer F.Cu) (net 41) (status 10))
  (segment (start 130.413989 81.180011) (end 130.413989 73.464989) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 73.464989) (end 129.974 73.025) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 129.974 73.025) (end 128.649 73.025) (width 0.35) (layer F.Cu) (net 41) (status 20))
  (segment (start 111.379 81.8) (end 111.379 82.55) (width 0.35) (layer F.Cu) (net 42) (status 20))
  (segment (start 114.554 73.66) (end 114.554 78.625) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 114.554 78.625) (end 111.379 81.8) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.919 73.025) (end 114.554 73.66) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 112.014 73.025) (end 113.919 73.025) (width 0.35) (layer F.Cu) (net 42) (status 10))
  (segment (start 115.189 79.26) (end 112.649 81.8) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 114.554 71.755) (end 115.189 72.39) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 112.649 81.8) (end 112.649 82.55) (width 0.35) (layer F.Cu) (net 43) (status 20))
  (segment (start 115.189 72.39) (end 115.189 79.26) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 112.014 71.755) (end 114.554 71.755) (width 0.35) (layer F.Cu) (net 43) (status 10))
  (segment (start 113.919 81.8) (end 113.919 82.55) (width 0.35) (layer F.Cu) (net 44) (status 20))
  (segment (start 115.824 71.12) (end 115.824 79.895) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.189 70.485) (end 115.824 71.12) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 79.895) (end 113.919 81.8) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 112.014 70.485) (end 115.189 70.485) (width 0.35) (layer F.Cu) (net 44) (status 10))
  (segment (start 115.189 81.8) (end 115.189 82.55) (width 0.35) (layer F.Cu) (net 45) (status 20))
  (segment (start 116.459 69.85) (end 116.459 80.53) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.824 69.215) (end 116.459 69.85) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 80.53) (end 115.189 81.8) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 112.014 69.215) (end 115.824 69.215) (width 0.35) (layer F.Cu) (net 45) (status 10))
  (segment (start 116.459 81.8) (end 117.094 81.165) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 116.459 82.55) (end 116.459 81.8) (width 0.35) (layer F.Cu) (net 46) (status 10))
  (segment (start 117.094 69.85) (end 117.729 69.215) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 81.165) (end 117.094 69.85) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.729 69.215) (end 121.414 69.215) (width 0.35) (layer F.Cu) (net 46) (status 20))
  (segment (start 117.729 71.12) (end 118.364 70.485) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 82.55) (end 117.729 71.12) (width 0.35) (layer F.Cu) (net 47) (status 10))
  (segment (start 118.364 70.485) (end 121.414 70.485) (width 0.35) (layer F.Cu) (net 47) (status 20))
  (segment (start 118.999 81.915) (end 118.999 82.55) (width 0.35) (layer F.Cu) (net 48) (status 20))
  (segment (start 118.364 72.39) (end 118.999 71.755) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 81.28) (end 118.364 72.39) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 121.414 71.755) (end 118.999 71.755) (width 0.35) (layer F.Cu) (net 48) (status 10))
  (segment (start 118.364 81.28) (end 118.999 81.915) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.269 82.55) (end 120.269 81.8) (width 0.35) (layer F.Cu) (net 49) (status 10))
  (segment (start 121.414 73.025) (end 120.269 73.025) (width 0.35) (layer F.Cu) (net 49) (status 10))
  (segment (start 118.999 73.66) (end 119.634 73.025) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 80.53) (end 118.999 73.66) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 120.269 81.8) (end 118.999 80.53) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 119.634 73.025) (end 120.269 73.025) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 105.664 73.66) (end 106.299 73.025) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 106.299 73.025) (end 108.839 73.025) (width 0.35) (layer F.Cu) (net 50) (status 20))
  (segment (start 109.474 81.8) (end 105.664 77.99) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 105.664 77.99) (end 105.664 73.66) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 109.474 82.55) (end 109.474 81.8) (width 0.35) (layer F.Cu) (net 50) (status 10))
  (segment (start 106.934 71.755) (end 108.839 71.755) (width 0.35) (layer F.Cu) (net 51) (status 20))
  (segment (start 105.029 72.39) (end 105.664 71.755) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 78.625) (end 105.029 72.39) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 108.204 81.8) (end 105.029 78.625) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 108.204 82.55) (end 108.204 81.8) (width 0.35) (layer F.Cu) (net 51) (status 10))
  (segment (start 105.664 71.755) (end 106.934 71.755) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 70.485) (end 108.839 70.485) (width 0.35) (layer F.Cu) (net 52) (status 20))
  (segment (start 106.934 81.8) (end 104.394 79.26) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 71.12) (end 105.029 70.485) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 79.26) (end 104.394 71.12) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 106.934 82.55) (end 106.934 81.8) (width 0.35) (layer F.Cu) (net 52) (status 10))
  (segment (start 107.569 69.215) (end 108.839 69.215) (width 0.35) (layer F.Cu) (net 53) (status 20))
  (segment (start 103.759 69.85) (end 104.394 69.215) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 103.759 79.895) (end 103.759 69.85) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 105.664 81.8) (end 103.759 79.895) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 105.664 82.55) (end 105.664 81.8) (width 0.35) (layer F.Cu) (net 53) (status 10))
  (segment (start 104.394 69.215) (end 107.569 69.215) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 104.394 82.55) (end 104.394 81.8) (width 0.35) (layer F.Cu) (net 54) (status 10))
  (segment (start 103.124 80.53) (end 103.124 69.85) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 101.219 69.215) (end 99.439 69.215) (width 0.35) (layer F.Cu) (net 54) (status 20))
  (segment (start 103.124 69.85) (end 102.489 69.215) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 104.394 81.8) (end 103.124 80.53) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 102.489 69.215) (end 101.219 69.215) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.124 82.55) (end 103.124 81.8) (width 0.35) (layer F.Cu) (net 55) (status 10))
  (segment (start 102.489 81.165) (end 102.489 71.12) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.854 70.485) (end 100.584 70.485) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 103.124 81.8) (end 102.489 81.165) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 102.489 71.12) (end 101.854 70.485) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 100.584 70.485) (end 99.439 70.485) (width 0.35) (layer F.Cu) (net 55) (status 20))
  (segment (start 101.219 71.755) (end 99.439 71.755) (width 0.35) (layer F.Cu) (net 56) (status 20))
  (segment (start 101.854 72.39) (end 101.219 71.755) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 101.854 82.55) (end 101.854 72.39) (width 0.35) (layer F.Cu) (net 56) (status 10))
  (segment (start 100.584 73.025) (end 99.439 73.025) (width 0.35) (layer F.Cu) (net 57) (status 20))
  (segment (start 101.219 73.66) (end 100.584 73.025) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 101.219 81.165) (end 101.219 73.66) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 100.584 81.8) (end 101.219 81.165) (width 0.35) (layer F.Cu) (net 57))
  (segment (start 100.584 82.55) (end 100.584 81.8) (width 0.35) (layer F.Cu) (net 57) (status 10))
  (segment (start 171.466915 92.08733) (end 170.44633 92.08733) (width 0.35) (layer F.Cu) (net 58) (status 10))
  (segment (start 169.799 91.44) (end 169.799 90.17) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.44633 92.08733) (end 169.799 91.44) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 169.799 90.17) (end 169.799 84.05) (width 0.35) (layer F.Cu) (net 58) (status 20))
  (segment (start 170.954 89.769755) (end 171.466915 90.28267) (width 0.35) (layer F.Cu) (net 59) (status 30))
  (segment (start 170.954 84.05) (end 170.954 89.769755) (width 0.35) (layer F.Cu) (net 59) (status 30))
  (segment (start 172.224 88.519003) (end 172.527667 88.82267) (width 0.35) (layer F.Cu) (net 60) (status 30))
  (segment (start 172.224 84.05) (end 172.224 88.519003) (width 0.35) (layer F.Cu) (net 60) (status 30))
  (segment (start 173.609 84.05) (end 173.609 85.725) (width 0.35) (layer F.Cu) (net 61) (status 10))
  (segment (start 174.244 86.36) (end 174.244 88.265) (width 0.35) (layer F.Cu) (net 61) (status 20))
  (segment (start 173.609 85.725) (end 174.244 86.36) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 174.879 84.05) (end 174.879 85.09) (width 0.35) (layer F.Cu) (net 62) (status 10))
  (segment (start 175.960333 86.171333) (end 175.960333 88.82267) (width 0.35) (layer F.Cu) (net 62) (status 20))
  (segment (start 174.879 85.09) (end 175.960333 86.171333) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 177.664828 89.638927) (end 177.021085 90.28267) (width 0.35) (layer F.Cu) (net 63) (status 30))
  (segment (start 177.664828 86.315828) (end 177.664828 89.638927) (width 0.35) (layer F.Cu) (net 63) (status 20))
  (segment (start 176.149 84.8) (end 177.664828 86.315828) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 176.149 84.05) (end 176.149 84.8) (width 0.35) (layer F.Cu) (net 63) (status 10))
  (segment (start 178.689 86.07) (end 177.419 84.8) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 178.689 91.44) (end 178.689 86.07) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 178.04167 92.08733) (end 178.689 91.44) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 177.419 84.8) (end 177.419 84.05) (width 0.35) (layer F.Cu) (net 64) (status 20))
  (segment (start 177.021085 92.08733) (end 178.04167 92.08733) (width 0.35) (layer F.Cu) (net 64) (status 10))
  (segment (start 178.689 84.8) (end 178.689 84.05) (width 0.35) (layer F.Cu) (net 65) (status 20))
  (segment (start 179.324 85.435) (end 178.689 84.8) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 177.85167 93.54733) (end 179.324 92.075) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.324 92.075) (end 179.324 85.435) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 175.960333 93.54733) (end 177.85167 93.54733) (width 0.35) (layer F.Cu) (net 65) (status 10))
  (segment (start 167.259 93.535) (end 165.165333 93.535) (width 0.35) (layer F.Cu) (net 66) (status 20))
  (segment (start 168.619 92.175) (end 167.259 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.619 85.525) (end 168.619 92.175) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.894 84.8) (end 168.619 85.525) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.894 84.05) (end 167.894 84.8) (width 0.35) (layer F.Cu) (net 66) (status 10))
  (segment (start 166.624 84.8) (end 166.624 84.05) (width 0.35) (layer F.Cu) (net 67) (status 20))
  (segment (start 167.894 86.07) (end 166.624 84.8) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.894 91.44) (end 167.894 86.07) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.259 92.075) (end 167.894 91.44) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 92.075) (end 167.259 92.075) (width 0.35) (layer F.Cu) (net 67) (status 10))
  (segment (start 165.354 84.05) (end 165.354 85.09) (width 0.35) (layer F.Cu) (net 68) (status 10))
  (segment (start 166.869828 89.626597) (end 166.226085 90.27034) (width 0.35) (layer F.Cu) (net 68) (status 30))
  (segment (start 166.869828 86.605828) (end 166.869828 89.626597) (width 0.35) (layer F.Cu) (net 68) (status 20))
  (segment (start 165.354 85.09) (end 166.869828 86.605828) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.084 84.05) (end 164.084 85.725) (width 0.35) (layer F.Cu) (net 69) (status 10))
  (segment (start 165.165333 86.806333) (end 165.165333 88.81034) (width 0.35) (layer F.Cu) (net 69) (status 20))
  (segment (start 164.084 85.725) (end 165.165333 86.806333) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 162.814 84.8) (end 162.814 84.05) (width 0.35) (layer F.Cu) (net 70) (status 20))
  (segment (start 163.449 87.05267) (end 162.814 86.41767) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 163.449 88.25267) (end 163.449 87.05267) (width 0.35) (layer F.Cu) (net 70) (status 10))
  (segment (start 162.814 86.41767) (end 162.814 84.8) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.544 88.621673) (end 161.732667 88.81034) (width 0.35) (layer F.Cu) (net 71) (status 30))
  (segment (start 161.544 84.05) (end 161.544 88.621673) (width 0.35) (layer F.Cu) (net 71) (status 30))
  (segment (start 160.274 84.8) (end 160.274 84.05) (width 0.35) (layer F.Cu) (net 72) (status 20))
  (segment (start 160.671915 89.539463) (end 160.274 89.141548) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 160.671915 90.27034) (end 160.671915 89.539463) (width 0.35) (layer F.Cu) (net 72) (status 10))
  (segment (start 160.274 89.141548) (end 160.274 84.8) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.004 90.407085) (end 159.004 84.455) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 160.671915 92.075) (end 159.004 90.407085) (width 0.35) (layer F.Cu) (net 73) (status 10))
  (segment (start 159.004 84.455) (end 159.004 84.05) (width 0.35) (layer F.Cu) (net 73) (status 20))
  (segment (start 140.589 90.419415) (end 140.589 84.05) (width 0.35) (layer F.Cu) (net 74) (status 20))
  (segment (start 142.256915 92.08733) (end 140.589 90.419415) (width 0.35) (layer F.Cu) (net 74) (status 10))
  (segment (start 141.859 84.8) (end 141.859 84.05) (width 0.35) (layer F.Cu) (net 75) (status 20))
  (segment (start 142.256915 89.551793) (end 141.859 89.153878) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.256915 90.28267) (end 142.256915 89.551793) (width 0.35) (layer F.Cu) (net 75) (status 10))
  (segment (start 141.859 89.153878) (end 141.859 84.8) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 143.129 88.634003) (end 143.317667 88.82267) (width 0.35) (layer F.Cu) (net 76) (status 30))
  (segment (start 143.129 84.05) (end 143.129 88.634003) (width 0.35) (layer F.Cu) (net 76) (status 30))
  (segment (start 145.034 87.065) (end 144.399 86.43) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 145.034 88.265) (end 145.034 87.065) (width 0.35) (layer F.Cu) (net 77) (status 10))
  (segment (start 144.399 86.43) (end 144.399 84.05) (width 0.35) (layer F.Cu) (net 77) (status 20))
  (segment (start 145.669 85.09) (end 145.669 84.05) (width 0.35) (layer F.Cu) (net 78) (status 20))
  (segment (start 146.750333 86.171333) (end 145.669 85.09) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 146.750333 88.82267) (end 146.750333 86.171333) (width 0.35) (layer F.Cu) (net 78) (status 10))
  (segment (start 146.939 85.09) (end 146.939 84.05) (width 0.35) (layer F.Cu) (net 79) (status 20))
  (segment (start 148.209 86.36) (end 146.939 85.09) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 148.209 89.153878) (end 148.209 86.36) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 147.811085 89.551793) (end 148.209 89.153878) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 147.811085 90.28267) (end 147.811085 89.551793) (width 0.35) (layer F.Cu) (net 79) (status 10))
  (segment (start 148.83167 92.08733) (end 147.811085 92.08733) (width 0.35) (layer F.Cu) (net 80) (status 20))
  (segment (start 149.479 91.44) (end 148.83167 92.08733) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 149.479 86.36) (end 149.479 91.44) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 148.209 85.09) (end 149.479 86.36) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 148.209 84.05) (end 148.209 85.09) (width 0.35) (layer F.Cu) (net 80) (status 10))
  (segment (start 149.479 85.09) (end 150.114 85.725) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.64167 93.54733) (end 146.750333 93.54733) (width 0.35) (layer F.Cu) (net 81) (status 20))
  (segment (start 150.114 92.075) (end 148.64167 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.114 85.725) (end 150.114 92.075) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 149.479 84.05) (end 149.479 85.09) (width 0.35) (layer F.Cu) (net 81) (status 10))
  (segment (start 136.764882 93.54733) (end 135.955333 93.54733) (width 0.35) (layer F.Cu) (net 82) (status 20))
  (segment (start 139.409 92.18733) (end 138.049 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 139.409 85.725) (end 139.409 92.18733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.684 85) (end 139.409 85.725) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.684 84.05) (end 138.684 85) (width 0.35) (layer F.Cu) (net 82) (status 10))
  (segment (start 138.049 93.54733) (end 136.764882 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.03667 92.08733) (end 137.016085 92.08733) (width 0.35) (layer F.Cu) (net 83) (status 20))
  (segment (start 138.684 86.36) (end 138.684 91.44) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 138.684 91.44) (end 138.03667 92.08733) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.414 85.09) (end 138.684 86.36) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.414 84.05) (end 137.414 85.09) (width 0.35) (layer F.Cu) (net 83) (status 10))
  (segment (start 137.414 86.36) (end 137.414 89.535) (width 0.35) (layer F.Cu) (net 84) (status 20))
  (segment (start 136.144 85.09) (end 137.414 86.36) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 136.144 84.05) (end 136.144 85.09) (width 0.35) (layer F.Cu) (net 84) (status 10))
  (segment (start 134.874 85.278667) (end 135.955333 86.36) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 134.874 84.05) (end 134.874 85.278667) (width 0.35) (layer F.Cu) (net 85) (status 10))
  (segment (start 135.955333 88.82267) (end 135.955333 86.36) (width 0.35) (layer F.Cu) (net 85) (status 10))
  (segment (start 133.604 84.05) (end 133.604 85.725) (width 0.35) (layer F.Cu) (net 86) (status 10))
  (segment (start 134.239 86.36) (end 134.239 88.265) (width 0.35) (layer F.Cu) (net 86) (status 20))
  (segment (start 133.604 85.725) (end 134.239 86.36) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 132.334 88.634003) (end 132.522667 88.82267) (width 0.35) (layer F.Cu) (net 87) (status 30))
  (segment (start 132.334 84.05) (end 132.334 88.634003) (width 0.35) (layer F.Cu) (net 87) (status 30))
  (segment (start 131.064 89.884755) (end 131.461915 90.28267) (width 0.35) (layer F.Cu) (net 88) (status 30))
  (segment (start 131.064 84.05) (end 131.064 89.884755) (width 0.35) (layer F.Cu) (net 88) (status 30))
  (segment (start 129.794 84.05) (end 129.794 91.44) (width 0.35) (layer F.Cu) (net 89) (status 10))
  (segment (start 130.44133 92.08733) (end 129.794 91.44) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 131.461915 92.08733) (end 130.44133 92.08733) (width 0.35) (layer F.Cu) (net 89) (status 10))
  (segment (start 111.77233 92.08733) (end 113.046915 92.08733) (width 0.35) (layer F.Cu) (net 90) (tstamp 5BB2973C) (status 20))
  (segment (start 111.379 91.694) (end 111.77233 92.08733) (width 0.35) (layer F.Cu) (net 90) (tstamp 5BB29739))
  (segment (start 111.379 91.694) (end 111.379 90.17) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 111.379 90.17) (end 111.379 90.424) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 111.379 84.05) (end 111.379 90.17) (width 0.35) (layer F.Cu) (net 90) (status 10))
  (segment (start 112.649 89.153878) (end 112.649 88.265) (width 0.35) (layer F.Cu) (net 91) (tstamp 5BB29757))
  (segment (start 112.649 89.153878) (end 113.046915 89.551793) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 112.649 86.36) (end 112.649 89.153878) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.046915 89.551793) (end 113.046915 90.28267) (width 0.35) (layer F.Cu) (net 91) (status 20))
  (segment (start 112.649 84.05) (end 112.649 86.36) (width 0.35) (layer F.Cu) (net 91) (status 10))
  (segment (start 112.649 86.36) (end 112.649 86.995) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.919 84.05) (end 113.919 85.725) (width 0.35) (layer F.Cu) (net 92) (status 10))
  (segment (start 113.919 88.634003) (end 114.107667 88.82267) (width 0.35) (layer F.Cu) (net 92) (status 30))
  (segment (start 113.919 84.05) (end 113.919 88.634003) (width 0.35) (layer F.Cu) (net 92) (status 30))
  (segment (start 113.919 86.36) (end 113.919 87.364003) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 115.189 85.725) (end 115.824 86.36) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 115.824 86.36) (end 115.824 88.265) (width 0.35) (layer F.Cu) (net 93) (status 20))
  (segment (start 115.189 85.725) (end 115.189 84.05) (width 0.35) (layer F.Cu) (net 93) (status 20))
  (segment (start 117.540333 88.82267) (end 117.04007 88.322407) (width 0.35) (layer F.Cu) (net 94) (status 10))
  (segment (start 117.04007 88.322407) (end 117.04007 86.995) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 117.04007 87.052407) (end 117.04007 86.995) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 117.04007 85.67107) (end 116.459 85.09) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 116.459 85.09) (end 116.459 84.05) (width 0.35) (layer F.Cu) (net 94) (status 20))
  (segment (start 117.04007 86.995) (end 117.04007 85.67107) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 118.601085 90.28267) (end 119.244828 89.638927) (width 0.35) (layer F.Cu) (net 95) (tstamp 5BB29745) (status 30))
  (segment (start 118.601085 92.08733) (end 120.049989 90.638426) (width 0.35) (layer F.Cu) (net 96) (status 10))
  (segment (start 120.049989 86.140989) (end 118.999 85.09) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.049989 90.638426) (end 120.049989 86.140989) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 118.999 85.09) (end 118.999 84.8) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 118.999 84.8) (end 118.999 84.05) (width 0.35) (layer F.Cu) (net 96) (status 20))
  (segment (start 120.06667 93.54733) (end 117.540333 93.54733) (width 0.35) (layer F.Cu) (net 97) (status 20))
  (segment (start 120.269 84.05) (end 120.269 85.09) (width 0.35) (layer F.Cu) (net 97) (status 10))
  (segment (start 120.65 85.471) (end 120.269 85.09) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 120.65 92.964) (end 120.65 85.471) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 120.65 92.964) (end 120.06667 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 110.274 92.424996) (end 110.274 85.45) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 106.745333 93.54733) (end 109.151666 93.54733) (width 0.35) (layer F.Cu) (net 98) (status 10))
  (segment (start 110.274 85.45) (end 109.474 84.65) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.151666 93.54733) (end 110.274 92.424996) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.474 84.65) (end 109.474 84.05) (width 0.35) (layer F.Cu) (net 98) (status 20))
  (segment (start 108.204 85.09) (end 108.204 84.05) (width 0.35) (layer F.Cu) (net 99) (status 20))
  (segment (start 108.839 85.725) (end 108.204 85.09) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.093 85.979) (end 108.204 85.09) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.347 91.567) (end 109.347 86.233) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 108.82667 92.08733) (end 109.347 91.567) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 107.806085 92.08733) (end 108.82667 92.08733) (width 0.35) (layer F.Cu) (net 99) (status 10))
  (segment (start 109.347 86.233) (end 109.093 85.979) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 108.449828 89.638927) (end 107.806085 90.28267) (width 0.35) (layer F.Cu) (net 100) (status 20))
  (segment (start 108.449828 86.605828) (end 108.449828 89.638927) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.934 85.09) (end 108.449828 86.605828) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.934 84.05) (end 106.934 85.09) (width 0.35) (layer F.Cu) (net 100) (status 10))
  (segment (start 106.745333 88.82267) (end 106.745333 86.806333) (width 0.35) (layer F.Cu) (net 101) (status 10))
  (segment (start 105.664 85.725) (end 105.664 84.8) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 106.745333 86.806333) (end 105.664 85.725) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 105.664 84.8) (end 105.664 84.05) (width 0.35) (layer F.Cu) (net 101) (status 20))
  (segment (start 104.394 84.8) (end 104.394 84.05) (width 0.35) (layer F.Cu) (net 102) (status 20))
  (segment (start 105.029 87.065) (end 104.394 86.43) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 105.029 88.265) (end 105.029 87.065) (width 0.35) (layer F.Cu) (net 102) (status 10))
  (segment (start 104.394 86.43) (end 104.394 84.8) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.124 88.634003) (end 103.312667 88.82267) (width 0.35) (layer F.Cu) (net 103) (status 30))
  (segment (start 103.124 84.05) (end 103.124 88.634003) (width 0.35) (layer F.Cu) (net 103) (status 30))
  (segment (start 101.854 89.884755) (end 102.251915 90.28267) (width 0.35) (layer F.Cu) (net 104) (status 30))
  (segment (start 101.854 84.05) (end 101.854 89.884755) (width 0.35) (layer F.Cu) (net 104) (status 30))
  (segment (start 101.23133 92.08733) (end 102.251915 92.08733) (width 0.35) (layer F.Cu) (net 105) (status 20))
  (segment (start 100.584 91.44) (end 101.23133 92.08733) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 100.584 84.05) (end 100.584 91.44) (width 0.35) (layer F.Cu) (net 105) (status 10))
  (segment (start 170.434 74.295) (end 167.259 74.295) (width 0.35) (layer F.Cu) (net 106) (status 30))
  (segment (start 167.259 74.295) (end 166.584 74.295) (width 0.35) (layer F.Cu) (net 106) (status 30))
  (segment (start 141.224 74.295) (end 138.049 74.295) (width 0.35) (layer F.Cu) (net 107) (status 30))
  (segment (start 150.624 74.295) (end 157.859 74.295) (width 0.35) (layer F.Cu) (net 108) (status 30))
  (segment (start 121.414 74.295) (end 128.649 74.295) (width 0.35) (layer F.Cu) (net 109) (status 30))
  (segment (start 108.839 74.295) (end 112.014 74.295) (width 0.35) (layer F.Cu) (net 110) (status 30))
  (segment (start 104.023 38.765) (end 104.648 38.765) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 101.854 36.596) (end 104.023 38.765) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 101.854 34.925) (end 101.854 36.596) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 117.348 36.195) (end 117.348 34.9264) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 114.348 39.195) (end 117.348 36.195) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 114.348 40.465) (end 114.348 39.195) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 106.248 50.165) (end 106.248 51.232) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 104.521 54.102) (end 104.521 53.467) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 106.248 51.74) (end 106.248 50.165) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 104.521 53.467) (end 106.248 51.74) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 115.951 35.525) (end 115.951 34.925) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 115.951 36.087) (end 115.951 35.525) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.273 38.765) (end 115.951 36.087) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 112.648 38.765) (end 113.273 38.765) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 115.448 46.065) (end 114.348 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.6485 46.065) (end 115.448 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 117.5735 46.99) (end 116.6485 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 118.1735 46.99) (end 117.5735 46.99) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 106.045 35.56) (end 106.045 34.913) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 107.048 36.563) (end 106.045 35.56) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 107.048 38.765) (end 107.048 36.563) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 104.66 34.913) (end 104.66 35.548) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 106.248 37.136) (end 106.248 38.765) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 104.66 35.548) (end 106.248 37.136) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 110.363 34.925) (end 110.363 35.56) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 109.448 36.475) (end 109.448 38.765) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 110.363 35.56) (end 109.448 36.475) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 110.248 37.037) (end 110.248 37.665) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.76 35.525) (end 110.248 37.037) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 110.248 37.665) (end 110.248 38.765) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.76 34.925) (end 111.76 35.525) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.048 37.288) (end 113.157 35.179) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 113.157 35.179) (end 113.157 34.925) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 111.048 38.765) (end 111.048 37.288) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 103.124 53.589) (end 103.124 53.975) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 105.448 51.265) (end 103.124 53.589) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 105.448 50.165) (end 105.448 51.265) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 103.124 53.975) (end 103.124 54.102) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 149.299 66.675) (end 148.844 66.22) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 150.624 66.675) (end 149.299 66.675) (width 0.35) (layer F.Cu) (net 123) (status 10))
  (segment (start 136.724 66.675) (end 136.144 66.095) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 138.049 66.675) (end 136.724 66.675) (width 0.35) (layer F.Cu) (net 123) (status 10))
  (segment (start 136.144 66.095) (end 136.144 59.69) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 120.089 66.675) (end 119.634 66.22) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 121.414 66.675) (end 120.089 66.675) (width 0.35) (layer F.Cu) (net 123) (status 10))
  (via (at 119.634 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (segment (start 119.634 66.22) (end 119.634 59.69) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 119.634 59.69) (end 136.144 59.69) (width 0.35) (layer B.Cu) (net 123))
  (segment (start 107.514 66.675) (end 106.934 66.095) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 108.839 66.675) (end 107.514 66.675) (width 0.35) (layer F.Cu) (net 123) (status 10))
  (via (at 106.934 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (segment (start 106.934 66.095) (end 106.934 59.69) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 106.934 59.69) (end 119.634 59.69) (width 0.35) (layer B.Cu) (net 123))
  (via (at 165.354 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (segment (start 165.934 66.675) (end 167.259 66.675) (width 0.35) (layer F.Cu) (net 123) (status 20))
  (segment (start 165.354 66.095) (end 165.934 66.675) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 165.354 59.69) (end 165.354 66.095) (width 0.35) (layer F.Cu) (net 123))
  (via (at 178.054 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (segment (start 165.354 59.69) (end 178.054 59.69) (width 0.35) (layer B.Cu) (net 123))
  (segment (start 178.054 66.22) (end 178.509 66.675) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 178.509 66.675) (end 179.834 66.675) (width 0.35) (layer F.Cu) (net 123) (status 20))
  (segment (start 178.054 59.69) (end 178.054 66.22) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 162.052 59.69) (end 165.354 59.69) (width 0.35) (layer B.Cu) (net 123))
  (via (at 136.144 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (via (at 148.844 59.69) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123))
  (segment (start 148.844 66.22) (end 148.844 59.69) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 148.844 59.69) (end 162.052 59.69) (width 0.35) (layer B.Cu) (net 123))
  (segment (start 136.144 59.69) (end 148.844 59.69) (width 0.35) (layer B.Cu) (net 123))
  (segment (start 114.348 46.865) (end 115.953 46.865) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 117.475 48.387) (end 118.1735 48.387) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 115.953 46.865) (end 117.475 48.387) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 115.448 47.665) (end 114.348 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 117.5735 49.784) (end 115.4545 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 115.4545 47.665) (end 115.448 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 118.1735 49.784) (end 117.5735 49.784) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 114.348 48.465) (end 114.348 49.09) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 116.439 51.181) (end 118.1735 51.181) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 115.443 50.185) (end 116.439 51.181) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 114.348 49.09) (end 115.443 50.185) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 100.827 37.719) (end 99.406 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 102.948 39.84) (end 100.827 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 99.406 37.719) (end 98.806 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 102.948 40.465) (end 102.948 39.84) (width 0.35) (layer F.Cu) (net 129))
  (via (at 98.425 55.118) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 130))
  (segment (start 98.425 56.388) (end 98.425 55.118) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 100.076 56.769) (end 99.822 56.515) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 99.822 56.515) (end 98.425 55.118) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 103.124 56.388) (end 102.743 56.769) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 102.743 56.769) (end 100.076 56.769) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 103.124 55.602) (end 103.124 56.388) (width 0.35) (layer F.Cu) (net 130))
  (via (at 97.028 53.594) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 131))
  (segment (start 97.028 54.737) (end 97.028 53.594) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 97.028 56.388) (end 97.028 54.737) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 97.028 53.594) (end 98.679 53.594) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 98.933 53.594) (end 98.679 53.594) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.927 55.602) (end 100.457 55.132) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 101.727 55.602) (end 100.927 55.602) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.457 55.132) (end 100.457 55.118) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.457 55.118) (end 98.933 53.594) (width 0.35) (layer F.Cu) (net 131))
  (via (at 95.758 51.816) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 132))
  (segment (start 95.389 51.828) (end 95.377 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 95.77 51.828) (end 95.758 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 97.294 51.828) (end 95.77 51.828) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 92.317 51.816) (end 95.758 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 95.631 51.943) (end 95.758 51.816) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 95.631 56.388) (end 95.631 51.943) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 92.329 50.419) (end 94.107 50.419) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 97.306 50.419) (end 94.107 50.419) (width 0.35) (layer F.Cu) (net 133))
  (via (at 94.107 50.419) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 133))
  (segment (start 94.234 50.546) (end 94.107 50.419) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 94.234 56.388) (end 94.234 50.546) (width 0.35) (layer B.Cu) (net 133))
  (via (at 95.758 49.022) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 134))
  (segment (start 97.306 49.022) (end 95.758 49.022) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 92.329 49.022) (end 95.758 49.022) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 93.345 49.022) (end 95.758 49.022) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 92.837 49.53) (end 93.345 49.022) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 92.837 56.388) (end 92.837 49.53) (width 0.35) (layer B.Cu) (net 134))
  (via (at 94.107 47.625) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 135))
  (segment (start 97.306 47.625) (end 94.107 47.625) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 94.107 47.625) (end 92.329 47.625) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 92.329 47.625) (end 94.107 47.625) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 91.44 48.514) (end 92.329 47.625) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 91.44 56.388) (end 91.44 48.514) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 114.348 43.665) (end 116.863 43.665) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 118.237 42.291) (end 120.65 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 116.863 43.665) (end 118.237 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 121.2596 42.9006) (end 120.65 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 123.2662 42.9006) (end 121.2596 42.9006) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 115.443 42.865) (end 115.758 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 114.348 42.865) (end 115.443 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 119.1 38.591) (end 120.65 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 117.729 39.962) (end 119.1 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 117.729 41.849) (end 117.729 39.962) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 116.713 42.865) (end 117.729 41.849) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 115.443 42.865) (end 116.713 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 121.2426 37.9984) (end 120.65 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 123.2662 37.9984) (end 121.2426 37.9984) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 99.568 46.228) (end 97.282 46.228) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 100.531 45.265) (end 99.568 46.228) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 102.948 45.265) (end 100.531 45.265) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 115.453 41.265) (end 114.348 41.265) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 116.078 40.64) (end 115.453 41.265) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 116.078 38.608) (end 116.078 40.64) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 118.745 35.941) (end 116.078 38.608) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 118.745 34.9384) (end 118.745 35.941) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 111.848 37.631) (end 113.538 35.941) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 113.538 35.941) (end 114.554 34.925) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BC7BC0F))
  (segment (start 111.848 38.765) (end 111.848 37.631) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 120.142 35.814) (end 120.142 34.9384) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.84 39.116) (end 120.142 35.814) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.304 42.065) (end 116.84 41.529) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.84 41.529) (end 116.84 39.116) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 114.348 42.065) (end 116.304 42.065) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 105.918 53.502) (end 105.918 54.102) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 105.918 53.467) (end 105.918 53.502) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 107.048 52.337) (end 105.918 53.467) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 107.048 50.165) (end 107.048 52.337) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 179.705 18.8595) (end 179.705 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DF1) (status 20))
  (segment (start 173.355 18.0995) (end 173.355 21.4745) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DE8) (status 30))
  (segment (start 137.795 19.05) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DEE) (status 30))
  (segment (start 139.065 15.24) (end 139.065 17.272) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DEB) (status 30))
  (segment (start 139.065 17.272) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DDF) (status 30))
  (segment (start 173.355 18.0995) (end 173.355 17.5895) (width 0.7) (layer F.Cu) (net 151) (tstamp 5BC64DDC) (status 30))
  (segment (start 173.355 18.0995) (end 173.355 17.3495) (width 0.7) (layer F.Cu) (net 151) (tstamp 5BC64DE5) (status 30))
  (segment (start 179.07 17.5895) (end 179.705 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DE2) (status 20))
  (segment (start 177.925 18.0995) (end 178.435 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DCD))
  (segment (start 173.355 18.0995) (end 177.925 18.0995) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DCA) (status 10))
  (segment (start 178.435 17.5895) (end 179.07 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D6D))
  (segment (start 139.065 19.685) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D73) (status 20))
  (segment (start 179.705 21.8745) (end 179.705 18.8595) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D70) (status 10))
  (segment (start 139.065 21.905) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D61))
  (segment (start 133.223 19.05) (end 131.953 17.78) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64E7B))
  (segment (start 137.795 19.05) (end 133.223 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64E69))
  (segment (start 132.715 17.78) (end 132.715 21.105) (width 0.7) (layer F.Cu) (net 151) (tstamp 5BC64E72))
  (segment (start 178.435 21.8745) (end 177.165 21.8745) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DD9) (status 30))
  (segment (start 177.165 22.4945) (end 177.165 21.8745) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DD6) (status 30))
  (segment (start 177.165 27.2745) (end 177.165 22.4945) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DD3) (status 30))
  (segment (start 177.132 27.2415) (end 177.165 27.2745) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DD0) (status 30))
  (segment (start 175.462 27.6745) (end 175.895 27.2415) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DBE))
  (segment (start 175.895 27.2415) (end 177.132 27.2415) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DBB) (status 20))
  (segment (start 173.355 27.6745) (end 175.462 27.6745) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DC7) (status 10))
  (segment (start 179.705 28.4995) (end 179.705 27.2745) (width 0.35) (layer F.Cu) (net 153) (tstamp 5BC64DC4) (status 20))
  (segment (start 180.86 29.6545) (end 179.705 28.4995) (width 0.35) (layer F.Cu) (net 153) (tstamp 5BC64DC1) (status 10))
  (segment (start 183.6155 19.4945) (end 183.635 19.475) (width 0.35) (layer F.Cu) (net 154) (tstamp 5BC64E78))
  (segment (start 180.655 19.4945) (end 183.6155 19.4945) (width 0.35) (layer F.Cu) (net 154) (tstamp 5BC64E6C))
  (segment (start 185.928 19.468) (end 185.935 19.475) (width 0.35) (layer F.Cu) (net 155) (tstamp 5BC64D1F))
  (segment (start 185.928 17.145) (end 185.928 19.468) (width 0.35) (layer F.Cu) (net 155) (tstamp 5BC64D13))
  (segment (start 152.9715 14.1285) (end 152.915 14.185) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64D28))
  (segment (start 152.9715 12.5095) (end 152.9715 14.1285) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64D2E))
  (segment (start 152.915 12.185) (end 153.035 12.065) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64E3C))
  (segment (start 152.915 14.185) (end 152.915 12.185) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64E36))
  (segment (start 150.495 14.065) (end 150.615 14.185) (width 0.35) (layer F.Cu) (net 157) (tstamp 5BC64E54))
  (segment (start 150.495 12.065) (end 150.495 14.065) (width 0.35) (layer F.Cu) (net 157) (tstamp 5BC64E45))
  (segment (start 139.065 29.21) (end 139.065 27.305) (width 0.35) (layer F.Cu) (net 158) (tstamp 5BC64E57))
  (segment (start 184.15 21.8745) (end 180.975 21.8745) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E2A))
  (segment (start 184.785 22.5095) (end 184.15 21.8745) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E30))
  (segment (start 184.785 24.975) (end 184.785 22.5095) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E3F))
  (segment (start 146.7485 18.05) (end 146.7485 16.256) (width 0.35) (layer F.Cu) (net 161) (tstamp 5BC64D9A) (status 30))
  (segment (start 142.245 20.27) (end 142.24 20.265) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D97) (status 30))
  (segment (start 142.245 20.32) (end 142.245 20.27) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D94) (status 30))
  (segment (start 141.605 19.05) (end 140.565 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D91) (status 20))
  (segment (start 145.7985 19.25) (end 145.7985 20.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DAC) (status 20))
  (segment (start 145.5985 19.05) (end 145.7985 19.25) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DA9))
  (segment (start 142.245 20.05) (end 142.245 19.055) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB8) (status 10))
  (segment (start 142.24 19.05) (end 145.5985 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB5))
  (segment (start 142.245 19.055) (end 142.24 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB2))
  (segment (start 146.746 14.2925) (end 146.746 13.716) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DAF))
  (segment (start 145.7985 15.24) (end 146.746 14.2925) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D8E))
  (segment (start 145.7985 19.25) (end 145.7985 15.24) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D8B))
  (segment (start 146.746 13.716) (end 146.746 11.446) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D6A) (status 20))
  (segment (start 141.605 19.05) (end 142.24 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D67))
  (segment (start 142.417 17.272) (end 143.195 18.05) (width 0.35) (layer F.Cu) (net 163) (tstamp 5BC64DA6) (status 20))
  (segment (start 140.965 17.272) (end 142.417 17.272) (width 0.35) (layer F.Cu) (net 163) (tstamp 5BC64DA3) (status 10))
  (segment (start 142.494 13.5128) (end 144.2052 13.5128) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64DA0) (status 30))
  (segment (start 142.494 11.938) (end 142.494 13.5128) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64D9D) (status 30))
  (segment (start 144.272 13.446) (end 144.2052 13.5128) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64D7C) (status 30))
  (segment (start 145.796 13.446) (end 144.272 13.446) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64D79) (status 30))
  (segment (start 145.7292 13.5128) (end 145.796 13.446) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64D88) (status 30))
  (segment (start 142.494 13.5128) (end 145.7292 13.5128) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BC64D85) (status 30))
  (segment (start 141.605 15.24) (end 140.565 15.24) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D82) (status 20))
  (segment (start 142.621 16.256) (end 141.605 15.24) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D7F))
  (segment (start 144.6485 16.256) (end 142.621 16.256) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D76) (status 10))
  (segment (start 92.58 20.32) (end 92.33 20.32) (width 0.7) (layer F.Cu) (net 168) (status 30))
  (segment (start 98.54 14.36) (end 92.58 20.32) (width 0.7) (layer F.Cu) (net 168) (status 30))
  (segment (start 99.45 14.36) (end 98.54 14.36) (width 0.7) (layer F.Cu) (net 168) (status 30))
  (segment (start 93.825 24.765) (end 92.33 23.27) (width 0.7) (layer F.Cu) (net 168))
  (segment (start 103.505 24.765) (end 93.825 24.765) (width 0.7) (layer F.Cu) (net 168))
  (segment (start 104.13 25.39) (end 103.505 24.765) (width 0.7) (layer F.Cu) (net 168))
  (segment (start 92.33 23.27) (end 92.33 20.32) (width 0.7) (layer F.Cu) (net 168) (status 20))
  (segment (start 104.13 27.305) (end 104.13 25.39) (width 0.7) (layer F.Cu) (net 168) (status 10))
  (segment (start 99.695 20.76) (end 99.695 20.51) (width 0.7) (layer F.Cu) (net 169) (status 30))
  (segment (start 102.87 22.86) (end 100.33 20.32) (width 0.7) (layer F.Cu) (net 169) (status 20))
  (segment (start 141.224 66.675) (end 142.494 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (segment (start 142.494 66.675) (end 143.129 66.04) (width 0.35) (layer F.Cu) (net 171))
  (via (at 143.129 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 143.129 66.04) (end 143.129 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 128.649 66.675) (end 129.794 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (segment (start 129.794 66.675) (end 130.429 66.04) (width 0.35) (layer F.Cu) (net 171))
  (via (at 130.429 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 130.429 66.04) (end 130.429 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 143.129 63.5) (end 130.429 63.5) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 112.014 66.675) (end 112.689 66.675) (width 0.35) (layer F.Cu) (net 171) (status 30))
  (segment (start 112.689 66.675) (end 113.284 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (via (at 113.919 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC6731C))
  (segment (start 113.919 66.04) (end 113.919 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 113.284 66.675) (end 113.919 66.04) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 113.919 63.5) (end 130.429 63.5) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 99.439 66.675) (end 100.584 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (segment (start 100.584 66.675) (end 101.219 66.04) (width 0.35) (layer F.Cu) (net 171))
  (via (at 101.219 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 101.219 66.04) (end 101.219 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 101.219 63.5) (end 113.919 63.5) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 159.184 66.675) (end 159.639 66.22) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 157.859 66.675) (end 159.184 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (via (at 159.639 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 159.639 66.22) (end 159.639 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 159.639 63.5) (end 143.129 63.5) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 171.759 66.675) (end 172.339 66.095) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 170.434 66.675) (end 171.759 66.675) (width 0.35) (layer F.Cu) (net 171) (status 10))
  (via (at 172.339 63.5) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 172.339 66.095) (end 172.339 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 172.339 63.5) (end 159.639 63.5) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 110.236 59.817) (end 113.919 63.5) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 110.236 55.602) (end 110.236 59.817) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 163.449 60.96) (end 146.939 60.96) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 164.084 67.945) (end 163.449 67.31) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 163.449 67.31) (end 163.449 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 167.259 67.945) (end 164.084 67.945) (width 0.35) (layer F.Cu) (net 172) (status 10))
  (segment (start 105.029 60.96) (end 117.729 60.96) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 105.664 67.945) (end 105.029 67.31) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 105.029 67.31) (end 105.029 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 108.839 67.945) (end 105.664 67.945) (width 0.35) (layer F.Cu) (net 172) (status 10))
  (segment (start 117.729 60.96) (end 134.239 60.96) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 117.729 67.31) (end 117.729 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 118.364 67.945) (end 117.729 67.31) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 121.414 67.945) (end 118.364 67.945) (width 0.35) (layer F.Cu) (net 172) (status 10))
  (segment (start 146.939 60.96) (end 134.239 60.96) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 134.874 67.945) (end 134.239 67.31) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 134.239 67.31) (end 134.239 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 138.049 67.945) (end 134.874 67.945) (width 0.35) (layer F.Cu) (net 172) (status 10))
  (segment (start 147.574 67.945) (end 146.939 67.31) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 146.939 67.31) (end 146.939 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 150.624 67.945) (end 147.574 67.945) (width 0.35) (layer F.Cu) (net 172) (status 10))
  (via (at 163.449 60.96) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 172))
  (via (at 105.029 60.96) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 172))
  (via (at 117.729 60.96) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 172))
  (via (at 134.239 60.96) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 172))
  (via (at 146.939 60.96) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 172))
  (segment (start 175.26 60.96) (end 163.449 60.96) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 114.427 57.658) (end 117.729 60.96) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 114.427 55.602) (end 114.427 57.658) (width 0.35) (layer F.Cu) (net 172))
  (segment (start 126.365 88.315) (end 126.365 91.186) (width 0.35) (layer F.Cu) (net 184) (status 30))
  (segment (start 155.321 91.186) (end 155.321 88.265) (width 0.35) (layer F.Cu) (net 186) (status 30))
  (segment (start 123.825 90.17) (end 123.825 88.38) (width 0.35) (layer F.Cu) (net 187) (status 20))
  (segment (start 123.825 91.186) (end 123.825 90.17) (width 0.35) (layer F.Cu) (net 187) (status 10))
  (segment (start 123.825 90.17) (end 123.825 88.9) (width 0.35) (layer F.Cu) (net 187))
  (segment (start 152.654 91.059) (end 152.781 91.186) (width 0.35) (layer F.Cu) (net 188) (status 30))
  (segment (start 152.654 88.38) (end 152.654 91.059) (width 0.35) (layer F.Cu) (net 188) (status 30))
  (segment (start 139.296002 102.235) (end 139.385 102.146002) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 139.0015 102.235) (end 139.296002 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 139.385 102.146002) (end 139.385 98.965) (width 0.35) (layer B.Cu) (net 193) (status 20))
  (segment (start 110.302 102.185499) (end 110.302 98.965) (width 0.35) (layer B.Cu) (net 193) (status 20))
  (segment (start 110.351501 102.235) (end 110.302 102.185499) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 139.192 102.235) (end 151.13 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 139.0015 102.235) (end 139.192 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 139.192 102.235) (end 139.371001 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 151.13 102.235) (end 152.019 103.124) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 152.019 103.124) (end 153.924 103.124) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 153.924 103.124) (end 154.738001 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 169.357 99.638) (end 169.3545 99.6405) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 169.3545 99.6405) (end 169.3545 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 169.357 98.838) (end 169.357 99.638) (width 0.35) (layer B.Cu) (net 193) (status 10))
  (segment (start 164.158999 102.309999) (end 169.3545 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 172.743501 102.309999) (end 171.831 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 173.355 102.2985) (end 172.755 102.2985) (width 0.35) (layer B.Cu) (net 193) (status 10))
  (segment (start 172.755 102.2985) (end 172.743501 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 171.831 102.309999) (end 172.137001 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 169.3545 102.309999) (end 171.831 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 129.0955 102.235) (end 139.0015 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 129.1615 102.169) (end 129.0955 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 129.1615 99.0285) (end 129.1615 102.169) (width 0.35) (layer B.Cu) (net 193) (status 10))
  (segment (start 158.308 102.243999) (end 158.242 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 158.308 98.838) (end 158.308 102.243999) (width 0.35) (layer B.Cu) (net 193) (status 10))
  (segment (start 154.738001 102.309999) (end 158.242 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 110.351501 102.235) (end 123.825 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 106.1085 102.235) (end 110.351501 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 99.568 101.727) (end 100.076 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 99.5705 99.8285) (end 99.568 99.831) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 99.568 99.831) (end 99.568 101.727) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 99.5705 99.0285) (end 99.5705 99.8285) (width 0.35) (layer B.Cu) (net 193) (status 10))
  (segment (start 100.076 102.235) (end 106.1085 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 123.825 102.235) (end 129.0955 102.235) (width 0.35) (layer B.Cu) (net 193))
  (segment (start 158.242 102.309999) (end 164.158999 102.309999) (width 0.35) (layer B.Cu) (net 193))
  (via (at 110.744 93.472) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 194))
  (segment (start 113.588 93.472) (end 110.744 93.472) (width 0.25) (layer F.Cu) (net 194))
  (segment (start 115.274 91.786) (end 113.588 93.472) (width 0.25) (layer F.Cu) (net 194))
  (segment (start 115.274 91.186) (end 115.274 91.786) (width 0.25) (layer F.Cu) (net 194) (status 10))
  (segment (start 111.252 100.965) (end 111.252 97.917) (width 0.35) (layer B.Cu) (net 194) (status 10))
  (segment (start 109.982 96.647) (end 109.982 94.234) (width 0.35) (layer B.Cu) (net 194))
  (segment (start 111.252 97.917) (end 109.982 96.647) (width 0.35) (layer B.Cu) (net 194))
  (segment (start 110.744 93.472) (end 109.982 94.234) (width 0.35) (layer B.Cu) (net 194))
  (via (at 128.905 93.218) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 195))
  (segment (start 133.689 91.786) (end 132.257 93.218) (width 0.25) (layer F.Cu) (net 195))
  (segment (start 133.689 91.186) (end 133.689 91.786) (width 0.25) (layer F.Cu) (net 195) (status 10))
  (segment (start 130.175 93.218) (end 128.905 93.218) (width 0.25) (layer F.Cu) (net 195))
  (segment (start 130.1115 94.4245) (end 128.905 93.218) (width 0.35) (layer B.Cu) (net 195))
  (segment (start 130.1115 95.885) (end 130.1115 94.4245) (width 0.35) (layer B.Cu) (net 195))
  (segment (start 130.1115 101.0285) (end 130.1115 95.885) (width 0.35) (layer B.Cu) (net 195) (status 10))
  (segment (start 132.257 93.218) (end 130.175 93.218) (width 0.25) (layer F.Cu) (net 195))
  (via (at 139.954 93.472) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 196))
  (segment (start 140.335 100.965) (end 140.335 97.79) (width 0.35) (layer B.Cu) (net 196) (status 10))
  (segment (start 140.335 97.79) (end 139.065 96.52) (width 0.35) (layer B.Cu) (net 196))
  (segment (start 139.065 94.361) (end 139.954 93.472) (width 0.35) (layer B.Cu) (net 196))
  (segment (start 139.065 96.52) (end 139.065 94.361) (width 0.35) (layer B.Cu) (net 196))
  (segment (start 139.954 93.472) (end 140.548528 93.472) (width 0.25) (layer F.Cu) (net 196))
  (via (at 157.6705 92.456) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 197))
  (segment (start 162.8355 91.8495) (end 161.558101 93.126899) (width 0.25) (layer F.Cu) (net 197))
  (segment (start 162.8355 91.2495) (end 162.8355 91.8495) (width 0.25) (layer F.Cu) (net 197) (status 10))
  (segment (start 159.258 94.0435) (end 159.258 94.234) (width 0.35) (layer B.Cu) (net 197))
  (segment (start 157.6705 92.456) (end 159.258 94.0435) (width 0.35) (layer B.Cu) (net 197))
  (segment (start 158.341399 93.126899) (end 157.6705 92.456) (width 0.25) (layer F.Cu) (net 197))
  (segment (start 159.9565 93.126899) (end 158.341399 93.126899) (width 0.25) (layer F.Cu) (net 197))
  (segment (start 161.558101 93.126899) (end 159.9565 93.126899) (width 0.25) (layer F.Cu) (net 197))
  (segment (start 159.258 100.838) (end 159.258 94.234) (width 0.35) (layer B.Cu) (net 197) (status 10))
  (via (at 169.545 93.345) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 198))
  (segment (start 172.135 93.345) (end 169.545 93.345) (width 0.25) (layer F.Cu) (net 198))
  (segment (start 173.694 91.786) (end 172.135 93.345) (width 0.25) (layer F.Cu) (net 198))
  (segment (start 173.694 91.186) (end 173.694 91.786) (width 0.25) (layer F.Cu) (net 198) (status 10))
  (segment (start 170.307 100.838) (end 170.307 98.044) (width 0.35) (layer B.Cu) (net 198) (status 10))
  (segment (start 170.307 98.044) (end 168.656 96.393) (width 0.35) (layer B.Cu) (net 198))
  (segment (start 168.656 94.234) (end 169.545 93.345) (width 0.35) (layer B.Cu) (net 198))
  (segment (start 168.656 96.393) (end 168.656 94.234) (width 0.35) (layer B.Cu) (net 198))
  (via (at 137.668 95.25) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 199))
  (segment (start 145.584 91.186) (end 145.584 91.786) (width 0.25) (layer F.Cu) (net 199) (status 10))
  (segment (start 140.635002 94.234) (end 139.619002 95.25) (width 0.25) (layer F.Cu) (net 199))
  (segment (start 143.136 94.234) (end 140.635002 94.234) (width 0.25) (layer F.Cu) (net 199))
  (segment (start 145.584 91.786) (end 143.136 94.234) (width 0.25) (layer F.Cu) (net 199))
  (segment (start 139.619002 95.25) (end 138.516528 95.25) (width 0.25) (layer F.Cu) (net 199))
  (segment (start 137.16 95.758) (end 137.668 95.25) (width 0.35) (layer B.Cu) (net 199))
  (segment (start 137.16 101.485) (end 137.16 95.758) (width 0.35) (layer B.Cu) (net 199) (status 10))
  (segment (start 138.516528 95.25) (end 137.668 95.25) (width 0.25) (layer F.Cu) (net 199))
  (segment (start 134.789 91.786) (end 132.341 94.234) (width 0.25) (layer F.Cu) (net 200))
  (segment (start 134.789 91.186) (end 134.789 91.786) (width 0.25) (layer F.Cu) (net 200) (status 10))
  (via (at 126.8095 94.996) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 200))
  (segment (start 128.905 94.234) (end 127.5715 94.234) (width 0.25) (layer F.Cu) (net 200))
  (segment (start 127.5715 94.234) (end 126.8095 94.996) (width 0.25) (layer F.Cu) (net 200))
  (segment (start 126.8095 94.996) (end 126.8095 101.473) (width 0.35) (layer B.Cu) (net 200) (status 20))
  (segment (start 132.341 94.234) (end 128.905 94.234) (width 0.25) (layer F.Cu) (net 200))
  (segment (start 163.9355 91.8495) (end 161.805 93.98) (width 0.25) (layer F.Cu) (net 201))
  (segment (start 163.9355 91.2495) (end 163.9355 91.8495) (width 0.25) (layer F.Cu) (net 201) (status 10))
  (segment (start 161.805 93.98) (end 155.575 93.98) (width 0.25) (layer F.Cu) (net 201))
  (via (at 155.575 93.98) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 201))
  (segment (start 155.575 101.5485) (end 155.575 93.98) (width 0.35) (layer B.Cu) (net 201) (status 10))
  (via (at 166.497 95.377) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 202))
  (segment (start 167.436062 94.437938) (end 166.497 95.377) (width 0.25) (layer F.Cu) (net 202))
  (segment (start 172.142062 94.437938) (end 167.436062 94.437938) (width 0.25) (layer F.Cu) (net 202))
  (segment (start 174.794 91.786) (end 172.142062 94.437938) (width 0.25) (layer F.Cu) (net 202))
  (segment (start 174.794 91.186) (end 174.794 91.786) (width 0.25) (layer F.Cu) (net 202) (status 10))
  (segment (start 166.37 95.504) (end 166.497 95.377) (width 0.35) (layer B.Cu) (net 202))
  (segment (start 166.37 101.5485) (end 166.37 95.504) (width 0.35) (layer B.Cu) (net 202) (status 10))
  (via (at 107.95 95.25) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 203))
  (segment (start 116.374 91.786) (end 116.374 91.186) (width 0.25) (layer F.Cu) (net 203) (status 20))
  (segment (start 111.343999 94.650001) (end 112.014 93.98) (width 0.25) (layer F.Cu) (net 203))
  (segment (start 114.18 93.98) (end 116.374 91.786) (width 0.25) (layer F.Cu) (net 203))
  (segment (start 112.014 93.98) (end 114.18 93.98) (width 0.25) (layer F.Cu) (net 203))
  (segment (start 108.549999 94.650001) (end 111.343999 94.650001) (width 0.25) (layer F.Cu) (net 203))
  (segment (start 107.95 95.25) (end 108.549999 94.650001) (width 0.25) (layer F.Cu) (net 203))
  (segment (start 107.95 101.358) (end 107.95 100.758) (width 0.35) (layer B.Cu) (net 203) (status 10))
  (segment (start 107.95 101.485) (end 107.95 95.25) (width 0.35) (layer B.Cu) (net 203) (status 10))
  (segment (start 107.95 100.758) (end 107.95 100.0125) (width 0.35) (layer B.Cu) (net 203))
  (segment (start 71.755 66.74) (end 72.225 66.27) (width 0.35) (layer F.Cu) (net 207))
  (segment (start 72.225 69.076) (end 71.755 68.606) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BC33073))
  (segment (start 72.225 66.27) (end 73.025 66.27) (width 0.35) (layer F.Cu) (net 207) (status 20))
  (segment (start 71.755 68.606) (end 71.755 66.74) (width 0.35) (layer F.Cu) (net 207))
  (segment (start 73.025 69.076) (end 72.225 69.076) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BC33070) (status 10))
  (segment (start 74.815 69.076) (end 75.057 68.834) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BC3306D) (status 30))
  (segment (start 73.025 69.076) (end 74.815 69.076) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BC3306A) (status 30))
  (segment (start 73.631 66.97) (end 75.057 66.97) (width 0.35) (layer F.Cu) (net 208) (status 20))
  (segment (start 73.025 67.576) (end 73.631 66.97) (width 0.35) (layer F.Cu) (net 208) (status 10))
  (segment (start 107.55 103.03) (end 107.95 103.43) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 104.775 103.03) (end 107.55 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 118.42 103.03) (end 118.745 103.355) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 115.57 103.03) (end 118.42 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 136.835 103.03) (end 137.16 103.355) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 133.985 103.03) (end 136.835 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 144.94 103.03) (end 147.63 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 165.97 103.03) (end 166.37 103.43) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 163.195 103.03) (end 165.97 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 176.765 103.03) (end 177.165 103.43) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (segment (start 173.99 103.03) (end 176.765 103.03) (width 0.35) (layer F.Cu) (net 210) (status 30))
  (via (at 107.95 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 107.95 103.43) (end 107.95 105.41) (width 0.7) (layer F.Cu) (net 210) (status 10))
  (via (at 118.745 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 118.745 105.41) (end 118.745 103.355) (width 0.7) (layer F.Cu) (net 210) (status 20))
  (via (at 166.37 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 166.37 105.41) (end 166.37 103.43) (width 0.7) (layer F.Cu) (net 210) (status 20))
  (via (at 177.165 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 177.165 105.41) (end 177.165 103.43) (width 0.7) (layer F.Cu) (net 210) (status 20))
  (segment (start 176.365001 104.610001) (end 177.165 105.41) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 166.37 105.41) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 166.37 104.610001) (end 176.365001 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 165.570001 104.610001) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (via (at 147.955 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 148.03 105.335) (end 147.955 105.41) (width 0.7) (layer F.Cu) (net 210))
  (segment (start 148.03 103.43) (end 148.03 105.335) (width 0.7) (layer F.Cu) (net 210) (status 10))
  (segment (start 147.955 105.41) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 148.754999 104.610001) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 147.955 104.610001) (end 138.43 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 137.16 104.610001) (end 137.16 105.41) (width 0.7) (layer B.Cu) (net 210))
  (via (at 137.16 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 137.16 105.41) (end 137.16 103.355) (width 0.7) (layer F.Cu) (net 210) (status 20))
  (segment (start 119.38 104.610001) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 118.745 104.775) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 118.745 105.41) (end 118.745 104.775) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 137.16 102.985) (end 137.16 105.41) (width 0.35) (layer B.Cu) (net 210) (status 10))
  (segment (start 107.95 105.41) (end 107.95 102.858) (width 0.35) (layer B.Cu) (net 210) (status 20))
  (segment (start 107.95 102.985) (end 107.95 105.41) (width 0.35) (layer B.Cu) (net 210) (status 10))
  (segment (start 119.38 104.610001) (end 109.22 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 109.22 104.610001) (end 108.749999 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 107.95 105.41) (end 107.95 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 109.22 104.610001) (end 107.95 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 166.37 103.0485) (end 166.37 105.41) (width 0.35) (layer B.Cu) (net 210) (status 10))
  (segment (start 126.8095 103.573) (end 126.8095 104.610001) (width 0.35) (layer B.Cu) (net 210))
  (segment (start 126.8095 104.610001) (end 119.38 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 137.16 104.610001) (end 126.8095 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 155.575 103.6485) (end 155.575 104.610001) (width 0.35) (layer B.Cu) (net 210))
  (segment (start 155.575 103.0485) (end 155.575 103.6485) (width 0.35) (layer B.Cu) (net 210) (status 10))
  (segment (start 126.8095 102.973) (end 126.8095 103.573) (width 0.35) (layer B.Cu) (net 210) (status 10))
  (segment (start 138.43 104.610001) (end 137.16 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 148.754999 104.610001) (end 165.570001 104.610001) (width 0.7) (layer B.Cu) (net 210))
  (segment (start 163.047 20.066) (end 164.211 20.066) (width 0.7) (layer F.Cu) (net 210) (tstamp 5BC64E24))
  (segment (start 165.227 20.066) (end 164.211 20.066) (width 0.7) (layer F.Cu) (net 210) (tstamp 5BC64D22))
  (segment (start 165.227 14.41) (end 165.227 16.51) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D46))
  (segment (start 155.362 12.065) (end 155.362 12.7) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D16))
  (segment (start 154.945 10.165) (end 155.362 10.582) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D34))
  (segment (start 155.362 10.582) (end 155.362 12.065) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D10))
  (segment (start 153.035 10.165) (end 154.945 10.165) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64E39))
  (segment (start 164.787 13.97) (end 165.227 14.41) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64DF7))
  (segment (start 155.362 12.7) (end 156.632 13.97) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D5E))
  (segment (start 156.632 13.97) (end 164.787 13.97) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64DF4))
  (segment (start 165.227 18.542) (end 165.227 20.066) (width 0.7) (layer F.Cu) (net 210) (tstamp 5BC64E2D))
  (segment (start 165.227 18.542) (end 165.227 16.51) (width 0.7) (layer F.Cu) (net 210) (tstamp 5BC64E33))
  (segment (start 144.145 20.955) (end 144.145 20.05) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64D5B))
  (segment (start 148.545 21.905) (end 150.765 19.685) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64D55))
  (segment (start 140.335 21.905) (end 142.875 21.905) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64D4F))
  (segment (start 150.765 19.685) (end 151.765 19.685) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64D49))
  (segment (start 142.875 21.905) (end 143.195 21.905) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64D4C))
  (segment (start 144.145 20.955) (end 144.145 21.905) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64E51))
  (segment (start 144.145 21.905) (end 148.545 21.905) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64E5A))
  (segment (start 142.875 21.905) (end 144.145 21.905) (width 0.35) (layer F.Cu) (net 219) (tstamp 5BC64E4E))
  (segment (start 137.795 29.53) (end 137.795 27.305) (width 0.35) (layer F.Cu) (net 229) (tstamp 5BC64D19))
  (segment (start 139.065 23.815) (end 142.24 23.815) (width 0.35) (layer F.Cu) (net 229) (tstamp 5BC64E42))
  (segment (start 137.795 25.085) (end 139.065 23.815) (width 0.35) (layer F.Cu) (net 229) (tstamp 5BC64E48))
  (segment (start 137.795 27.305) (end 137.795 25.085) (width 0.35) (layer F.Cu) (net 229) (tstamp 5BC64E4B))
  (segment (start 119.6735 49.784) (end 121.285 49.784) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 128.905 48.641) (end 128.905 46.228) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 121.92 49.149) (end 128.397 49.149) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 121.285 49.784) (end 121.92 49.149) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 128.397 49.149) (end 132.207 49.149) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 128.905 48.641) (end 128.905 49.022) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 132.207 47.47) (end 132.207 49.149) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 126.365 47.879) (end 126.365 46.228) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 125.857 48.387) (end 126.365 47.879) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 119.6735 48.387) (end 125.857 48.387) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 121.285 46.99) (end 119.6735 46.99) (width 0.35) (layer F.Cu) (net 246))
  (via (at 92.71 100.203) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 247))
  (segment (start 92.837 58.801) (end 92.837 57.888) (width 0.35) (layer B.Cu) (net 247))
  (segment (start 92.202 59.436) (end 92.837 58.801) (width 0.35) (layer B.Cu) (net 247))
  (segment (start 92.202 98.56363) (end 92.202 59.436) (width 0.35) (layer B.Cu) (net 247))
  (segment (start 92.71 99.07163) (end 92.202 98.56363) (width 0.35) (layer B.Cu) (net 247))
  (segment (start 92.71 100.203) (end 92.71 99.07163) (width 0.35) (layer B.Cu) (net 247))
  (segment (start 94.107 100.203) (end 92.71 100.203) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 95.504 101.6) (end 94.107 100.203) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 109.68 101.6) (end 95.504 101.6) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 111.11 103.03) (end 109.68 101.6) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 111.76 103.03) (end 111.11 103.03) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 101.727 53.561) (end 101.727 54.102) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 104.648 50.165) (end 104.013 50.165) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 101.727 52.451) (end 101.727 53.561) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 104.013 50.165) (end 101.727 52.451) (width 0.35) (layer F.Cu) (net 248))
  (via (at 98.552 94.361) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 249))
  (segment (start 170.18 99.949) (end 170.18 102.555) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 170.18 102.555) (end 170.18 103.03) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 98.552 94.361) (end 98.552 97.409) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 169.291 99.06) (end 170.18 99.949) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 100.203 99.06) (end 169.291 99.06) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 98.552 97.409) (end 100.203 99.06) (width 0.35) (layer F.Cu) (net 249))
  (segment (start 95.885 94.361) (end 98.552 94.361) (width 0.35) (layer B.Cu) (net 249))
  (segment (start 95.25 93.726) (end 95.885 94.361) (width 0.35) (layer B.Cu) (net 249))
  (segment (start 95.25 62.103) (end 95.25 93.726) (width 0.35) (layer B.Cu) (net 249))
  (segment (start 98.425 58.928) (end 95.25 62.103) (width 0.35) (layer B.Cu) (net 249))
  (segment (start 98.425 57.888) (end 98.425 58.928) (width 0.35) (layer B.Cu) (net 249))
  (segment (start 99.70663 99.695) (end 99.822 99.695) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 96.901 95.758) (end 96.901 96.88937) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 159.385 103.03) (end 159.385 100.457) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 96.901 96.88937) (end 99.70663 99.695) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 100.076 99.695) (end 99.822 99.695) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 159.385 100.457) (end 158.623 99.695) (width 0.35) (layer F.Cu) (net 250))
  (via (at 96.901 95.758) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 250))
  (segment (start 158.623 99.695) (end 129.794 99.695) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 129.794 99.695) (end 100.076 99.695) (width 0.35) (layer F.Cu) (net 250))
  (segment (start 95.123 95.758) (end 96.901 95.758) (width 0.35) (layer B.Cu) (net 250))
  (segment (start 94.488 61.595) (end 94.488 95.123) (width 0.35) (layer B.Cu) (net 250))
  (segment (start 97.028 59.055) (end 94.488 61.595) (width 0.35) (layer B.Cu) (net 250))
  (segment (start 94.488 95.123) (end 95.123 95.758) (width 0.35) (layer B.Cu) (net 250))
  (segment (start 97.028 57.888) (end 97.028 59.055) (width 0.35) (layer B.Cu) (net 250))
  (segment (start 100.21 51.828) (end 99.394 51.828) (width 0.35) (layer F.Cu) (net 251))
  (segment (start 99.394 51.828) (end 98.794 51.828) (width 0.35) (layer F.Cu) (net 251))
  (segment (start 102.948 49.09) (end 100.21 51.828) (width 0.35) (layer F.Cu) (net 251))
  (segment (start 102.948 48.465) (end 102.948 49.09) (width 0.35) (layer F.Cu) (net 251))
  (segment (start 99.406 50.419) (end 102.16 47.665) (width 0.35) (layer F.Cu) (net 252))
  (segment (start 102.16 47.665) (end 102.948 47.665) (width 0.35) (layer F.Cu) (net 252))
  (segment (start 98.806 50.419) (end 99.406 50.419) (width 0.35) (layer F.Cu) (net 252))
  (segment (start 91.44 57.888) (end 91.44 98.044) (width 0.35) (layer B.Cu) (net 253))
  (via (at 91.44 101.727) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 253))
  (segment (start 91.44 98.044) (end 91.44 101.727) (width 0.35) (layer B.Cu) (net 253))
  (segment (start 94.107 101.727) (end 91.44 101.727) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 95.41 103.03) (end 94.107 101.727) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 100.965 103.03) (end 95.41 103.03) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 102.948 46.865) (end 101.598 46.865) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 99.441 49.022) (end 98.806 49.022) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 101.598 46.865) (end 99.441 49.022) (width 0.35) (layer F.Cu) (net 254))
  (via (at 95.377 97.155) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 255))
  (segment (start 97.79 99.568) (end 95.377 97.155) (width 0.35) (layer F.Cu) (net 255))
  (segment (start 98.552 100.33) (end 97.79 99.568) (width 0.35) (layer F.Cu) (net 255))
  (segment (start 137.62 100.33) (end 98.552 100.33) (width 0.35) (layer F.Cu) (net 255))
  (segment (start 140.32 103.03) (end 137.62 100.33) (width 0.35) (layer F.Cu) (net 255))
  (segment (start 140.97 103.03) (end 140.32 103.03) (width 0.35) (layer F.Cu) (net 255))
  (segment (start 93.726 96.647) (end 94.234 97.155) (width 0.35) (layer B.Cu) (net 255))
  (segment (start 93.726 60.96) (end 93.726 96.647) (width 0.35) (layer B.Cu) (net 255))
  (segment (start 95.631 59.055) (end 93.726 60.96) (width 0.35) (layer B.Cu) (net 255))
  (segment (start 94.234 97.155) (end 95.377 97.155) (width 0.35) (layer B.Cu) (net 255))
  (segment (start 95.631 57.888) (end 95.631 59.055) (width 0.35) (layer B.Cu) (net 255))
  (segment (start 92.964 60.452) (end 92.964 96.901) (width 0.35) (layer B.Cu) (net 256))
  (segment (start 94.234 59.182) (end 92.964 60.452) (width 0.35) (layer B.Cu) (net 256))
  (segment (start 94.234 57.888) (end 94.234 59.182) (width 0.35) (layer B.Cu) (net 256))
  (segment (start 92.964 97.663) (end 93.98 98.679) (width 0.35) (layer B.Cu) (net 256))
  (segment (start 92.964 96.901) (end 92.964 97.663) (width 0.35) (layer B.Cu) (net 256))
  (via (at 93.98 98.679) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 256))
  (segment (start 96.266 100.965) (end 93.98 98.679) (width 0.35) (layer F.Cu) (net 256))
  (segment (start 129.235 100.965) (end 96.266 100.965) (width 0.35) (layer F.Cu) (net 256))
  (segment (start 130.175 101.905) (end 129.235 100.965) (width 0.35) (layer F.Cu) (net 256))
  (segment (start 130.175 103.03) (end 130.175 101.905) (width 0.35) (layer F.Cu) (net 256))
  (segment (start 102.948 46.065) (end 101.128 46.065) (width 0.35) (layer F.Cu) (net 257))
  (segment (start 99.568 47.625) (end 98.806 47.625) (width 0.35) (layer F.Cu) (net 257))
  (segment (start 101.128 46.065) (end 99.568 47.625) (width 0.35) (layer F.Cu) (net 257))
  (segment (start 132.715 27.305) (end 136.525 27.305) (width 0.7) (layer F.Cu) (net 268) (tstamp 5BC64E60))
  (segment (start 136.525 27.305) (end 136.525 21.905) (width 0.7) (layer F.Cu) (net 268) (tstamp 5BC64D25))
  (segment (start 136.525 21.905) (end 137.795 21.905) (width 0.7) (layer F.Cu) (net 268) (tstamp 5BC64D2B))
  (segment (start 132.715 27.305) (end 132.715 28.6) (width 0.7) (layer F.Cu) (net 268) (tstamp 5BC64D40))
  (segment (start 135.895 30.53) (end 135.895 29.53) (width 0.35) (layer F.Cu) (net 266) (tstamp 5BC64E5D))
  (segment (start 135.895 30.765) (end 135.895 30.53) (width 0.35) (layer F.Cu) (net 266) (tstamp 5BC64E81))
  (segment (start 134.91 31.75) (end 135.895 30.765) (width 0.35) (layer F.Cu) (net 266) (tstamp 5BC64E84))
  (segment (start 133.985 31.75) (end 134.91 31.75) (width 0.35) (layer F.Cu) (net 266) (tstamp 5BC64E66))
  (segment (start 102.948 42.865) (end 100.523 42.865) (width 0.35) (layer F.Cu) (net 269))
  (segment (start 99.568 41.91) (end 98.806 41.91) (width 0.35) (layer F.Cu) (net 269))
  (segment (start 100.523 42.865) (end 99.568 41.91) (width 0.35) (layer F.Cu) (net 269))
  (segment (start 98.806 40.513) (end 99.441 40.513) (width 0.35) (layer F.Cu) (net 272))
  (segment (start 100.993 42.065) (end 102.948 42.065) (width 0.35) (layer F.Cu) (net 272))
  (segment (start 99.441 40.513) (end 100.993 42.065) (width 0.35) (layer F.Cu) (net 272))
  (segment (start 99.406 39.116) (end 98.806 39.116) (width 0.35) (layer F.Cu) (net 273))
  (segment (start 101.555 41.265) (end 99.406 39.116) (width 0.35) (layer F.Cu) (net 273))
  (segment (start 102.948 41.265) (end 101.555 41.265) (width 0.35) (layer F.Cu) (net 273))
  (segment (start 105.448 37.665) (end 103.251 35.468) (width 0.35) (layer F.Cu) (net 276))
  (segment (start 105.448 38.765) (end 105.448 37.665) (width 0.35) (layer F.Cu) (net 276))
  (segment (start 103.251 35.468) (end 103.251 34.925) (width 0.35) (layer F.Cu) (net 276))
  (segment (start 115.824 53.502) (end 115.824 54.102) (width 0.35) (layer F.Cu) (net 277))
  (segment (start 115.824 52.716) (end 115.824 53.502) (width 0.35) (layer F.Cu) (net 277))
  (segment (start 113.273 50.165) (end 115.824 52.716) (width 0.35) (layer F.Cu) (net 277))
  (segment (start 112.648 50.165) (end 113.273 50.165) (width 0.35) (layer F.Cu) (net 277))
  (segment (start 114.427 53.594) (end 114.427 53.848) (width 0.35) (layer F.Cu) (net 279))
  (segment (start 114.427 53.848) (end 114.427 54.102) (width 0.35) (layer F.Cu) (net 279))
  (segment (start 111.848 51.054) (end 111.887 51.054) (width 0.35) (layer F.Cu) (net 279))
  (segment (start 111.887 51.054) (end 114.427 53.594) (width 0.35) (layer F.Cu) (net 279))
  (segment (start 111.848 50.165) (end 111.848 51.054) (width 0.35) (layer F.Cu) (net 279))
  (segment (start 113.03 53.502) (end 113.03 54.102) (width 0.35) (layer F.Cu) (net 280))
  (segment (start 111.048 51.52) (end 113.03 53.502) (width 0.35) (layer F.Cu) (net 280))
  (segment (start 111.048 50.165) (end 111.048 51.52) (width 0.35) (layer F.Cu) (net 280))
  (segment (start 111.633 53.514) (end 111.633 54.114) (width 0.35) (layer F.Cu) (net 282))
  (segment (start 110.248 52.129) (end 111.633 53.514) (width 0.35) (layer F.Cu) (net 282))
  (segment (start 110.248 50.165) (end 110.248 52.129) (width 0.35) (layer F.Cu) (net 282))
  (segment (start 110.236 53.34) (end 110.236 54.102) (width 0.35) (layer F.Cu) (net 283))
  (segment (start 109.448 52.552) (end 110.236 53.34) (width 0.35) (layer F.Cu) (net 283))
  (segment (start 109.448 50.165) (end 109.448 52.552) (width 0.35) (layer F.Cu) (net 283))

  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BC646F5) (hatch full 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 172.72 37.465) (xy 172.72 34.29) (xy 168.275 34.29) (xy 168.275 27.10845) (xy 171.45 27.10845)
        (xy 171.45 29.21) (xy 177.165 29.21) (xy 177.165 37.465)
      )
    )
  )
  (zone (net 160) (net_name "/5V PSU /SwE") (layer F.Cu) (tstamp 5BC646F2) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 177.8 37.465) (xy 177.8 26.4795) (xy 179.07 26.4795) (xy 179.07 31.115) (xy 187.325 31.115)
        (xy 187.325 37.465)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (tstamp 5BB8CC5B) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 8.255) (xy 189.23 8.255) (xy 189.23 107.95) (xy 89.535 107.95)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (tstamp 5BB8CC58) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 8.255) (xy 189.23 8.255) (xy 189.23 107.95) (xy 89.535 107.95)
      )
    )
  )
  (zone (net 267) (net_name "/3_3V PSU/HC_Plain") (layer F.Cu) (tstamp 5BC64CC5) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.35 30.48) (xy 140.97 30.48) (xy 143.51 27.94) (xy 143.51 22.86) (xy 150.495 22.86)
        (xy 150.495 38.1) (xy 133.35 38.1)
      )
    )
  )
  (zone (net 241) (net_name "/3_3V PSU/MC34063_HC_A") (layer F.Cu) (tstamp 5BC64D0D) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 156.083 13.97) (xy 156.083 37.846) (xy 167.767 37.846) (xy 167.767 22.098) (xy 161.163 22.098)
        (xy 161.163 13.97)
      )
    )
  )
  (zone (net 268) (net_name "/3_3V PSU/HC_Plain_b") (layer F.Cu) (tstamp 5BC64929) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 127.127 26.67) (xy 134.747 26.67) (xy 134.747 38.354) (xy 124.587 38.354) (xy 124.587 26.67)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 112.141 48.641) (xy 104.521 48.641) (xy 104.521 40.259) (xy 112.903 40.259) (xy 112.903 48.641)
      )
    )
  )
)
