(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")

  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 1602)
    (zones 0)
    (modules 277)
    (nets 269)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 1)
    (trace_clearance 0.24)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.9)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (user_via 1.4 0.9)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_fffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "../../../Desktop/"))
  )

  (net 0 "")
  (net 1 "Net-(C802-Pad1)")
  (net 2 "Net-(C702-Pad1)")
  (net 3 "Net-(C602-Pad1)")
  (net 4 "Net-(C502-Pad1)")
  (net 5 "Net-(C402-Pad1)")
  (net 6 "Net-(C302-Pad1)")
  (net 7 VCC)
  (net 8 GND)
  (net 9 "Net-(R808-Pad2)")
  (net 10 "Net-(R807-Pad2)")
  (net 11 "Net-(R806-Pad2)")
  (net 12 "Net-(R805-Pad2)")
  (net 13 ~enable_Shiftregister)
  (net 14 "Net-(R804-Pad2)")
  (net 15 "Net-(R803-Pad2)")
  (net 16 "Net-(R802-Pad2)")
  (net 17 "Net-(R801-Pad2)")
  (net 18 "Net-(R701-Pad2)")
  (net 19 "Net-(R702-Pad2)")
  (net 20 "Net-(R703-Pad2)")
  (net 21 "Net-(R704-Pad2)")
  (net 22 "Net-(R705-Pad2)")
  (net 23 "Net-(R706-Pad2)")
  (net 24 "Net-(R707-Pad2)")
  (net 25 "Net-(R708-Pad2)")
  (net 26 "Net-(R608-Pad2)")
  (net 27 "Net-(R607-Pad2)")
  (net 28 "Net-(R606-Pad2)")
  (net 29 "Net-(R605-Pad2)")
  (net 30 "Net-(R604-Pad2)")
  (net 31 "Net-(R603-Pad2)")
  (net 32 "Net-(R602-Pad2)")
  (net 33 "Net-(R601-Pad2)")
  (net 34 "Net-(R501-Pad2)")
  (net 35 "Net-(R502-Pad2)")
  (net 36 "Net-(R503-Pad2)")
  (net 37 "Net-(R504-Pad2)")
  (net 38 "Net-(R505-Pad2)")
  (net 39 "Net-(R506-Pad2)")
  (net 40 "Net-(R507-Pad2)")
  (net 41 "Net-(R508-Pad2)")
  (net 42 "Net-(R408-Pad2)")
  (net 43 "Net-(R407-Pad2)")
  (net 44 "Net-(R406-Pad2)")
  (net 45 "Net-(R405-Pad2)")
  (net 46 "Net-(R404-Pad2)")
  (net 47 "Net-(R403-Pad2)")
  (net 48 "Net-(R402-Pad2)")
  (net 49 "Net-(R401-Pad2)")
  (net 50 "Net-(R301-Pad2)")
  (net 51 "Net-(R302-Pad2)")
  (net 52 "Net-(R303-Pad2)")
  (net 53 "Net-(R304-Pad2)")
  (net 54 "Net-(R305-Pad2)")
  (net 55 "Net-(R306-Pad2)")
  (net 56 "Net-(R307-Pad2)")
  (net 57 "Net-(R308-Pad2)")
  (net 58 /Tubes/sheet5BB3E86D/e)
  (net 59 /Tubes/sheet5BB3E86D/d)
  (net 60 /Tubes/sheet5BB3E86D/g)
  (net 61 /Tubes/sheet5BB3E86D/f)
  (net 62 /Tubes/sheet5BB3E86D/a)
  (net 63 /Tubes/sheet5BB3E86D/c)
  (net 64 /Tubes/sheet5BB3E86D/b)
  (net 65 /Tubes/sheet5BB3E86D/Dot)
  (net 66 /Tubes/sheet5BB3E86C/Dot)
  (net 67 /Tubes/sheet5BB3E86C/b)
  (net 68 /Tubes/sheet5BB3E86C/c)
  (net 69 /Tubes/sheet5BB3E86C/a)
  (net 70 /Tubes/sheet5BB3E86C/f)
  (net 71 /Tubes/sheet5BB3E86C/g)
  (net 72 /Tubes/sheet5BB3E86C/d)
  (net 73 /Tubes/sheet5BB3E86C/e)
  (net 74 /Tubes/sheet5BB3BB93/e)
  (net 75 /Tubes/sheet5BB3BB93/d)
  (net 76 /Tubes/sheet5BB3BB93/g)
  (net 77 /Tubes/sheet5BB3BB93/f)
  (net 78 /Tubes/sheet5BB3BB93/a)
  (net 79 /Tubes/sheet5BB3BB93/c)
  (net 80 /Tubes/sheet5BB3BB93/b)
  (net 81 /Tubes/sheet5BB3BB93/Dot)
  (net 82 /Tubes/sheet5BB36ADE/Dot)
  (net 83 /Tubes/sheet5BB36ADE/b)
  (net 84 /Tubes/sheet5BB36ADE/c)
  (net 85 /Tubes/sheet5BB36ADE/a)
  (net 86 /Tubes/sheet5BB36ADE/f)
  (net 87 /Tubes/sheet5BB36ADE/g)
  (net 88 /Tubes/sheet5BB36ADE/d)
  (net 89 /Tubes/sheet5BB36ADE/e)
  (net 90 /Tubes/sheet5BB32DC8/e)
  (net 91 /Tubes/sheet5BB32DC8/d)
  (net 92 /Tubes/sheet5BB32DC8/g)
  (net 93 /Tubes/sheet5BB32DC8/f)
  (net 94 /Tubes/sheet5BB32DC8/a)
  (net 95 /Tubes/sheet5BB32DC8/c)
  (net 96 /Tubes/sheet5BB32DC8/b)
  (net 97 /Tubes/sheet5BB32DC8/Dot)
  (net 98 /Tubes/IV-9_Tube/Dot)
  (net 99 /Tubes/IV-9_Tube/b)
  (net 100 /Tubes/IV-9_Tube/c)
  (net 101 /Tubes/IV-9_Tube/a)
  (net 102 /Tubes/IV-9_Tube/f)
  (net 103 /Tubes/IV-9_Tube/g)
  (net 104 /Tubes/IV-9_Tube/d)
  (net 105 /Tubes/IV-9_Tube/e)
  (net 106 /Tubes/sheet5BB3E86C/Data_in)
  (net 107 /Tubes/sheet5BB36ADE/Data_in)
  (net 108 /Tubes/sheet5BB3BB93/Data_in)
  (net 109 /Tubes/sheet5BB32DC8/Data_in)
  (net 110 /Tubes/IV-9_Tube/Data_in)
  (net 111 "Net-(R902-Pad2)")
  (net 112 "Net-(R914-Pad2)")
  (net 113 "Net-(R916-Pad2)")
  (net 114 "Net-(R915-Pad2)")
  (net 115 "Net-(R901-Pad2)")
  (net 116 "Net-(R913-Pad2)")
  (net 117 "Net-(R912-Pad2)")
  (net 118 "Net-(R911-Pad2)")
  (net 119 "Net-(R910-Pad2)")
  (net 120 "Net-(R909-Pad2)")
  (net 121 "Net-(R908-Pad2)")
  (net 122 "Net-(R907-Pad2)")
  (net 123 clk)
  (net 124 "Net-(R906-Pad2)")
  (net 125 "Net-(R905-Pad2)")
  (net 126 MISO)
  (net 127 MOSI)
  (net 128 "Net-(R904-Pad2)")
  (net 129 "Net-(R903-Pad2)")
  (net 130 Currentsensing_Tube_6)
  (net 131 Currentsensing_Tube_5)
  (net 132 Currentsensing_Tube_4)
  (net 133 Currentsensing_Tube_3)
  (net 134 Currentsensing_Tube_2)
  (net 135 Currentsensing_Tube_1)
  (net 136 /uC/XTAL2)
  (net 137 /uC/XTAL1)
  (net 138 "Net-(C901-Pad1)")
  (net 139 "Net-(R921-Pad2)")
  (net 140 "Net-(R918-Pad2)")
  (net 141 "Net-(R924-Pad2)")
  (net 142 "Net-(R923-Pad2)")
  (net 143 "Net-(R922-Pad2)")
  (net 144 "Net-(R920-Pad2)")
  (net 145 "Net-(R919-Pad2)")
  (net 146 SCL)
  (net 147 SDA)
  (net 148 "Net-(U1101-Pad4)")
  (net 149 "Net-(U1101-Pad3)")
  (net 150 "Net-(U1101-Pad1)")
  (net 151 +12V)
  (net 152 "Net-(R1201-Pad1)")
  (net 153 "Net-(C1203-Pad1)")
  (net 154 "Net-(R1202-Pad2)")
  (net 155 "Net-(R1203-Pad1)")
  (net 156 "Net-(R1302-Pad2)")
  (net 157 "Net-(R1303-Pad1)")
  (net 158 "Net-(C1303-Pad1)")
  (net 159 "Net-(RV1201-Pad2)")
  (net 160 "/5V PSU /SwE")
  (net 161 "Net-(D1303-Pad1)")
  (net 162 "Net-(Q1301-Pad3)")
  (net 163 "Net-(Q1302-Pad3)")
  (net 164 "Net-(C1306-Pad1)")
  (net 165 "Net-(D1303-Pad2)")
  (net 166 enable_2.5V_PSU)
  (net 167 "Net-(D1401-Pad1)")
  (net 168 "Net-(F1401-Pad2)")
  (net 169 /Tubes/IV-9_Tube/Data_out)
  (net 170 reset_Shiftregister)
  (net 171 ~latch_Shiftregister)
  (net 172 "Net-(U503-Pad4)")
  (net 173 "Net-(U803-Pad4)")
  (net 174 "Net-(U703-Pad4)")
  (net 175 "Net-(U303-Pad4)")
  (net 176 "Net-(U603-Pad4)")
  (net 177 "Net-(U403-Pad4)")
  (net 178 Encoder_B)
  (net 179 "Net-(R1501-Pad1)")
  (net 180 "Net-(R1502-Pad1)")
  (net 181 Encoder_A)
  (net 182 Encoder_push)
  (net 183 "Net-(D202-Pad1)")
  (net 184 Dot)
  (net 185 "Net-(D201-Pad1)")
  (net 186 "Net-(D202-Pad2)")
  (net 187 "Net-(D201-Pad2)")
  (net 188 Dip_3)
  (net 189 Dip_2)
  (net 190 Dip_1)
  (net 191 Tube_LED)
  (net 192 LED_Error)
  (net 193 Rx)
  (net 194 +3V3)
  (net 195 "Net-(U1601-Pad2)")
  (net 196 "Net-(U1601-Pad4)")
  (net 197 "Net-(U1601-Pad5)")
  (net 198 "Net-(U1601-Pad6)")
  (net 199 "Net-(U1601-Pad14)")
  (net 200 "Net-(U1601-Pad16)")
  (net 201 "Net-(U1601-Pad17)")
  (net 202 Tx)
  (net 203 "/3_3V PSU/MC34063_Feedback")
  (net 204 "Net-(D1601-Pad2)")
  (net 205 "Net-(R1601-Pad1)")
  (net 206 PSU_3.3V_feedback)
  (net 207 enable_3.3V_PSU)
  (net 208 "Net-(U1601-Pad1)")
  (net 209 "Net-(U1601-Pad15)")
  (net 210 "/3_3V PSU/SwE")
  (net 211 "Net-(L1601-Pad2)")
  (net 212 "Net-(R1607-Pad1)")
  (net 213 V_Bat)
  (net 214 "Net-(D1602-Pad1)")
  (net 215 "/3_3V PSU/MC34063_HC_A")
  (net 216 /uC/MOSI_ISP)
  (net 217 /uC/MISO_ISP)
  (net 218 /uC/clk_ISP)
  (net 219 /uC/~Reset_ISP)
  (net 220 "Net-(R411-Pad2)")
  (net 221 "Net-(R933-Pad2)")
  (net 222 "Net-(R711-Pad2)")
  (net 223 "Net-(R811-Pad2)")
  (net 224 "Net-(R934-Pad2)")
  (net 225 "Net-(R935-Pad2)")
  (net 226 "Net-(R311-Pad2)")
  (net 227 "Net-(R936-Pad2)")
  (net 228 "Net-(R611-Pad2)")
  (net 229 "Net-(R511-Pad2)")
  (net 230 "Net-(R937-Pad2)")
  (net 231 "Net-(Q1201-Pad4)")
  (net 232 "/3_3V PSU/HC_Plain")
  (net 233 "/3_3V PSU/HC_Plain_b")
  (net 234 "Net-(R946-Pad2)")
  (net 235 "Net-(R946-Pad1)")
  (net 236 "Net-(R945-Pad1)")
  (net 237 "Net-(R945-Pad2)")
  (net 238 "Net-(R944-Pad2)")
  (net 239 "Net-(R944-Pad1)")
  (net 240 "Net-(R943-Pad1)")
  (net 241 "Net-(R943-Pad2)")
  (net 242 "Net-(R942-Pad2)")
  (net 243 "Net-(R942-Pad1)")
  (net 244 "Net-(R941-Pad2)")
  (net 245 "Net-(R940-Pad2)")
  (net 246 "Net-(R940-Pad1)")
  (net 247 "Net-(R939-Pad2)")
  (net 248 "Net-(R938-Pad2)")
  (net 249 "Net-(R908-Pad1)")
  (net 250 "Net-(R909-Pad1)")
  (net 251 "Net-(R910-Pad1)")
  (net 252 "Net-(SW1401-Pad3)")
  (net 253 "Net-(U1601-Pad19)")
  (net 254 "Net-(U1601-Pad18)")
  (net 255 "Net-(D1603-Pad1)")
  (net 256 "Net-(D1604-Pad1)")
  (net 257 "Net-(D1603-Pad2)")
  (net 258 /WiFi/Antenna)
  (net 259 "Net-(U1502-Pad3)")
  (net 260 "Net-(U1501-Pad3)")
  (net 261 "Net-(R1606-Pad2)")
  (net 262 /Tubes/IV-9_Tube/Tube_LED)
  (net 263 "Net-(D801-Pad2)")
  (net 264 "Net-(D401-Pad2)")
  (net 265 "Net-(D701-Pad2)")
  (net 266 "Net-(D601-Pad2)")
  (net 267 "Net-(D301-Pad2)")
  (net 268 "Net-(D501-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.24)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net "/3_3V PSU/HC_Plain")
    (add_net "/3_3V PSU/HC_Plain_b")
    (add_net "/3_3V PSU/MC34063_Feedback")
    (add_net "/3_3V PSU/MC34063_HC_A")
    (add_net "/3_3V PSU/SwE")
    (add_net "/5V PSU /SwE")
    (add_net /Tubes/IV-9_Tube/Data_in)
    (add_net /Tubes/IV-9_Tube/Data_out)
    (add_net /Tubes/IV-9_Tube/Dot)
    (add_net /Tubes/IV-9_Tube/Tube_LED)
    (add_net /Tubes/IV-9_Tube/a)
    (add_net /Tubes/IV-9_Tube/b)
    (add_net /Tubes/IV-9_Tube/c)
    (add_net /Tubes/IV-9_Tube/d)
    (add_net /Tubes/IV-9_Tube/e)
    (add_net /Tubes/IV-9_Tube/f)
    (add_net /Tubes/IV-9_Tube/g)
    (add_net /Tubes/sheet5BB32DC8/Data_in)
    (add_net /Tubes/sheet5BB32DC8/Dot)
    (add_net /Tubes/sheet5BB32DC8/a)
    (add_net /Tubes/sheet5BB32DC8/b)
    (add_net /Tubes/sheet5BB32DC8/c)
    (add_net /Tubes/sheet5BB32DC8/d)
    (add_net /Tubes/sheet5BB32DC8/e)
    (add_net /Tubes/sheet5BB32DC8/f)
    (add_net /Tubes/sheet5BB32DC8/g)
    (add_net /Tubes/sheet5BB36ADE/Data_in)
    (add_net /Tubes/sheet5BB36ADE/Dot)
    (add_net /Tubes/sheet5BB36ADE/a)
    (add_net /Tubes/sheet5BB36ADE/b)
    (add_net /Tubes/sheet5BB36ADE/c)
    (add_net /Tubes/sheet5BB36ADE/d)
    (add_net /Tubes/sheet5BB36ADE/e)
    (add_net /Tubes/sheet5BB36ADE/f)
    (add_net /Tubes/sheet5BB36ADE/g)
    (add_net /Tubes/sheet5BB3BB93/Data_in)
    (add_net /Tubes/sheet5BB3BB93/Dot)
    (add_net /Tubes/sheet5BB3BB93/a)
    (add_net /Tubes/sheet5BB3BB93/b)
    (add_net /Tubes/sheet5BB3BB93/c)
    (add_net /Tubes/sheet5BB3BB93/d)
    (add_net /Tubes/sheet5BB3BB93/e)
    (add_net /Tubes/sheet5BB3BB93/f)
    (add_net /Tubes/sheet5BB3BB93/g)
    (add_net /Tubes/sheet5BB3E86C/Data_in)
    (add_net /Tubes/sheet5BB3E86C/Dot)
    (add_net /Tubes/sheet5BB3E86C/a)
    (add_net /Tubes/sheet5BB3E86C/b)
    (add_net /Tubes/sheet5BB3E86C/c)
    (add_net /Tubes/sheet5BB3E86C/d)
    (add_net /Tubes/sheet5BB3E86C/e)
    (add_net /Tubes/sheet5BB3E86C/f)
    (add_net /Tubes/sheet5BB3E86C/g)
    (add_net /Tubes/sheet5BB3E86D/Dot)
    (add_net /Tubes/sheet5BB3E86D/a)
    (add_net /Tubes/sheet5BB3E86D/b)
    (add_net /Tubes/sheet5BB3E86D/c)
    (add_net /Tubes/sheet5BB3E86D/d)
    (add_net /Tubes/sheet5BB3E86D/e)
    (add_net /Tubes/sheet5BB3E86D/f)
    (add_net /Tubes/sheet5BB3E86D/g)
    (add_net /uC/MISO_ISP)
    (add_net /uC/MOSI_ISP)
    (add_net /uC/XTAL1)
    (add_net /uC/XTAL2)
    (add_net /uC/clk_ISP)
    (add_net /uC/~Reset_ISP)
    (add_net Currentsensing_Tube_1)
    (add_net Currentsensing_Tube_2)
    (add_net Currentsensing_Tube_3)
    (add_net Currentsensing_Tube_4)
    (add_net Currentsensing_Tube_5)
    (add_net Currentsensing_Tube_6)
    (add_net Dip_1)
    (add_net Dip_2)
    (add_net Dip_3)
    (add_net Dot)
    (add_net Encoder_A)
    (add_net Encoder_B)
    (add_net Encoder_push)
    (add_net GND)
    (add_net LED_Error)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1203-Pad1)")
    (add_net "Net-(C1303-Pad1)")
    (add_net "Net-(C1306-Pad1)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C602-Pad1)")
    (add_net "Net-(C702-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C901-Pad1)")
    (add_net "Net-(D1303-Pad1)")
    (add_net "Net-(D1303-Pad2)")
    (add_net "Net-(D1401-Pad1)")
    (add_net "Net-(D1601-Pad2)")
    (add_net "Net-(D1602-Pad1)")
    (add_net "Net-(D1603-Pad1)")
    (add_net "Net-(D1603-Pad2)")
    (add_net "Net-(D1604-Pad1)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad1)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D401-Pad2)")
    (add_net "Net-(D501-Pad2)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D701-Pad2)")
    (add_net "Net-(D801-Pad2)")
    (add_net "Net-(F1401-Pad2)")
    (add_net "Net-(L1601-Pad2)")
    (add_net "Net-(Q1201-Pad4)")
    (add_net "Net-(Q1301-Pad3)")
    (add_net "Net-(Q1302-Pad3)")
    (add_net "Net-(R1201-Pad1)")
    (add_net "Net-(R1202-Pad2)")
    (add_net "Net-(R1203-Pad1)")
    (add_net "Net-(R1302-Pad2)")
    (add_net "Net-(R1303-Pad1)")
    (add_net "Net-(R1501-Pad1)")
    (add_net "Net-(R1502-Pad1)")
    (add_net "Net-(R1601-Pad1)")
    (add_net "Net-(R1606-Pad2)")
    (add_net "Net-(R1607-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad2)")
    (add_net "Net-(R306-Pad2)")
    (add_net "Net-(R307-Pad2)")
    (add_net "Net-(R308-Pad2)")
    (add_net "Net-(R311-Pad2)")
    (add_net "Net-(R401-Pad2)")
    (add_net "Net-(R402-Pad2)")
    (add_net "Net-(R403-Pad2)")
    (add_net "Net-(R404-Pad2)")
    (add_net "Net-(R405-Pad2)")
    (add_net "Net-(R406-Pad2)")
    (add_net "Net-(R407-Pad2)")
    (add_net "Net-(R408-Pad2)")
    (add_net "Net-(R411-Pad2)")
    (add_net "Net-(R501-Pad2)")
    (add_net "Net-(R502-Pad2)")
    (add_net "Net-(R503-Pad2)")
    (add_net "Net-(R504-Pad2)")
    (add_net "Net-(R505-Pad2)")
    (add_net "Net-(R506-Pad2)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R508-Pad2)")
    (add_net "Net-(R511-Pad2)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad2)")
    (add_net "Net-(R605-Pad2)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R607-Pad2)")
    (add_net "Net-(R608-Pad2)")
    (add_net "Net-(R611-Pad2)")
    (add_net "Net-(R701-Pad2)")
    (add_net "Net-(R702-Pad2)")
    (add_net "Net-(R703-Pad2)")
    (add_net "Net-(R704-Pad2)")
    (add_net "Net-(R705-Pad2)")
    (add_net "Net-(R706-Pad2)")
    (add_net "Net-(R707-Pad2)")
    (add_net "Net-(R708-Pad2)")
    (add_net "Net-(R711-Pad2)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad2)")
    (add_net "Net-(R805-Pad2)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R807-Pad2)")
    (add_net "Net-(R808-Pad2)")
    (add_net "Net-(R811-Pad2)")
    (add_net "Net-(R901-Pad2)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R904-Pad2)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(R907-Pad2)")
    (add_net "Net-(R908-Pad1)")
    (add_net "Net-(R908-Pad2)")
    (add_net "Net-(R909-Pad1)")
    (add_net "Net-(R909-Pad2)")
    (add_net "Net-(R910-Pad1)")
    (add_net "Net-(R910-Pad2)")
    (add_net "Net-(R911-Pad2)")
    (add_net "Net-(R912-Pad2)")
    (add_net "Net-(R913-Pad2)")
    (add_net "Net-(R914-Pad2)")
    (add_net "Net-(R915-Pad2)")
    (add_net "Net-(R916-Pad2)")
    (add_net "Net-(R918-Pad2)")
    (add_net "Net-(R919-Pad2)")
    (add_net "Net-(R920-Pad2)")
    (add_net "Net-(R921-Pad2)")
    (add_net "Net-(R922-Pad2)")
    (add_net "Net-(R923-Pad2)")
    (add_net "Net-(R924-Pad2)")
    (add_net "Net-(R933-Pad2)")
    (add_net "Net-(R934-Pad2)")
    (add_net "Net-(R935-Pad2)")
    (add_net "Net-(R936-Pad2)")
    (add_net "Net-(R937-Pad2)")
    (add_net "Net-(R938-Pad2)")
    (add_net "Net-(R939-Pad2)")
    (add_net "Net-(R940-Pad1)")
    (add_net "Net-(R940-Pad2)")
    (add_net "Net-(R941-Pad2)")
    (add_net "Net-(R942-Pad1)")
    (add_net "Net-(R942-Pad2)")
    (add_net "Net-(R943-Pad1)")
    (add_net "Net-(R943-Pad2)")
    (add_net "Net-(R944-Pad1)")
    (add_net "Net-(R944-Pad2)")
    (add_net "Net-(R945-Pad1)")
    (add_net "Net-(R945-Pad2)")
    (add_net "Net-(R946-Pad1)")
    (add_net "Net-(R946-Pad2)")
    (add_net "Net-(RV1201-Pad2)")
    (add_net "Net-(SW1401-Pad3)")
    (add_net "Net-(U1101-Pad1)")
    (add_net "Net-(U1101-Pad3)")
    (add_net "Net-(U1101-Pad4)")
    (add_net "Net-(U1501-Pad3)")
    (add_net "Net-(U1502-Pad3)")
    (add_net "Net-(U1601-Pad1)")
    (add_net "Net-(U1601-Pad14)")
    (add_net "Net-(U1601-Pad15)")
    (add_net "Net-(U1601-Pad16)")
    (add_net "Net-(U1601-Pad17)")
    (add_net "Net-(U1601-Pad18)")
    (add_net "Net-(U1601-Pad19)")
    (add_net "Net-(U1601-Pad2)")
    (add_net "Net-(U1601-Pad4)")
    (add_net "Net-(U1601-Pad5)")
    (add_net "Net-(U1601-Pad6)")
    (add_net "Net-(U303-Pad4)")
    (add_net "Net-(U403-Pad4)")
    (add_net "Net-(U503-Pad4)")
    (add_net "Net-(U603-Pad4)")
    (add_net "Net-(U703-Pad4)")
    (add_net "Net-(U803-Pad4)")
    (add_net PSU_3.3V_feedback)
    (add_net Rx)
    (add_net SCL)
    (add_net SDA)
    (add_net Tube_LED)
    (add_net Tx)
    (add_net VCC)
    (add_net V_Bat)
    (add_net clk)
    (add_net enable_2.5V_PSU)
    (add_net enable_3.3V_PSU)
    (add_net reset_Shiftregister)
    (add_net ~enable_Shiftregister)
    (add_net ~latch_Shiftregister)
  )

  (net_class Antenna ""
    (clearance 0.3)
    (trace_width 1.40626)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /WiFi/Antenna)
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB40647)
    (at 145.034 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3BB9E/5BB249BA)
    (fp_text reference U602 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B218)
    (at 159.004 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249EB)
    (attr smd)
    (fp_text reference R707 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B248)
    (at 160.401 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F2)
    (attr smd)
    (fp_text reference R706 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B278)
    (at 161.798 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F9)
    (attr smd)
    (fp_text reference R705 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2A8)
    (at 163.195 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249C8)
    (attr smd)
    (fp_text reference R704 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2D8)
    (at 164.592 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249CF)
    (attr smd)
    (fp_text reference R703 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B308)
    (at 165.989 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249D6)
    (attr smd)
    (fp_text reference R702 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B338)
    (at 157.607 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249E4)
    (attr smd)
    (fp_text reference R708 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B368)
    (at 140.97 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249E4)
    (attr smd)
    (fp_text reference R608 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B398)
    (at 142.367 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249EB)
    (attr smd)
    (fp_text reference R607 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3C8)
    (at 143.764 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F2)
    (attr smd)
    (fp_text reference R606 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3F8)
    (at 145.161 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F9)
    (attr smd)
    (fp_text reference R605 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B428)
    (at 146.558 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249C8)
    (attr smd)
    (fp_text reference R604 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D171)
    (at 147.955 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249CF)
    (attr smd)
    (fp_text reference R603 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D0DE)
    (at 149.352 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249D6)
    (attr smd)
    (fp_text reference R602 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4B8)
    (at 128.397 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249E4)
    (attr smd)
    (fp_text reference R508 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4E8)
    (at 129.794 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249EB)
    (attr smd)
    (fp_text reference R507 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B518)
    (at 131.191 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F2)
    (attr smd)
    (fp_text reference R506 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B548)
    (at 132.588 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F9)
    (attr smd)
    (fp_text reference R505 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B578)
    (at 133.985 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249C8)
    (attr smd)
    (fp_text reference R504 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5A8)
    (at 135.382 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249CF)
    (attr smd)
    (fp_text reference R503 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5D8)
    (at 136.779 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249D6)
    (attr smd)
    (fp_text reference R502 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B608)
    (at 111.76 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249E4)
    (attr smd)
    (fp_text reference R408 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B638)
    (at 113.157 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249EB)
    (attr smd)
    (fp_text reference R407 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B668)
    (at 114.554 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F2)
    (attr smd)
    (fp_text reference R406 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B698)
    (at 115.951 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F9)
    (attr smd)
    (fp_text reference R405 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6C8)
    (at 117.348 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249C8)
    (attr smd)
    (fp_text reference R404 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6F8)
    (at 118.745 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249CF)
    (attr smd)
    (fp_text reference R403 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.627 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B728)
    (at 120.142 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249D6)
    (attr smd)
    (fp_text reference R402 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B758)
    (at 99.187 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249E4)
    (attr smd)
    (fp_text reference R308 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B788)
    (at 100.584 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249EB)
    (attr smd)
    (fp_text reference R307 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7B8)
    (at 101.981 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F2)
    (attr smd)
    (fp_text reference R306 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7E8)
    (at 103.378 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F9)
    (attr smd)
    (fp_text reference R305 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B818)
    (at 104.775 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249C8)
    (attr smd)
    (fp_text reference R304 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B848)
    (at 106.172 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249CF)
    (attr smd)
    (fp_text reference R303 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B878)
    (at 107.569 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249D6)
    (attr smd)
    (fp_text reference R302 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8A8)
    (at 178.5747 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249D6)
    (attr smd)
    (fp_text reference R802 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B908)
    (at 177.1777 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249CF)
    (attr smd)
    (fp_text reference R803 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B938)
    (at 175.7807 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249C8)
    (attr smd)
    (fp_text reference R804 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B968)
    (at 174.3837 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F9)
    (attr smd)
    (fp_text reference R805 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B998)
    (at 172.9987 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F2)
    (attr smd)
    (fp_text reference R806 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B9C8)
    (at 171.6017 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249EB)
    (attr smd)
    (fp_text reference R807 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8D8)
    (at 170.1927 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249E4)
    (attr smd)
    (fp_text reference R808 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8544)
    (at 104.902 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB247DF/5BB7D8C2)
    (attr smd)
    (fp_text reference D301 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(D301-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8530)
    (at 115.824 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB32DD3/5BB7D8C2)
    (attr smd)
    (fp_text reference D401 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF851C)
    (at 134.239 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB36AE9/5BB7D8C2)
    (attr smd)
    (fp_text reference D501 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 268 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8508)
    (at 144.996 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3BB9E/5BB7D8C2)
    (attr smd)
    (fp_text reference D601 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84F4)
    (at 174.075 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E89F/5BB7D8C2)
    (attr smd)
    (fp_text reference D701 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(D701-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84E0)
    (at 163.28 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E878/5BB7D8C2)
    (attr smd)
    (fp_text reference D801 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 263 "Net-(D801-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCF18A5)
    (at 203.2 78.867)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BCF2CFF)
    (attr smd)
    (fp_text reference R203 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 191 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7B9FF)
    (at 115.316 111.252 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC38F55)
    (attr smd)
    (fp_text reference R510 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 268 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCE36B9)
    (at 217.17 61.341 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BCBB79A)
    (attr smd)
    (fp_text reference C1504 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCE3689)
    (at 215.011 61.329 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BCBB793)
    (attr smd)
    (fp_text reference C1505 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCE081D)
    (at 216.111 58.039 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5BC18D95/5BCBB7BA)
    (attr smd)
    (fp_text reference U1501 (at 0 -2.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN74LVC1T45DBV (at 0 2.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.9 -1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 -1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U1501-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 193 Rx))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R1606-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCE36EE)
    (at 216.111 64.704 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (path /5BC18D95/5BCB6D91)
    (attr smd)
    (fp_text reference U1502 (at 0 -2.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN74LVC1T45DBV (at 0 2.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -1.9 -1.8) (end -1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.9 1.8) (end 1.9 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 1.8) (end 1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.9 -1.8) (end -1.9 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 202 Tx))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U1502-Pad3)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BCDD2FF)
    (at 242.062 63.119 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BC18D95/5BBF235B)
    (attr smd)
    (fp_text reference U1603 (at 0 -3.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 24AA32A (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(U1601-Pad19)"))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(U1601-Pad18)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCBC5FF)
    (at 171.335 49.53 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B465E)
    (attr smd)
    (fp_text reference R1501 (at 0 1.45 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(R1501-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 178 Encoder_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCBC3E1)
    (at 171.323 48.133 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B4628)
    (attr smd)
    (fp_text reference R1502 (at 0 1.45 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 181 Encoder_A))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 180 "Net-(R1502-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_THT:SW_DIP_x3_W7.62mm_Slide (layer F.Cu) (tedit 5923F251) (tstamp 5BCB58CA)
    (at 215.265 95.758 90)
    (descr "3x-dip-switch, Slide, row spacing 7.62 mm (300 mils)")
    (tags "DIP Switch Slide 7.62mm 300mil")
    (path /5BBCA088/5BC054E9)
    (fp_text reference SW1503 (at 3.81 -3.48 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_DIP_x03 (at 3.81 8.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9 -2.7) (end -1.4 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9 7.7) (end 9 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 7.7) (end 9 7.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -2.7) (end -1.4 7.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.81 4.445) (end 3.81 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 4.445) (end 1.78 4.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 5.715) (end 5.84 4.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.715) (end 5.84 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.445) (end 1.78 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.81 1.905) (end 3.81 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 1.905) (end 1.78 1.905) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 3.175) (end 5.84 1.905) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 3.175) (end 5.84 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 1.905) (end 1.78 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.81 -0.635) (end 3.81 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 -0.635) (end 1.78 -0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 0.635) (end 5.84 -0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.635) (end 5.84 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.635) (end 1.78 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.2 7.56) (end -1.2 -2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.82 7.56) (end -1.2 7.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.82 -2.48) (end 8.82 7.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.2 -2.48) (end 8.82 -2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.81 4.445) (end 3.81 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 4.445) (end 1.78 4.445) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 5.715) (end 5.84 4.445) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.715) (end 5.84 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.445) (end 1.78 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 1.905) (end 3.81 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 1.905) (end 1.78 1.905) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 3.175) (end 5.84 1.905) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 3.175) (end 5.84 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 1.905) (end 1.78 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -0.635) (end 3.81 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 -0.635) (end 1.78 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 0.635) (end 5.84 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.635) (end 5.84 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.635) (end 1.78 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.08 -1.36) (end -0.08 -2.36) (layer F.Fab) (width 0.1))
    (fp_line (start -1.08 7.44) (end -1.08 -1.36) (layer F.Fab) (width 0.1))
    (fp_line (start 8.7 7.44) (end -1.08 7.44) (layer F.Fab) (width 0.1))
    (fp_line (start 8.7 -2.36) (end 8.7 7.44) (layer F.Fab) (width 0.1))
    (fp_line (start -0.08 -2.36) (end 8.7 -2.36) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -2.68) (end 1.14 -2.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -2.68) (end -1.4 -1.41) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 3.81 2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 6 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 188 Dip_3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 189 Dip_2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 190 Dip_1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_DIP_x3_W7.62mm_Slide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BCAF030)
    (at 57.285001 69.451001)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BCA1C95/5BCA1D0E)
    (attr smd)
    (fp_text reference D1604 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(D1604-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BCAE787)
    (at 56.585001 71.451001)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BCA1CF3)
    (attr smd)
    (fp_text reference D1603 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(D1603-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCADD2D)
    (at 62.385001 72.616001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D07)
    (attr smd)
    (fp_text reference R1609 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(D1603-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(D1604-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCADC7C)
    (at 59.835001 72.616001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D00)
    (attr smd)
    (fp_text reference R1604 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(D1604-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCADB6B)
    (at 55.885001 73.066001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D21)
    (attr smd)
    (fp_text reference R1603 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 LED_Error))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCAD802)
    (at 61.685001 70.101001)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BCA1CEC)
    (attr smd)
    (fp_text reference Q1601 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 192 LED_Error))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5BB5DBAF) (tstamp 5BB853D5)
    (at 107.824 22.0345 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5BB7D616/5BB7D6F8)
    (fp_text reference J1401 (at 2.794 -0.507 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.8 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 168 "Net-(F1401-Pad2)"))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC9ABE5)
    (at 132.9055 49.899 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC1BD67)
    (attr smd)
    (fp_text reference R932 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 /uC/clk_ISP))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C) (tstamp 5BC80D5F)
    (at 120.65 40.441 270)
    (descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (path /5BB48B05/5BB3A603)
    (attr smd)
    (fp_text reference Y901 (at 0 -2.8 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 0 2.8 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.093333 0) (layer F.Adhes) (width 0.186667))
    (fp_circle (center 0 0) (end 0.213333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.333333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.4 0) (layer F.Adhes) (width 0.1))
    (fp_line (start 3.1 -1.9) (end -3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 1.9) (end 3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.9) (end 3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.9) (end -3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.05 1.8) (end 2.7 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.05 -1.8) (end -3.05 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -1.8) (end -3.05 -1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 0.6) (end -1.5 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -1.4) (end -2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 1.4) (end -2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 1.6) (end -2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 1.6) (end -2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.4) (end 2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -1.4) (end 2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -1.6) (end 2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 -1.6) (end 2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (pad 1 smd rect (at -1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_5032-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F39)
    (at 103.251 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC662F3)
    (attr smd)
    (fp_text reference R943 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(R943-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(R943-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC79BE2)
    (at 108.204 34.798 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B3DE)
    (attr smd)
    (fp_text reference C906 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC1B200) (tstamp 5BC7B6C2)
    (at 108.089 53.975)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B34B)
    (attr smd)
    (fp_text reference C907 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48) (tstamp 5BC7BD1A)
    (at 108.648 44.465 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5BB48B05/5BC060C8)
    (attr smd)
    (fp_text reference U902 (at 0 -7.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega32-16AU (at 0 7.45 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.175 -4.6) (end -6.45 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -5.175 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 -4) (end -4 -5) (layer F.Fab) (width 0.15))
    (fp_line (start -5 5) (end -5 -4) (layer F.Fab) (width 0.15))
    (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.15))
    (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.15))
    (fp_line (start -4 -5) (end 5 -5) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R942-Pad2)"))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(R941-Pad2)"))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R940-Pad2)"))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R939-Pad2)"))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R938-Pad2)"))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R919-Pad2)"))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R907-Pad2)"))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R933-Pad2)"))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R934-Pad2)"))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(R935-Pad2)"))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R936-Pad2)"))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R937-Pad2)"))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(C901-Pad1)"))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(R946-Pad2)"))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(R945-Pad2)"))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(R944-Pad2)"))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R903-Pad2)"))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(R943-Pad2)"))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R911-Pad2)"))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R912-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R910-Pad2)"))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R909-Pad2)"))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R908-Pad2)"))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R918-Pad2)"))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R921-Pad2)"))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R920-Pad2)"))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R913-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R906-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7200E)
    (at 110.236 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5FA00)
    (attr smd)
    (fp_text reference R938 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(R938-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F7D)
    (at 111.633 54.864 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F9F9)
    (attr smd)
    (fp_text reference R939 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(R939-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F6C)
    (at 113.03 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D25)
    (attr smd)
    (fp_text reference R940 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(R940-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(R940-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F5B)
    (at 114.427 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D1E)
    (attr smd)
    (fp_text reference R941 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(R941-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC71F4A)
    (at 115.824 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC64046)
    (attr smd)
    (fp_text reference R942 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R942-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(R942-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B019)
    (at 98.056 39.116)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC685A2)
    (attr smd)
    (fp_text reference R944 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(R944-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(R944-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B049)
    (at 98.056 40.513)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D766)
    (attr smd)
    (fp_text reference R945 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(R945-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(R945-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AFE9)
    (at 98.056 41.91)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D75F)
    (attr smd)
    (fp_text reference R946 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(R946-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(R946-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC649EC)
    (at 184.978 17.145 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D469D9)
    (attr smd)
    (fp_text reference R1203 (at 0.828 3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R1203-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BC64797)
    (at 166.227 20.066)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB8D2EE/5BC34D02)
    (attr smd)
    (fp_text reference C1206 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-669_LFPAK_ThermalVias-2 (layer F.Cu) (tedit 59217BD0) (tstamp 5BCA4509)
    (at 133.182 33.655 180)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT669 Thermical Vias Power-SO8")
    (path /5BB8D2EE/5BC31987)
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference Q1201 (at 1.085 -5.26 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PHPT60406NY (at 1.085 5.58 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.66 4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.66 4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.855 2.5) (end 1.855 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 2.5) (end 1.855 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -2.5) (end -2.245 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.855 -2.5) (end -2.245 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 1.855 -2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 2.2) (end 1.855 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 3.155 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -1.65) (end -2.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -2.245 -2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -3.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.4) (end -2.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.85) (end -3.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -0.85) (end -3.245 -0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.85) (end -2.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.4) (end -3.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 0.4) (end -3.245 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 2.15) (end -2.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 1.7) (end -3.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 1.7) (end -3.245 1.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.345 -2.6) (end -2.345 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.345 2.4) (end -2.345 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 2.6) (end -1.155 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 -2.6) (end -1.205 -2.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 thru_hole rect (at 4.745 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 4 smd rect (at -2.835 1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(Q1201-Pad4)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 0.445 0 90) (size 4.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 2.645 0 90) (size 4.7 1.55) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.835 0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 232 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.835 -1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 232 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at -2.835 -0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 232 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.895 -0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 -1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 -1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers B.Cu B.Paste B.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC39110)
    (at 126.365 56.995 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E24)
    (attr smd)
    (fp_text reference D902 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 216 /uC/MOSI_ISP))
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC390F7)
    (at 126.365 41.303 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54DD6)
    (attr smd)
    (fp_text reference D903 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 218 /uC/clk_ISP))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_6.3x6.3_H3 (layer F.Cu) (tedit 5990349C) (tstamp 5BC64847)
    (at 179.07 33.655)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (path /5BB73C46/5BB49522)
    (attr smd)
    (fp_text reference L1201 (at 0 -4.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 4.45) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0 0) (end 1.91 1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end -1.91 -1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end -3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end -3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end 3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -3.4) (end -3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.4) (end 3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.4) (end 3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.4) (end -3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.3 -3.2) (end 3.3 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -3.2) (end 3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -1.5) (end -3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 3.2) (end -3.3 1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.2) (end -3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 1.5) (end 3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.75 0) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (pad 1 smd rect (at -2.75 0) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_Vishay_IHLP-6767 (layer F.Cu) (tedit 5990349D) (tstamp 5BCF3FDE)
    (at 155.575 30.48 180)
    (descr "Inductor, Vishay, IHLP series, 17.0mmx17.0mm")
    (tags "inductor vishay ihlp smd")
    (path /5BB8D2EE/59D4542E)
    (attr smd)
    (fp_text reference L1301 (at 0 -9.509 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 10.009 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.3 -8.8) (end -10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.3 8.8) (end 10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 8.8) (end 10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 -8.8) (end -10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.609 8.609) (end 8.609 6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 8.609) (end 8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 6.46) (end -8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.609 -8.609) (end 8.609 -6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -8.609) (end 8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -6.46) (end -8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.509 -8.509) (end -8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start 8.509 8.509) (end 8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 8.509) (end 8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 -8.509) (end -8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 232 "/3_3V PSU/HC_Plain"))
    (pad 1 smd rect (at -8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 215 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Vishay_IHLP-6767.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC648CC)
    (at 139.815 29.21)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/59D455EA)
    (attr smd)
    (fp_text reference C1303 (at 3.81 1.016) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1303-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMC (layer F.Cu) (tedit 5864295D) (tstamp 5BC6488E)
    (at 141.478 36.674 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (path /5BB8D2EE/5BB49523)
    (attr smd)
    (fp_text reference D1301 (at 0 -4.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VSSC8L45-M3/9AT (at 0 4.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.8 -3.25) (end 3.6 -3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.8 3.25) (end 3.6 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -4.9 3.35) (end -4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 3.35) (end -4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -3.35) (end 4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -3.35) (end 4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 -3.1) (end 3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 3.1) (end -3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -4.8 3.25) (end -4.8 -3.25) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 232 "/3_3V PSU/HC_Plain"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBA573E)
    (at 85.09 63.615 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB967B8)
    (attr smd)
    (fp_text reference R1309 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC64591)
    (at 184.785 22.225 90)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB73C46/5BB49537)
    (attr smd)
    (fp_text reference RV1201 (at 0 3.4925 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 155 "Net-(R1203-Pad1)"))
    (pad 2 smd rect (at -2.75 0 90) (size 2 1.3) (layers F.Cu F.Mask)
      (net 159 "Net-(RV1201-Pad2)"))
    (pad 1 smd rect (at 2.75 -1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 154 "Net-(R1202-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC3216F)
    (at 235.065 67.945)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA0467)
    (attr smd)
    (fp_text reference C1603 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34523)
    (at 25.666 42.2656)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC06246)
    (attr smd)
    (fp_text reference R1506 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 Dip_1))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34512)
    (at 25.666 40.7416)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC0636F)
    (attr smd)
    (fp_text reference R1507 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 Dip_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC34501)
    (at 25.666 39.2176)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC0639A)
    (attr smd)
    (fp_text reference R1508 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 Dip_3))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AEF9)
    (at 98.056 37.719)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F7)
    (attr smd)
    (fp_text reference R903 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R903-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 184 Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B90F)
    (at 118.9235 51.181 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F0)
    (attr smd)
    (fp_text reference R904 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 216 /uC/MOSI_ISP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B93F)
    (at 118.9235 49.784 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E9)
    (attr smd)
    (fp_text reference R905 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 217 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88E45)
    (at 101.854 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6FE)
    (attr smd)
    (fp_text reference R902 (at 0 9.853 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC645F2)
    (at 165.227 13.81 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BC3EDF8)
    (attr smd)
    (fp_text reference C1307 (at 0 4.43 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21F8E)
    (at 91.579 50.419 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC237F5)
    (attr smd)
    (fp_text reference C504 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21FBE)
    (at 91.567 51.816 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC237F5)
    (attr smd)
    (fp_text reference C604 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC21FEE)
    (at 88.637401 69.310601)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC237F5)
    (attr smd)
    (fp_text reference C704 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC220AE)
    (at 76.927401 77.370601)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BC237F5)
    (attr smd)
    (fp_text reference C804 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC220DE)
    (at 91.579 49.022 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC237F5)
    (attr smd)
    (fp_text reference C404 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC8616A)
    (at 91.579 47.625 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BC237F5)
    (attr smd)
    (fp_text reference C304 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_1206 (layer F.Cu) (tedit 58307BE8) (tstamp 5BC6454E)
    (at 161.597 20.066)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BC1CECA)
    (attr smd)
    (fp_text reference L1202 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BLM31KN601SN1L (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.07) (end 1 -1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 1.07) (end -1 1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 215 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC827E3)
    (at 98.056 47.625)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F151)
    (attr smd)
    (fp_text reference R937 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R937-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC221CE)
    (at 94.234 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC2388D)
    (attr smd)
    (fp_text reference R511 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 229 "Net-(R511-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 133 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC221FE)
    (at 95.631 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC2388D)
    (attr smd)
    (fp_text reference R611 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 132 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 228 "Net-(R611-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82873)
    (at 98.056 49.022)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5CD4F)
    (attr smd)
    (fp_text reference R936 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R936-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2225E)
    (at 91.44 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC2388D)
    (attr smd)
    (fp_text reference R311 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 135 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 226 "Net-(R311-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82843)
    (at 98.056 50.419)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5AA8D)
    (attr smd)
    (fp_text reference R935 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(R935-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC82813)
    (at 98.044 51.828)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC58906)
    (attr smd)
    (fp_text reference R934 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R934-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC222EE)
    (at 97.028 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC2388D)
    (attr smd)
    (fp_text reference R811 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(R811-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 131 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2231E)
    (at 98.425 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC2388D)
    (attr smd)
    (fp_text reference R711 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 130 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 222 "Net-(R711-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA0D)
    (at 101.727 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC568B6)
    (attr smd)
    (fp_text reference R933 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R933-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC223AE)
    (at 118.9348 52.6288)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC14A1B)
    (attr smd)
    (fp_text reference R931 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 216 /uC/MOSI_ISP))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC223DE)
    (at 131.445 49.899 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC12BB4)
    (attr smd)
    (fp_text reference R930 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 MISO))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 217 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC2201E)
    (at 92.837 57.138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC2388D)
    (attr smd)
    (fp_text reference R411 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 220 "Net-(R411-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 134 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64767)
    (at 136.845 29.53)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC25F71)
    (attr smd)
    (fp_text reference R1311 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(Q1201-Pad4)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 210 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64737)
    (at 142.24 24.765 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC1FD35)
    (attr smd)
    (fp_text reference R1310 (at 0 -1.65 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 210 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BCA440F)
    (at 83.3755 34.671)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BB48B05/5BB3C67E)
    (attr smd)
    (fp_text reference SW901 (at -5.034 1.175 -90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 219 /uC/~Reset_ISP))
    (pad 1 smd rect (at -2.875 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 219 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCB5E4A)
    (at 239.268 72.517)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BC191B1)
    (attr smd)
    (fp_text reference R1608 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D1602-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 213 V_Bat))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Axial Connector SMD:Ceramic_GPS_Antenna_SMD" (layer B.Cu) (tedit 5BB8BE91) (tstamp 5BC3EE0C)
    (at 219.2162 3.8212 180)
    (path /5BC18D95/5BC0A07F)
    (fp_text reference J1601 (at 11.75 -15.75 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x01_Female (at -8.5 -16 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -8.75 12.25) (end 8.75 12.25) (layer B.SilkS) (width 0.15))
    (fp_line (start 12.25 9.75) (end 12.25 -9.75) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.75 -12.25) (end -8.5 -12.25) (layer B.SilkS) (width 0.15))
    (fp_line (start -12.5 -9.75) (end -12.5 9.75) (layer B.SilkS) (width 0.15))
    (pad 1 smd rect (at -12 12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 12 -12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -12 -12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 12 12 90) (size 4 6) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
  )

  (module NEO-6M_24P-16X12.2MM_:GPS24P-SMD-1.1-16X12.2MM (layer F.Cu) (tedit 0) (tstamp 5BCC1D4D)
    (at 228.516 60.071 270)
    (path /5BC18D95/5BB887E8)
    (attr smd)
    (fp_text reference U1601 (at -8.3915 5.631 180) (layer F.SilkS)
      (effects (font (size 1.00332 1.00332) (thickness 0.05)))
    )
    (fp_text value "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)" (at -10.233 7.0026 180) (layer F.SilkS)
      (effects (font (size 1.00302 1.00302) (thickness 0.05)))
    )
    (fp_poly (pts (xy -4.45094 -8.255) (xy 4.445 -8.255) (xy 4.445 8.26603) (xy -4.45094 8.26603)) (layer F.SilkS) (width 0))
    (fp_circle (center -6.985 -8.255) (end -6.731 -8.255) (layer F.SilkS) (width 0.508))
    (fp_line (start -5.334 -8.636) (end -6.096 -7.874) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.096 -8.636) (end -5.334 -8.636) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.096 -7.874) (end 6.096 -8.636) (layer F.SilkS) (width 0.127))
    (fp_line (start -6.096 8.636) (end -6.096 8.001) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.096 8.636) (end -6.096 8.636) (layer F.SilkS) (width 0.127))
    (fp_line (start 6.096 8.001) (end 6.096 8.636) (layer F.SilkS) (width 0.127))
    (pad 24 smd rect (at 5.896 -6.888 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 23 smd rect (at 5.896 -5.788 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 22 smd rect (at 5.896 -4.688 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D1602-Pad1)"))
    (pad 21 smd rect (at 5.896 -3.588 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 259 "Net-(U1502-Pad3)"))
    (pad 20 smd rect (at 5.896 -2.488 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 260 "Net-(U1501-Pad3)"))
    (pad 19 smd rect (at 5.896 -1.388 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(U1601-Pad19)"))
    (pad 18 smd rect (at 5.896 -0.288 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(U1601-Pad18)"))
    (pad 17 smd rect (at 5.896 2.712 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(U1601-Pad17)"))
    (pad 16 smd rect (at 5.896 3.812 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(U1601-Pad16)"))
    (pad 15 smd rect (at 5.896 4.912 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U1601-Pad15)"))
    (pad 14 smd rect (at 5.896 6.012 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(U1601-Pad14)"))
    (pad 13 smd rect (at 5.896 7.112 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at -5.904 7.112 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at -5.904 6.012 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 258 /WiFi/Antenna))
    (pad 10 smd rect (at -5.904 4.912 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -5.904 3.812 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R1607-Pad1)"))
    (pad 8 smd rect (at -5.904 2.712 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R1607-Pad1)"))
    (pad 7 smd rect (at -5.904 -0.288 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -5.904 -1.388 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(U1601-Pad6)"))
    (pad 5 smd rect (at -5.904 -2.488 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(U1601-Pad5)"))
    (pad 4 smd rect (at -5.904 -3.588 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(U1601-Pad4)"))
    (pad 3 smd rect (at -5.904 -4.688 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R1601-Pad1)"))
    (pad 2 smd rect (at -5.904 -5.788 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(U1601-Pad2)"))
    (pad 1 smd rect (at -5.904 -6.888 90) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(U1601-Pad1)"))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FC6) (tstamp 5BB8D6F4)
    (at 121.285 46.24 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BE4C)
    (attr smd)
    (fp_text reference R917 (at 0.9405 -2.159) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 219 /uC/~Reset_ISP))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC9CE3C)
    (at 241.947 58.42)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBE487C)
    (attr smd)
    (fp_text reference C1601 (at 0.2032 1.2954) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Axial Connector SMD:U.FL Coaxial Connector" (layer F.Cu) (tedit 5BB8ACB6) (tstamp 5BBD2D4F)
    (at 227.685 35.814 90)
    (path /5BC18D95/5BBCE948)
    (fp_text reference J1602 (at 3 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Antenna_Conc (at 0 3.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 -1.75) (end 1.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.75 1.75) (end 0.75 1.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 -1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 1.75) (end -0.75 1.75) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.75 1.75) (end 1.75 1.25) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.75 -1.75) (end -1.75 -1.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 1.25) (end -1.75 1.75) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -1.4 0 180) (size 2.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 1.4 0 180) (size 2.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0 1.55 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 258 /WiFi/Antenna))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7BA2F)
    (at 118.9235 46.99 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BA78)
    (attr smd)
    (fp_text reference R913 (at -3.06 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R913-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 219 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 5BB890DB) (tstamp 5BBC5F2A)
    (at 71.7686 41.2496)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BC18D95/5BBAE28A)
    (attr smd)
    (fp_text reference D1602 (at 1.6755 -1.397) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value D (at 0 -1.4) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.3 0.57) (end 0.8 0.57) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.57) (end 0.8 -0.57) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.45) (end 0.8 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.45) (end 0.8 -0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.45) (end -0.8 -0.45) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.45) (end -0.8 0.45) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end -0.1 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end 0.2 0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0.2) (end -0.1 -0.2) (layer B.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer B.Fab) (width 0.1))
    (fp_line (start 1.4 0.67) (end -1.4 0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.67) (end -1.4 -0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.67) (end 1.4 -0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.67) (end 1.4 0.67) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.57) (end -1.3 -0.57) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 1.4) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 194 +3V3))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 214 "Net-(D1602-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCD24C8)
    (at 212.61 58.039)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BB9A675)
    (attr smd)
    (fp_text reference R1606 (at 3.6068 -0.0254) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "10k " (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 261 "Net-(R1606-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBA9425)
    (at 217.17 67.945 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA317C)
    (attr smd)
    (fp_text reference C1604 (at 0.901 -6.5786 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBA9414)
    (at 215.011 67.945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BC18D95/5BBA3100)
    (attr smd)
    (fp_text reference C1605 (at 0.7366 -2.9972) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8) (tstamp 5BBA8E72)
    (at 235.839 69.85)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (path /5BC18D95/5BB9F9F1)
    (attr smd)
    (fp_text reference C1602 (at 0 -1.75) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 0 2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end -2.25 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -1.05) (end 2.25 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 1.02) (end 1 1.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 -1.02) (end -1 -1.02) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 58307A47) (tstamp 5BCD7E9D)
    (at 223.254 51.816)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBA9401)
    (attr smd)
    (fp_text reference L1601 (at -0.127 -4.5085) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 27uH (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 258 /WiFi/Antenna))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BBA84E2)
    (at 229.024 51.816)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BC18D95/5BB8AC9C)
    (attr smd)
    (fp_text reference D1601 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED (at 0 1.55) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(D1601-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC22694)
    (at 225.679 51.816 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BBA78F0)
    (attr smd)
    (fp_text reference R1607 (at 0 -4.2545 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(L1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R1607-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBA44BD)
    (at 232.422 51.816 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BC18D95/5BB8A952)
    (attr smd)
    (fp_text reference R1601 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(D1601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R1601-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Encoder:STEC11B01 (layer F.Cu) (tedit 5BB61B4C) (tstamp 5BBFC26E)
    (at 177.165 48.895 270)
    (path /5BBCA088/5BBCA305)
    (fp_text reference SW1501 (at 1.048 11.564999 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Rotary_Encoder_Switch (at 0 7.119999 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -18) (end 1 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -18) (end 1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -29) (end -1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3 -29) (end 3 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -29) (end 3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -28) (end -3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -11) (end -3 -28) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3.5 -11) (end -3.5 -4) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -11) (end -3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -4) (end 3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -6 -4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 4) (end 6 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4) (end -6 4) (layer F.SilkS) (width 0.15))
    (pad B thru_hole circle (at -2.54 -1.27 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 180 "Net-(R1502-Pad1)"))
    (pad C thru_hole circle (at 0 -1.27 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad A thru_hole circle (at 2.54 -1.27 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 179 "Net-(R1501-Pad1)"))
    (pad S2 thru_hole circle (at 2.54 1.27 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad S1 thru_hole circle (at -2.54 1.27 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 182 Encoder_push))
    (pad "" thru_hole circle (at -5.842 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.842 0 270) (size 4 4) (drill 2) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB8AD77)
    (at 165.735 111.252 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE22E8)
    (attr smd)
    (fp_text reference R205 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 262 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB8C91E)
    (at 97.79 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC38F55)
    (attr smd)
    (fp_text reference R310 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 267 "Net-(D301-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AF48)
    (at 108.966 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249DD)
    (attr smd)
    (fp_text reference R301 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B068)
    (at 121.539 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249DD)
    (attr smd)
    (fp_text reference R401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC2EA1B) (tstamp 5BC3AF78)
    (at 110.363 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC38F55)
    (attr smd)
    (fp_text reference R410 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 264 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B008)
    (at 138.176 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249DD)
    (attr smd)
    (fp_text reference R501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BB7BB02)
    (at 170.053 111.24 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC38F55)
    (attr smd)
    (fp_text reference R810 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100R (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 263 "Net-(D801-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AFD8)
    (at 179.9717 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249DD)
    (attr smd)
    (fp_text reference R801 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BA70)
    (at 168.783 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC38F55)
    (attr smd)
    (fp_text reference R710 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 265 "Net-(D701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D07E)
    (at 150.6855 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249DD)
    (attr smd)
    (fp_text reference R601 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B8ED)
    (at 139.573 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC38F55)
    (attr smd)
    (fp_text reference R610 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 266 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B038)
    (at 167.386 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249DD)
    (attr smd)
    (fp_text reference R701 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BC64946)
    (at 173.355 14.48 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB73C46/5BB49533)
    (attr smd)
    (fp_text reference C1202 (at 6.0325 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC3E015)
    (at 155.321 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBD4644)
    (fp_text reference D201 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 185 "Net-(D201-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 187 "Net-(D201-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC23268)
    (at 126.365 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBEEFA5)
    (fp_text reference D202 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 186 "Net-(D202-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 183 "Net-(D202-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AF18)
    (at 125.095 73.914 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE40CE)
    (attr smd)
    (fp_text reference R201 (at 0.012 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 184 Dot))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC23018)
    (at 152.781 87.63 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBD471C)
    (attr smd)
    (fp_text reference R202 (at 0 -1.397 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 187 "Net-(D201-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC22FD6)
    (at 123.825 87.63 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBEEFB2)
    (attr smd)
    (fp_text reference R204 (at 0 -1.27 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 186 "Net-(D202-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22B05)
    (at 155.321 95.012 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBDEA3D)
    (attr smd)
    (fp_text reference Q201 (at 0 2.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 184 Dot))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 185 "Net-(D201-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22AF0)
    (at 124.206 93.329 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBEEFBB)
    (attr smd)
    (fp_text reference Q202 (at 0 2.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 183 "Net-(D202-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 184 Dot))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB75445) (tstamp 5BC33049)
    (at 171.311 51.054)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46FC)
    (attr smd)
    (fp_text reference C1501 (at -0.115 -3.302) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 178 Encoder_B))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB7544A) (tstamp 5BCB6561)
    (at 171.311 46.609)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46B9)
    (attr smd)
    (fp_text reference C1502 (at -0.115 -2.921) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 181 Encoder_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BC1566E)
    (at 168.275 42.43 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0DEE19)
    (attr smd)
    (fp_text reference C1503 (at 0 1.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 182 Encoder_push))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCB5CCC)
    (at 181.495 46.355 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3FA)
    (attr smd)
    (fp_text reference R1503 (at 0.647 4.826 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 180 "Net-(R1502-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC14464)
    (at 181.495 51.435 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3C9)
    (attr smd)
    (fp_text reference R1504 (at 0.647 4.318 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(R1501-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCE3B86)
    (at 172.72 41.402 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F47F)
    (attr smd)
    (fp_text reference R1505 (at 0.647 5.334 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 182 Encoder_push))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89025)
    (at 111.76 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D785)
    (attr smd)
    (fp_text reference R909 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R909-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(R909-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC647FF)
    (at 169.291 26.162 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB73C46/5BB4952F)
    (attr smd)
    (fp_text reference D1202 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BBE7DB5)
    (at 104.9573 94.119204 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB247DF/5BB249BA)
    (fp_text reference U302 (at 7.124204 -4.3733 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Battery_Holders:BatteryHolder_CoinCell_Keystone_3000 (layer F.Cu) (tedit 0) (tstamp 5BBE2D03)
    (at 130.836 12.573 180)
    (descr "Keystone type 3000 coin cell retainer")
    (path /5BB6494F/5BB6519B)
    (fp_text reference BT1101 (at 0 -8.1 180) (layer F.SilkS)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_text value Battery_Cell (at 0 6.9 180) (layer F.Fab)
      (effects (font (size 1.524 1.524) (thickness 0.15)))
    )
    (fp_line (start 0.6096 2.921) (end 1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start 1.8542 3.1496) (end 3.0988 3.6576) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.0988 3.6576) (end 4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.064 4.5212) (end 4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.7244 5.1816) (end 5.2832 5.4356) (layer F.SilkS) (width 0.381))
    (fp_line (start 0 2.8956) (end 0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -4.064 4.5212) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.064 4.5212) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -5.2832 5.4356) (end -4.7244 5.1816) (layer F.SilkS) (width 0.381))
    (fp_line (start -3.0988 3.6576) (end -1.8542 3.1496) (layer F.SilkS) (width 0.381))
    (fp_line (start -1.8542 3.1496) (end -0.6096 2.921) (layer F.SilkS) (width 0.381))
    (fp_line (start -0.6096 2.921) (end 0 2.8956) (layer F.SilkS) (width 0.381))
    (fp_arc (start 5.2832 4.1148) (end 6.604 4.1148) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_arc (start -5.2832 4.1148) (end -5.2832 5.4356) (angle 90) (layer F.SilkS) (width 0.381))
    (fp_line (start 6.604 -3.429) (end 6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start -6.604 -3.429) (end -6.604 4.064) (layer F.SilkS) (width 0.381))
    (fp_line (start 4.0005 -5.969) (end 6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -5.969) (end -6.604 -3.429) (layer F.SilkS) (width 0.381))
    (fp_line (start 3.9995 -6.731) (end 3.9995 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end -4.0005 -5.969) (layer F.SilkS) (width 0.381))
    (fp_line (start -4.0005 -6.731) (end 4.0005 -6.731) (layer F.SilkS) (width 0.381))
    (pad 1 smd rect (at -7.9 0 180) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 213 V_Bat))
    (pad 1 smd rect (at 7.9 0 180) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 213 V_Bat))
    (pad 2 smd rect (at 0 0 180) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Battery_Holders.3dshapes/BatteryHolder_CoinCell_Keystone_3000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EAE)
    (at 107.95 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB247DF/5BB24A0E)
    (attr smd)
    (fp_text reference R309 (at -4.6355 -0.0635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E8E)
    (at 137.16 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB36AE9/5BB24A0E)
    (attr smd)
    (fp_text reference R509 (at -4.7105 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EEE)
    (at 148.03 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3BB9E/5BB24A0E)
    (attr smd)
    (fp_text reference R609 (at -4.6355 -0.0115 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EDE)
    (at 177.165 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E89F/5BB24A0E)
    (attr smd)
    (fp_text reference R809 (at -4.6355 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6ECE)
    (at 118.745 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB32DD3/5BB24A0E)
    (attr smd)
    (fp_text reference R409 (at -4.647 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E9E)
    (at 166.37 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E878/5BB24A0E)
    (attr smd)
    (fp_text reference R709 (at -4.6355 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD3416)
    (at 112.28 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BBBEA7E)
    (attr smd)
    (fp_text reference C403 (at -0.012 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD33E5)
    (at 113.55 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB26FB6)
    (attr smd)
    (fp_text reference C402 (at 2.044 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF88)
    (at 113.665 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BBB5EFE)
    (attr smd)
    (fp_text reference U403 (at 0 3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U403-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(R411-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF6C)
    (at 142.875 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BBB5EFE)
    (attr smd)
    (fp_text reference U603 (at 0 3.2385 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(R611-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U603-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB97560)
    (at 102.87 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BBB5EFE)
    (attr smd)
    (fp_text reference U303 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U303-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(R311-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEC4)
    (at 172.085 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BBB5EFE)
    (attr smd)
    (fp_text reference U703 (at -0.0635 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(R711-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U703-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEA8)
    (at 161.29 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BBB5EFE)
    (attr smd)
    (fp_text reference U803 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U803-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(R811-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEE1C)
    (at 132.08 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BBB5EFE)
    (attr smd)
    (fp_text reference U503 (at 0 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(R511-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U503-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532) (tstamp 5BC970B3)
    (at 126.365 48.753 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (path /5BB48B05/5BB4F230)
    (attr smd)
    (fp_text reference J901 (at 5.207 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.9 -4.35) (end -5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.9 4.35) (end 5.9 -4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 4.35) (end 5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.9 -4.35) (end -5.9 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.6 0.76) (end 2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 0.76) (end -2.6 1.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -1.78) (end 2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.78) (end -2.6 -0.76) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 3.3) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.3) (end -2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 -3.87) (end 2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.04 -3.3) (end -2.6 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 3.87) (end 2.6 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -3.87) (end 2.6 -3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.6 2.86) (end 2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 2.22) (end 3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 2.22) (end 3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.86) (end -2.54 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 2.22) (end -3.6 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 2.22) (end -3.6 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 0.32) (end 2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -0.32) (end 3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -0.32) (end 3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 0.32) (end -2.54 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -0.32) (end -3.6 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -0.32) (end -3.6 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.22) (end 2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 3.6 -2.86) (end 3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -2.86) (end 3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.22) (end -2.54 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -3.6 -2.86) (end -3.6 -2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -3.6 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -3.81) (end 2.54 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 -2.86) (end -1.59 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -2.54 3.81) (end -2.54 -2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -1.59 -3.81) (end 2.54 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 3.81) (end -2.54 3.81) (layer F.Fab) (width 0.1))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 219 /uC/~Reset_ISP))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 216 /uC/MOSI_ISP))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 218 /uC/clk_ISP))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 217 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC6429E)
    (at 171.45 33.942 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49527)
    (attr smd)
    (fp_text reference C1204 (at 5.4915 1.143) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Kippschalter:B12AV (layer F.Cu) (tedit 5BB5DE12) (tstamp 5BBAFE9F)
    (at 101.092 30.988)
    (path /5BB7D616/5BB7EDAF)
    (fp_text reference SW1401 (at -7.8105 -4.826) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_SPDT (at -9.5 5.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7 -4) (end 7 1) (layer F.SilkS) (width 0.15))
    (fp_line (start 7 -4) (end -11.75 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -4) (end -11.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 4) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -1.25) (end -21.75 -1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 -1.25) (end -21.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 1.25) (end -11.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start 7 1) (end -0.75 1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.75 1) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (pad "" thru_hole rect (at -5.08 1.27) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" thru_hole rect (at -5.08 -1.27) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 252 "Net-(SW1401-Pad3)"))
    (pad 2 thru_hole circle (at 2.53 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 167 "Net-(D1401-Pad1)"))
    (pad 1 thru_hole circle (at 5.08 -1.27) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 151 +12V))
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB983B0)
    (at 237.49 43.97 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5BB9689B)
    (attr smd)
    (fp_text reference D1304 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 206 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Fuse Holder:Nano Fuse Holder" (layer F.Cu) (tedit 5BB4B4A4) (tstamp 5BB8397E)
    (at 96.076 23.876)
    (path /5BB7D616/5BB7D87A)
    (fp_text reference F1401 (at -3.25 -3.25) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 0.5 3.25) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.5 -2.5) (end 5.5 -2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 -2.5) (end 5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 2.5) (end -5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.5 2.5) (end -5.5 -2.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4 0 90) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D1401-Pad1)"))
    (pad 2 smd rect (at 4 0 90) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(F1401-Pad2)"))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E14) (tstamp 5BB763E2)
    (at 93.345 12.065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB8682A)
    (fp_text reference MH1401 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E06) (tstamp 5BB7BA9E)
    (at 186.055 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB86916)
    (fp_text reference MH1402 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60F0C) (tstamp 5BC63C85)
    (at 93.472 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868BC)
    (fp_text reference MH1403 (at 0 -3.048 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E19) (tstamp 5BB763CA)
    (at 185.42 12.065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868ED)
    (fp_text reference MH1404 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BB66FA0)
    (at 125.349 24.384 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB7D616/5BB7DD24)
    (attr smd)
    (fp_text reference C1402 (at 0 5.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (fp_text user + (at -2.27 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BB66F84)
    (at 116.84 24.386 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB7D616/5BB7F33C)
    (attr smd)
    (fp_text reference C1401 (at -0.002 3.175 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 90) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB669BC)
    (at 52.07 47.625)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB7D616/5BB7DDC7)
    (attr smd)
    (fp_text reference C1403 (at 0 1.397) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BB85027)
    (at 94.225 18.288)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB7D616/5BB7D945)
    (attr smd)
    (fp_text reference D1401 (at 0 -3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 0 3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D1401-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB6128D) (tstamp 5BC6451E)
    (at 143.51 11.684 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB5DF23)
    (attr smd)
    (fp_text reference C1306 (at -1.131 -1.3462 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4) (tstamp 5BC644E0)
    (at 145.6985 16.256 180)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BB8D2EE/5BB6A6ED)
    (attr smd)
    (fp_text reference D1303 (at -1.3675 1.397) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_2.5VPSU_off_red (at 0 1.7 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -0.8) (end 1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1 0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.65) (end 1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.65) (end 1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.65) (end -1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.65) (end -1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end -0.1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end 0.2 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 -0.2) (end -0.1 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.88) (end 1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -0.88) (end 1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 0.88) (end -1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 0.88) (end -1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D1303-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB61283) (tstamp 5BCA41CD)
    (at 143.51 13.462 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5CFDD)
    (attr smd)
    (fp_text reference R1304 (at 2.4758 -1.2032 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 enable_3.3V_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB612A8) (tstamp 5BC64479)
    (at 143.522 10.033 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5D0B6)
    (attr smd)
    (fp_text reference R1305 (at 2.171 1.651 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64449)
    (at 139.815 19.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5A81D)
    (attr smd)
    (fp_text reference R1306 (at -2.401 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64419)
    (at 139.815 15.24)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB71DFD)
    (attr smd)
    (fp_text reference R1308 (at -2.401 -3.7465) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643E9)
    (at 140.015 17.272)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB57E62)
    (attr smd)
    (fp_text reference R1307 (at -2.601 -4.572) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(Q1302-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC643B1)
    (at 146.746 12.446 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB59C86)
    (attr smd)
    (fp_text reference Q1301 (at 2.286 0.447 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB610FE) (tstamp 5BC64375)
    (at 143.195 19.05 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB57D85)
    (attr smd)
    (fp_text reference Q1302 (at -2.286 -0.066 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BC850 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/MC34063_Feedback"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(Q1302-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB61104) (tstamp 5BC64339)
    (at 146.7485 19.05 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB6719E)
    (attr smd)
    (fp_text reference Q1303 (at -2.286 0.127 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D1303-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC642EF)
    (at 158.115 13.81 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/59D46505)
    (attr smd)
    (fp_text reference C1304 (at 5.6185 0 -180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 215 "/3_3V PSU/MC34063_HC_A"))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_8x10.5 (layer F.Cu) (tedit 58AA8BC3) (tstamp 5BCA3930)
    (at 116.84 13.718 90)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (path /5BB8D2EE/5BB80A8D)
    (attr smd)
    (fp_text reference C1302 (at 0.887 -3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.3 4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.3 4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end -5.3 4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -4.29) (end 5.3 -4.29) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.43 -4.19) (end 4.19 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -3.43 -4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.43 4.19) (end -4.19 3.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end -3.43 4.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 -4.19) (end 4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.19 4.19) (end 4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 -3.43) (end -4.19 -1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.19 3.43) (end -4.19 1.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.04 -4.04) (end -3.37 -4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 -4.04) (end -4.04 -3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 -3.37) (end -4.04 3.37) (layer F.Fab) (width 0.1))
    (fp_line (start -4.04 3.37) (end -3.37 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start -3.37 4.04) (end 4.04 4.04) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.04) (end 4.04 -4.04) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 5.45 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.78 3.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -2.27 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.3 3.7) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.05 0 270) (size 4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC647C7)
    (at 137.795 18.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB81889)
    (attr smd)
    (fp_text reference C1301 (at 1.0915 -1.7145 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64680)
    (at 155.829 20.066 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB49531)
    (attr smd)
    (fp_text reference C1305 (at 1.9805 -1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 215 "/3_3V PSU/MC34063_HC_A"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC64640)
    (at 163.957 6.858 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5AAD3380)
    (attr smd)
    (fp_text reference D1302 (at 1.425 -1.778 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_2.7V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC64BC7)
    (at 151.765 16.935 90)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB8D2EE/5BB85821)
    (attr smd)
    (fp_text reference RV1301 (at -4.87 1.016 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 156 "Net-(R1302-Pad2)"))
    (pad 2 smd rect (at -2.75 0 90) (size 2 1.3) (layers F.Cu F.Mask)
      (net 203 "/3_3V PSU/MC34063_Feedback"))
    (pad 1 smd rect (at 2.75 -1.15 90) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 157 "Net-(R1303-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC649BC)
    (at 150.495 11.115 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB4952A)
    (attr smd)
    (fp_text reference R1303 (at 3.6855 -7.8105 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BB6113F) (tstamp 5BC6498C)
    (at 153.035 11.115 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB49529)
    (attr smd)
    (fp_text reference R1302 (at -3.1115 0.6985 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 27k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(R1302-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 194 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BB611A5) (tstamp 5BC64707)
    (at 132.715 24.436 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB8D2EE/59D44D00)
    (attr smd)
    (fp_text reference R1301 (at 3.3135 -2.667 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64B84)
    (at 181.61 29.6545)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49524)
    (attr smd)
    (fp_text reference C1203 (at 0.8255 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 83pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1203-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BC64CDE)
    (at 185.665 30.48 90)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB73C46/59D454FD)
    (attr smd)
    (fp_text reference D1201 (at -1.397 2.9845 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SB350 (at 0 3.1 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64B24)
    (at 173.355 24.5745 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB73C46/5BB49521)
    (attr smd)
    (fp_text reference R1201 (at 0 -2.413 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC64ADC)
    (at 179.07 24.5745 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB73C46/5BB74814)
    (attr smd)
    (fp_text reference U1201 (at 0 -3.302 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 "/5V PSU /SwE"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1203-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(RV1201-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC64A88)
    (at 138.43 24.605 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB8D2EE/5BB49532)
    (attr smd)
    (fp_text reference U1301 (at 0 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/MC34063_Feedback"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1303-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 210 "/3_3V PSU/SwE"))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 233 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64A4C)
    (at 180.455 17.5895)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49534)
    (attr smd)
    (fp_text reference C1201 (at -0.496 -2.794) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 151 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC64A1C)
    (at 181.229 40.398 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB47F9D)
    (attr smd)
    (fp_text reference C1205 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC64B54)
    (at 179.705 19.4945)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D46945)
    (attr smd)
    (fp_text reference R1202 (at 0.254 -3.3655) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22k (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R1202-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC9CE0C)
    (at 112.383 29.464 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CF46)
    (attr smd)
    (fp_text reference R925 (at 3.2505 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FBD) (tstamp 5BB8D7A8)
    (at 110.363 29.579 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CFEE)
    (attr smd)
    (fp_text reference R926 (at 2.667 -0.254 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC9CDDC)
    (at 139.446 51.562 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB6494F/5BB64C0D)
    (attr smd)
    (fp_text reference C1101 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB8D730)
    (at 139.573 54.61)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB6494F/5BB64ADA)
    (attr smd)
    (fp_text reference U1101 (at -4.445 -0.0635 -270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS3231MZ (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 213 V_Bat))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U1101-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U1101-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U1101-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA9D)
    (at 105.918 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60B72)
    (attr smd)
    (fp_text reference R919 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R919-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 PSU_3.3V_feedback))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D64)
    (at 120.142 34.1884 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63D55)
    (attr smd)
    (fp_text reference R920 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 Rx))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R920-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89406)
    (at 87.515 40.259)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DF5)
    (attr smd)
    (fp_text reference R922 (at -3.1235 -0.0635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R922-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 Dip_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB893D6)
    (at 87.515 41.656)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB62DFC)
    (attr smd)
    (fp_text reference R923 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 Dip_2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R923-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB893A6)
    (at 87.515 43.053)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CA3)
    (attr smd)
    (fp_text reference R924 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R924-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 Dip_1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7BBCC)
    (at 114.554 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60C0B)
    (attr smd)
    (fp_text reference R918 (at -3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 Encoder_B))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R918-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D34)
    (at 118.745 34.1884 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CF7)
    (attr smd)
    (fp_text reference R921 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R921-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 202 Tx))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC7AFB9)
    (at 97.282 45.478 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A35B)
    (attr smd)
    (fp_text reference C901 (at 3.187 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(C901-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19AE4) (tstamp 5BB89244)
    (at 118.3005 44.8945 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A26C)
    (attr smd)
    (fp_text reference C902 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB89214)
    (at 98.679 44.069 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB39CC9)
    (attr smd)
    (fp_text reference C903 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB891E4)
    (at 123.2662 38.7484 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A69F)
    (attr smd)
    (fp_text reference C904 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 137 /uC/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19B2A) (tstamp 5BB891B4)
    (at 123.2662 42.1506 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A72A)
    (attr smd)
    (fp_text reference C905 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB397FA)
    (at 128.905 41.303 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E76)
    (attr smd)
    (fp_text reference D901 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 217 /uC/MISO_ISP))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7B99F)
    (at 118.9235 48.387 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E2)
    (attr smd)
    (fp_text reference R906 (at -3.2505 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 /uC/clk_ISP))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R906-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC7AA6D)
    (at 103.124 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC50B36)
    (attr smd)
    (fp_text reference R907 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R907-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB89055)
    (at 113.157 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D7AF)
    (attr smd)
    (fp_text reference R908 (at -3.1235 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(R908-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R908-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88FF5)
    (at 110.363 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D75D)
    (attr smd)
    (fp_text reference R910 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(R910-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R910-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88FC5)
    (at 104.66 34.163 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D737)
    (attr smd)
    (fp_text reference R911 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R911-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F95)
    (at 106.045 34.163 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D711)
    (attr smd)
    (fp_text reference R912 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 SCL))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R912-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F35)
    (at 87.515 44.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB43320)
    (attr smd)
    (fp_text reference R901 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 LED_Error))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R901-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB88F05)
    (at 115.951 34.175 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E7E0)
    (attr smd)
    (fp_text reference R915 (at 0.0254 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 Encoder_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC1B239) (tstamp 5BC7AA3D)
    (at 104.521 54.852 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB4E3C2)
    (attr smd)
    (fp_text reference R916 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 166 enable_2.5V_PSU))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC81D04)
    (at 117.348 34.1764 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E361)
    (attr smd)
    (fp_text reference R914 (at -3.048 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 Encoder_push))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B188)
    (at 175.259 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BB249C1)
    (attr smd)
    (fp_text reference U801 (at -0.001 7.62 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 127 MOSI))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B5BB)
    (at 142.99 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB26FB6)
    (attr smd)
    (fp_text reference C602 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B110)
    (at 162.559 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BB249C1)
    (attr smd)
    (fp_text reference U701 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B4CB)
    (at 102.87 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB26FB6)
    (attr smd)
    (fp_text reference C302 (at 2.159 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B49B)
    (at 101.485 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BBBEA7E)
    (attr smd)
    (fp_text reference C303 (at -0.012 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608EF) (tstamp 5BC3B0C8)
    (at 123.444 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2618D)
    (attr smd)
    (fp_text reference C401 (at -0.242 -1.3335 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60CBD) (tstamp 5BC3B098)
    (at 140.474 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2618D)
    (attr smd)
    (fp_text reference C501 (at -0.242 -1.2065 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B3DB)
    (at 132.195 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB26FB6)
    (attr smd)
    (fp_text reference C502 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA2D)
    (at 130.695 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BBBEA7E)
    (attr smd)
    (fp_text reference C503 (at 0.0515 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60E26) (tstamp 5BC3B1E8)
    (at 152.781 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2618D)
    (attr smd)
    (fp_text reference C601 (at -0.3055 -1.2065 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABB6)
    (at 141.49 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BBBEA7E)
    (attr smd)
    (fp_text reference C603 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DA1) (tstamp 5BC3BA58)
    (at 169.672 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2618D)
    (attr smd)
    (fp_text reference C701 (at -0.242 -1.27 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD8FE6)
    (at 161.29 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB26FB6)
    (attr smd)
    (fp_text reference C702 (at 2.159 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA96)
    (at 159.905 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BBBEA7E)
    (attr smd)
    (fp_text reference C703 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DE8) (tstamp 5BC3BA28)
    (at 181.991 78.244 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2618D)
    (attr smd)
    (fp_text reference C801 (at -0.3055 -1.27 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608D4) (tstamp 5BC3B9F8)
    (at 111.264 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2618D)
    (attr smd)
    (fp_text reference C301 (at -0.369 -1.27) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABE6)
    (at 171.97 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB26FB6)
    (attr smd)
    (fp_text reference C802 (at 2.044 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39C36)
    (at 170.7 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BBBEA7E)
    (attr smd)
    (fp_text reference C803 (at 0 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BC08)
    (at 104.139 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BB249C1)
    (attr smd)
    (fp_text reference U301 (at 0 7.366 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 /Tubes/IV-9_Tube/Data_out))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB90)
    (at 116.714 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BB249C1)
    (attr smd)
    (fp_text reference U401 (at 0.763 7.493 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB18)
    (at 133.349 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BB249C1)
    (attr smd)
    (fp_text reference U501 (at -0.0645 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BAA0)
    (at 146.049 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BB249C1)
    (attr smd)
    (fp_text reference U601 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 171 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB29692)
    (at 115.824 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB32DD3/5BB249BA)
    (fp_text reference U402 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E57)
    (at 134.239 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB36AE9/5BB249BA)
    (fp_text reference U502 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E2D)
    (at 163.449 94.09267 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E878/5BB249BA)
    (fp_text reference U702 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E18)
    (at 174.244 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E89F/5BB249BA)
    (fp_text reference U802 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text 9-24VDC (at 100.838 10.16 180) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "IV-9 Clock  Max Nowka  10.2018 V1.0 " (at 114.173 108.331) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )

  (segment (start 172.72 95.25) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 173.99 95.25) (end 173.99 94.359) (width 0.35) (layer F.Cu) (net 1) (status 20))
  (segment (start 173.99 97.63) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 176.765 97.63) (end 177.165 97.23) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 173.99 97.63) (end 176.765 97.63) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 165.97 97.63) (end 166.37 97.23) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 163.195 97.63) (end 165.97 97.63) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 162.04 95.25) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 163.195 95.25) (end 163.195 94.34667) (width 0.35) (layer F.Cu) (net 2) (status 20))
  (segment (start 163.195 97.63) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 144.94 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 143.74 95.25) (end 144.78 95.25) (width 0.35) (layer F.Cu) (net 3) (status 10))
  (segment (start 144.78 95.25) (end 144.78 97.63) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 147.63 97.63) (end 148.03 97.23) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 94.359) (end 145.034 94.105) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 95.25) (end 144.78 94.359) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 133.985 97.63) (end 136.365 97.63) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.84 97.155) (end 137.16 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.365 97.63) (end 136.84 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 133.985 94.359) (end 134.239 94.105) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 132.945 95.25) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 133.985 95.25) (end 133.985 94.359) (width 0.35) (layer F.Cu) (net 4) (status 20))
  (segment (start 133.985 97.63) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 118.27 97.63) (end 118.745 97.155) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 115.57 97.63) (end 118.27 97.63) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 114.3 95.25) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 97.63) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 94.359) (end 115.824 94.105) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 115.57 95.25) (end 115.57 94.359) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 107.55 97.63) (end 107.95 97.23) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 97.63) (end 107.55 97.63) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 94.359) (end 105.029 94.105) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 103.62 95.25) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 104.775 95.25) (end 104.775 94.359) (width 0.35) (layer F.Cu) (net 6) (status 20))
  (segment (start 104.775 97.63) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (via (at 121.412 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1FC))
  (segment (start 136.779 76.962) (end 136.144 77.597) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23E))
  (segment (start 136.779 76.962) (end 138.049 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCEF) (status 20))
  (via (at 108.585 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F6))
  (segment (start 107.514 76.962) (end 106.934 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB6))
  (segment (start 108.839 76.962) (end 107.514 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCE) (status 10))
  (segment (start 106.934 77.542) (end 106.934 78.74) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD4))
  (via (at 167.005 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F3))
  (segment (start 167.259 80.137) (end 167.005 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C22C))
  (segment (start 167.259 76.962) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C244) (status 10))
  (segment (start 165.354 77.542) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD31))
  (segment (start 165.354 79.502) (end 165.354 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD1))
  (segment (start 108.585 80.391) (end 120.904 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD07))
  (segment (start 108.839 80.137) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCF5))
  (segment (start 138.049 80.391) (end 150.114 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCD7))
  (segment (start 178.054 77.542) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC2))
  (segment (start 178.634 76.962) (end 178.054 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C232))
  (segment (start 178.054 79.732) (end 178.459 80.137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD0A) (status 20))
  (segment (start 179.959 76.962) (end 178.634 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBF) (status 10))
  (segment (start 167.005 80.391) (end 177.673 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD4F))
  (segment (start 172.255 30.9245) (end 170.815 30.9245) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64DFA) (status 20))
  (segment (start 102.235 104.775) (end 102.235 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 113.03 104.775) (end 113.03 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 131.445 104.775) (end 131.445 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 142.24 104.775) (end 142.24 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 160.655 104.775) (end 160.655 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 171.45 103.03) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (via (at 113.03 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 106.045 106.68) (end 113.03 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 113.03 106.68) (end 113.03 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 102.235 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 102.235 106.68) (end 102.235 105.41) (width 0.35) (layer F.Cu) (net 7))
  (via (at 131.445 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 113.03 106.68) (end 131.445 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 131.445 106.68) (end 131.445 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 142.24 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 131.445 106.68) (end 142.24 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 142.24 106.68) (end 142.24 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 160.655 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 160.655 106.68) (end 160.655 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 160.655 106.68) (end 171.45 106.68) (width 0.35) (layer B.Cu) (net 7))
  (via (at 171.45 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 171.45 106.68) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (via (at 153.035 106.68) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 153.035 106.68) (end 160.655 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 142.24 106.68) (end 153.035 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 120.904 80.391) (end 122.555 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCEC))
  (segment (start 122.555 80.391) (end 126.365 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3C238))
  (segment (start 170.491 27.404) (end 170.773 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E09))
  (segment (start 169.291 27.404) (end 170.491 27.404) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E0C) (status 10))
  (segment (start 170.773 27.686) (end 170.815 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64DFD))
  (segment (start 170.815 30.9245) (end 170.815 27.686) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E00) (status 10))
  (segment (start 176.53 19.4945) (end 178.755 19.4945) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E03) (status 20))
  (segment (start 175.895 20.1295) (end 176.53 19.4945) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E06))
  (segment (start 175.895 25.4) (end 175.895 20.1295) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E18))
  (segment (start 172.085 26.035) (end 175.26 26.035) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E1B))
  (segment (start 170.815 27.305) (end 172.085 26.035) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E0F))
  (segment (start 175.26 26.035) (end 175.895 25.4) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E12))
  (segment (start 170.815 27.686) (end 170.815 27.305) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC64E15))
  (segment (start 128.27 80.391) (end 138.049 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCA4))
  (segment (start 24.916 39.2176) (end 24.916 40.7416) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 24.916 42.2656) (end 24.916 40.7416) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 126.365 80.391) (end 128.27 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD01))
  (segment (start 102.235 105.41) (end 102.235 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 106.045 106.68) (end 102.235 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 107.823 50.19) (end 107.848 50.165) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 51.265) (end 107.848 50.165) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 52.741) (end 107.848 51.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.339 53.25) (end 107.848 52.741) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.339 53.975) (end 107.339 53.25) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC7AD3F))
  (segment (start 108.648 37.665) (end 108.648 38.765) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.648 35.944) (end 108.648 37.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.954 35.638) (end 108.648 35.944) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.954 34.798) (end 108.954 35.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 117.196 45.265) (end 115.448 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 115.448 45.265) (end 114.348 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 117.5755 45.6445) (end 117.196 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 118.3005 45.6445) (end 117.5755 45.6445) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 114.348 45.265) (end 110.617 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.922 45.265) (end 107.848 45.339) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 110.617 45.265) (end 107.922 45.265) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 102.948 43.665) (end 107.719 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 43.794) (end 107.719 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 50.165) (end 107.848 45.847) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 45.847) (end 107.848 45.339) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.719 43.665) (end 107.782 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.648 38.765) (end 108.648 42.799) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 43.599) (end 108.14 43.307) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.14 43.307) (end 108.648 42.799) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 44.323) (end 107.848 43.599) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.782 43.665) (end 108.14 43.307) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 45.847) (end 107.848 44.323) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.848 44.323) (end 107.848 43.794) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 102.948 43.665) (end 100.053 43.665) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.707 43.319) (end 98.679 43.319) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 100.053 43.665) (end 99.707 43.319) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 120.015 45.49) (end 121.285 45.49) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 119.8605 45.6445) (end 120.015 45.49) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 118.3005 45.6445) (end 119.8605 45.6445) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 150.114 80.391) (end 150.749 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCDD))
  (via (at 150.749 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F0))
  (segment (start 150.749 80.391) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAA))
  (segment (start 149.424 76.962) (end 150.749 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCFB))
  (segment (start 148.844 77.542) (end 149.424 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCE0))
  (segment (start 148.844 79.629) (end 148.844 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCDA))
  (segment (start 149.606 80.391) (end 148.844 79.629) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB3))
  (segment (start 150.749 80.391) (end 149.606 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA1))
  (segment (start 151.88037 80.391) (end 167.005 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3C247))
  (segment (start 150.749 80.391) (end 151.88037 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD94))
  (via (at 179.959 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1ED))
  (segment (start 177.673 80.391) (end 179.959 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3C22F))
  (segment (start 181.991 80.391) (end 179.959 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD1F))
  (segment (start 178.713 80.391) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBC))
  (segment (start 179.959 80.391) (end 178.713 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB9))
  (segment (start 167.005 80.391) (end 168.922 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23B))
  (segment (start 139.724 80.391) (end 138.049 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCB))
  (segment (start 120.269 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC8))
  (segment (start 119.634 79.756) (end 120.269 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C241))
  (segment (start 119.634 77.417) (end 119.634 79.756) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA7))
  (segment (start 120.089 76.962) (end 119.634 77.417) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAD))
  (segment (start 121.414 76.962) (end 120.089 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC5))
  (segment (start 123.444 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB0))
  (segment (start 110.514 80.391) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC9E))
  (segment (start 188.087 78.994) (end 179.959 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 79.121) (end 188.087 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 180.975 106.68) (end 171.45 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 101.092) (end 187.452 101.854) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 182.372 105.283) (end 180.975 106.68) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 79.121) (end 188.214 101.092) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 182.372 104.14) (end 184.658 101.854) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 187.452 101.854) (end 184.658 101.854) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 182.372 104.14) (end 182.372 105.283) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 40.513) (end 188.214 39.624) (width 0.35) (layer B.Cu) (net 7))
  (via (at 188.214 39.116) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 188.214 41.275) (end 188.214 40.513) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 39.116) (end 188.214 41.275) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 188.214 79.121) (end 188.214 41.275) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 182.245 46.355) (end 183.515 46.355) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 183.515 46.355) (end 183.515 50.8) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 183.515 50.8) (end 182.88 51.435) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 182.88 51.435) (end 182.245 51.435) (width 0.35) (layer B.Cu) (net 7))
  (via (at 183.515 39.37) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 183.515 46.355) (end 183.515 39.37) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 215.011 67.195) (end 215.011 65.654) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 215.011 60.579) (end 215.011 58.989) (width 0.35) (layer F.Cu) (net 7))
  (via (at 173.736 39.37) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 172.72 40.386) (end 173.736 39.37) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 172.72 40.652) (end 172.72 40.386) (width 0.35) (layer B.Cu) (net 7))
  (via (at 211.836 67.183) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 214.999 67.183) (end 215.011 67.195) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 211.836 67.183) (end 214.999 67.183) (width 0.35) (layer F.Cu) (net 7))
  (via (at 211.778664 61.971905) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 211.836 62.029241) (end 211.778664 61.971905) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 211.836 67.183) (end 211.836 62.029241) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 215.011 60.579) (end 213.171569 60.579) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 213.171569 60.579) (end 212.578663 61.171906) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 212.578663 61.171906) (end 211.778664 61.971905) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 123.825 80.772) (end 123.444 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD19))
  (segment (start 152.654 80.518) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24A))
  (segment (start 110.363 83.347) (end 110.363 83.947) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24D))
  (segment (start 110.363 83.30037) (end 110.363 83.347) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C277))
  (segment (start 106.934 79.87137) (end 108.966 81.90337) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC6E))
  (segment (start 106.934 78.74) (end 106.934 79.87137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC62))
  (segment (start 108.966 81.90337) (end 110.363 83.30037) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC71))
  (segment (start 108.46963 80.391) (end 107.96163 80.899) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C280))
  (segment (start 108.585 80.391) (end 108.46963 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C28C))
  (segment (start 165.354 79.918) (end 165.354 79.502) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.947) (end 168.783 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.913 80.391) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.37 80.934) (end 165.354 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 167.005 80.391) (end 166.913 80.391) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.347) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.573 83.347) (end 139.065 82.839) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.144 79.918) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.573 83.947) (end 139.573 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.144 77.597) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (via (at 138.049 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 137.449001 81.152999) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.449001 80.990999) (end 137.449001 81.152999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.414 81.188) (end 136.144 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 138.049 80.391) (end 137.449001 80.990999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.573 83.347) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 122.555 80.391) (end 122.174 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCF8))
  (segment (start 123.825 82.804) (end 121.412 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 86.88) (end 123.825 82.804) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.781 82.423) (end 152.527 82.169) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.781 86.88) (end 152.781 82.423) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.527 82.169) (end 150.749 80.391) (width 0.35) (layer B.Cu) (net 7))
  (via (at 99.441 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 108.585 80.391) (end 99.441 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 97.79 83.947) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.441 81.696) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.441 80.391) (end 99.441 81.696) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.014 76.962) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE3) (status 30))
  (segment (start 108.839 78.232) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC95) (status 30))
  (segment (start 112.014 80.137) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD3A) (status 30))
  (segment (start 141.224 79.883) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC98) (status 30))
  (segment (start 138.049 78.232) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC92) (status 30))
  (segment (start 141.224 79.883) (end 141.224 78.867) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD79) (status 10))
  (segment (start 112.014 79.883) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA6) (status 10))
  (segment (start 167.259 78.232) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD28) (status 30))
  (segment (start 170.434 78.232) (end 170.434 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE9) (status 30))
  (segment (start 157.859 78.232) (end 157.859 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA3) (status 30))
  (segment (start 128.649 76.962) (end 128.649 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD1C) (status 30))
  (segment (start 141.224 80.137) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDF7) (status 30))
  (segment (start 114.3 97.63) (end 113.03 97.63) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 169.54 23.655) (end 169.291 23.904) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E21) (status 30))
  (segment (start 147.6985 20.05) (end 147.6985 20.1) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E1E) (status 30))
  (via (at 139.7 66.167) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1EA))
  (segment (start 139.573 66.167) (end 139.7 66.04) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD88))
  (segment (start 139.573 66.802) (end 139.573 66.167) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA9))
  (segment (start 138.049 66.802) (end 139.573 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BEB1) (status 10))
  (segment (start 139.573 66.802) (end 141.224 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD52) (status 20))
  (via (at 168.91 66.294) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1E7))
  (segment (start 168.783 66.421) (end 168.91 66.294) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BEF0))
  (segment (start 167.259 66.802) (end 168.783 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD4C) (status 10))
  (segment (start 168.783 66.802) (end 168.783 66.421) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD70))
  (segment (start 168.783 66.802) (end 170.434 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD85) (status 20))
  (segment (start 112.014 66.802) (end 110.49 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD49) (status 10))
  (segment (start 110.49 66.802) (end 108.839 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD16) (status 20))
  (segment (start 112.014 80.137) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9A) (status 10))
  (segment (start 141.224 77.597) (end 141.224 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD34) (status 20))
  (segment (start 141.224 78.867) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCFE) (status 20))
  (segment (start 140.565 27.535) (end 140.335 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E6F))
  (segment (start 140.565 29.21) (end 140.565 27.535) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E63))
  (via (at 142.24 27.305) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC64E87))
  (segment (start 140.335 27.305) (end 142.24 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64E7E))
  (segment (start 142.24 25.715) (end 142.24 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D31))
  (segment (start 147.696 20.0475) (end 147.6985 20.05) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D1C))
  (segment (start 147.696 13.446) (end 147.696 20.0475) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D3A))
  (segment (start 182.8495 27.2745) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D58))
  (via (at 182.88 27.305) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC64E27))
  (segment (start 180.975 27.2745) (end 182.8495 27.2745) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D52))
  (segment (start 182.36 27.825) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D3D))
  (segment (start 182.36 29.6545) (end 182.36 27.825) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D37))
  (segment (start 183.905 28.33) (end 182.88 27.305) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D43))
  (segment (start 185.665 28.33) (end 183.905 28.33) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC64D64))
  (segment (start 169.291 20.066) (end 167.227 20.066) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 53.9) (end 108.573 53.975) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.839 52.959) (end 108.839 53.975) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 52.768) (end 108.839 52.959) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 108.648 50.165) (end 108.648 52.768) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.848 35.802) (end 107.848 37.665) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.848 37.665) (end 107.848 38.765) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.569 35.523) (end 107.848 35.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 107.569 34.798) (end 107.569 35.523) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 118.3005 44.1445) (end 117.463 44.1445) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 117.1425 44.465) (end 114.348 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 117.463 44.1445) (end 117.1425 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 123.2662 41.4006) (end 123.2662 39.4984) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.948 44.465) (end 100.188 44.465) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 99.834 44.819) (end 98.679 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 100.188 44.465) (end 99.834 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 97.373 44.819) (end 97.282 44.728) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 98.679 44.819) (end 97.373 44.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 47.625) (end 90.829 49.022) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 49.022) (end 90.829 50.419) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 51.804) (end 90.817 51.816) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.829 50.419) (end 90.829 51.804) (width 0.35) (layer F.Cu) (net 8))
  (via (at 126.365 66.802) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1E4))
  (segment (start 128.649 66.802) (end 126.365 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD73))
  (via (at 97.155 66.802) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 99.439 66.802) (end 97.155 66.802) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD3D))
  (segment (start 169.291 20.828) (end 169.291 21.844) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 169.291 24.412) (end 169.291 21.844) (width 0.35) (layer F.Cu) (net 8))
  (via (at 169.291 21.844) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 169.291 20.828) (end 169.291 20.066) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 179.959 78.232) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD61))
  (segment (start 181.991 78.891) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC9B))
  (segment (start 170.422 80.391) (end 170.422 79.006) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8E))
  (segment (start 170.422 79.006) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD10))
  (segment (start 170.434 78.994) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9D))
  (segment (start 170.434 80.137) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD55))
  (segment (start 141.224 80.391) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD46))
  (segment (start 141.224 77.851) (end 141.224 77.597) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD64))
  (segment (start 141.224 78.232) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8B))
  (segment (start 112.014 80.391) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD5B))
  (segment (start 112.014 79.375) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD82))
  (segment (start 112.014 79.883) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDCD))
  (via (at 140.208 82.042) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1E1))
  (segment (start 141.224 80.391) (end 141.224 80.645) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD67))
  (via (at 169.418 82.042) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1DE))
  (segment (start 170.422 80.391) (end 170.422 80.657) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD40))
  (via (at 111.125 82.042) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1DB))
  (segment (start 110.998 82.169) (end 110.49 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6D))
  (segment (start 112.014 81.153) (end 110.998 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BF53))
  (segment (start 112.014 80.391) (end 112.014 81.153) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE39))
  (segment (start 141.224 80.391) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDAC))
  (segment (start 141.224 81.116) (end 141.224 81.28) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6A))
  (segment (start 140.870999 81.469001) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDB5))
  (segment (start 140.399999 81.469001) (end 140.870999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE7E))
  (segment (start 139.7 82.169) (end 140.399999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDC1))
  (segment (start 152.781 78.232) (end 152.781 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE00))
  (segment (start 150.749 78.232) (end 152.781 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD91))
  (segment (start 123.444 78.486) (end 123.444 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE30))
  (segment (start 123.444 78.232) (end 123.444 78.486) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE75))
  (segment (start 121.414 78.232) (end 123.444 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE48))
  (segment (start 142.76 10.045) (end 142.772 10.033) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 142.76 11.684) (end 142.76 10.045) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 150.495 10.165) (end 149.093 10.165) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 147.696 13.446) (end 148.955 13.446) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 148.844 13.335) (end 148.844 10.414) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 148.955 13.446) (end 148.844 13.335) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 149.093 10.165) (end 148.844 10.414) (width 0.35) (layer F.Cu) (net 8))
  (via (at 181.864 48.895) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 178.435 48.895) (end 182.245 48.895) (width 0.35) (layer B.Cu) (net 8))
  (via (at 121.445503 51.274497) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 123.825 51.278) (end 121.449006 51.278) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 121.449006 51.278) (end 121.445503 51.274497) (width 0.35) (layer F.Cu) (net 8))
  (via (at 172.085 52.705) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 172.061 52.681) (end 172.085 52.705) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 172.061 51.054) (end 172.061 52.681) (width 0.35) (layer B.Cu) (net 8))
  (via (at 172.085 45.085) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 172.061 45.109) (end 172.085 45.085) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 172.061 46.609) (end 172.061 45.109) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 241.427 58.65) (end 241.197 58.42) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 241.427 60.419) (end 241.427 58.65) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 240.157 60.419) (end 241.427 60.419) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 235.404 67.534) (end 235.815 67.945) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 235.404 65.967) (end 235.404 67.534) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 236.855 67.945) (end 235.815 67.945) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 237.339 68.429) (end 236.855 67.945) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 237.339 69.85) (end 237.339 68.429) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 228.054 54.167) (end 228.804 54.167) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 227.924 54.037) (end 228.054 54.167) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 227.924 51.816) (end 227.924 54.037) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 241.427 65.819) (end 240.157 65.819) (width 0.35) (layer F.Cu) (net 8))
  (via (at 238.252 64.389) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 239.682 65.819) (end 238.252 64.389) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 240.157 65.819) (end 239.682 65.819) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 217.211 64.704) (end 215.011 64.704) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 217.158 62.079) (end 217.17 62.091) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 215.011 62.079) (end 217.158 62.079) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 215.011 68.695) (end 217.17 68.695) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 213.638 62.079) (end 213.614 62.103) (width 0.35) (layer F.Cu) (net 8))
  (via (at 213.614 62.103) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 215.011 62.079) (end 213.638 62.079) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 218.44 58.039) (end 218.821 58.42) (width 0.35) (layer F.Cu) (net 8))
  (via (at 218.821 58.42) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BCE3D23))
  (segment (start 217.211 58.039) (end 218.44 58.039) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 112.8 95.25) (end 111.125 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 140.335 95.25) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 142.24 95.25) (end 140.335 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 129.54 95.25) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 131.445 95.25) (end 129.54 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 158.75 95.25) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 160.54 95.25) (end 158.75 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 169.545 95.25) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 171.22 95.25) (end 169.545 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 100.33 95.25) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 102.12 95.25) (end 100.33 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 103.505 97.63) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 97.515) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 95.25) (end 102.12 97.515) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 170.1927 83.3247) (end 172.974 80.5434) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.339 74.422) (end 170.434 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 75.057) (end 172.339 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 80.5434) (end 172.974 75.057) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.1927 83.9724) (end 170.1927 83.3247) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 171.6017 83.3724) (end 171.6621 83.312) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 171.6017 83.9724) (end 171.6017 83.3724) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 81.3651) (end 171.6017 83.3724) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 73.787) (end 173.609 81.3651) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.974 73.152) (end 173.609 73.787) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 170.434 73.152) (end 172.974 73.152) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.9987 83.3724) (end 173.0591 83.312) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.9987 83.9724) (end 172.9987 83.3724) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 82.1271) (end 172.9987 83.3724) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 72.517) (end 174.244 82.1271) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 173.609 71.882) (end 174.244 72.517) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 170.434 71.882) (end 173.609 71.882) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.879 71.247) (end 174.244 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.879 82.8294) (end 174.879 71.247) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.244 70.612) (end 170.434 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.3247) (end 174.879 82.8294) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.9724) (end 174.3837 83.3247) (width 0.35) (layer F.Cu) (net 12))
  (via (at 145.034 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1D8))
  (segment (start 128.649 69.342) (end 131.064 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE2A) (status 10))
  (segment (start 131.699 69.342) (end 132.334 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BDC4))
  (via (at 132.334 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1D5))
  (segment (start 132.334 68.707) (end 132.334 63.627) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE06))
  (segment (start 132.334 63.627) (end 145.034 63.627) (width 0.35) (layer B.Cu) (net 13) (tstamp 5BC3BF4D))
  (segment (start 112.014 69.342) (end 113.339 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BD43) (status 10))
  (segment (start 112.014 69.342) (end 115.189 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BDAF) (status 10))
  (via (at 115.824 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1D2))
  (segment (start 115.824 68.707) (end 115.824 63.627) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE4E))
  (segment (start 115.189 69.342) (end 115.824 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE03))
  (segment (start 115.824 63.627) (end 132.334 63.627) (width 0.35) (layer B.Cu) (net 13) (tstamp 5BC3BE3F))
  (segment (start 99.439 69.342) (end 101.854 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE15) (status 10))
  (segment (start 102.489 69.342) (end 103.124 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE51))
  (via (at 103.124 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1CF))
  (segment (start 103.124 68.707) (end 103.124 63.627) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BEB7))
  (segment (start 103.124 63.627) (end 115.824 63.627) (width 0.35) (layer B.Cu) (net 13) (tstamp 5BC3BE12))
  (via (at 161.544 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1CC))
  (segment (start 145.034 63.627) (end 161.544 63.627) (width 0.35) (layer B.Cu) (net 13) (tstamp 5BC3BE9C))
  (segment (start 161.544 63.627) (end 161.544 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE21))
  (segment (start 160.909 69.342) (end 157.859 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE1B) (status 20))
  (segment (start 161.544 68.707) (end 160.909 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE24))
  (via (at 174.244 63.627) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13) (tstamp 5BC3C1C9))
  (segment (start 161.544 63.627) (end 174.244 63.627) (width 0.35) (layer B.Cu) (net 13) (tstamp 5BC3BE5D))
  (segment (start 174.244 63.627) (end 174.244 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BDEE))
  (segment (start 173.609 69.342) (end 170.434 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE96) (status 20))
  (segment (start 174.244 68.707) (end 173.609 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BDCA))
  (segment (start 101.854 69.342) (end 102.489 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE33))
  (segment (start 131.064 69.342) (end 131.699 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BDD9))
  (segment (start 145.034 63.627) (end 145.034 68.707) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE81))
  (segment (start 144.399 69.342) (end 141.349 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE18))
  (segment (start 145.034 68.707) (end 144.399 69.342) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BC3BE3C))
  (segment (start 111.633 58.039) (end 115.824 62.23) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 111.633 55.614) (end 111.633 58.039) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 175.514 83.058) (end 175.7807 83.3247) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.514 71.247) (end 175.514 83.058) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 176.149 70.612) (end 175.514 71.247) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.7807 83.3247) (end 175.7807 83.9724) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 179.959 70.612) (end 176.149 70.612) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 176.784 71.882) (end 179.834 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 82.296) (end 176.149 72.517) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 72.517) (end 176.784 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.3247) (end 176.149 82.296) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.9724) (end 177.1777 83.3247) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.784 73.787) (end 177.419 73.152) (width 0.35) (layer F.Cu) (net 16) (tstamp 5BC3BD37))
  (segment (start 177.419 73.152) (end 179.834 73.152) (width 0.35) (layer F.Cu) (net 16) (tstamp 5BC3BE27) (status 20))
  (segment (start 178.5747 83.3724) (end 178.562 83.3597) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.5747 83.9724) (end 178.5747 83.3724) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.3597) (end 178.562 83.312) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 81.534) (end 176.784 73.787) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.312) (end 176.784 81.534) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 177.419 80.8863) (end 179.9717 83.439) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.9717 83.439) (end 179.9717 83.9724) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 75.057) (end 177.419 80.8863) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 178.054 74.422) (end 177.419 75.057) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.834 74.422) (end 178.054 74.422) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 164.084 75.057) (end 164.719 74.422) (width 0.35) (layer F.Cu) (net 18) (tstamp 5BC3BE54))
  (segment (start 164.719 74.422) (end 167.259 74.422) (width 0.35) (layer F.Cu) (net 18) (tstamp 5BC3BE0F) (status 20))
  (segment (start 167.386 83.347) (end 164.084 80.045) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 167.386 83.947) (end 167.386 83.347) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 80.045) (end 164.084 79.121) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 79.121) (end 164.084 75.057) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 73.152) (end 163.449 73.787) (width 0.35) (layer F.Cu) (net 19) (tstamp 5BC3BFF5))
  (segment (start 163.449 73.787) (end 163.449 80.022) (width 0.35) (layer F.Cu) (net 19) (tstamp 5BC3BEAB))
  (segment (start 167.259 73.152) (end 164.084 73.152) (width 0.35) (layer F.Cu) (net 19) (tstamp 5BC3BFA4) (status 10))
  (segment (start 163.449 80.807) (end 163.449 80.022) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.347) (end 163.449 80.807) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.947) (end 165.989 83.347) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 163.449 71.882) (end 167.259 71.882) (width 0.35) (layer F.Cu) (net 20) (tstamp 5BC3C01F) (status 20))
  (segment (start 162.814 72.517) (end 163.449 71.882) (width 0.35) (layer F.Cu) (net 20) (tstamp 5BC3BF7A))
  (segment (start 164.592 83.347) (end 162.814 81.569) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 81.569) (end 162.814 80.391) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.592 83.947) (end 164.592 83.347) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 80.391) (end 162.814 72.517) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 70.612) (end 162.179 71.247) (width 0.35) (layer F.Cu) (net 21) (tstamp 5BC3BE90))
  (segment (start 167.259 70.612) (end 162.814 70.612) (width 0.35) (layer F.Cu) (net 21) (tstamp 5BC3BF47) (status 10))
  (segment (start 163.195 83.347) (end 162.179 82.331) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 82.331) (end 162.179 81.153) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 163.195 83.947) (end 163.195 83.347) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 71.247) (end 162.179 81.153) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 160.909 70.612) (end 157.859 70.612) (width 0.35) (layer F.Cu) (net 22) (tstamp 5BC3BEE4) (status 20))
  (segment (start 161.544 71.247) (end 160.909 70.612) (width 0.35) (layer F.Cu) (net 22) (tstamp 5BC3BFB3))
  (segment (start 161.544 83.093) (end 161.798 83.347) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 83.093) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.798 83.347) (end 161.798 83.947) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.927) (end 161.544 81.534) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 71.247) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 160.274 71.882) (end 160.943989 72.551989) (width 0.35) (layer F.Cu) (net 23) (tstamp 5BC3BF11))
  (segment (start 157.859 71.882) (end 160.274 71.882) (width 0.35) (layer F.Cu) (net 23) (tstamp 5BC3BECC) (status 10))
  (segment (start 160.401 83.347) (end 160.401 83.947) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 82.804011) (end 160.401 83.347) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.804011) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 72.551989) (end 160.943989 81.534) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.596989) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 159.004 83.947) (end 159.004 83.347) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 82.159011) (end 160.191989 74.159989) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 74.159989) (end 159.184 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.004 83.347) (end 160.191989 82.159011) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 73.152) (end 157.859 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 74.422) (end 159.524 74.762) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BEED))
  (segment (start 157.859 74.422) (end 159.184 74.422) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BF23) (status 10))
  (segment (start 157.607 83.347) (end 159.524 81.43) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 81.43) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 157.607 83.947) (end 157.607 83.347) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 74.762) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 143.129 74.422) (end 141.224 74.422) (width 0.35) (layer F.Cu) (net 26) (tstamp 5BC3BED8) (status 20))
  (segment (start 143.764 75.057) (end 143.129 74.422) (width 0.35) (layer F.Cu) (net 26) (tstamp 5BC3BECF))
  (segment (start 140.97 83.347) (end 143.764 80.553) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 143.764 80.553) (end 143.764 79.756) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.97 83.947) (end 140.97 83.347) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 143.764 79.756) (end 143.764 75.057) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 144.354011 81.359989) (end 144.354011 73.742011) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.347) (end 144.354011 81.359989) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 143.764 73.152) (end 141.224 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 144.354011 73.742011) (end 143.764 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.947) (end 142.367 83.347) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 141.224 71.882) (end 142.549 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.347) (end 145.034 82.077) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 144.399 71.882) (end 141.224 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 82.077) (end 145.034 72.517) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 72.517) (end 144.399 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.947) (end 143.764 83.347) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 70.612) (end 145.669 71.247) (width 0.35) (layer F.Cu) (net 29) (tstamp 5BC3BF86))
  (segment (start 141.224 70.612) (end 145.034 70.612) (width 0.35) (layer F.Cu) (net 29) (tstamp 5BC3BF6E) (status 10))
  (segment (start 145.669 82.839) (end 145.669 81.788) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.947) (end 145.161 83.347) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.347) (end 145.669 82.839) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 81.788) (end 145.669 81.927) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 71.247) (end 145.669 81.788) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 146.304 71.247) (end 146.939 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.304 83.093) (end 146.304 71.247) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.347) (end 146.304 83.093) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.939 70.612) (end 150.624 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.947) (end 146.558 83.347) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 147.955 83.312) (end 147.955 83.947) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 82.296) (end 147.955 83.312) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 72.517) (end 146.939 82.296) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 147.574 71.882) (end 146.939 72.517) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 150.624 71.882) (end 147.574 71.882) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 148.209 73.152) (end 150.624 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 81.534) (end 147.574 73.787) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 73.787) (end 148.209 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.312) (end 147.574 81.534) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.947) (end 149.352 83.312) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 148.844 74.422) (end 150.624 74.422) (width 0.35) (layer F.Cu) (net 33) (tstamp 5BC3BF41) (status 20))
  (segment (start 148.209 75.057) (end 148.844 74.422) (width 0.35) (layer F.Cu) (net 33) (tstamp 5BC3BF56))
  (segment (start 148.209 75.057) (end 148.209 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 150.6855 83.347) (end 150.6855 83.947) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.2375 80.899) (end 150.6855 83.347) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.209 80.899) (end 148.2375 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 134.874 79.387) (end 134.874 75.057) (width 0.35) (layer F.Cu) (net 34) (tstamp 5BC3BF38))
  (segment (start 135.509 74.422) (end 138.049 74.422) (width 0.35) (layer F.Cu) (net 34) (tstamp 5BC3BF9B) (status 20))
  (segment (start 134.874 75.057) (end 135.509 74.422) (width 0.35) (layer F.Cu) (net 34) (tstamp 5BC3BF92))
  (segment (start 138.176 83.947) (end 138.176 83.347) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 80.045) (end 138.176 83.347) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 79.387) (end 134.874 80.045) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.239 80.022) (end 134.239 73.787) (width 0.35) (layer F.Cu) (net 35) (tstamp 5BC3BF5C))
  (segment (start 134.874 73.152) (end 138.049 73.152) (width 0.35) (layer F.Cu) (net 35) (tstamp 5BC3BF5F) (status 20))
  (segment (start 134.239 73.787) (end 134.874 73.152) (width 0.35) (layer F.Cu) (net 35) (tstamp 5BC3C067))
  (segment (start 136.779 83.947) (end 136.779 83.312) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 80.772) (end 136.779 83.312) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 80.022) (end 134.239 80.772) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 71.882) (end 138.049 71.882) (width 0.35) (layer F.Cu) (net 36) (tstamp 5BC3BF62) (status 20))
  (segment (start 133.604 72.517) (end 134.239 71.882) (width 0.35) (layer F.Cu) (net 36) (tstamp 5BC3C06A))
  (segment (start 133.604 80.657) (end 133.604 72.517) (width 0.35) (layer F.Cu) (net 36) (tstamp 5BC3BF89))
  (segment (start 133.604 80.657) (end 133.604 81.534) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 135.382 83.312) (end 135.382 83.347) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 135.382 83.347) (end 135.382 83.947) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 81.534) (end 135.382 83.312) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 132.969 81.292) (end 132.969 71.247) (width 0.35) (layer F.Cu) (net 37) (tstamp 5BC3BE93))
  (segment (start 133.604 70.612) (end 138.049 70.612) (width 0.35) (layer F.Cu) (net 37) (tstamp 5BC3BFAD) (status 20))
  (segment (start 132.969 71.247) (end 133.604 70.612) (width 0.35) (layer F.Cu) (net 37) (tstamp 5BC3BF9E))
  (segment (start 133.985 83.347) (end 133.95 83.312) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 133.985 83.947) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 82.331) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 81.292) (end 132.969 82.331) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 131.699 70.612) (end 128.649 70.612) (width 0.35) (layer F.Cu) (net 38) (tstamp 5BC3BF8C) (status 20))
  (segment (start 132.334 71.247) (end 131.699 70.612) (width 0.35) (layer F.Cu) (net 38) (tstamp 5BC3BF6B))
  (segment (start 132.334 83.093) (end 132.334 81.534) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.588 83.947) (end 132.588 83.347) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 81.534) (end 132.334 71.247) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.588 83.347) (end 132.334 83.093) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 131.064 71.882) (end 131.699 72.517) (width 0.35) (layer F.Cu) (net 39) (tstamp 5BC3BFCE))
  (segment (start 128.649 71.882) (end 131.064 71.882) (width 0.35) (layer F.Cu) (net 39) (tstamp 5BC3BFD1) (status 10))
  (segment (start 131.699 82.839) (end 131.699 82.296) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.191 83.347) (end 131.699 82.839) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.191 83.947) (end 131.191 83.347) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 72.517) (end 131.699 82.296) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.064 73.787) (end 130.429 73.152) (width 0.35) (layer F.Cu) (net 40) (tstamp 5BC3BF95))
  (segment (start 130.429 73.152) (end 128.649 73.152) (width 0.35) (layer F.Cu) (net 40) (tstamp 5BC3BFE9) (status 20))
  (segment (start 131.064 82.077) (end 131.064 81.026) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 131.064 81.026) (end 131.064 73.787) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 129.794 83.347) (end 131.064 82.077) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 129.794 83.947) (end 129.794 83.347) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 130.413989 74.861989) (end 129.974 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFBF))
  (segment (start 129.974 74.422) (end 128.649 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFEF) (status 20))
  (segment (start 130.413989 81.330011) (end 130.413989 80.772) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 128.397 83.347) (end 130.413989 81.330011) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 128.397 83.947) (end 128.397 83.347) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 80.772) (end 130.413989 74.861989) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 114.554 80.518) (end 111.76 83.312) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 111.76 83.312) (end 111.76 83.947) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 114.554 75.057) (end 114.554 80.518) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.919 74.422) (end 114.554 75.057) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 112.014 74.422) (end 113.919 74.422) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 115.189 73.787) (end 115.189 81.28) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.157 83.312) (end 113.157 83.947) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.189 81.28) (end 113.157 83.312) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 114.554 73.152) (end 115.189 73.787) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 112.014 73.152) (end 114.554 73.152) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.824 82.042) (end 114.554 83.312) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.189 71.882) (end 115.824 72.517) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 114.554 83.312) (end 114.554 83.947) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 72.517) (end 115.824 82.042) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 112.014 71.882) (end 115.189 71.882) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 70.612) (end 112.014 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 82.55) (end 116.459 71.247) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.058) (end 116.459 82.55) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 71.247) (end 115.824 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.947) (end 115.951 83.058) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 117.094 71.247) (end 117.729 70.612) (width 0.35) (layer F.Cu) (net 46) (tstamp 5BC3C06D))
  (segment (start 117.094 82.562) (end 117.094 71.247) (width 0.35) (layer F.Cu) (net 46) (tstamp 5BC3C037))
  (segment (start 117.729 70.612) (end 121.414 70.612) (width 0.35) (layer F.Cu) (net 46) (tstamp 5BC3C025) (status 20))
  (segment (start 117.348 82.816) (end 117.348 83.947) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 82.562) (end 117.348 82.816) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.729 72.517) (end 118.364 71.882) (width 0.35) (layer F.Cu) (net 47) (tstamp 5BC3BDE8))
  (segment (start 118.364 71.882) (end 121.414 71.882) (width 0.35) (layer F.Cu) (net 47) (tstamp 5BC3C02E) (status 20))
  (segment (start 118.745 83.347) (end 117.729 82.331) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 82.331) (end 117.729 81.28) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.745 83.947) (end 118.745 83.347) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 81.28) (end 117.729 72.517) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.364 73.787) (end 118.999 73.152) (width 0.35) (layer F.Cu) (net 48) (tstamp 5BC3BE0C))
  (segment (start 121.414 73.152) (end 118.999 73.152) (width 0.35) (layer F.Cu) (net 48) (tstamp 5BC3C0AF) (status 10))
  (segment (start 120.142 83.347) (end 118.364 81.569) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.142 83.947) (end 120.142 83.347) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 81.569) (end 118.364 81.026) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 81.026) (end 118.364 73.787) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 121.414 74.422) (end 120.269 74.422) (width 0.35) (layer F.Cu) (net 49) (tstamp 5BC3C00A) (status 10))
  (segment (start 118.999 75.057) (end 119.634 74.422) (width 0.35) (layer F.Cu) (net 49) (tstamp 5BC3BDA0))
  (segment (start 119.634 74.422) (end 120.269 74.422) (width 0.35) (layer F.Cu) (net 49) (tstamp 5BC3C04C))
  (segment (start 118.999 80.807) (end 118.999 80.645) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 121.539 83.347) (end 118.999 80.807) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 121.539 83.947) (end 121.539 83.347) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 80.645) (end 118.999 75.057) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 105.664 75.057) (end 106.299 74.422) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3C03A))
  (segment (start 106.299 74.422) (end 108.839 74.422) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3C013) (status 20))
  (segment (start 105.664 79.387) (end 105.664 75.057) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3C016))
  (segment (start 105.664 80.045) (end 105.664 79.387) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3BC59))
  (segment (start 108.966 83.347) (end 105.664 80.045) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3BC83))
  (segment (start 108.966 83.947) (end 108.966 83.347) (width 0.35) (layer F.Cu) (net 50) (tstamp 5BC3BC7A))
  (segment (start 106.934 73.152) (end 108.839 73.152) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C019) (status 20))
  (segment (start 105.029 73.787) (end 105.664 73.152) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C0B2))
  (segment (start 105.029 80.022) (end 105.029 73.787) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3BF65))
  (segment (start 105.664 73.152) (end 106.934 73.152) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C052))
  (segment (start 105.029 80.807) (end 105.029 80.022) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C271))
  (segment (start 107.569 83.347) (end 105.029 80.807) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C27A))
  (segment (start 107.569 83.947) (end 107.569 83.347) (width 0.35) (layer F.Cu) (net 51) (tstamp 5BC3C26E))
  (segment (start 105.029 71.882) (end 108.839 71.882) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3C02B) (status 20))
  (segment (start 104.394 72.517) (end 105.029 71.882) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3C004))
  (segment (start 104.394 80.657) (end 104.394 72.517) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3BF17))
  (segment (start 104.394 81.581) (end 104.394 80.657) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3C25F))
  (segment (start 106.172 83.359) (end 104.394 81.581) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3C268))
  (segment (start 106.172 83.959) (end 106.172 83.359) (width 0.35) (layer F.Cu) (net 52) (tstamp 5BC3C26B))
  (segment (start 107.569 70.612) (end 108.839 70.612) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3C010) (status 20))
  (segment (start 103.759 71.247) (end 104.394 70.612) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3C03D))
  (segment (start 103.759 81.292) (end 103.759 71.247) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3C046))
  (segment (start 104.394 70.612) (end 107.569 70.612) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3BF32))
  (segment (start 103.759 81.292) (end 103.759 82.296) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3BC5C))
  (segment (start 104.775 83.312) (end 104.775 83.947) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3C289))
  (segment (start 103.759 82.296) (end 104.775 83.312) (width 0.35) (layer F.Cu) (net 53) (tstamp 5BC3C27D))
  (segment (start 103.124 81.927) (end 103.124 71.247) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3BFF8))
  (segment (start 101.219 70.612) (end 99.439 70.612) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3C049) (status 20))
  (segment (start 103.124 71.247) (end 102.489 70.612) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3C043))
  (segment (start 102.489 70.612) (end 101.219 70.612) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3BFA1))
  (segment (start 103.378 83.347) (end 103.124 83.093) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3BC80))
  (segment (start 103.124 83.093) (end 103.124 81.927) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3BC74))
  (segment (start 103.378 83.947) (end 103.378 83.347) (width 0.35) (layer F.Cu) (net 54) (tstamp 5BC3BC65))
  (segment (start 101.854 71.882) (end 100.584 71.882) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C0A3))
  (segment (start 102.489 72.517) (end 101.854 71.882) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C0A6))
  (segment (start 100.584 71.882) (end 99.439 71.882) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3BE57) (status 20))
  (segment (start 102.489 82.839) (end 102.489 82.042) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C274))
  (segment (start 102.489 82.042) (end 102.489 72.517) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C253))
  (segment (start 101.981 83.347) (end 102.489 82.839) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C256))
  (segment (start 101.981 83.947) (end 101.981 83.347) (width 0.35) (layer F.Cu) (net 55) (tstamp 5BC3C259))
  (segment (start 101.219 73.152) (end 99.439 73.152) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C0A0) (status 20))
  (segment (start 101.854 73.787) (end 101.219 73.152) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C040))
  (segment (start 100.584 83.347) (end 101.854 82.077) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C286))
  (segment (start 100.584 83.947) (end 100.584 83.347) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C298))
  (segment (start 101.854 82.077) (end 101.854 81.407) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C292))
  (segment (start 101.854 81.407) (end 101.854 73.787) (width 0.35) (layer F.Cu) (net 56) (tstamp 5BC3C28F))
  (segment (start 100.584 74.422) (end 99.439 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BF29) (status 20))
  (segment (start 101.219 75.057) (end 100.584 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3C0AC))
  (segment (start 101.219 81.327) (end 101.219 79.502) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC77))
  (segment (start 99.187 83.959) (end 99.187 83.359) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC6B))
  (segment (start 101.219 79.502) (end 101.219 75.057) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC5F))
  (segment (start 99.187 83.359) (end 101.219 81.327) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC7D))
  (segment (start 170.1927 90.813115) (end 171.466915 92.08733) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.1927 85.4724) (end 170.1927 90.813115) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.823172 89.638927) (end 171.466915 90.28267) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 170.823172 86.850928) (end 170.823172 89.638927) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 86.0724) (end 170.823172 86.850928) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 85.4724) (end 171.6017 86.0724) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 172.9987 86.0724) (end 172.5841 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.9987 85.4724) (end 172.9987 86.0724) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.5841 86.487) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.527667 88.82267) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 174.3837 88.1253) (end 174.244 88.265) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 174.3837 85.4724) (end 174.3837 88.1253) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 175.7807 88.643037) (end 175.960333 88.82267) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 175.7807 85.4724) (end 175.7807 88.643037) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 177.1777 90.126055) (end 177.021085 90.28267) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 177.1777 85.4724) (end 177.1777 90.126055) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 178.5747 90.533715) (end 177.021085 92.08733) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 178.5747 85.4724) (end 178.5747 90.533715) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 176.769882 93.54733) (end 175.960333 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 177.310383 93.54733) (end 176.769882 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 90.886013) (end 177.310383 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 85.4724) (end 179.9717 90.886013) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 165.974882 93.535) (end 165.165333 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.068505 91.981878) (end 166.515383 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 87.172199) (end 168.068505 87.854704) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 166.515383 93.535) (end 165.974882 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.068505 87.854704) (end 168.068505 91.981878) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 85.447) (end 167.386 87.172199) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.478494 89.773451) (end 167.478494 90.612721) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 165.989 85.447) (end 165.989 86.6096) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.478494 90.612721) (end 166.226085 91.86513) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.459838 88.080438) (end 167.459838 89.754795) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 165.989 86.6096) (end 167.459838 88.080438) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.459838 89.754795) (end 167.478494 89.773451) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 91.86513) (end 166.226085 92.075) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.869828 89.626597) (end 166.226085 90.27034) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 166.869828 88.324828) (end 166.869828 89.626597) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 86.047) (end 166.869828 88.324828) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 85.447) (end 164.592 86.047) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 165.165333 88.017333) (end 165.165333 88.81034) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 86.047) (end 165.165333 88.017333) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 85.447) (end 163.195 86.047) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.449 88.00267) (end 163.449 88.25267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 86.35167) (end 163.449 88.00267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 85.447) (end 161.798 86.35167) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 160.401 87.478673) (end 161.732667 88.81034) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 160.401 85.447) (end 160.401 87.478673) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 159.004 88.602425) (end 160.671915 90.27034) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.004 85.447) (end 159.004 88.602425) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 157.607 89.010085) (end 160.671915 92.075) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 157.607 85.447) (end 157.607 89.010085) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 140.97 90.800415) (end 142.256915 92.08733) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.97 85.447) (end 140.97 90.800415) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 141.613172 89.638927) (end 142.256915 90.28267) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 86.047) (end 141.613172 86.800828) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 141.613172 86.800828) (end 141.613172 89.638927) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 85.447) (end 142.367 86.047) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 143.764 85.447) (end 143.764 85.979) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.317667 86.425333) (end 143.317667 88.82267) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.764 85.979) (end 143.317667 86.425333) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 145.161 88.138) (end 145.034 88.265) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 145.161 85.447) (end 145.161 88.138) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 146.558 88.630337) (end 146.750333 88.82267) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 146.558 85.447) (end 146.558 88.630337) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 147.955 90.138755) (end 147.811085 90.28267) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 147.955 85.447) (end 147.955 90.138755) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 149.352 90.546415) (end 147.811085 92.08733) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 149.352 85.447) (end 149.352 90.546415) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 147.559882 93.54733) (end 146.750333 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.100383 93.54733) (end 147.559882 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 90.962213) (end 148.100383 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 85.447) (end 150.6855 90.962213) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 138.938 91.914713) (end 137.305383 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 136.764882 93.54733) (end 135.955333 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.938 86.995) (end 138.938 91.914713) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 137.305383 93.54733) (end 136.764882 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.176 86.233) (end 138.938 86.995) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.176 85.447) (end 138.176 86.233) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.268494 90.834921) (end 137.559254 91.544161) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 138.268494 87.536494) (end 138.268494 90.834921) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 86.047) (end 138.268494 87.536494) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 85.447) (end 136.779 86.047) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.559254 91.544161) (end 137.016085 92.08733) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.659828 89.638927) (end 137.016085 90.28267) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 86.047) (end 137.659828 88.324828) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 137.659828 88.324828) (end 137.659828 89.638927) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 85.447) (end 135.382 86.047) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.955333 88.017333) (end 135.955333 88.82267) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 86.047) (end 135.955333 88.017333) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 85.447) (end 133.985 86.047) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 132.588 86.364) (end 132.588 85.447) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.015) (end 132.588 86.364) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.265) (end 134.239 88.015) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 131.191 87.491003) (end 132.522667 88.82267) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 131.191 85.447) (end 131.191 87.491003) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 129.794 88.614755) (end 131.461915 90.28267) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 129.794 85.447) (end 129.794 88.614755) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 128.397 89.022415) (end 131.461915 92.08733) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 128.397 85.447) (end 128.397 89.022415) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 111.76 90.800415) (end 113.046915 92.08733) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 111.76 85.447) (end 111.76 90.800415) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 112.403172 89.638927) (end 113.046915 90.28267) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 112.403172 86.800828) (end 112.403172 89.638927) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 86.047) (end 112.403172 86.800828) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 85.447) (end 113.157 86.047) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 114.554 85.979) (end 114.554 85.447) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 86.425333) (end 114.554 85.979) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 88.82267) (end 114.107667 86.425333) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 115.951 88.138) (end 115.824 88.265) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 115.951 85.447) (end 115.951 88.138) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 117.348 88.630337) (end 117.540333 88.82267) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 117.348 85.447) (end 117.348 88.630337) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 118.745 90.138755) (end 118.601085 90.28267) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 118.745 85.447) (end 118.745 90.138755) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 120.142 90.546415) (end 118.601085 92.08733) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.142 85.447) (end 120.142 90.546415) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 118.349882 93.54733) (end 117.540333 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 118.890383 93.54733) (end 118.349882 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 121.539 90.898713) (end 118.890383 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 121.539 85.447) (end 121.539 90.898713) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 108.966 86.047) (end 108.966 85.447) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.855 86.936) (end 108.966 86.047) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.855 91.730217) (end 109.855 86.936) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.023683 93.561534) (end 109.855 91.730217) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 106.673633 93.561534) (end 108.023683 93.561534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 107.569 86.047) (end 109.22 87.698) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 107.569 85.447) (end 107.569 86.047) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 90.615919) (end 107.734385 92.101534) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 87.698) (end 109.22 90.615919) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 108.378128 89.653131) (end 107.734385 90.296874) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 108.378128 88.265128) (end 108.378128 89.653131) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 86.059) (end 108.378128 88.265128) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 85.459) (end 106.172 86.059) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.673633 87.945633) (end 106.673633 87.95306) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 106.673633 87.95306) (end 106.673633 88.836874) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 86.047) (end 106.673633 87.945633) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 85.447) (end 104.775 86.047) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.9573 88.029204) (end 104.9573 88.279204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 86.449904) (end 104.9573 88.029204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 85.447) (end 103.378 86.449904) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 101.981 87.576907) (end 103.240967 88.836874) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 101.981 85.447) (end 101.981 87.576907) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 100.584 88.700659) (end 102.180215 90.296874) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 100.584 85.447) (end 100.584 88.700659) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 99.187 89.108319) (end 102.180215 92.101534) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 99.187 85.459) (end 99.187 89.108319) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 170.434 75.692) (end 167.259 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0BB) (status 30))
  (segment (start 167.259 75.692) (end 166.584 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0C4) (status 30))
  (segment (start 141.224 75.692) (end 138.049 75.692) (width 0.35) (layer F.Cu) (net 107) (tstamp 5BC3C0C1) (status 30))
  (segment (start 150.624 75.692) (end 157.859 75.692) (width 0.35) (layer F.Cu) (net 108) (tstamp 5BC3C0BE) (status 30))
  (segment (start 121.414 75.692) (end 128.649 75.692) (width 0.35) (layer F.Cu) (net 109) (tstamp 5BC3C0C7) (status 30))
  (segment (start 108.839 75.692) (end 112.014 75.692) (width 0.35) (layer F.Cu) (net 110) (tstamp 5BC3C0CA) (status 30))
  (segment (start 104.023 38.765) (end 104.648 38.765) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 101.854 36.596) (end 104.023 38.765) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 101.854 34.925) (end 101.854 36.596) (width 0.35) (layer F.Cu) (net 111))
  (segment (start 117.348 36.195) (end 117.348 34.9264) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 114.348 39.195) (end 117.348 36.195) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 114.348 40.465) (end 114.348 39.195) (width 0.35) (layer F.Cu) (net 112))
  (segment (start 106.248 50.165) (end 106.248 51.232) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 104.521 54.102) (end 104.521 53.467) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 106.248 51.74) (end 106.248 50.165) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 104.521 53.467) (end 106.248 51.74) (width 0.35) (layer F.Cu) (net 113))
  (segment (start 115.951 35.525) (end 115.951 34.925) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 115.951 36.087) (end 115.951 35.525) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 113.273 38.765) (end 115.951 36.087) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 112.648 38.765) (end 113.273 38.765) (width 0.35) (layer F.Cu) (net 114))
  (segment (start 115.448 46.065) (end 114.348 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 116.6485 46.065) (end 115.448 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 117.5735 46.99) (end 116.6485 46.065) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 118.1735 46.99) (end 117.5735 46.99) (width 0.35) (layer F.Cu) (net 116))
  (segment (start 106.045 35.56) (end 106.045 34.913) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 107.048 36.563) (end 106.045 35.56) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 107.048 38.765) (end 107.048 36.563) (width 0.35) (layer F.Cu) (net 117))
  (segment (start 104.66 34.913) (end 104.66 35.548) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 106.248 37.136) (end 106.248 38.765) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 104.66 35.548) (end 106.248 37.136) (width 0.35) (layer F.Cu) (net 118))
  (segment (start 110.363 34.925) (end 110.363 35.56) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 109.448 36.475) (end 109.448 38.765) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 110.363 35.56) (end 109.448 36.475) (width 0.35) (layer F.Cu) (net 119))
  (segment (start 110.248 37.037) (end 110.248 37.665) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.76 35.525) (end 110.248 37.037) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 110.248 37.665) (end 110.248 38.765) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.76 34.925) (end 111.76 35.525) (width 0.35) (layer F.Cu) (net 120))
  (segment (start 111.048 37.288) (end 113.157 35.179) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 113.157 35.179) (end 113.157 34.925) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 111.048 38.765) (end 111.048 37.288) (width 0.35) (layer F.Cu) (net 121))
  (segment (start 103.124 53.589) (end 103.124 53.975) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 105.448 51.265) (end 103.124 53.589) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 105.448 50.165) (end 105.448 51.265) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 103.124 53.975) (end 103.124 54.102) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 149.299 68.072) (end 148.844 67.617) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0CD))
  (segment (start 150.624 68.072) (end 149.299 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0D3) (status 10))
  (segment (start 136.724 68.072) (end 136.144 67.492) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0D0))
  (segment (start 138.049 68.072) (end 136.724 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0D6) (status 10))
  (segment (start 136.144 67.492) (end 136.144 61.087) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0D9))
  (segment (start 120.089 68.072) (end 119.634 67.617) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0DC))
  (segment (start 121.414 68.072) (end 120.089 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0EB) (status 10))
  (via (at 119.634 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1C6))
  (segment (start 119.634 67.617) (end 119.634 61.087) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0EE))
  (segment (start 119.634 61.087) (end 136.144 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C0DF))
  (segment (start 107.514 68.072) (end 106.934 67.492) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0E2))
  (segment (start 108.839 68.072) (end 107.514 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0E5) (status 10))
  (via (at 106.934 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1C3))
  (segment (start 106.934 67.492) (end 106.934 61.087) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0E8))
  (segment (start 106.934 61.087) (end 119.634 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C0F7))
  (via (at 165.354 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1C0))
  (segment (start 165.934 68.072) (end 167.259 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0F1) (status 20))
  (segment (start 165.354 67.492) (end 165.934 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3BE9F))
  (segment (start 165.354 61.087) (end 165.354 67.492) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C0F4))
  (via (at 178.054 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1BD))
  (segment (start 165.354 61.087) (end 178.054 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C0FD))
  (segment (start 178.054 67.617) (end 178.509 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C100))
  (segment (start 178.509 68.072) (end 179.834 68.072) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C103) (status 20))
  (segment (start 178.054 61.087) (end 178.054 67.617) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C10C))
  (segment (start 162.052 61.087) (end 165.354 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C106))
  (via (at 136.144 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1BA))
  (via (at 148.844 61.087) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 123) (tstamp 5BC3C1B7))
  (segment (start 148.844 67.617) (end 148.844 61.087) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C109))
  (segment (start 148.844 61.087) (end 162.052 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C118))
  (segment (start 136.144 61.087) (end 148.844 61.087) (width 0.35) (layer B.Cu) (net 123) (tstamp 5BC3C0FA))
  (segment (start 133.9215 61.087) (end 136.144 61.087) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BC3C112))
  (segment (start 132.9055 60.071) (end 133.9215 61.087) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 132.9055 50.649) (end 132.9055 58.674) (width 0.35) (layer F.Cu) (net 123))
  (segment (start 114.348 46.865) (end 115.953 46.865) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 117.475 48.387) (end 118.1735 48.387) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 115.953 46.865) (end 117.475 48.387) (width 0.35) (layer F.Cu) (net 124))
  (segment (start 115.448 47.665) (end 114.348 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 117.5735 49.784) (end 115.4545 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 115.4545 47.665) (end 115.448 47.665) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 118.1735 49.784) (end 117.5735 49.784) (width 0.35) (layer F.Cu) (net 125))
  (via (at 118.11 54.4576) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 127))
  (segment (start 118.1848 54.3828) (end 118.11 54.4576) (width 0.35) (layer F.Cu) (net 127))
  (segment (start 118.1848 52.6288) (end 118.1848 54.3828) (width 0.35) (layer F.Cu) (net 127))
  (via (at 182.245 58.42) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 127))
  (segment (start 182.245 58.42) (end 182.245 73.66) (width 0.35) (layer F.Cu) (net 127))
  (segment (start 181.61 75.692) (end 179.959 75.692) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BC3C115))
  (segment (start 182.245 75.057) (end 181.61 75.692) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BC3C10F))
  (segment (start 120.002401 55.257599) (end 118.909999 55.257599) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 120.015 55.245) (end 120.002401 55.257599) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 172.72 55.245) (end 120.015 55.245) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 175.895 58.42) (end 172.72 55.245) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 118.909999 55.257599) (end 118.11 54.4576) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 182.245 58.42) (end 175.895 58.42) (width 0.35) (layer B.Cu) (net 127))
  (segment (start 114.348 48.465) (end 114.348 49.09) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 116.439 51.181) (end 118.1735 51.181) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 115.443 50.185) (end 116.439 51.181) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 114.348 49.09) (end 115.443 50.185) (width 0.35) (layer F.Cu) (net 128))
  (segment (start 100.827 37.719) (end 99.406 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 102.948 39.84) (end 100.827 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 99.406 37.719) (end 98.806 37.719) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 102.948 40.465) (end 102.948 39.84) (width 0.35) (layer F.Cu) (net 129))
  (via (at 98.425 55.118) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 130))
  (segment (start 98.425 56.388) (end 98.425 55.118) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 100.076 56.769) (end 99.822 56.515) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 99.822 56.515) (end 98.425 55.118) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 103.124 56.388) (end 102.743 56.769) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 102.743 56.769) (end 100.076 56.769) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 103.124 55.602) (end 103.124 56.388) (width 0.35) (layer F.Cu) (net 130))
  (via (at 97.028 53.594) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 131))
  (segment (start 97.028 54.737) (end 97.028 53.594) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 97.028 56.388) (end 97.028 54.737) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 97.028 53.594) (end 98.679 53.594) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 98.933 53.594) (end 98.679 53.594) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.927 55.602) (end 100.457 55.132) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 101.727 55.602) (end 100.927 55.602) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.457 55.132) (end 100.457 55.118) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 100.457 55.118) (end 98.933 53.594) (width 0.35) (layer F.Cu) (net 131))
  (via (at 95.758 51.816) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 132))
  (segment (start 95.389 51.828) (end 95.377 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 95.77 51.828) (end 95.758 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 97.294 51.828) (end 95.77 51.828) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 92.317 51.816) (end 95.758 51.816) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 95.631 51.943) (end 95.758 51.816) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 95.631 56.388) (end 95.631 51.943) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 92.329 50.419) (end 94.107 50.419) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 97.306 50.419) (end 94.107 50.419) (width 0.35) (layer F.Cu) (net 133))
  (via (at 94.107 50.419) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 133))
  (segment (start 94.234 50.546) (end 94.107 50.419) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 94.234 56.388) (end 94.234 50.546) (width 0.35) (layer B.Cu) (net 133))
  (via (at 95.758 49.022) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 134))
  (segment (start 97.306 49.022) (end 95.758 49.022) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 92.329 49.022) (end 95.758 49.022) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 93.345 49.022) (end 95.758 49.022) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 92.837 49.53) (end 93.345 49.022) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 92.837 56.388) (end 92.837 49.53) (width 0.35) (layer B.Cu) (net 134))
  (via (at 94.107 47.625) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 135))
  (segment (start 97.306 47.625) (end 94.107 47.625) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 94.107 47.625) (end 92.329 47.625) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 91.44 49.16063) (end 91.44 50.165) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 94.107 47.625) (end 92.97563 47.625) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 92.97563 47.625) (end 91.44 49.16063) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 91.44 56.388) (end 91.44 50.165) (width 0.35) (layer B.Cu) (net 135))
  (segment (start 114.348 43.665) (end 116.863 43.665) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 118.237 42.291) (end 120.65 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 116.863 43.665) (end 118.237 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 121.2596 42.9006) (end 120.65 42.291) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 123.2662 42.9006) (end 121.2596 42.9006) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 115.443 42.865) (end 115.758 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 114.348 42.865) (end 115.443 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 119.1 38.591) (end 120.65 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 117.729 39.962) (end 119.1 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 117.729 41.849) (end 117.729 39.962) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 116.713 42.865) (end 117.729 41.849) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 115.443 42.865) (end 116.713 42.865) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 121.2426 37.9984) (end 120.65 38.591) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 123.2662 37.9984) (end 121.2426 37.9984) (width 0.35) (layer F.Cu) (net 137))
  (segment (start 99.568 46.228) (end 97.282 46.228) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 100.531 45.265) (end 99.568 46.228) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 102.948 45.265) (end 100.531 45.265) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 115.453 41.265) (end 114.348 41.265) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 116.078 40.64) (end 115.453 41.265) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 116.078 38.608) (end 116.078 40.64) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 118.745 35.941) (end 116.078 38.608) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 118.745 34.9384) (end 118.745 35.941) (width 0.35) (layer F.Cu) (net 139))
  (segment (start 111.848 37.631) (end 113.538 35.941) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 113.538 35.941) (end 114.554 34.925) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BC7BC0F))
  (segment (start 111.848 38.765) (end 111.848 37.631) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 120.142 35.814) (end 120.142 34.9384) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.84 39.116) (end 120.142 35.814) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.304 42.065) (end 116.84 41.529) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 116.84 41.529) (end 116.84 39.116) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 114.348 42.065) (end 116.304 42.065) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 105.918 53.502) (end 105.918 54.102) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 105.918 53.467) (end 105.918 53.502) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 107.048 52.337) (end 105.918 53.467) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 107.048 50.165) (end 107.048 52.337) (width 0.35) (layer F.Cu) (net 145))
  (segment (start 179.705 18.8595) (end 179.705 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DF1) (status 20))
  (segment (start 137.795 19.05) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DEE) (status 30))
  (segment (start 139.065 15.24) (end 139.065 17.272) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DEB) (status 30))
  (segment (start 139.065 17.272) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DDF) (status 30))
  (segment (start 173.355 18.0995) (end 173.355 17.5895) (width 0.7) (layer F.Cu) (net 151) (tstamp 5BC64DDC) (status 30))
  (segment (start 173.355 18.0995) (end 173.355 17.3495) (width 0.7) (layer F.Cu) (net 151) (tstamp 5BC64DE5) (status 30))
  (segment (start 179.07 17.5895) (end 179.705 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DE2) (status 20))
  (segment (start 177.925 18.0995) (end 178.435 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DCD))
  (segment (start 173.355 18.0995) (end 177.925 18.0995) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64DCA) (status 10))
  (segment (start 178.435 17.5895) (end 179.07 17.5895) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D6D))
  (segment (start 139.065 19.685) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D73) (status 20))
  (segment (start 179.705 21.8745) (end 179.705 18.8595) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D70) (status 10))
  (segment (start 139.065 21.905) (end 139.065 19.05) (width 0.35) (layer F.Cu) (net 151) (tstamp 5BC64D61))
  (segment (start 173.355 18.0995) (end 173.355 20.32) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 173.355 20.32) (end 173.355 17.53) (width 0.7) (layer F.Cu) (net 151))
  (segment (start 173.355 20.32) (end 173.355 21.4745) (width 0.7) (layer F.Cu) (net 151))
  (via (at 173.355 20.32) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 151))
  (segment (start 173.355 21.4745) (end 173.355 17.53) (width 1) (layer F.Cu) (net 151))
  (segment (start 137.795 19.05) (end 133.35 19.05) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 132.715 19.685) (end 132.715 21.105) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 133.35 19.05) (end 132.715 19.685) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 116.84 16.768) (end 116.84 21.336) (width 1) (layer F.Cu) (net 151))
  (segment (start 132.715 21.336) (end 125.476 21.336) (width 1) (layer F.Cu) (net 151))
  (segment (start 115.57 20.32) (end 106.172 29.718) (width 1) (layer B.Cu) (net 151))
  (via (at 121.031 20.32) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 151))
  (segment (start 173.355 20.32) (end 121.031 20.32) (width 1) (layer B.Cu) (net 151))
  (segment (start 121.031 20.32) (end 115.57 20.32) (width 1) (layer B.Cu) (net 151))
  (segment (start 121.031 21.209) (end 120.904 21.336) (width 1) (layer F.Cu) (net 151))
  (segment (start 121.031 20.32) (end 121.031 21.209) (width 1) (layer F.Cu) (net 151))
  (segment (start 120.904 21.336) (end 125.476 21.336) (width 1) (layer F.Cu) (net 151))
  (segment (start 116.84 21.336) (end 120.904 21.336) (width 1) (layer F.Cu) (net 151))
  (segment (start 177.132 27.2415) (end 177.165 27.2745) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DD0) (status 30))
  (segment (start 175.895 27.2415) (end 177.132 27.2415) (width 0.35) (layer F.Cu) (net 152) (tstamp 5BC64DBB) (status 20))
  (segment (start 177.165 21.8745) (end 177.165 27.2745) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 175.655 27.6745) (end 175.895 27.4345) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 173.355 27.6745) (end 175.655 27.6745) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 176.055 27.2745) (end 175.655 27.6745) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 177.165 27.2745) (end 176.055 27.2745) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 177.165 21.8745) (end 178.435 21.8745) (width 0.7) (layer F.Cu) (net 152))
  (segment (start 179.705 28.4995) (end 179.705 27.2745) (width 0.35) (layer F.Cu) (net 153) (tstamp 5BC64DC4) (status 20))
  (segment (start 180.86 29.6545) (end 179.705 28.4995) (width 0.35) (layer F.Cu) (net 153) (tstamp 5BC64DC1) (status 10))
  (segment (start 183.6155 19.4945) (end 183.635 19.475) (width 0.35) (layer F.Cu) (net 154) (tstamp 5BC64E78))
  (segment (start 180.655 19.4945) (end 183.6155 19.4945) (width 0.35) (layer F.Cu) (net 154) (tstamp 5BC64E6C))
  (segment (start 185.928 19.468) (end 185.935 19.475) (width 0.35) (layer F.Cu) (net 155) (tstamp 5BC64D1F))
  (segment (start 185.928 17.145) (end 185.928 19.468) (width 0.35) (layer F.Cu) (net 155) (tstamp 5BC64D13))
  (segment (start 152.9715 14.1285) (end 152.915 14.185) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64D28))
  (segment (start 152.9715 12.5095) (end 152.9715 14.1285) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64D2E))
  (segment (start 152.915 12.185) (end 153.035 12.065) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64E3C))
  (segment (start 152.915 14.185) (end 152.915 12.185) (width 0.35) (layer F.Cu) (net 156) (tstamp 5BC64E36))
  (segment (start 150.495 14.065) (end 150.615 14.185) (width 0.35) (layer F.Cu) (net 157) (tstamp 5BC64E54))
  (segment (start 150.495 12.065) (end 150.495 14.065) (width 0.35) (layer F.Cu) (net 157) (tstamp 5BC64E45))
  (segment (start 139.065 29.21) (end 139.065 27.305) (width 0.35) (layer F.Cu) (net 158) (tstamp 5BC64E57))
  (segment (start 184.15 21.8745) (end 180.975 21.8745) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E2A))
  (segment (start 184.785 22.5095) (end 184.15 21.8745) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E30))
  (segment (start 184.785 24.975) (end 184.785 22.5095) (width 0.35) (layer F.Cu) (net 159) (tstamp 5BC64E3F))
  (segment (start 146.7485 18.05) (end 146.7485 16.256) (width 0.35) (layer F.Cu) (net 161) (tstamp 5BC64D9A) (status 30))
  (segment (start 142.245 20.27) (end 142.24 20.265) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D97) (status 30))
  (segment (start 142.245 20.32) (end 142.245 20.27) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D94) (status 30))
  (segment (start 141.605 19.05) (end 140.565 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D91) (status 20))
  (segment (start 145.7985 19.25) (end 145.7985 20.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DAC) (status 20))
  (segment (start 145.5985 19.05) (end 145.7985 19.25) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DA9))
  (segment (start 142.245 20.05) (end 142.245 19.055) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB8) (status 10))
  (segment (start 142.24 19.05) (end 145.5985 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB5))
  (segment (start 142.245 19.055) (end 142.24 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DB2))
  (segment (start 146.746 14.2925) (end 146.746 13.716) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64DAF))
  (segment (start 145.7985 15.24) (end 146.746 14.2925) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D8E))
  (segment (start 145.7985 19.25) (end 145.7985 15.24) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D8B))
  (segment (start 146.746 13.716) (end 146.746 11.446) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D6A) (status 20))
  (segment (start 141.605 19.05) (end 142.24 19.05) (width 0.35) (layer F.Cu) (net 162) (tstamp 5BC64D67))
  (segment (start 142.417 17.272) (end 143.195 18.05) (width 0.35) (layer F.Cu) (net 163) (tstamp 5BC64DA6) (status 20))
  (segment (start 140.965 17.272) (end 142.417 17.272) (width 0.35) (layer F.Cu) (net 163) (tstamp 5BC64DA3) (status 10))
  (segment (start 144.276 13.446) (end 144.26 13.462) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 145.796 13.446) (end 144.276 13.446) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 144.272 11.672) (end 144.26 11.684) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 144.272 10.033) (end 144.272 11.672) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 144.26 11.684) (end 144.26 13.462) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 141.605 15.24) (end 140.565 15.24) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D82) (status 20))
  (segment (start 142.621 16.256) (end 141.605 15.24) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D7F))
  (segment (start 144.6485 16.256) (end 142.621 16.256) (width 0.35) (layer F.Cu) (net 165) (tstamp 5BC64D76) (status 10))
  (segment (start 92.076 27.126) (end 92.382 27.432) (width 1) (layer F.Cu) (net 167))
  (segment (start 92.076 23.876) (end 92.076 27.126) (width 1) (layer F.Cu) (net 167))
  (segment (start 92.382 27.432) (end 102.87 27.432) (width 1) (layer F.Cu) (net 167))
  (segment (start 103.622 28.184) (end 103.622 29.718) (width 1) (layer F.Cu) (net 167))
  (segment (start 102.87 27.432) (end 103.622 28.184) (width 1) (layer F.Cu) (net 167))
  (segment (start 92.075 23.875) (end 92.076 23.876) (width 1) (layer F.Cu) (net 167))
  (segment (start 92.075 18.288) (end 92.075 23.875) (width 1) (layer F.Cu) (net 167))
  (segment (start 105.9825 23.876) (end 107.824 22.0345) (width 1) (layer F.Cu) (net 168))
  (segment (start 100.076 23.876) (end 105.9825 23.876) (width 1) (layer F.Cu) (net 168))
  (segment (start 141.224 68.072) (end 142.494 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C121) (status 10))
  (segment (start 142.494 68.072) (end 143.129 67.437) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C11B))
  (via (at 143.129 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1B4))
  (segment (start 143.129 67.437) (end 143.129 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C12A))
  (segment (start 128.649 68.072) (end 129.794 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C11E) (status 10))
  (segment (start 129.794 68.072) (end 130.429 67.437) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C124))
  (via (at 130.429 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1B1))
  (segment (start 130.429 67.437) (end 130.429 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C12D))
  (segment (start 143.129 64.897) (end 130.429 64.897) (width 0.35) (layer B.Cu) (net 170) (tstamp 5BC3C13F))
  (segment (start 112.014 68.072) (end 112.689 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C142) (status 30))
  (segment (start 112.689 68.072) (end 113.284 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C130) (status 10))
  (via (at 113.919 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1AE))
  (segment (start 113.919 67.437) (end 113.919 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C133))
  (segment (start 113.284 68.072) (end 113.919 67.437) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C127))
  (segment (start 113.919 64.897) (end 130.429 64.897) (width 0.35) (layer B.Cu) (net 170) (tstamp 5BC3C136))
  (segment (start 99.439 68.072) (end 100.584 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C154) (status 10))
  (segment (start 100.584 68.072) (end 101.219 67.437) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C145))
  (via (at 101.219 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1AB))
  (segment (start 101.219 67.437) (end 101.219 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C151))
  (segment (start 101.219 64.897) (end 113.919 64.897) (width 0.35) (layer B.Cu) (net 170) (tstamp 5BC3C13C))
  (segment (start 159.184 68.072) (end 159.639 67.617) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C139))
  (segment (start 157.859 68.072) (end 159.184 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C148) (status 10))
  (via (at 159.639 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1A8))
  (segment (start 159.639 67.617) (end 159.639 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C15D))
  (segment (start 159.639 64.897) (end 143.129 64.897) (width 0.35) (layer B.Cu) (net 170) (tstamp 5BC3C15A))
  (segment (start 171.759 68.072) (end 172.339 67.492) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C14E))
  (segment (start 170.434 68.072) (end 171.759 68.072) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C16F) (status 10))
  (via (at 172.339 64.897) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170) (tstamp 5BC3C1A5))
  (segment (start 172.339 67.492) (end 172.339 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C16C))
  (segment (start 172.339 64.897) (end 159.639 64.897) (width 0.35) (layer B.Cu) (net 170) (tstamp 5BC3C14B))
  (segment (start 110.236 61.214) (end 113.919 64.897) (width 0.35) (layer F.Cu) (net 170) (tstamp 5BC3C157))
  (segment (start 110.236 55.602) (end 110.236 59.817) (width 0.35) (layer F.Cu) (net 170))
  (segment (start 163.449 62.357) (end 146.939 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C160))
  (segment (start 164.084 69.342) (end 163.449 68.707) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C181))
  (segment (start 163.449 68.707) (end 163.449 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C17E))
  (segment (start 167.259 69.342) (end 164.084 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C169) (status 10))
  (segment (start 105.029 62.357) (end 117.729 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C175))
  (segment (start 105.664 69.342) (end 105.029 68.707) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C166))
  (segment (start 105.029 68.707) (end 105.029 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C163))
  (segment (start 108.839 69.342) (end 105.664 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C202) (status 10))
  (segment (start 117.729 62.357) (end 134.239 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C17B))
  (segment (start 117.729 68.707) (end 117.729 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C172))
  (segment (start 118.364 69.342) (end 117.729 68.707) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C187))
  (segment (start 121.414 69.342) (end 118.364 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C184) (status 10))
  (segment (start 146.939 62.357) (end 134.239 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C178))
  (segment (start 134.874 69.342) (end 134.239 68.707) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C18A))
  (segment (start 134.239 68.707) (end 134.239 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C226))
  (segment (start 138.049 69.342) (end 134.874 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C214) (status 10))
  (segment (start 147.574 69.342) (end 146.939 68.707) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C1FF))
  (segment (start 146.939 68.707) (end 146.939 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C208))
  (segment (start 150.624 69.342) (end 147.574 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C205) (status 10))
  (via (at 163.449 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C1A2))
  (via (at 105.029 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C19F))
  (via (at 117.729 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C19C))
  (via (at 134.239 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C199))
  (via (at 146.939 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C196))
  (segment (start 114.427 57.658) (end 117.729 60.96) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 114.427 55.602) (end 114.427 57.658) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 179.959 69.342) (end 177.165 69.342) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C223))
  (via (at 176.276 62.357) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BC3C193))
  (segment (start 176.276 68.453) (end 176.276 62.357) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C20B))
  (segment (start 177.165 69.342) (end 176.276 68.453) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BC3C20E))
  (segment (start 174.752 62.357) (end 163.449 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C21A))
  (segment (start 176.276 62.357) (end 174.752 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C211))
  (segment (start 175.26 62.357) (end 174.752 62.357) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BC3C217))
  (via (at 114.554 32.004) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 178) (tstamp 5BCBC56E))
  (segment (start 114.554 32.004) (end 114.554 33.425) (width 0.35) (layer F.Cu) (net 178))
  (segment (start 170.561 49.554) (end 170.585 49.53) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 170.561 51.054) (end 170.561 49.554) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 114.554 32.004) (end 114.554 48.514) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 167.386 54.61) (end 170.561 51.435) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 120.65 54.61) (end 167.386 54.61) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 114.554 48.514) (end 120.65 54.61) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 170.561 51.435) (end 170.561 51.054) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 180.745 51.435) (end 178.435 51.435) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 176.53 49.53) (end 176.657 49.657) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 172.085 49.53) (end 176.53 49.53) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 176.657 49.657) (end 178.435 51.435) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 180.745 46.355) (end 178.435 46.355) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 176.657 48.133) (end 172.073 48.133) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 178.435 46.355) (end 176.657 48.133) (width 0.35) (layer B.Cu) (net 180))
  (via (at 115.951 30.607) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 181))
  (segment (start 115.951 30.607) (end 115.951 33.425) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 170.561 48.121) (end 170.573 48.133) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 170.561 46.609) (end 170.561 48.121) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 169.672 48.133) (end 170.573 48.133) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 168.91 48.895) (end 169.672 48.133) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 115.951 30.607) (end 115.951 48.641) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 167.005 53.975) (end 168.91 52.07) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 121.285 53.975) (end 167.005 53.975) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 168.91 52.07) (end 168.91 48.895) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 115.951 48.641) (end 121.285 53.975) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 117.348 32.004) (end 117.348 48.768) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 117.348 33.4264) (end 117.348 32.004) (width 0.35) (layer F.Cu) (net 182))
  (via (at 117.348 32.004) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 182))
  (segment (start 117.348 48.768) (end 121.92 53.34) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 121.92 53.34) (end 166.37 53.34) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 166.37 53.34) (end 168.275 51.435) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 168.275 51.435) (end 168.275 43.815) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 172.72 43.18) (end 175.895 46.355) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 172.72 41.91) (end 172.72 43.18) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 169.164 43.18) (end 168.275 43.18) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 168.91 43.18) (end 169.164 43.18) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 169.164 43.18) (end 172.72 43.18) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 168.275 43.815) (end 168.275 43.18) (width 0.35) (layer B.Cu) (net 182))
  (segment (start 155.321 91.186) (end 155.321 94.012) (width 0.35) (layer B.Cu) (net 185))
  (segment (start 123.825 91.186) (end 123.825 90.17) (width 0.35) (layer F.Cu) (net 186) (status 10))
  (segment (start 123.825 88.38) (end 123.825 91.186) (width 0.35) (layer B.Cu) (net 186))
  (segment (start 152.654 91.059) (end 152.781 91.186) (width 0.35) (layer F.Cu) (net 187) (status 30))
  (segment (start 152.781 91.186) (end 152.781 88.38) (width 0.35) (layer B.Cu) (net 187))
  (segment (start 215.011 57.089) (end 211.008 57.089) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 107.55 103.03) (end 107.95 103.43) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 104.775 103.03) (end 107.55 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 118.42 103.03) (end 118.745 103.355) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 115.57 103.03) (end 118.42 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 136.835 103.03) (end 137.16 103.355) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 133.985 103.03) (end 136.835 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 144.94 103.03) (end 147.63 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 163.195 103.03) (end 165.97 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 176.765 103.03) (end 177.165 103.43) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 173.99 103.03) (end 176.765 103.03) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (via (at 107.95 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 107.95 103.43) (end 107.95 105.41) (width 0.7) (layer F.Cu) (net 194) (status 10))
  (via (at 118.745 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 118.745 105.41) (end 118.745 103.355) (width 0.7) (layer F.Cu) (net 194) (status 20))
  (via (at 166.37 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 166.37 105.41) (end 166.37 103.43) (width 0.7) (layer F.Cu) (net 194) (status 20))
  (via (at 177.165 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 177.165 105.41) (end 177.165 103.43) (width 0.7) (layer F.Cu) (net 194) (status 20))
  (segment (start 176.365001 104.610001) (end 177.165 105.41) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 166.37 105.41) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 166.37 104.610001) (end 176.365001 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 165.570001 104.610001) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (via (at 147.955 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 148.03 105.335) (end 147.955 105.41) (width 0.7) (layer F.Cu) (net 194))
  (segment (start 148.03 103.43) (end 148.03 105.335) (width 0.7) (layer F.Cu) (net 194) (status 10))
  (segment (start 147.955 105.41) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 148.754999 104.610001) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 147.955 104.610001) (end 138.43 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 137.16 104.610001) (end 137.16 105.41) (width 0.7) (layer B.Cu) (net 194))
  (via (at 137.16 105.41) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 137.16 105.41) (end 137.16 103.355) (width 0.7) (layer F.Cu) (net 194) (status 20))
  (segment (start 119.38 104.610001) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 118.745 104.775) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 118.745 105.41) (end 118.745 104.775) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 119.38 104.610001) (end 109.22 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 109.22 104.610001) (end 108.749999 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 107.95 105.41) (end 107.95 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 109.22 104.610001) (end 107.95 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 126.8095 104.610001) (end 119.38 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 137.16 104.610001) (end 126.8095 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 138.43 104.610001) (end 137.16 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 148.754999 104.610001) (end 165.570001 104.610001) (width 0.7) (layer B.Cu) (net 194))
  (segment (start 163.047 20.066) (end 164.211 20.066) (width 0.7) (layer F.Cu) (net 194) (tstamp 5BC64E24))
  (segment (start 165.227 20.066) (end 164.211 20.066) (width 0.7) (layer F.Cu) (net 194) (tstamp 5BC64D22))
  (segment (start 165.227 14.41) (end 165.227 16.51) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64D46))
  (segment (start 155.362 12.065) (end 155.362 12.7) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64D16))
  (segment (start 154.945 10.165) (end 155.362 10.582) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64D34))
  (segment (start 155.362 10.582) (end 155.362 12.065) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64D10))
  (segment (start 153.035 10.165) (end 154.945 10.165) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64E39))
  (segment (start 164.787 13.97) (end 165.227 14.41) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64DF7))
  (segment (start 155.362 12.7) (end 156.632 13.97) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64D5E))
  (segment (start 156.632 13.97) (end 164.787 13.97) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BC64DF4))
  (segment (start 165.227 18.542) (end 165.227 20.066) (width 0.7) (layer F.Cu) (net 194) (tstamp 5BC64E2D))
  (segment (start 165.227 18.542) (end 165.227 16.51) (width 0.7) (layer F.Cu) (net 194) (tstamp 5BC64E33))
  (segment (start 176.365001 104.610001) (end 179.996999 104.610001) (width 1) (layer B.Cu) (net 194))
  (segment (start 186.309 100.584) (end 186.944 99.949) (width 1) (layer B.Cu) (net 194))
  (segment (start 184.023 100.584) (end 186.309 100.584) (width 1) (layer B.Cu) (net 194))
  (segment (start 179.996999 104.610001) (end 184.023 100.584) (width 1) (layer B.Cu) (net 194))
  (via (at 168.91 15.748) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 165.989 15.748) (end 165.227 16.51) (width 1) (layer F.Cu) (net 194))
  (segment (start 168.91 15.748) (end 165.989 15.748) (width 1) (layer F.Cu) (net 194))
  (segment (start 186.309 100.584) (end 186.309 93.726) (width 1) (layer B.Cu) (net 194))
  (via (at 186.309 80.645) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 186.309 93.726) (end 186.309 80.645) (width 1) (layer B.Cu) (net 194))
  (via (at 186.309 77.47) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 186.309 80.645) (end 186.309 77.47) (width 1) (layer F.Cu) (net 194))
  (segment (start 186.309 77.47) (end 186.309 17.78) (width 1) (layer B.Cu) (net 194))
  (segment (start 186.309 17.78) (end 184.277 15.748) (width 1) (layer B.Cu) (net 194))
  (segment (start 168.91 15.748) (end 184.277 15.748) (width 1) (layer B.Cu) (net 194))
  (segment (start 242.697 58.42) (end 242.697 60.419) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 234.339 67.969) (end 234.315 67.945) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 234.339 69.85) (end 234.339 67.969) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 234.304 67.934) (end 234.315 67.945) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 234.304 65.967) (end 234.304 67.934) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 217.17 65.695) (end 217.211 65.654) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 217.17 67.195) (end 217.17 65.695) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 217.211 60.55) (end 217.17 60.591) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 217.211 58.989) (end 217.211 60.55) (width 0.35) (layer F.Cu) (net 194))
  (via (at 218.821 60.579) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 218.809 60.591) (end 218.821 60.579) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 217.17 60.591) (end 218.809 60.591) (width 0.35) (layer F.Cu) (net 194))
  (via (at 218.821 67.183) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 218.821 60.579) (end 218.821 67.183) (width 0.35) (layer B.Cu) (net 194))
  (segment (start 217.182 67.183) (end 217.17 67.195) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 218.821 67.183) (end 217.182 67.183) (width 0.35) (layer F.Cu) (net 194))
  (via (at 211.836 59.817) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 194))
  (segment (start 211.86 59.793) (end 211.836 59.817) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 211.86 58.039) (end 211.86 59.793) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 218.059 59.817) (end 218.821 60.579) (width 0.35) (layer B.Cu) (net 194))
  (segment (start 211.836 59.817) (end 218.059 59.817) (width 0.35) (layer B.Cu) (net 194))
  (segment (start 165.97 103.03) (end 166.37 103.43) (width 0.35) (layer F.Cu) (net 194) (status 30))
  (segment (start 215.011 63.754) (end 210.566 63.754) (width 0.35) (layer F.Cu) (net 202))
  (segment (start 144.145 20.955) (end 144.145 20.05) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64D5B))
  (segment (start 148.545 21.905) (end 150.765 19.685) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64D55))
  (segment (start 140.335 21.905) (end 142.875 21.905) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64D4F))
  (segment (start 150.765 19.685) (end 151.765 19.685) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64D49))
  (segment (start 142.875 21.905) (end 143.195 21.905) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64D4C))
  (segment (start 144.145 20.955) (end 144.145 21.905) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64E51))
  (segment (start 144.145 21.905) (end 148.545 21.905) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64E5A))
  (segment (start 142.875 21.905) (end 144.145 21.905) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BC64E4E))
  (segment (start 231.672 51.816) (end 230.124 51.816) (width 0.35) (layer F.Cu) (net 204))
  (segment (start 233.172 54.135) (end 233.204 54.167) (width 0.35) (layer F.Cu) (net 205))
  (segment (start 233.172 51.816) (end 233.172 54.135) (width 0.35) (layer F.Cu) (net 205))
  (segment (start 137.795 29.53) (end 137.795 27.305) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64D19))
  (segment (start 139.065 23.815) (end 142.24 23.815) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64E42))
  (segment (start 137.795 25.085) (end 139.065 23.815) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64E48))
  (segment (start 137.795 27.305) (end 137.795 25.085) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BC64E4B))
  (segment (start 224.929 51.816) (end 224.004 51.816) (width 0.35) (layer F.Cu) (net 211))
  (segment (start 225.794 54.157) (end 225.804 54.167) (width 0.35) (layer F.Cu) (net 212))
  (segment (start 224.704 54.167) (end 225.804 54.167) (width 0.35) (layer F.Cu) (net 212))
  (segment (start 226.429 53.542) (end 225.804 54.167) (width 0.35) (layer F.Cu) (net 212))
  (segment (start 226.429 51.816) (end 226.429 53.542) (width 0.35) (layer F.Cu) (net 212))
  (via (at 122.936 17.78) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 213))
  (segment (start 122.936 12.573) (end 122.936 17.78) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 123.735999 18.579999) (end 123.989999 18.579999) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 122.936 17.78) (end 123.735999 18.579999) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 123.989999 18.579999) (end 124.079 18.669) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 124.079 18.669) (end 163.068 18.669) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 163.068 18.669) (end 174.752 18.669) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 174.752 18.669) (end 184.277 18.669) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 184.277 18.669) (end 185.039 19.431) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 185.039 19.431) (end 185.039 40.767) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 119.6735 52.6175) (end 119.6848 52.6288) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 119.6735 51.181) (end 119.6735 52.6175) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 126.365 53.213) (end 126.365 51.278) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 120.65 53.975) (end 125.603 53.975) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 119.6848 53.0098) (end 120.65 53.975) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 119.6848 52.6288) (end 119.6848 53.0098) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 125.603 53.975) (end 126.365 53.975) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 126.365 53.975) (end 126.365 51.278) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 126.365 55.245) (end 126.365 53.975) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 128.905 43.053) (end 128.905 46.228) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 128.905 48.641) (end 128.905 46.228) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 128.905 49.149) (end 128.905 48.641) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 121.92 49.149) (end 128.905 49.149) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 121.285 49.784) (end 121.92 49.149) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 119.6735 49.784) (end 121.285 49.784) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 128.905 49.149) (end 131.445 49.149) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 126.365 47.879) (end 126.365 46.228) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 125.857 48.387) (end 126.365 47.879) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 119.6735 48.387) (end 125.857 48.387) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 126.365 43.053) (end 126.365 46.228) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 126.365 43.053) (end 126.365 42.053) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 130.318 41.418) (end 127 41.418) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 130.81 41.91) (end 130.318 41.418) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 126.365 42.053) (end 127 41.418) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 132.9055 47.8155) (end 130.81 45.72) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 132.9055 49.149) (end 132.9055 47.8155) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 130.81 45.72) (end 130.81 41.91) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 121.285 46.99) (end 119.6735 46.99) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 122.975 46.228) (end 123.825 46.228) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 122.213 46.99) (end 122.975 46.228) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 121.285 46.99) (end 122.213 46.99) (width 0.35) (layer F.Cu) (net 219))
  (via (at 92.71 100.203) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 220))
  (segment (start 92.837 58.801) (end 92.837 57.888) (width 0.35) (layer B.Cu) (net 220))
  (segment (start 92.202 59.436) (end 92.837 58.801) (width 0.35) (layer B.Cu) (net 220))
  (segment (start 92.202 98.56363) (end 92.202 59.436) (width 0.35) (layer B.Cu) (net 220))
  (segment (start 92.71 99.07163) (end 92.202 98.56363) (width 0.35) (layer B.Cu) (net 220))
  (segment (start 92.71 100.203) (end 92.71 99.07163) (width 0.35) (layer B.Cu) (net 220))
  (segment (start 94.107 100.203) (end 92.71 100.203) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 95.504 101.6) (end 94.107 100.203) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 109.68 101.6) (end 95.504 101.6) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 111.11 103.03) (end 109.68 101.6) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 111.76 103.03) (end 111.11 103.03) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 101.727 53.561) (end 101.727 54.102) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 104.648 50.165) (end 104.013 50.165) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 101.727 52.451) (end 101.727 53.561) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 104.013 50.165) (end 101.727 52.451) (width 0.35) (layer F.Cu) (net 221))
  (via (at 98.552 94.361) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 222))
  (segment (start 170.18 99.949) (end 170.18 102.555) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 170.18 102.555) (end 170.18 103.03) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 98.552 94.361) (end 98.552 97.409) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 169.291 99.06) (end 170.18 99.949) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 100.203 99.06) (end 169.291 99.06) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 98.552 97.409) (end 100.203 99.06) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 95.885 94.361) (end 98.552 94.361) (width 0.35) (layer B.Cu) (net 222))
  (segment (start 95.25 93.726) (end 95.885 94.361) (width 0.35) (layer B.Cu) (net 222))
  (segment (start 95.25 62.103) (end 95.25 93.726) (width 0.35) (layer B.Cu) (net 222))
  (segment (start 98.425 58.928) (end 95.25 62.103) (width 0.35) (layer B.Cu) (net 222))
  (segment (start 98.425 57.888) (end 98.425 58.928) (width 0.35) (layer B.Cu) (net 222))
  (segment (start 99.70663 99.695) (end 99.822 99.695) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 96.901 95.758) (end 96.901 96.88937) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 159.385 103.03) (end 159.385 100.457) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 96.901 96.88937) (end 99.70663 99.695) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 100.076 99.695) (end 99.822 99.695) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 159.385 100.457) (end 158.623 99.695) (width 0.35) (layer F.Cu) (net 223))
  (via (at 96.901 95.758) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 223))
  (segment (start 158.623 99.695) (end 129.794 99.695) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 129.794 99.695) (end 100.076 99.695) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 95.123 95.758) (end 96.901 95.758) (width 0.35) (layer B.Cu) (net 223))
  (segment (start 94.488 61.595) (end 94.488 95.123) (width 0.35) (layer B.Cu) (net 223))
  (segment (start 97.028 59.055) (end 94.488 61.595) (width 0.35) (layer B.Cu) (net 223))
  (segment (start 94.488 95.123) (end 95.123 95.758) (width 0.35) (layer B.Cu) (net 223))
  (segment (start 97.028 57.888) (end 97.028 59.055) (width 0.35) (layer B.Cu) (net 223))
  (segment (start 100.21 51.828) (end 99.394 51.828) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 99.394 51.828) (end 98.794 51.828) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 102.948 49.09) (end 100.21 51.828) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 102.948 48.465) (end 102.948 49.09) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 99.406 50.419) (end 102.16 47.665) (width 0.35) (layer F.Cu) (net 225))
  (segment (start 102.16 47.665) (end 102.948 47.665) (width 0.35) (layer F.Cu) (net 225))
  (segment (start 98.806 50.419) (end 99.406 50.419) (width 0.35) (layer F.Cu) (net 225))
  (segment (start 91.44 57.888) (end 91.44 98.044) (width 0.35) (layer B.Cu) (net 226))
  (via (at 91.44 101.727) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 226))
  (segment (start 91.44 98.044) (end 91.44 101.727) (width 0.35) (layer B.Cu) (net 226))
  (segment (start 94.107 101.727) (end 91.44 101.727) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 95.41 103.03) (end 94.107 101.727) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 100.965 103.03) (end 95.41 103.03) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 102.948 46.865) (end 101.598 46.865) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 99.441 49.022) (end 98.806 49.022) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 101.598 46.865) (end 99.441 49.022) (width 0.35) (layer F.Cu) (net 227))
  (via (at 95.377 97.155) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 228))
  (segment (start 97.79 99.568) (end 95.377 97.155) (width 0.35) (layer F.Cu) (net 228))
  (segment (start 98.552 100.33) (end 97.79 99.568) (width 0.35) (layer F.Cu) (net 228))
  (segment (start 137.62 100.33) (end 98.552 100.33) (width 0.35) (layer F.Cu) (net 228))
  (segment (start 140.32 103.03) (end 137.62 100.33) (width 0.35) (layer F.Cu) (net 228))
  (segment (start 140.97 103.03) (end 140.32 103.03) (width 0.35) (layer F.Cu) (net 228))
  (segment (start 93.726 96.647) (end 94.234 97.155) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 93.726 60.96) (end 93.726 96.647) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 95.631 59.055) (end 93.726 60.96) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 94.234 97.155) (end 95.377 97.155) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 95.631 57.888) (end 95.631 59.055) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 92.964 60.452) (end 92.964 96.901) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 94.234 59.182) (end 92.964 60.452) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 94.234 57.888) (end 94.234 59.182) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 92.964 97.663) (end 93.98 98.679) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 92.964 96.901) (end 92.964 97.663) (width 0.35) (layer B.Cu) (net 229))
  (via (at 93.98 98.679) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 229))
  (segment (start 96.266 100.965) (end 93.98 98.679) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 129.235 100.965) (end 96.266 100.965) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 130.175 101.905) (end 129.235 100.965) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 130.175 103.03) (end 130.175 101.905) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 102.948 46.065) (end 101.128 46.065) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 99.568 47.625) (end 98.806 47.625) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 101.128 46.065) (end 99.568 47.625) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 135.895 31.623) (end 136.017 31.745) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 135.895 29.53) (end 135.895 31.623) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 132.715 27.305) (end 136.525 27.305) (width 0.7) (layer F.Cu) (net 233) (tstamp 5BC64E60))
  (segment (start 136.525 27.305) (end 136.525 21.905) (width 0.7) (layer F.Cu) (net 233) (tstamp 5BC64D25))
  (segment (start 136.525 21.905) (end 137.795 21.905) (width 0.7) (layer F.Cu) (net 233) (tstamp 5BC64D2B))
  (segment (start 102.948 42.865) (end 100.523 42.865) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 99.568 41.91) (end 98.806 41.91) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 100.523 42.865) (end 99.568 41.91) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 98.806 40.513) (end 99.441 40.513) (width 0.35) (layer F.Cu) (net 237))
  (segment (start 100.993 42.065) (end 102.948 42.065) (width 0.35) (layer F.Cu) (net 237))
  (segment (start 99.441 40.513) (end 100.993 42.065) (width 0.35) (layer F.Cu) (net 237))
  (segment (start 99.406 39.116) (end 98.806 39.116) (width 0.35) (layer F.Cu) (net 238))
  (segment (start 101.555 41.265) (end 99.406 39.116) (width 0.35) (layer F.Cu) (net 238))
  (segment (start 102.948 41.265) (end 101.555 41.265) (width 0.35) (layer F.Cu) (net 238))
  (segment (start 105.448 37.665) (end 103.251 35.468) (width 0.35) (layer F.Cu) (net 241))
  (segment (start 105.448 38.765) (end 105.448 37.665) (width 0.35) (layer F.Cu) (net 241))
  (segment (start 103.251 35.468) (end 103.251 34.925) (width 0.35) (layer F.Cu) (net 241))
  (segment (start 115.824 53.502) (end 115.824 54.102) (width 0.35) (layer F.Cu) (net 242))
  (segment (start 115.824 52.716) (end 115.824 53.502) (width 0.35) (layer F.Cu) (net 242))
  (segment (start 113.273 50.165) (end 115.824 52.716) (width 0.35) (layer F.Cu) (net 242))
  (segment (start 112.648 50.165) (end 113.273 50.165) (width 0.35) (layer F.Cu) (net 242))
  (segment (start 114.427 53.594) (end 114.427 53.848) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 114.427 53.848) (end 114.427 54.102) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 111.848 51.054) (end 111.887 51.054) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 111.887 51.054) (end 114.427 53.594) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 111.848 50.165) (end 111.848 51.054) (width 0.35) (layer F.Cu) (net 244))
  (segment (start 113.03 53.502) (end 113.03 54.102) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 111.048 51.52) (end 113.03 53.502) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 111.048 50.165) (end 111.048 51.52) (width 0.35) (layer F.Cu) (net 245))
  (segment (start 111.633 53.514) (end 111.633 54.114) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 110.248 52.129) (end 111.633 53.514) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 110.248 50.165) (end 110.248 52.129) (width 0.35) (layer F.Cu) (net 247))
  (segment (start 110.236 53.34) (end 110.236 54.102) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 109.448 52.552) (end 110.236 53.34) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 109.448 50.165) (end 109.448 52.552) (width 0.35) (layer F.Cu) (net 248))
  (segment (start 243.967 67.056) (end 243.967 65.819) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 243.586 67.437) (end 243.967 67.056) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 239.395 67.437) (end 243.586 67.437) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 229.904 64.617) (end 230.505 64.016) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 235.974 64.016) (end 239.395 67.437) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 230.505 64.016) (end 235.974 64.016) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 229.904 65.967) (end 229.904 64.617) (width 0.35) (layer F.Cu) (net 253))
  (segment (start 242.697 63.754) (end 242.697 65.819) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 242.062 63.119) (end 242.697 63.754) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 229.997 63.119) (end 242.062 63.119) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 228.804 64.312) (end 229.997 63.119) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 228.804 65.967) (end 228.804 64.312) (width 0.35) (layer F.Cu) (net 254))
  (segment (start 222.504 51.816) (end 222.504 49.95974) (width 1.40626) (layer F.Cu) (net 258))
  (segment (start 222.504 49.95974) (end 222.504 46.101) (width 1.40626) (layer F.Cu) (net 258))
  (segment (start 222.504 54.167) (end 222.504 51.816) (width 0.7) (layer F.Cu) (net 258))
  (segment (start 232.104 65.967) (end 232.104 67.489) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 230.886 68.707) (end 227.838 68.707) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 227.838 68.707) (end 226.822 67.691) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 232.104 67.489) (end 230.886 68.707) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 226.187 63.754) (end 226.822 64.389) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 226.822 67.691) (end 226.822 64.389) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 217.211 63.754) (end 218.821 63.754) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 218.821 63.754) (end 226.187 63.754) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 217.973 63.754) (end 218.821 63.754) (width 0.35) (layer F.Cu) (net 259))
  (segment (start 228.346 67.818) (end 227.838 67.31) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 231.013 67.326) (end 231.013 67.437) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 230.632 67.818) (end 228.346 67.818) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 231.004 67.317) (end 231.013 67.326) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 231.013 67.437) (end 230.632 67.818) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 231.004 65.967) (end 231.004 67.317) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 217.211 57.089) (end 218.091 57.089) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 227.772 64.262) (end 220.599 57.089) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 227.838 64.262) (end 227.772 64.262) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 220.599 57.089) (end 217.973 57.089) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 227.838 67.31) (end 227.838 64.262) (width 0.35) (layer F.Cu) (net 260))
  (segment (start 215.011 58.039) (end 213.36 58.039) (width 0.35) (layer F.Cu) (net 261))
  (via (at 116.928503 91.12853) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 116.185973 90.386) (end 116.928503 91.12853) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 115.824 90.386) (end 116.185973 90.386) (width 0.35) (layer F.Cu) (net 262))
  (via (at 106.172 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 105.372 90.386) (end 106.172 91.186) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 104.902 90.386) (end 105.372 90.386) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 103.251 93.258472) (end 105.323472 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 105.323472 91.186) (end 106.172 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 103.251 95.885) (end 103.251 93.258472) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 116.928503 91.12853) (end 116.38947 91.12853) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 103.886 96.52) (end 103.251 95.885) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 114.173 96.52) (end 103.886 96.52) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 116.38947 91.12853) (end 114.173 93.345) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 114.173 93.345) (end 114.173 96.52) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 114.173 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 262))
  (via (at 135.382 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 134.582 90.386) (end 135.382 91.186) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 134.239 90.386) (end 134.582 90.386) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 134.533472 91.186) (end 132.842 92.877472) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 135.382 91.186) (end 134.533472 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 132.842 92.877472) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 132.842 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 262))
  (via (at 146.177 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 145.377 90.386) (end 146.177 91.186) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 144.996 90.386) (end 145.377 90.386) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 145.328472 91.186) (end 143.637 92.877472) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 146.177 91.186) (end 145.328472 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 143.637 92.877472) (end 143.637 96.52) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 143.637 96.52) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 143.637 96.52) (end 143.994001 96.877001) (width 0.35) (layer B.Cu) (net 262))
  (via (at 164.592 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 163.792 90.386) (end 164.592 91.186) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 163.28 90.386) (end 163.792 90.386) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 162.052 92.877472) (end 162.052 96.877001) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 163.743472 91.186) (end 162.052 92.877472) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 164.592 91.186) (end 163.743472 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 143.994001 96.877001) (end 162.052 96.877001) (width 0.35) (layer B.Cu) (net 262))
  (via (at 175.387 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 262))
  (segment (start 174.587 90.386) (end 175.387 91.186) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 174.075 90.386) (end 174.587 90.386) (width 0.35) (layer F.Cu) (net 262))
  (segment (start 175.387 91.186) (end 174.498 91.186) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 174.498 91.186) (end 172.847 92.837) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 171.854999 96.877001) (end 172.847 95.885) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 171.577 96.877001) (end 171.854999 96.877001) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 172.847 92.837) (end 172.847 95.885) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 162.052 96.877001) (end 171.577 96.877001) (width 0.35) (layer B.Cu) (net 262))
  (segment (start 115.786 91.986) (end 115.824 91.986) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 114.3 93.472) (end 115.786 91.986) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 112.141 93.472) (end 114.3 93.472) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 110.871 92.202) (end 112.141 93.472) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 110.363 86.233) (end 110.871 86.741) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 110.871 86.741) (end 110.871 92.202) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 110.363 85.447) (end 110.363 86.233) (width 0.35) (layer F.Cu) (net 264))
  (segment (start 168.783 85.447) (end 168.783 91.152713) (width 0.35) (layer F.Cu) (net 265))
  (segment (start 139.573 85.447) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 266))
  (segment (start 139.954 92.964) (end 140.335 93.345) (width 0.35) (layer F.Cu) (net 266))
  (segment (start 139.954 86.614) (end 139.954 92.964) (width 0.35) (layer F.Cu) (net 266))
  (segment (start 140.335 93.345) (end 140.716 93.726) (width 0.35) (layer F.Cu) (net 266))
  (segment (start 139.954 86.614) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 266))
  (segment (start 104.864 91.986) (end 104.902 91.986) (width 0.35) (layer F.Cu) (net 267))
  (segment (start 97.79 85.447) (end 97.79 90.17) (width 0.35) (layer F.Cu) (net 267))
  (segment (start 103.378 93.472) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 267))
  (segment (start 97.79 90.17) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 267))
  (segment (start 103.378 93.472) (end 104.864 91.986) (width 0.35) (layer F.Cu) (net 267))

  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BC646F5) (hatch full 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 172.72 40.386) (xy 172.72 34.29) (xy 168.275 34.29) (xy 168.275 27.10845) (xy 171.45 27.10845)
        (xy 171.45 29.21) (xy 177.165 29.21) (xy 177.165 37.846) (xy 189.23 37.973) (xy 189.23 40.386)
      )
    )
  )
  (zone (net 160) (net_name "/5V PSU /SwE") (layer F.Cu) (tstamp 5BC646F2) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 177.8 37.465) (xy 177.8 26.4795) (xy 179.07 26.4795) (xy 179.07 31.115) (xy 187.325 31.115)
        (xy 187.325 37.465)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (tstamp 5BB8CC5B) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 8.255) (xy 189.23 8.255) (xy 189.23 107.95) (xy 89.535 107.95)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (tstamp 5BB8CC58) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.535 8.255) (xy 189.23 8.255) (xy 189.23 107.95) (xy 89.535 107.95)
      )
    )
  )
  (zone (net 232) (net_name "/3_3V PSU/HC_Plain") (layer F.Cu) (tstamp 5BC64CC5) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.35 30.48) (xy 140.97 30.48) (xy 143.51 27.94) (xy 143.51 22.86) (xy 150.495 22.86)
        (xy 150.495 38.1) (xy 133.35 38.1)
      )
    )
  )
  (zone (net 215) (net_name "/3_3V PSU/MC34063_HC_A") (layer F.Cu) (tstamp 5BC64D0D) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 156.083 13.97) (xy 156.083 37.846) (xy 167.767 37.846) (xy 167.767 22.098) (xy 161.163 22.098)
        (xy 161.163 13.97)
      )
    )
  )
  (zone (net 233) (net_name "/3_3V PSU/HC_Plain_b") (layer F.Cu) (tstamp 5BC64929) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 127.127 26.67) (xy 134.747 26.67) (xy 134.747 38.354) (xy 124.587 38.354) (xy 124.587 26.67)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 112.141 48.641) (xy 104.521 48.641) (xy 104.521 40.259) (xy 112.903 40.259) (xy 112.903 48.641)
      )
    )
  )
)
