(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")

  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 1794)
    (zones 0)
    (modules 261)
    (nets 243)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.35)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 1)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.9)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (user_via 1.4 0.9)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_fffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "../../../Desktop/"))
  )

  (net 0 "")
  (net 1 "Net-(C802-Pad1)")
  (net 2 "Net-(C702-Pad1)")
  (net 3 "Net-(C602-Pad1)")
  (net 4 "Net-(C502-Pad1)")
  (net 5 "Net-(C402-Pad1)")
  (net 6 "Net-(C302-Pad1)")
  (net 7 VCC)
  (net 8 GND)
  (net 9 "Net-(R808-Pad2)")
  (net 10 "Net-(R807-Pad2)")
  (net 11 "Net-(R806-Pad2)")
  (net 12 "Net-(R805-Pad2)")
  (net 13 ~enable_Shiftregister)
  (net 14 "Net-(R804-Pad2)")
  (net 15 "Net-(R803-Pad2)")
  (net 16 "Net-(R802-Pad2)")
  (net 17 "Net-(R801-Pad2)")
  (net 18 "Net-(R701-Pad2)")
  (net 19 "Net-(R702-Pad2)")
  (net 20 "Net-(R703-Pad2)")
  (net 21 "Net-(R704-Pad2)")
  (net 22 "Net-(R705-Pad2)")
  (net 23 "Net-(R706-Pad2)")
  (net 24 "Net-(R707-Pad2)")
  (net 25 "Net-(R708-Pad2)")
  (net 26 "Net-(R608-Pad2)")
  (net 27 "Net-(R607-Pad2)")
  (net 28 "Net-(R606-Pad2)")
  (net 29 "Net-(R605-Pad2)")
  (net 30 "Net-(R604-Pad2)")
  (net 31 "Net-(R603-Pad2)")
  (net 32 "Net-(R602-Pad2)")
  (net 33 "Net-(R601-Pad2)")
  (net 34 "Net-(R501-Pad2)")
  (net 35 "Net-(R502-Pad2)")
  (net 36 "Net-(R503-Pad2)")
  (net 37 "Net-(R504-Pad2)")
  (net 38 "Net-(R505-Pad2)")
  (net 39 "Net-(R506-Pad2)")
  (net 40 "Net-(R507-Pad2)")
  (net 41 "Net-(R508-Pad2)")
  (net 42 "Net-(R408-Pad2)")
  (net 43 "Net-(R407-Pad2)")
  (net 44 "Net-(R406-Pad2)")
  (net 45 "Net-(R405-Pad2)")
  (net 46 "Net-(R404-Pad2)")
  (net 47 "Net-(R403-Pad2)")
  (net 48 "Net-(R402-Pad2)")
  (net 49 "Net-(R401-Pad2)")
  (net 50 "Net-(R301-Pad2)")
  (net 51 "Net-(R302-Pad2)")
  (net 52 "Net-(R303-Pad2)")
  (net 53 "Net-(R304-Pad2)")
  (net 54 "Net-(R305-Pad2)")
  (net 55 "Net-(R306-Pad2)")
  (net 56 "Net-(R307-Pad2)")
  (net 57 "Net-(R308-Pad2)")
  (net 58 /Tubes/sheet5BB3E86D/e)
  (net 59 /Tubes/sheet5BB3E86D/d)
  (net 60 /Tubes/sheet5BB3E86D/g)
  (net 61 /Tubes/sheet5BB3E86D/f)
  (net 62 /Tubes/sheet5BB3E86D/a)
  (net 63 /Tubes/sheet5BB3E86D/c)
  (net 64 /Tubes/sheet5BB3E86D/b)
  (net 65 /Tubes/sheet5BB3E86D/Dot)
  (net 66 /Tubes/sheet5BB3E86C/Dot)
  (net 67 /Tubes/sheet5BB3E86C/b)
  (net 68 /Tubes/sheet5BB3E86C/c)
  (net 69 /Tubes/sheet5BB3E86C/a)
  (net 70 /Tubes/sheet5BB3E86C/f)
  (net 71 /Tubes/sheet5BB3E86C/g)
  (net 72 /Tubes/sheet5BB3E86C/d)
  (net 73 /Tubes/sheet5BB3E86C/e)
  (net 74 /Tubes/sheet5BB3BB93/e)
  (net 75 /Tubes/sheet5BB3BB93/d)
  (net 76 /Tubes/sheet5BB3BB93/g)
  (net 77 /Tubes/sheet5BB3BB93/f)
  (net 78 /Tubes/sheet5BB3BB93/a)
  (net 79 /Tubes/sheet5BB3BB93/c)
  (net 80 /Tubes/sheet5BB3BB93/b)
  (net 81 /Tubes/sheet5BB3BB93/Dot)
  (net 82 /Tubes/sheet5BB36ADE/Dot)
  (net 83 /Tubes/sheet5BB36ADE/b)
  (net 84 /Tubes/sheet5BB36ADE/c)
  (net 85 /Tubes/sheet5BB36ADE/a)
  (net 86 /Tubes/sheet5BB36ADE/f)
  (net 87 /Tubes/sheet5BB36ADE/g)
  (net 88 /Tubes/sheet5BB36ADE/d)
  (net 89 /Tubes/sheet5BB36ADE/e)
  (net 90 /Tubes/sheet5BB32DC8/e)
  (net 91 /Tubes/sheet5BB32DC8/d)
  (net 92 /Tubes/sheet5BB32DC8/g)
  (net 93 /Tubes/sheet5BB32DC8/f)
  (net 94 /Tubes/sheet5BB32DC8/a)
  (net 95 /Tubes/sheet5BB32DC8/c)
  (net 96 /Tubes/sheet5BB32DC8/b)
  (net 97 /Tubes/sheet5BB32DC8/Dot)
  (net 98 /Tubes/IV-9_Tube/Dot)
  (net 99 /Tubes/IV-9_Tube/b)
  (net 100 /Tubes/IV-9_Tube/c)
  (net 101 /Tubes/IV-9_Tube/a)
  (net 102 /Tubes/IV-9_Tube/f)
  (net 103 /Tubes/IV-9_Tube/g)
  (net 104 /Tubes/IV-9_Tube/d)
  (net 105 /Tubes/IV-9_Tube/e)
  (net 106 /Tubes/sheet5BB3E86C/Data_in)
  (net 107 /Tubes/sheet5BB36ADE/Data_in)
  (net 108 /Tubes/sheet5BB3BB93/Data_in)
  (net 109 /Tubes/sheet5BB32DC8/Data_in)
  (net 110 /Tubes/IV-9_Tube/Data_in)
  (net 111 "Net-(R902-Pad2)")
  (net 112 "Net-(R914-Pad2)")
  (net 113 "Net-(R916-Pad2)")
  (net 114 "Net-(R915-Pad2)")
  (net 115 "Net-(R913-Pad2)")
  (net 116 "Net-(R912-Pad2)")
  (net 117 "Net-(R911-Pad2)")
  (net 118 "Net-(R910-Pad2)")
  (net 119 "Net-(R909-Pad2)")
  (net 120 "Net-(R908-Pad2)")
  (net 121 "Net-(R907-Pad2)")
  (net 122 clk)
  (net 123 "Net-(R906-Pad2)")
  (net 124 "Net-(R905-Pad2)")
  (net 125 MISO)
  (net 126 MOSI)
  (net 127 "Net-(R904-Pad2)")
  (net 128 "Net-(R903-Pad2)")
  (net 129 Currentsensing_Tube_6)
  (net 130 Currentsensing_Tube_5)
  (net 131 Currentsensing_Tube_4)
  (net 132 Currentsensing_Tube_3)
  (net 133 Currentsensing_Tube_2)
  (net 134 Currentsensing_Tube_1)
  (net 135 /uC/XTAL2)
  (net 136 /uC/XTAL1)
  (net 137 "Net-(C901-Pad1)")
  (net 138 "Net-(R921-Pad2)")
  (net 139 "Net-(R918-Pad2)")
  (net 140 "Net-(R920-Pad2)")
  (net 141 "Net-(R919-Pad2)")
  (net 142 SCL)
  (net 143 SDA)
  (net 144 "Net-(U1101-Pad4)")
  (net 145 "Net-(U1101-Pad3)")
  (net 146 "Net-(U1101-Pad1)")
  (net 147 +12V)
  (net 148 "Net-(R1201-Pad1)")
  (net 149 "Net-(C1203-Pad1)")
  (net 150 "Net-(R1202-Pad2)")
  (net 151 "Net-(R1302-Pad2)")
  (net 152 "Net-(R1303-Pad1)")
  (net 153 "Net-(C1303-Pad1)")
  (net 154 "/5V PSU /SwE")
  (net 155 "Net-(D1303-Pad1)")
  (net 156 "Net-(Q1301-Pad3)")
  (net 157 "Net-(Q1302-Pad3)")
  (net 158 "Net-(C1306-Pad1)")
  (net 159 "Net-(D1303-Pad2)")
  (net 160 "Net-(D1401-Pad1)")
  (net 161 "Net-(F1401-Pad2)")
  (net 162 /Tubes/IV-9_Tube/Data_out)
  (net 163 reset_Shiftregister)
  (net 164 ~latch_Shiftregister)
  (net 165 "Net-(U503-Pad4)")
  (net 166 "Net-(U803-Pad4)")
  (net 167 "Net-(U703-Pad4)")
  (net 168 "Net-(U303-Pad4)")
  (net 169 "Net-(U603-Pad4)")
  (net 170 "Net-(U403-Pad4)")
  (net 171 Encoder_B)
  (net 172 "Net-(R1501-Pad1)")
  (net 173 "Net-(R1502-Pad1)")
  (net 174 Encoder_A)
  (net 175 Encoder_push)
  (net 176 "Net-(D202-Pad1)")
  (net 177 Dot)
  (net 178 "Net-(D201-Pad1)")
  (net 179 "Net-(D202-Pad2)")
  (net 180 "Net-(D201-Pad2)")
  (net 181 Tube_LED)
  (net 182 Rx)
  (net 183 +3V3)
  (net 184 Tx)
  (net 185 "/3_3V PSU/MC34063_Feedback")
  (net 186 "/3_3V PSU/SwE")
  (net 187 V_Bat)
  (net 188 "/3_3V PSU/MC34063_HC_A")
  (net 189 /uC/~Reset_ISP)
  (net 190 "Net-(R411-Pad2)")
  (net 191 "Net-(R933-Pad2)")
  (net 192 "Net-(R711-Pad2)")
  (net 193 "Net-(R811-Pad2)")
  (net 194 "Net-(R934-Pad2)")
  (net 195 "Net-(R935-Pad2)")
  (net 196 "Net-(R311-Pad2)")
  (net 197 "Net-(R936-Pad2)")
  (net 198 "Net-(R611-Pad2)")
  (net 199 "Net-(R511-Pad2)")
  (net 200 "Net-(R937-Pad2)")
  (net 201 "Net-(Q1201-Pad4)")
  (net 202 "/3_3V PSU/HC_Plain")
  (net 203 "/3_3V PSU/HC_Plain_b")
  (net 204 "Net-(R946-Pad2)")
  (net 205 "Net-(R945-Pad2)")
  (net 206 "Net-(R944-Pad2)")
  (net 207 "Net-(R943-Pad2)")
  (net 208 "Net-(R942-Pad2)")
  (net 209 "Net-(R941-Pad2)")
  (net 210 "Net-(R940-Pad2)")
  (net 211 "Net-(R939-Pad2)")
  (net 212 "Net-(R938-Pad2)")
  (net 213 "Net-(R910-Pad1)")
  (net 214 "Net-(D1603-Pad1)")
  (net 215 "Net-(D1603-Pad2)")
  (net 216 /Tubes/IV-9_Tube/Tube_LED)
  (net 217 "Net-(D801-Pad2)")
  (net 218 "Net-(D401-Pad2)")
  (net 219 "Net-(D701-Pad2)")
  (net 220 "Net-(D601-Pad2)")
  (net 221 "Net-(D301-Pad2)")
  (net 222 "Net-(D501-Pad2)")
  (net 223 "Net-(R903-Pad1)")
  (net 224 "Net-(R1402-Pad2)")
  (net 225 Button_B)
  (net 226 Button_A)
  (net 227 "Net-(R1401-Pad2)")
  (net 228 feedback_Tube_PSU)
  (net 229 enable_Tube_PSU)
  (net 230 "Net-(R916-Pad1)")
  (net 231 "Net-(R1405-Pad2)")
  (net 232 "Net-(SW1401-Pad1)")
  (net 233 Status_LED_a)
  (net 234 "Net-(D1502-Pad1)")
  (net 235 Status_LED_c)
  (net 236 Status_LED_b)
  (net 237 "Net-(D1501-Pad1)")
  (net 238 "Net-(D1501-Pad2)")
  (net 239 "Net-(D1502-Pad2)")
  (net 240 RX)
  (net 241 TX)
  (net 242 "Net-(R902-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net "/3_3V PSU/HC_Plain")
    (add_net "/3_3V PSU/HC_Plain_b")
    (add_net "/3_3V PSU/MC34063_Feedback")
    (add_net "/3_3V PSU/MC34063_HC_A")
    (add_net "/3_3V PSU/SwE")
    (add_net "/5V PSU /SwE")
    (add_net /Tubes/IV-9_Tube/Data_in)
    (add_net /Tubes/IV-9_Tube/Data_out)
    (add_net /Tubes/IV-9_Tube/Dot)
    (add_net /Tubes/IV-9_Tube/Tube_LED)
    (add_net /Tubes/IV-9_Tube/a)
    (add_net /Tubes/IV-9_Tube/b)
    (add_net /Tubes/IV-9_Tube/c)
    (add_net /Tubes/IV-9_Tube/d)
    (add_net /Tubes/IV-9_Tube/e)
    (add_net /Tubes/IV-9_Tube/f)
    (add_net /Tubes/IV-9_Tube/g)
    (add_net /Tubes/sheet5BB32DC8/Data_in)
    (add_net /Tubes/sheet5BB32DC8/Dot)
    (add_net /Tubes/sheet5BB32DC8/a)
    (add_net /Tubes/sheet5BB32DC8/b)
    (add_net /Tubes/sheet5BB32DC8/c)
    (add_net /Tubes/sheet5BB32DC8/d)
    (add_net /Tubes/sheet5BB32DC8/e)
    (add_net /Tubes/sheet5BB32DC8/f)
    (add_net /Tubes/sheet5BB32DC8/g)
    (add_net /Tubes/sheet5BB36ADE/Data_in)
    (add_net /Tubes/sheet5BB36ADE/Dot)
    (add_net /Tubes/sheet5BB36ADE/a)
    (add_net /Tubes/sheet5BB36ADE/b)
    (add_net /Tubes/sheet5BB36ADE/c)
    (add_net /Tubes/sheet5BB36ADE/d)
    (add_net /Tubes/sheet5BB36ADE/e)
    (add_net /Tubes/sheet5BB36ADE/f)
    (add_net /Tubes/sheet5BB36ADE/g)
    (add_net /Tubes/sheet5BB3BB93/Data_in)
    (add_net /Tubes/sheet5BB3BB93/Dot)
    (add_net /Tubes/sheet5BB3BB93/a)
    (add_net /Tubes/sheet5BB3BB93/b)
    (add_net /Tubes/sheet5BB3BB93/c)
    (add_net /Tubes/sheet5BB3BB93/d)
    (add_net /Tubes/sheet5BB3BB93/e)
    (add_net /Tubes/sheet5BB3BB93/f)
    (add_net /Tubes/sheet5BB3BB93/g)
    (add_net /Tubes/sheet5BB3E86C/Data_in)
    (add_net /Tubes/sheet5BB3E86C/Dot)
    (add_net /Tubes/sheet5BB3E86C/a)
    (add_net /Tubes/sheet5BB3E86C/b)
    (add_net /Tubes/sheet5BB3E86C/c)
    (add_net /Tubes/sheet5BB3E86C/d)
    (add_net /Tubes/sheet5BB3E86C/e)
    (add_net /Tubes/sheet5BB3E86C/f)
    (add_net /Tubes/sheet5BB3E86C/g)
    (add_net /Tubes/sheet5BB3E86D/Dot)
    (add_net /Tubes/sheet5BB3E86D/a)
    (add_net /Tubes/sheet5BB3E86D/b)
    (add_net /Tubes/sheet5BB3E86D/c)
    (add_net /Tubes/sheet5BB3E86D/d)
    (add_net /Tubes/sheet5BB3E86D/e)
    (add_net /Tubes/sheet5BB3E86D/f)
    (add_net /Tubes/sheet5BB3E86D/g)
    (add_net /uC/XTAL1)
    (add_net /uC/XTAL2)
    (add_net /uC/~Reset_ISP)
    (add_net Button_A)
    (add_net Button_B)
    (add_net Currentsensing_Tube_1)
    (add_net Currentsensing_Tube_2)
    (add_net Currentsensing_Tube_3)
    (add_net Currentsensing_Tube_4)
    (add_net Currentsensing_Tube_5)
    (add_net Currentsensing_Tube_6)
    (add_net Dot)
    (add_net Encoder_A)
    (add_net Encoder_B)
    (add_net Encoder_push)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1203-Pad1)")
    (add_net "Net-(C1303-Pad1)")
    (add_net "Net-(C1306-Pad1)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C602-Pad1)")
    (add_net "Net-(C702-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C901-Pad1)")
    (add_net "Net-(D1303-Pad1)")
    (add_net "Net-(D1303-Pad2)")
    (add_net "Net-(D1401-Pad1)")
    (add_net "Net-(D1501-Pad1)")
    (add_net "Net-(D1501-Pad2)")
    (add_net "Net-(D1502-Pad1)")
    (add_net "Net-(D1502-Pad2)")
    (add_net "Net-(D1603-Pad1)")
    (add_net "Net-(D1603-Pad2)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad1)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D401-Pad2)")
    (add_net "Net-(D501-Pad2)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D701-Pad2)")
    (add_net "Net-(D801-Pad2)")
    (add_net "Net-(F1401-Pad2)")
    (add_net "Net-(Q1201-Pad4)")
    (add_net "Net-(Q1301-Pad3)")
    (add_net "Net-(Q1302-Pad3)")
    (add_net "Net-(R1201-Pad1)")
    (add_net "Net-(R1202-Pad2)")
    (add_net "Net-(R1302-Pad2)")
    (add_net "Net-(R1303-Pad1)")
    (add_net "Net-(R1401-Pad2)")
    (add_net "Net-(R1402-Pad2)")
    (add_net "Net-(R1405-Pad2)")
    (add_net "Net-(R1501-Pad1)")
    (add_net "Net-(R1502-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad2)")
    (add_net "Net-(R306-Pad2)")
    (add_net "Net-(R307-Pad2)")
    (add_net "Net-(R308-Pad2)")
    (add_net "Net-(R311-Pad2)")
    (add_net "Net-(R401-Pad2)")
    (add_net "Net-(R402-Pad2)")
    (add_net "Net-(R403-Pad2)")
    (add_net "Net-(R404-Pad2)")
    (add_net "Net-(R405-Pad2)")
    (add_net "Net-(R406-Pad2)")
    (add_net "Net-(R407-Pad2)")
    (add_net "Net-(R408-Pad2)")
    (add_net "Net-(R411-Pad2)")
    (add_net "Net-(R501-Pad2)")
    (add_net "Net-(R502-Pad2)")
    (add_net "Net-(R503-Pad2)")
    (add_net "Net-(R504-Pad2)")
    (add_net "Net-(R505-Pad2)")
    (add_net "Net-(R506-Pad2)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R508-Pad2)")
    (add_net "Net-(R511-Pad2)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad2)")
    (add_net "Net-(R605-Pad2)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R607-Pad2)")
    (add_net "Net-(R608-Pad2)")
    (add_net "Net-(R611-Pad2)")
    (add_net "Net-(R701-Pad2)")
    (add_net "Net-(R702-Pad2)")
    (add_net "Net-(R703-Pad2)")
    (add_net "Net-(R704-Pad2)")
    (add_net "Net-(R705-Pad2)")
    (add_net "Net-(R706-Pad2)")
    (add_net "Net-(R707-Pad2)")
    (add_net "Net-(R708-Pad2)")
    (add_net "Net-(R711-Pad2)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad2)")
    (add_net "Net-(R805-Pad2)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R807-Pad2)")
    (add_net "Net-(R808-Pad2)")
    (add_net "Net-(R811-Pad2)")
    (add_net "Net-(R902-Pad1)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad1)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R904-Pad2)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(R907-Pad2)")
    (add_net "Net-(R908-Pad2)")
    (add_net "Net-(R909-Pad2)")
    (add_net "Net-(R910-Pad1)")
    (add_net "Net-(R910-Pad2)")
    (add_net "Net-(R911-Pad2)")
    (add_net "Net-(R912-Pad2)")
    (add_net "Net-(R913-Pad2)")
    (add_net "Net-(R914-Pad2)")
    (add_net "Net-(R915-Pad2)")
    (add_net "Net-(R916-Pad1)")
    (add_net "Net-(R916-Pad2)")
    (add_net "Net-(R918-Pad2)")
    (add_net "Net-(R919-Pad2)")
    (add_net "Net-(R920-Pad2)")
    (add_net "Net-(R921-Pad2)")
    (add_net "Net-(R933-Pad2)")
    (add_net "Net-(R934-Pad2)")
    (add_net "Net-(R935-Pad2)")
    (add_net "Net-(R936-Pad2)")
    (add_net "Net-(R937-Pad2)")
    (add_net "Net-(R938-Pad2)")
    (add_net "Net-(R939-Pad2)")
    (add_net "Net-(R940-Pad2)")
    (add_net "Net-(R941-Pad2)")
    (add_net "Net-(R942-Pad2)")
    (add_net "Net-(R943-Pad2)")
    (add_net "Net-(R944-Pad2)")
    (add_net "Net-(R945-Pad2)")
    (add_net "Net-(R946-Pad2)")
    (add_net "Net-(SW1401-Pad1)")
    (add_net "Net-(U1101-Pad1)")
    (add_net "Net-(U1101-Pad3)")
    (add_net "Net-(U1101-Pad4)")
    (add_net "Net-(U303-Pad4)")
    (add_net "Net-(U403-Pad4)")
    (add_net "Net-(U503-Pad4)")
    (add_net "Net-(U603-Pad4)")
    (add_net "Net-(U703-Pad4)")
    (add_net "Net-(U803-Pad4)")
    (add_net RX)
    (add_net Rx)
    (add_net SCL)
    (add_net SDA)
    (add_net Status_LED_a)
    (add_net Status_LED_b)
    (add_net Status_LED_c)
    (add_net TX)
    (add_net Tube_LED)
    (add_net Tx)
    (add_net VCC)
    (add_net V_Bat)
    (add_net clk)
    (add_net enable_Tube_PSU)
    (add_net feedback_Tube_PSU)
    (add_net reset_Shiftregister)
    (add_net ~enable_Shiftregister)
    (add_net ~latch_Shiftregister)
  )

  (net_class Antenna ""
    (clearance 0.3)
    (trace_width 1.40626)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3ABC)
    (at 105.2322 35.8006 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D21)
    (attr smd)
    (fp_text reference R1603 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 Status_LED_a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC322E)
    (at 122.7455 35.8514 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B465E)
    (attr smd)
    (fp_text reference R1501 (at 0 1.45 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 172 "Net-(R1501-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 171 Encoder_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3AEC)
    (at 126.9238 56.5023 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4B0C4)
    (attr smd)
    (fp_text reference R1509 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(D1502-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5BC97ADC)
    (at 156.2227 10.414 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /5BB48B05/5BC4C86E)
    (fp_text reference J902 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 240 RX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 241 TX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC8A67E)
    (at 69.1642 52.7565 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4B0D2)
    (attr smd)
    (fp_text reference R1507 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 Status_LED_c))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC8A66E)
    (at 64.1858 52.705 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4AE55)
    (attr smd)
    (fp_text reference R1506 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 236 Status_LED_b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BC8618F)
    (at 70.8406 49.0552 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BC4B0BD)
    (attr smd)
    (fp_text reference D1502 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(D1502-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D1502-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BC86179)
    (at 68.4403 49.1187 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BC4AE40)
    (attr smd)
    (fp_text reference D1501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(D1501-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(D1501-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCA0D47)
    (at 66.675 52.9209)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BC4AE39)
    (attr smd)
    (fp_text reference Q1501 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 236 Status_LED_b))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(D1501-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC84F27)
    (at 71.8406 52.9438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BC4B0B6)
    (attr smd)
    (fp_text reference Q1502 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D1502-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 235 Status_LED_c))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB61104) (tstamp 5BC4AC69)
    (at 184.023 8.5344 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB6719E)
    (attr smd)
    (fp_text reference Q1303 (at -2.286 0.127 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(D1303-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC7A14E)
    (at 251.968 27.5463 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BB967B8)
    (attr smd)
    (fp_text reference R1309 (at 0 1.85 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.95 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.15 -1.1) (end -2.15 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.15 -1.1) (end 2.15 1.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.15 1.11) (end -2.15 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.15 1.11) (end 2.15 1.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 1.07) (end 1 1.07) (layer B.SilkS) (width 0.12))
    (fp_line (start 1 -1.07) (end -1 -1.07) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.7 0.7) (thickness 0.105)) (justify mirror))
    )
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 183 +3V3))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 228 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BC08)
    (at 104.139 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BB249C1)
    (attr smd)
    (fp_text reference U301 (at 0 7.366 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 162 /Tubes/IV-9_Tube/Data_out))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC6239E)
    (at 184.3456 2.0142 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB7D616/5BB7F33C)
    (attr smd)
    (fp_text reference C1401 (at 0 4.43 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC623B9)
    (at 87.9018 7.5438 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB7D616/5BB7DD24)
    (attr smd)
    (fp_text reference C1402 (at 0 4.43 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (fp_text user + (at -1.73 -0.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC62317)
    (at 198.0946 1.9507 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BB80A8D)
    (attr smd)
    (fp_text reference C1302 (at 0 4.43 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC622C6)
    (at 191.2366 1.9507 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49533)
    (attr smd)
    (fp_text reference C1202 (at 0 4.43 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5BB5DBAF) (tstamp 5BC3B6F2)
    (at 171.8945 39.878 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5BB7D616/5BB7D6F8)
    (fp_text reference J1401 (at 2.794 -0.507 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.8 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 161 "Net-(F1401-Pad2)"))
  )

  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5BC558B8)
    (at 79.6036 19.8628 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (path /5BB48B05/5BB4F230)
    (fp_text reference J901 (at 1.27 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AVR-ISP-6 (at 1.27 7.41 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 6.85) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 6.85) (end 4.35 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 6.41) (end 3.87 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 6.35) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 6.35) (end -1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 189 /uC/~Reset_ISP))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 MOSI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 clk))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC9B64A)
    (at 193.7886 61.6712 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F47F)
    (attr smd)
    (fp_text reference R1505 (at 0.647 -5.334 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(R1405-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC14464)
    (at 193.7505 71.882 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3C9)
    (attr smd)
    (fp_text reference R1504 (at 0.647 -4.318 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R1501-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCB5CCC)
    (at 193.7505 70.485 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3FA)
    (attr smd)
    (fp_text reference R1503 (at 0.647 -4.826 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R1502-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC3366)
    (at 124.1425 35.8274 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B4628)
    (attr smd)
    (fp_text reference R1502 (at 0 1.45 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 174 Encoder_A))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 173 "Net-(R1502-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC3336)
    (at 125.5395 35.8394 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC36391)
    (attr smd)
    (fp_text reference R1405 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 231 "Net-(R1405-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 175 Encoder_push))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module BatteryHolder:Battery_Holder (layer F.Cu) (tedit 5BC35560) (tstamp 5BCBEDAC)
    (at 104.2543 19.6342 180)
    (path /5BB6494F/5BB6519B)
    (fp_text reference BT1101 (at -9 4.25 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Battery_Cell (at -2.75 -4.25 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.6 -3.5) (end -6.6 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.6 3.5) (end -6.6 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.5 -3.5) (end 6.5 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 3.5) (end 11 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.5 -3.5) (end 10.5 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 3.5) (end 11 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 -3.5) (end 10.5 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.5 -3.5) (end -6.5 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.5 3.5) (end -11 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 3.5) (end -11 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -3.5) (end -6.5 -3.5) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -5 1.6 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 187 V_Bat))
    (pad 1 thru_hole circle (at 5 1.6 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 187 V_Bat))
    (pad 2 thru_hole circle (at 0 -1.6 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 GND))
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC574A7)
    (at 185.7316 15.1257)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB8D2EE/5BB85821)
    (attr smd)
    (fp_text reference RV1301 (at -4.87 1.016 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 151 "Net-(R1302-Pad2)"))
    (pad 2 smd rect (at -2.75 0) (size 2 1.3) (layers F.Cu F.Mask)
      (net 185 "/3_3V PSU/MC34063_Feedback"))
    (pad 1 smd rect (at 2.75 -1.15) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 152 "Net-(R1303-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BC3A49B)
    (at 135.7884 10.9321 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB73C46/5BB4952F)
    (attr smd)
    (fp_text reference D1202 (at 0 2 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC4AEBA)
    (at 214.249 27.8181 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB8D2EE/5BB49532)
    (attr smd)
    (fp_text reference U1301 (at 0 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 185 "/3_3V PSU/MC34063_Feedback"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1303-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 186 "/3_3V PSU/SwE"))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_Vishay_IHLP-6767 (layer F.Cu) (tedit 5990349D) (tstamp 5BC4AF06)
    (at 230.632 34.8361 180)
    (descr "Inductor, Vishay, IHLP series, 17.0mmx17.0mm")
    (tags "inductor vishay ihlp smd")
    (path /5BB8D2EE/59D4542E)
    (attr smd)
    (fp_text reference L1301 (at 0 -9.509 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 10.009 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.3 -8.8) (end -10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.3 8.8) (end 10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 8.8) (end 10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 -8.8) (end -10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.609 8.609) (end 8.609 6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 8.609) (end 8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 6.46) (end -8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.609 -8.609) (end 8.609 -6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -8.609) (end 8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -6.46) (end -8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.509 -8.509) (end -8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start 8.509 8.509) (end 8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 8.509) (end 8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 -8.509) (end -8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 202 "/3_3V PSU/HC_Plain"))
    (pad 1 smd rect (at -8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 188 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Vishay_IHLP-6767.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BCC32F6)
    (at 114.1095 54.8412 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5BB9689B)
    (attr smd)
    (fp_text reference D1304 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 228 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC4AE7E)
    (at 214.134 22.8219 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB81889)
    (attr smd)
    (fp_text reference C1301 (at 1.0915 -1.7145 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC7C948)
    (at 185.392 34.925)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB7D616/5BB7D945)
    (attr smd)
    (fp_text reference D1401 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(D1401-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Fuse Holder:Nano Fuse Holder" (layer F.Cu) (tedit 5BB4B4A4) (tstamp 5BC4C751)
    (at 179.5145 32.512 90)
    (path /5BB7D616/5BB7D87A)
    (fp_text reference F1401 (at -3.25 -3.25 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 0.5 3.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.5 -2.5) (end 5.5 -2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 -2.5) (end 5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 2.5) (end -5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.5 2.5) (end -5.5 -2.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4 0 180) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(D1401-Pad1)"))
    (pad 2 smd rect (at 4 0 180) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(F1401-Pad2)"))
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BCA440F)
    (at 92.869 65.8035 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BB48B05/5BB3C67E)
    (attr smd)
    (fp_text reference SW901 (at -5.034 1.175 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 189 /uC/~Reset_ISP))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 189 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BC665EA)
    (at 92.9005 74.93 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BBCA088/5BC50C98)
    (attr smd)
    (fp_text reference SW1402 (at 0 -4.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R1401-Pad2)"))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R1401-Pad2)"))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BC665D0)
    (at 92.9005 84.0105 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BBCA088/5BC55ACC)
    (attr smd)
    (fp_text reference SW1403 (at 0 -4.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1402-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC32BE)
    (at 99.7585 40.7289 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5BC52E3C)
    (attr smd)
    (fp_text reference C1404 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 226 Button_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC328E)
    (at 99.7705 42.3164 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5BC55AF2)
    (attr smd)
    (fp_text reference C1405 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 225 Button_B))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643F0)
    (at 92.075 90.551 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC52136)
    (attr smd)
    (fp_text reference R1401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R1401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643DF)
    (at 93.472 90.539 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC55ADB)
    (attr smd)
    (fp_text reference R1402 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643CE)
    (at 97.155 71.259 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC52D73)
    (attr smd)
    (fp_text reference R1403 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 Button_A))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R1401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643BD)
    (at 97.155 76.061 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC55AEB)
    (attr smd)
    (fp_text reference R1404 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 Button_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BC55271)
    (at 79.4893 5.2223 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BC3F0BE)
    (attr smd)
    (fp_text reference D904 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5BC359F7) (tstamp 5BC3C5BE)
    (at 96.581 82.915 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BCE9EA1)
    (attr smd)
    (fp_text reference Q203 (at 0 2.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 181 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC7C46C)
    (at 96.381 78.74)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BCF2CFF)
    (attr smd)
    (fp_text reference R203 (at 0 1.45) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 181 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC325E)
    (at 107.6325 27.8264 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CF46)
    (attr smd)
    (fp_text reference R925 (at 3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB40647)
    (at 145.034 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3BB9E/5BB249BA)
    (fp_text reference U602 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B218)
    (at 159.004 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249EB)
    (attr smd)
    (fp_text reference R707 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B248)
    (at 160.401 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F2)
    (attr smd)
    (fp_text reference R706 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B278)
    (at 161.798 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F9)
    (attr smd)
    (fp_text reference R705 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2A8)
    (at 163.195 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249C8)
    (attr smd)
    (fp_text reference R704 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2D8)
    (at 164.592 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249CF)
    (attr smd)
    (fp_text reference R703 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B308)
    (at 165.989 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249D6)
    (attr smd)
    (fp_text reference R702 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B338)
    (at 157.607 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249E4)
    (attr smd)
    (fp_text reference R708 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B368)
    (at 140.97 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249E4)
    (attr smd)
    (fp_text reference R608 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B398)
    (at 142.367 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249EB)
    (attr smd)
    (fp_text reference R607 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3C8)
    (at 143.764 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F2)
    (attr smd)
    (fp_text reference R606 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3F8)
    (at 145.161 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F9)
    (attr smd)
    (fp_text reference R605 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B428)
    (at 146.558 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249C8)
    (attr smd)
    (fp_text reference R604 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D171)
    (at 147.955 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249CF)
    (attr smd)
    (fp_text reference R603 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D0DE)
    (at 149.352 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249D6)
    (attr smd)
    (fp_text reference R602 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4B8)
    (at 128.397 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249E4)
    (attr smd)
    (fp_text reference R508 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4E8)
    (at 129.794 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249EB)
    (attr smd)
    (fp_text reference R507 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B518)
    (at 131.191 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F2)
    (attr smd)
    (fp_text reference R506 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B548)
    (at 132.588 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F9)
    (attr smd)
    (fp_text reference R505 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B578)
    (at 133.985 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249C8)
    (attr smd)
    (fp_text reference R504 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5A8)
    (at 135.382 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249CF)
    (attr smd)
    (fp_text reference R503 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5D8)
    (at 136.779 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249D6)
    (attr smd)
    (fp_text reference R502 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B608)
    (at 111.76 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249E4)
    (attr smd)
    (fp_text reference R408 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B638)
    (at 113.157 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249EB)
    (attr smd)
    (fp_text reference R407 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B668)
    (at 114.554 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F2)
    (attr smd)
    (fp_text reference R406 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B698)
    (at 115.951 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F9)
    (attr smd)
    (fp_text reference R405 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6C8)
    (at 117.348 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249C8)
    (attr smd)
    (fp_text reference R404 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6F8)
    (at 118.745 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249CF)
    (attr smd)
    (fp_text reference R403 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.627 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B728)
    (at 120.142 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249D6)
    (attr smd)
    (fp_text reference R402 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B758)
    (at 99.187 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249E4)
    (attr smd)
    (fp_text reference R308 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B788)
    (at 100.584 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249EB)
    (attr smd)
    (fp_text reference R307 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7B8)
    (at 101.981 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F2)
    (attr smd)
    (fp_text reference R306 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7E8)
    (at 103.378 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F9)
    (attr smd)
    (fp_text reference R305 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B818)
    (at 104.775 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249C8)
    (attr smd)
    (fp_text reference R304 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B848)
    (at 106.172 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249CF)
    (attr smd)
    (fp_text reference R303 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B878)
    (at 107.569 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249D6)
    (attr smd)
    (fp_text reference R302 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8A8)
    (at 178.5747 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249D6)
    (attr smd)
    (fp_text reference R802 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B908)
    (at 177.1777 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249CF)
    (attr smd)
    (fp_text reference R803 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B938)
    (at 175.7807 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249C8)
    (attr smd)
    (fp_text reference R804 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B968)
    (at 174.3837 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F9)
    (attr smd)
    (fp_text reference R805 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B998)
    (at 172.9987 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F2)
    (attr smd)
    (fp_text reference R806 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B9C8)
    (at 171.6017 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249EB)
    (attr smd)
    (fp_text reference R807 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8D8)
    (at 170.1927 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249E4)
    (attr smd)
    (fp_text reference R808 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8544)
    (at 104.902 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB247DF/5BB7D8C2)
    (attr smd)
    (fp_text reference D301 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(D301-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8530)
    (at 115.824 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB32DD3/5BB7D8C2)
    (attr smd)
    (fp_text reference D401 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF851C)
    (at 134.239 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB36AE9/5BB7D8C2)
    (attr smd)
    (fp_text reference D501 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8508)
    (at 144.996 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3BB9E/5BB7D8C2)
    (attr smd)
    (fp_text reference D601 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84F4)
    (at 174.075 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E89F/5BB7D8C2)
    (attr smd)
    (fp_text reference D701 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D701-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84E0)
    (at 163.28 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E878/5BB7D8C2)
    (attr smd)
    (fp_text reference D801 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D801-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B9FF)
    (at 127 84.721 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC38F55)
    (attr smd)
    (fp_text reference R510 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BCC31F4)
    (at 99.9871 37.2315 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BCA1CF3)
    (attr smd)
    (fp_text reference D1603 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D1603-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC31BF)
    (at 106.2355 37.9349 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D07)
    (attr smd)
    (fp_text reference R1609 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D1603-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BC38ABF) (tstamp 5BCC3187)
    (at 102.7082 35.6006 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BCA1CEC)
    (attr smd)
    (fp_text reference Q1601 (at 0 -2.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 -90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 233 Status_LED_a))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C) (tstamp 5BCC313F)
    (at 128.8415 42.1174 270)
    (descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (path /5BB48B05/5BB3A603)
    (attr smd)
    (fp_text reference Y901 (at 0 -2.8 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 0 2.8 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.093333 0) (layer F.Adhes) (width 0.186667))
    (fp_circle (center 0 0) (end 0.213333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.333333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.4 0) (layer F.Adhes) (width 0.1))
    (fp_line (start 3.1 -1.9) (end -3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 1.9) (end 3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.9) (end 3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.9) (end -3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.05 1.8) (end 2.7 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.05 -1.8) (end -3.05 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -1.8) (end -3.05 -1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 0.6) (end -1.5 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -1.4) (end -2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 1.4) (end -2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 1.6) (end -2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 1.6) (end -2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.4) (end 2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -1.4) (end 2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -1.6) (end 2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 -1.6) (end 2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (pad 1 smd rect (at -1.85 0 270) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_5032-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3105)
    (at 111.4425 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC662F3)
    (attr smd)
    (fp_text reference R943 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 233 Status_LED_a))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R943-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC32321) (tstamp 5BCC360C)
    (at 116.3955 36.4744 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B3DE)
    (attr smd)
    (fp_text reference C906 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC1B200) (tstamp 5BCC35DC)
    (at 116.2805 55.6514)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B34B)
    (attr smd)
    (fp_text reference C907 (at 0 -1.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48) (tstamp 5BCC3548)
    (at 116.8395 46.1414 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5BB48B05/5BC060C8)
    (attr smd)
    (fp_text reference U902 (at 0 -7.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega32-16AU (at 0 7.45 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.175 -4.6) (end -6.45 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -5.175 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 -4) (end -4 -5) (layer F.Fab) (width 0.15))
    (fp_line (start -5 5) (end -5 -4) (layer F.Fab) (width 0.15))
    (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.15))
    (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.15))
    (fp_line (start -4 -5) (end 5 -5) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R942-Pad2)"))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R941-Pad2)"))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R940-Pad2)"))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(R939-Pad2)"))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R938-Pad2)"))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R919-Pad2)"))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R907-Pad2)"))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R933-Pad2)"))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R934-Pad2)"))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R935-Pad2)"))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R936-Pad2)"))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(R937-Pad2)"))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C901-Pad1)"))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R946-Pad2)"))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R945-Pad2)"))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R944-Pad2)"))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R903-Pad2)"))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R943-Pad2)"))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R911-Pad2)"))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R912-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R910-Pad2)"))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R909-Pad2)"))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R908-Pad2)"))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R918-Pad2)"))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R921-Pad2)"))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R920-Pad2)"))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R913-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R906-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC34E6)
    (at 118.4275 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5FA00)
    (attr smd)
    (fp_text reference R938 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R938-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC34B6)
    (at 119.8245 56.5404 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F9F9)
    (attr smd)
    (fp_text reference R939 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(R939-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3486)
    (at 121.2215 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D25)
    (attr smd)
    (fp_text reference R940 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R940-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 236 Status_LED_b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3456)
    (at 122.6185 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D1E)
    (attr smd)
    (fp_text reference R941 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 229 enable_Tube_PSU))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R941-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3426)
    (at 124.0155 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC64046)
    (attr smd)
    (fp_text reference R942 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R942-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 Status_LED_c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC33F6)
    (at 106.2475 40.7924)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC685A2)
    (attr smd)
    (fp_text reference R944 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R944-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 Button_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC33C6)
    (at 106.2475 42.1894)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D766)
    (attr smd)
    (fp_text reference R945 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 Button_B))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R945-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3396)
    (at 106.2475 43.5864)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D75F)
    (attr smd)
    (fp_text reference R946 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R946-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 177 Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC5A93D)
    (at 126.9136 19.7739 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D469D9)
    (attr smd)
    (fp_text reference R1203 (at 0.828 3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R1202-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BC4791C)
    (at 241.046 23.0919 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB8D2EE/5BC34D02)
    (attr smd)
    (fp_text reference C1206 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-669_LFPAK_ThermalVias-2 (layer F.Cu) (tedit 59217BD0) (tstamp 5BC4AB42)
    (at 207.518 34.6506 180)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT669 Thermical Vias Power-SO8")
    (path /5BB8D2EE/5BC31987)
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference Q1201 (at 1.085 -5.26 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PHPT60406NY (at 1.085 5.58 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.66 4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.66 4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.855 2.5) (end 1.855 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 2.5) (end 1.855 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -2.5) (end -2.245 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.855 -2.5) (end -2.245 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 1.855 -2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 2.2) (end 1.855 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 3.155 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -1.65) (end -2.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -2.245 -2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -3.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.4) (end -2.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.85) (end -3.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -0.85) (end -3.245 -0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.85) (end -2.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.4) (end -3.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 0.4) (end -3.245 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 2.15) (end -2.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 1.7) (end -3.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 1.7) (end -3.245 1.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.345 -2.6) (end -2.345 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.345 2.4) (end -2.345 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 2.6) (end -1.155 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 -2.6) (end -1.205 -2.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 thru_hole rect (at 4.745 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 4 smd rect (at -2.835 1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(Q1201-Pad4)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 0.445 0 90) (size 4.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 2.645 0 90) (size 4.7 1.55) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.835 0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 202 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.835 -1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 202 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at -2.835 -0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 202 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.895 -0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 -1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 -1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers B.Cu B.Paste B.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BC39110)
    (at 83.8708 5.1588 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E24)
    (attr smd)
    (fp_text reference D902 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BC390F7)
    (at 86.0933 5.1663 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54DD6)
    (attr smd)
    (fp_text reference D903 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 122 clk))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_6.3x6.3_H3 (layer F.Cu) (tedit 5990349C) (tstamp 5BC5A8FD)
    (at 131.2096 9.6139 180)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (path /5BB73C46/5BB49522)
    (attr smd)
    (fp_text reference L1201 (at 0 -4.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 4.45 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0 0) (end 1.91 1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end -1.91 -1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end -3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end -3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end 3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -3.4) (end -3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.4) (end 3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.4) (end 3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.4) (end -3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.3 -3.2) (end 3.3 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -3.2) (end 3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -1.5) (end -3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 3.2) (end -3.3 1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.2) (end -3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 1.5) (end 3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.75 0 180) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 154 "/5V PSU /SwE"))
    (pad 1 smd rect (at -2.75 0 180) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC341FE) (tstamp 5BC4AAE5)
    (at 215.634 32.4231)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/59D455EA)
    (attr smd)
    (fp_text reference C1303 (at 3.81 1.016) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C1303-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMC (layer F.Cu) (tedit 5864295D) (tstamp 5BC4AAA7)
    (at 216.281 38.6171 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (path /5BB8D2EE/5BB49523)
    (attr smd)
    (fp_text reference D1301 (at 0 -4.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VSSC8L45-M3/9AT (at 0 4.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.8 -3.25) (end 3.6 -3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.8 3.25) (end 3.6 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -4.9 3.35) (end -4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 3.35) (end -4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -3.35) (end 4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -3.35) (end 4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 -3.1) (end 3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 3.1) (end -3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -4.8 3.25) (end -4.8 -3.25) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 202 "/3_3V PSU/HC_Plain"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3A2C)
    (at 125.476 56.515 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4AE47)
    (attr smd)
    (fp_text reference R1508 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(D1501-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC39FC)
    (at 106.2475 39.3954)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F7)
    (attr smd)
    (fp_text reference R903 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R903-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(R903-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC39CC)
    (at 127.115 52.8574 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F0)
    (attr smd)
    (fp_text reference R904 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC399C)
    (at 127.115 51.4604 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E9)
    (attr smd)
    (fp_text reference R905 (at 0 9.853 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC396C)
    (at 110.0455 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6FE)
    (attr smd)
    (fp_text reference R902 (at 0 9.853 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(R902-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC477AA)
    (at 246.159 30.5816)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BC3EDF8)
    (attr smd)
    (fp_text reference C1307 (at 0 4.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC393C)
    (at 133.8834 113.7165 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC237F5)
    (attr smd)
    (fp_text reference C504 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC390C)
    (at 135.2804 113.7285 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC237F5)
    (attr smd)
    (fp_text reference C604 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC38DC)
    (at 157.099 97.663 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC237F5)
    (attr smd)
    (fp_text reference C704 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC38AC)
    (at 136.6774 113.7165 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BC237F5)
    (attr smd)
    (fp_text reference C804 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC387C)
    (at 132.4864 113.7165 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC237F5)
    (attr smd)
    (fp_text reference C404 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC384C)
    (at 131.0894 113.7165 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BC237F5)
    (attr smd)
    (fp_text reference C304 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_1206 (layer F.Cu) (tedit 58307BE8) (tstamp 5BC4776F)
    (at 243.6495 35.3441)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BC1CECA)
    (attr smd)
    (fp_text reference L1202 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BLM31KN601SN1L (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.07) (end 1 -1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 1.07) (end -1 1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 188 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC381C)
    (at 106.2475 49.3014)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F151)
    (attr smd)
    (fp_text reference R937 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(R937-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC37EC)
    (at 127.901 102.9335)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC2388D)
    (attr smd)
    (fp_text reference R511 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(R511-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC37BC)
    (at 127.889 101.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC2388D)
    (attr smd)
    (fp_text reference R611 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R611-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC378C)
    (at 106.2475 50.6984)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5CD4F)
    (attr smd)
    (fp_text reference R936 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R936-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC375C)
    (at 98.679 103.251)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC2388D)
    (attr smd)
    (fp_text reference R311 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R311-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC372C)
    (at 106.2475 52.0954)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5AA8D)
    (attr smd)
    (fp_text reference R935 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R935-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC36FC)
    (at 106.2355 53.5044)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC58906)
    (attr smd)
    (fp_text reference R934 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R934-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC36CC)
    (at 157.099 102.997)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC2388D)
    (attr smd)
    (fp_text reference R811 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R811-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC369C)
    (at 157.099 101.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC2388D)
    (attr smd)
    (fp_text reference R711 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R711-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC366C)
    (at 109.9185 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC568B6)
    (attr smd)
    (fp_text reference R933 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R933-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC363C)
    (at 98.691 101.854)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC2388D)
    (attr smd)
    (fp_text reference R411 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R411-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AA70)
    (at 212.664 32.7431)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC25F71)
    (attr smd)
    (fp_text reference R1311 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(Q1201-Pad4)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 186 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AA40)
    (at 218.059 27.9781 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC1FD35)
    (attr smd)
    (fp_text reference R1310 (at 0 -1.65 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 186 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FC6) (tstamp 5BCC3A5C)
    (at 129.2225 47.9044 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BE4C)
    (attr smd)
    (fp_text reference R917 (at 0.9405 -2.159) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 /uC/~Reset_ISP))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3A8C)
    (at 127.115 48.6664 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BA78)
    (attr smd)
    (fp_text reference R913 (at -3.06 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R913-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Encoder:STEC11B01 (layer F.Cu) (tedit 5BC3907B) (tstamp 5BC9B72D)
    (at 94.0435 40.1955 90)
    (path /5BBCA088/5BBCA305)
    (fp_text reference SW1501 (at 1.048 11.564999 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Rotary_Encoder_Switch (at 0 7.119999 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -18) (end 1 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -18) (end 1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -29) (end -1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3 -29) (end 3 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -29) (end 3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -28) (end -3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -11) (end -3 -28) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3.5 -11) (end -3.5 -4) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -11) (end -3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -4) (end 3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -6 -4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 4) (end 6 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4) (end -6 4) (layer F.SilkS) (width 0.15))
    (pad B thru_hole circle (at -2.54 -1.27 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 173 "Net-(R1502-Pad1)"))
    (pad C thru_hole circle (at 0 -1.27 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad A thru_hole circle (at 2.54 -1.27 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 172 "Net-(R1501-Pad1)"))
    (pad S2 thru_hole circle (at 2.54 1.27 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad S1 thru_hole circle (at -2.54 1.27 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 231 "Net-(R1405-Pad2)"))
    (pad "" thru_hole circle (at -5.842 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.842 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB8C91E)
    (at 97.79 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC38F55)
    (attr smd)
    (fp_text reference R310 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(D301-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AF48)
    (at 108.966 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249DD)
    (attr smd)
    (fp_text reference R301 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B068)
    (at 121.539 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249DD)
    (attr smd)
    (fp_text reference R401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC2EA1B) (tstamp 5BC3AF78)
    (at 110.363 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC38F55)
    (attr smd)
    (fp_text reference R410 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B008)
    (at 138.176 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249DD)
    (attr smd)
    (fp_text reference R501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BB02)
    (at 156.21 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC38F55)
    (attr smd)
    (fp_text reference R810 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D801-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AFD8)
    (at 179.9717 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249DD)
    (attr smd)
    (fp_text reference R801 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BA70)
    (at 168.783 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC38F55)
    (attr smd)
    (fp_text reference R710 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D07E)
    (at 150.6855 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249DD)
    (attr smd)
    (fp_text reference R601 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B8ED)
    (at 139.573 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC38F55)
    (attr smd)
    (fp_text reference R610 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B038)
    (at 167.386 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249DD)
    (attr smd)
    (fp_text reference R701 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC3E015)
    (at 155.321 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBD4644)
    (fp_text reference D201 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 178 "Net-(D201-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 180 "Net-(D201-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC23268)
    (at 126.365 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBEEFA5)
    (fp_text reference D202 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 179 "Net-(D202-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 176 "Net-(D202-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2C5E)
    (at 99.7705 43.6499 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE40CE)
    (attr smd)
    (fp_text reference R201 (at 0.012 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 177 Dot))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC23018)
    (at 152.781 81.8515 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBD471C)
    (attr smd)
    (fp_text reference R202 (at 0 -1.397 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 180 "Net-(D201-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5BC3033A) (tstamp 5BC22FD6)
    (at 123.825 81.788 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBEEFB2)
    (attr smd)
    (fp_text reference R204 (at 0 -1.27 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(D202-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22B05)
    (at 155.321 84.852 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBDEA3D)
    (attr smd)
    (fp_text reference Q201 (at 0 2.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 177 Dot))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 178 "Net-(D201-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22AF0)
    (at 126.365 84.82 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBEEFBB)
    (attr smd)
    (fp_text reference Q202 (at 0 2.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(D202-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 177 Dot))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB75445) (tstamp 5BCC2CBE)
    (at 122.7455 29.8584 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46FC)
    (attr smd)
    (fp_text reference C1501 (at -0.115 -3.302 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 171 Encoder_B))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB7544A) (tstamp 5BCC2C8E)
    (at 124.1425 29.8824 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46B9)
    (attr smd)
    (fp_text reference C1502 (at -0.115 -2.921 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 174 Encoder_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BCC2CEE)
    (at 125.5395 29.8704 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0DEE19)
    (attr smd)
    (fp_text reference C1503 (at 0 1.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 175 Encoder_push))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2D1E)
    (at 119.9515 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D785)
    (attr smd)
    (fp_text reference R909 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R909-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BBE7DB5)
    (at 104.9573 94.119204 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB247DF/5BB249BA)
    (fp_text reference U302 (at 7.124204 -4.3733 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EAE)
    (at 107.95 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB247DF/5BB24A0E)
    (attr smd)
    (fp_text reference R309 (at -4.6355 -0.0635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E8E)
    (at 137.16 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB36AE9/5BB24A0E)
    (attr smd)
    (fp_text reference R509 (at -4.7105 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EEE)
    (at 148.03 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3BB9E/5BB24A0E)
    (attr smd)
    (fp_text reference R609 (at -4.6355 -0.0115 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EDE)
    (at 177.165 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E89F/5BB24A0E)
    (attr smd)
    (fp_text reference R809 (at -4.6355 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BC301D8) (tstamp 5BBD6ECE)
    (at 118.745 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB32DD3/5BB24A0E)
    (attr smd)
    (fp_text reference R409 (at -4.647 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E9E)
    (at 166.37 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E878/5BB24A0E)
    (attr smd)
    (fp_text reference R709 (at -4.6355 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD3416)
    (at 112.28 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BBBEA7E)
    (attr smd)
    (fp_text reference C403 (at -0.012 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD33E5)
    (at 113.55 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB26FB6)
    (attr smd)
    (fp_text reference C402 (at 2.044 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF88)
    (at 113.665 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BBB5EFE)
    (attr smd)
    (fp_text reference U403 (at 0 3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U403-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R411-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF6C)
    (at 142.875 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BBB5EFE)
    (attr smd)
    (fp_text reference U603 (at 0 3.2385 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R611-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U603-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB97560)
    (at 102.87 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BBB5EFE)
    (attr smd)
    (fp_text reference U303 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U303-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R311-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEC4)
    (at 172.085 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BBB5EFE)
    (attr smd)
    (fp_text reference U703 (at -0.0635 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R711-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U703-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEA8)
    (at 161.29 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BBB5EFE)
    (attr smd)
    (fp_text reference U803 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U803-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R811-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEE1C)
    (at 132.08 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BBB5EFE)
    (attr smd)
    (fp_text reference U503 (at 0 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(R511-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U503-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC5CB77)
    (at 141.3256 10.3454)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49527)
    (attr smd)
    (fp_text reference C1204 (at 5.4915 1.143 -270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Kippschalter:B12AV (layer F.Cu) (tedit 5BB5DE12) (tstamp 5BC76F0B)
    (at 176.9872 43.3832 180)
    (path /5BB7D616/5BB7EDAF)
    (fp_text reference SW1401 (at -7.8105 -4.826 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_SPDT (at -9.5 5.25 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7 -4) (end 7 1) (layer F.SilkS) (width 0.15))
    (fp_line (start 7 -4) (end -11.75 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -4) (end -11.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 4) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -1.25) (end -21.75 -1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 -1.25) (end -21.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 1.25) (end -11.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start 7 1) (end -0.75 1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.75 1) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (pad "" thru_hole rect (at -5.08 1.27 180) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" thru_hole rect (at -5.08 -1.27 180) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 160 "Net-(D1401-Pad1)"))
    (pad 2 thru_hole circle (at 2.53 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 147 +12V))
    (pad 1 thru_hole circle (at 5.08 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 232 "Net-(SW1401-Pad1)"))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E14) (tstamp 5BB763E2)
    (at 92.583 29.21)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB8682A)
    (fp_text reference MH1401 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E06) (tstamp 5BB7BA9E)
    (at 186.055 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB86916)
    (fp_text reference MH1402 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60F0C) (tstamp 5BC63C85)
    (at 93.472 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868BC)
    (fp_text reference MH1403 (at 0 -3.048 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E19) (tstamp 5BC419C9)
    (at 185.42 29.083)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868ED)
    (fp_text reference MH1404 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC382CF) (tstamp 5BC4AE4E)
    (at 188.3036 7.9502)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB5DF23)
    (attr smd)
    (fp_text reference C1306 (at -1.131 -1.3462) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4) (tstamp 5BC4AE10)
    (at 174.4685 12.446 180)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BB8D2EE/5BB6A6ED)
    (attr smd)
    (fp_text reference D1303 (at -1.3675 1.397) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_2.5VPSU_off_red (at 0 1.7 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -0.8) (end 1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1 0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.65) (end 1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.65) (end 1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.65) (end -1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.65) (end -1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end -0.1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end 0.2 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 -0.2) (end -0.1 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.88) (end 1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -0.88) (end 1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 0.88) (end -1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 0.88) (end -1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(D1303-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB61283) (tstamp 5BC4ADD9)
    (at 191.6818 9.5504)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5CFDD)
    (attr smd)
    (fp_text reference R1304 (at 2.4758 -1.2032 -270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 229 enable_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB612A8) (tstamp 5BC4ADA9)
    (at 191.6938 8.001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5D0B6)
    (attr smd)
    (fp_text reference R1305 (at 2.171 1.651) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AD79)
    (at 171.9453 13.0556 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5A81D)
    (attr smd)
    (fp_text reference R1306 (at -2.401 -5.08 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AD49)
    (at 172.6953 10.5156)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB71DFD)
    (attr smd)
    (fp_text reference R1308 (at -2.401 -3.7465) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(D1303-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AD19)
    (at 170.7617 15.4432)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB57E62)
    (attr smd)
    (fp_text reference R1307 (at -2.601 -4.572) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(Q1302-Pad3)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC7D270)
    (at 188.5282 10.5054)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB59C86)
    (attr smd)
    (fp_text reference Q1301 (at 2.286 0.447 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB610FE) (tstamp 5BC7D234)
    (at 174.4091 15.4432)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB57D85)
    (attr smd)
    (fp_text reference Q1302 (at -2.286 -0.066 90) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BC850 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 185 "/3_3V PSU/MC34063_Feedback"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(Q1302-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC47AEC)
    (at 246.0955 40.2336)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/59D46505)
    (attr smd)
    (fp_text reference C1304 (at 5.6185 0 -270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 188 "/3_3V PSU/MC34063_HC_A"))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC47A60)
    (at 240.3595 43.1546 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB49531)
    (attr smd)
    (fp_text reference C1305 (at 1.9805 -1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 188 "/3_3V PSU/MC34063_HC_A"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC47A20)
    (at 248.7295 35.3441)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5AAD3380)
    (attr smd)
    (fp_text reference D1302 (at 1.425 -1.778) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_2.7V (at 0.889 -2.568) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AC35)
    (at 191.1731 13.9852)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB4952A)
    (attr smd)
    (fp_text reference R1303 (at 3.6855 -7.8105) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BB6113F) (tstamp 5BC4AC05)
    (at 191.1706 16.2687 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB49529)
    (attr smd)
    (fp_text reference R1302 (at -3.1115 0.6985 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 27k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R1302-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 183 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BB611A5) (tstamp 5BC4ABD5)
    (at 209.169 25.9981 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB8D2EE/59D44D00)
    (attr smd)
    (fp_text reference R1301 (at 3.3135 -2.667 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 203 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC5AA9C)
    (at 126.9746 16.2814 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49524)
    (attr smd)
    (fp_text reference C1203 (at 0.8255 1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 83pF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C1203-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BC5AA5E)
    (at 124.6976 11.1379 270)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB73C46/59D454FD)
    (attr smd)
    (fp_text reference D1201 (at -1.397 2.9845 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SB350 (at 0 3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 154 "/5V PSU /SwE"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC5AA27)
    (at 137.8966 18.1979 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB73C46/5BB49521)
    (attr smd)
    (fp_text reference R1201 (at 0 -2.413 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC5A9DF)
    (at 131.2926 17.0434 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB73C46/5BB74814)
    (attr smd)
    (fp_text reference U1201 (at 0 -3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R1201-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 154 "/5V PSU /SwE"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(C1203-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R1202-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R1201-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC5A9A3)
    (at 126.9746 17.8689 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49534)
    (attr smd)
    (fp_text reference C1201 (at -0.496 -2.794 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 147 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BC44171)
    (at 133.5532 9.6647 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB47F9D)
    (attr smd)
    (fp_text reference C1205 (at 0 1.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value C (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC5A973)
    (at 135.0391 21.2369 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D46945)
    (attr smd)
    (fp_text reference R1202 (at 0.254 -3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R1202-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FBD) (tstamp 5BCC30D2)
    (at 106.1085 27.8384 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CFEE)
    (attr smd)
    (fp_text reference R926 (at 2.667 -0.254 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.294 -0.762 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC30A2)
    (at 115.7605 27.8384 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB6494F/5BB64C0D)
    (attr smd)
    (fp_text reference C1101 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BCC305A)
    (at 112.2045 29.8374 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB6494F/5BB64ADA)
    (attr smd)
    (fp_text reference U1101 (at -4.445 -0.0635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS3231MZ (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 187 V_Bat))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U1101-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U1101-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U1101-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC301E)
    (at 114.1095 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60B72)
    (attr smd)
    (fp_text reference R919 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R919-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 228 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2FEE)
    (at 128.3335 35.8648 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63D55)
    (attr smd)
    (fp_text reference R920 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 182 Rx))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R920-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2FBE)
    (at 122.7455 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60C0B)
    (attr smd)
    (fp_text reference R918 (at -3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 Encoder_B))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R918-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2F8E)
    (at 126.9365 35.8648 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CF7)
    (attr smd)
    (fp_text reference R921 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R921-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 184 Tx))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC2F5E)
    (at 105.4735 47.1544 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A35B)
    (attr smd)
    (fp_text reference C901 (at 3.187 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C901-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19AE4) (tstamp 5BCC2F2E)
    (at 126.492 46.5709 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A26C)
    (attr smd)
    (fp_text reference C902 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC2EFE)
    (at 106.8705 45.7454 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB39CC9)
    (attr smd)
    (fp_text reference C903 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC3DD04)
    (at 124.1298 21.3113 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A69F)
    (attr smd)
    (fp_text reference C904 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19B2A) (tstamp 5BB891B4)
    (at 80.5815 6.1334 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A72A)
    (attr smd)
    (fp_text reference C905 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BB397FA)
    (at 81.7118 5.2223 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E76)
    (attr smd)
    (fp_text reference D901 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC33ABB) (tstamp 5BCC2ECE)
    (at 127.115 50.0634 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E2)
    (attr smd)
    (fp_text reference R906 (at -3.2505 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R906-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2E9E)
    (at 111.3155 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC50B36)
    (attr smd)
    (fp_text reference R907 (at -3.1235 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R907-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2E6E)
    (at 121.3485 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D7AF)
    (attr smd)
    (fp_text reference R908 (at -3.1235 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R908-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2E3E)
    (at 118.5545 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D75D)
    (attr smd)
    (fp_text reference R910 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(R910-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R910-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2E0E)
    (at 112.8515 35.8394 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D737)
    (attr smd)
    (fp_text reference R911 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R911-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2DDE)
    (at 114.2365 35.8394 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D711)
    (attr smd)
    (fp_text reference R912 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R912-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2DAE)
    (at 124.1425 35.8514 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E7E0)
    (attr smd)
    (fp_text reference R915 (at 0.0254 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 174 Encoder_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC1B239) (tstamp 5BCC2D7E)
    (at 112.7125 56.5284 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB4E3C2)
    (attr smd)
    (fp_text reference R916 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(R916-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2D4E)
    (at 125.5395 35.8528 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E361)
    (attr smd)
    (fp_text reference R914 (at -3.048 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 Encoder_push))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B188)
    (at 175.259 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BB249C1)
    (attr smd)
    (fp_text reference U801 (at -0.001 7.62 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B5BB)
    (at 142.99 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB26FB6)
    (attr smd)
    (fp_text reference C602 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B110)
    (at 162.559 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BB249C1)
    (attr smd)
    (fp_text reference U701 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B4CB)
    (at 102.87 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB26FB6)
    (attr smd)
    (fp_text reference C302 (at 2.159 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B49B)
    (at 101.485 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BBBEA7E)
    (attr smd)
    (fp_text reference C303 (at -0.012 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608EF) (tstamp 5BC3B0C8)
    (at 123.444 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2618D)
    (attr smd)
    (fp_text reference C401 (at -0.242 -1.3335 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60CBD) (tstamp 5BC3B098)
    (at 140.474 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2618D)
    (attr smd)
    (fp_text reference C501 (at -0.242 -1.2065 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B3DB)
    (at 132.195 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB26FB6)
    (attr smd)
    (fp_text reference C502 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA2D)
    (at 130.695 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BBBEA7E)
    (attr smd)
    (fp_text reference C503 (at 0.0515 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60E26) (tstamp 5BC3B1E8)
    (at 152.781 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2618D)
    (attr smd)
    (fp_text reference C601 (at -0.3055 -1.2065 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABB6)
    (at 141.49 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BBBEA7E)
    (attr smd)
    (fp_text reference C603 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DA1) (tstamp 5BC3BA58)
    (at 169.672 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2618D)
    (attr smd)
    (fp_text reference C701 (at -0.242 -1.27 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD8FE6)
    (at 161.29 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB26FB6)
    (attr smd)
    (fp_text reference C702 (at 2.159 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA96)
    (at 159.905 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BBBEA7E)
    (attr smd)
    (fp_text reference C703 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DE8) (tstamp 5BC3BA28)
    (at 181.991 79.629 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2618D)
    (attr smd)
    (fp_text reference C801 (at -0.3055 -1.27 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608D4) (tstamp 5BC3B9F8)
    (at 111.264 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2618D)
    (attr smd)
    (fp_text reference C301 (at -0.369 -1.27) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABE6)
    (at 171.97 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB26FB6)
    (attr smd)
    (fp_text reference C802 (at 2.044 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39C36)
    (at 170.7 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BBBEA7E)
    (attr smd)
    (fp_text reference C803 (at 0 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB90)
    (at 116.714 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BB249C1)
    (attr smd)
    (fp_text reference U401 (at 0.763 7.493 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB18)
    (at 133.349 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BB249C1)
    (attr smd)
    (fp_text reference U501 (at -0.0645 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BAA0)
    (at 146.049 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BB249C1)
    (attr smd)
    (fp_text reference U601 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB29692)
    (at 115.824 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB32DD3/5BB249BA)
    (fp_text reference U402 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E57)
    (at 134.239 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB36AE9/5BB249BA)
    (fp_text reference U502 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E2D)
    (at 163.449 94.09267 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E878/5BB249BA)
    (fp_text reference U702 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E18)
    (at 174.244 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E89F/5BB249BA)
    (fp_text reference U802 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text 9-24VDC (at 100.838 10.16 180) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "IV-9 Clock  Max Nowka  10.2018 V1.0 " (at 114.173 108.331) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )

  (segment (start 172.72 95.25) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 173.99 95.25) (end 173.99 94.359) (width 0.35) (layer F.Cu) (net 1) (status 20))
  (segment (start 173.99 97.63) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 176.765 97.63) (end 177.165 97.23) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 173.99 97.63) (end 176.765 97.63) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 165.97 97.63) (end 166.37 97.23) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 163.195 97.63) (end 165.97 97.63) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 162.04 95.25) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 163.195 95.25) (end 163.195 94.34667) (width 0.35) (layer F.Cu) (net 2) (status 20))
  (segment (start 163.195 97.63) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 144.94 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 143.74 95.25) (end 144.78 95.25) (width 0.35) (layer F.Cu) (net 3) (status 10))
  (segment (start 144.78 95.25) (end 144.78 97.63) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 147.63 97.63) (end 148.03 97.23) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 94.359) (end 145.034 94.105) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 95.25) (end 144.78 94.359) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 133.985 97.63) (end 136.365 97.63) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.84 97.155) (end 137.16 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.365 97.63) (end 136.84 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 133.985 94.359) (end 134.239 94.105) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 132.945 95.25) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 133.985 95.25) (end 133.985 94.359) (width 0.35) (layer F.Cu) (net 4) (status 20))
  (segment (start 133.985 97.63) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 118.27 97.63) (end 118.745 97.155) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 115.57 97.63) (end 118.27 97.63) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 114.3 95.25) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 97.63) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 94.359) (end 115.824 94.105) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 115.57 95.25) (end 115.57 94.359) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 107.55 97.63) (end 107.95 97.23) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 97.63) (end 107.55 97.63) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 94.359) (end 105.029 94.105) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 103.62 95.25) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 104.775 95.25) (end 104.775 94.359) (width 0.35) (layer F.Cu) (net 6) (status 20))
  (segment (start 104.775 97.63) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 123.825 80.391) (end 126.365 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 157.861 80.391) (end 167.005 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 171.45 104.775) (end 171.45 106.299) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 122.555 80.391) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 139.573 83.947) (end 139.573 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 127 83.971) (end 127 83.439) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.934 78.74) (end 106.934 79.87137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC62))
  (segment (start 106.934 79.87137) (end 108.966 81.90337) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC6E))
  (segment (start 108.966 81.90337) (end 110.363 83.30037) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC71))
  (segment (start 136.144 77.597) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.144 79.918) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (via (at 157.861 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 138.049 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 167.005 80.391) (end 166.913 80.391) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.347) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.913 80.391) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 127 83.439) (end 127 83.312) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.37 80.934) (end 165.354 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 113.03 106.68) (end 113.03 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 110.514 80.391) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC9E))
  (segment (start 113.03 104.775) (end 113.03 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 150.749 80.391) (end 149.606 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA1))
  (segment (start 160.655 104.775) (end 160.655 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 119.634 77.417) (end 119.634 79.756) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA7))
  (segment (start 150.749 80.391) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAA))
  (segment (start 120.089 76.962) (end 119.634 77.417) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAD))
  (segment (start 123.444 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB0))
  (segment (start 149.606 80.391) (end 148.844 79.629) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB3))
  (segment (start 107.514 76.962) (end 106.934 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB6))
  (segment (start 171.45 103.03) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 179.959 80.391) (end 178.713 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB9))
  (segment (start 178.713 80.391) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBC))
  (segment (start 179.959 76.962) (end 178.634 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBF) (status 10))
  (segment (start 178.054 77.542) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC2))
  (segment (start 121.414 76.962) (end 120.089 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC5))
  (segment (start 120.269 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC8))
  (segment (start 139.724 80.391) (end 138.049 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCB))
  (segment (start 108.839 76.962) (end 107.514 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCE) (status 10))
  (segment (start 165.354 79.502) (end 165.354 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD1))
  (segment (start 102.235 105.41) (end 102.235 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 106.934 77.542) (end 106.934 78.74) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD4))
  (segment (start 102.235 106.68) (end 102.235 105.41) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.844 79.629) (end 148.844 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCDA))
  (segment (start 148.844 77.542) (end 149.424 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCE0))
  (segment (start 102.235 104.775) (end 102.235 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 120.904 80.391) (end 122.555 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCEC))
  (segment (start 136.779 76.962) (end 138.049 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCEF) (status 20))
  (segment (start 171.45 106.68) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 108.839 80.137) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCF5))
  (segment (start 122.555 80.391) (end 122.174 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCF8))
  (segment (start 149.424 76.962) (end 150.749 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCFB))
  (segment (start 131.445 106.68) (end 131.445 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 126.365 80.391) (end 128.27 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD01))
  (segment (start 108.585 80.391) (end 120.904 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD07))
  (segment (start 178.054 79.732) (end 178.459 80.137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD0A) (status 20))
  (segment (start 181.991 80.391) (end 179.959 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD1F))
  (segment (start 165.354 77.542) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD31))
  (segment (start 150.749 80.391) (end 151.88037 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD94))
  (via (at 179.959 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1ED))
  (via (at 150.749 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F0))
  (via (at 171.45 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 160.655 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 142.24 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 131.445 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 102.235 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 113.03 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 167.005 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F3))
  (via (at 108.585 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F6))
  (via (at 121.412 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1FC))
  (segment (start 167.259 80.137) (end 167.005 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C22C))
  (segment (start 178.634 76.962) (end 178.054 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C232))
  (segment (start 131.445 104.775) (end 131.445 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 160.655 106.68) (end 160.655 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 167.005 80.391) (end 168.922 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23B))
  (segment (start 142.24 106.68) (end 142.24 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 136.779 76.962) (end 136.144 77.597) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23E))
  (segment (start 119.634 79.756) (end 120.269 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C241))
  (segment (start 167.259 76.962) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C244) (status 10))
  (segment (start 152.654 80.518) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24A))
  (segment (start 142.24 104.775) (end 142.24 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 110.363 83.347) (end 110.363 83.947) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24D))
  (segment (start 157.861 81.696) (end 156.21 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 165.354 79.918) (end 165.354 79.502) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.947) (end 168.783 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 128.651 81.661) (end 127 83.312) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 128.651 80.391) (end 128.651 81.661) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 151.88037 80.391) (end 152.781 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 128.27 80.391) (end 128.651 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 139.573 83.347) (end 139.065 82.839) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 110.363 83.30037) (end 110.363 83.347) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C277))
  (segment (start 156.21 83.947) (end 156.21 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 152.781 80.391) (end 157.861 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 157.861 80.391) (end 157.861 81.696) (width 0.35) (layer F.Cu) (net 7))
  (via (at 128.651 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 108.46963 80.391) (end 107.96163 80.899) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C280))
  (segment (start 179.971 80.379) (end 179.959 80.391) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 177.927 106.299) (end 171.45 106.299) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 138.049 80.391) (end 137.449001 80.990999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.449001 81.152999) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.585 80.391) (end 108.46963 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C28C))
  (segment (start 181.991 80.379) (end 179.971 80.379) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.414 81.188) (end 136.144 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.573 83.347) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 178.562 106.299) (end 177.927 106.299) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 137.449001 80.990999) (end 137.449001 81.152999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 123.825 80.946) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 80.438) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 81.038) (end 123.825 80.438) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7645 80.4545) (end 152.781 80.4545) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7175 80.5015) (end 152.7645 80.4545) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.781 80.4545) (end 152.781 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7175 81.1015) (end 152.7175 80.5015) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 108.585 80.391) (end 99.441 80.391) (width 0.35) (layer B.Cu) (net 7))
  (via (at 99.8855 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 97.79 83.947) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 83.058) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 93.46 91.301) (end 93.472 91.289) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 92.075 91.301) (end 93.46 91.301) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 98.73087 82.677) (end 98.171 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.8855 81.52237) (end 98.73087 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.8855 80.391) (end 99.8855 81.52237) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 83.058) (end 97.79 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 82.677) (end 98.171 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 94.742 91.289) (end 93.472 91.289) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 95.274 91.289) (end 94.742 91.289) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 96.52 83.058) (end 96.52 90.043) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 96.52 90.043) (end 95.274 91.289) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 96.901 82.677) (end 96.52 83.058) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 82.677) (end 96.901 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 194.4765 69.088) (end 194.4765 70.461) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 113.4745 28.5884) (end 114.6175 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D17))
  (segment (start 112.8395 28.5884) (end 113.4745 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D1A))
  (segment (start 108.4325 27.0764) (end 108.6865 27.3304) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D1D))
  (segment (start 109.928498 28.5884) (end 108.6865 27.346402) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D20))
  (segment (start 107.8325 27.0764) (end 107.9595 27.2034) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3CED))
  (segment (start 194.4765 70.461) (end 194.5005 70.485) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.6325 27.0764) (end 107.8325 27.0764) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D29))
  (segment (start 108.6865 27.346402) (end 108.6865 27.3304) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D32))
  (segment (start 113.4745 28.5884) (end 109.928498 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D35))
  (segment (start 107.6205 27.0884) (end 107.6325 27.0764) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D38))
  (segment (start 106.1085 27.0884) (end 107.6205 27.0884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D3B))
  (segment (start 194.5005 69.596) (end 194.5005 70.231) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.8395 28.2624) (end 112.8395 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D3E))
  (segment (start 113.1655 28.5884) (end 112.8395 28.2624) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3C5D))
  (segment (start 194.5005 69.596) (end 194.5245 69.572) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.8395 28.2624) (end 112.8395 27.1374) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3C0C))
  (segment (start 115.7605 28.5884) (end 114.6175 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3C48))
  (segment (start 114.6175 28.5884) (end 113.1655 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3E9A))
  (segment (start 194.5005 70.485) (end 194.5005 71.882) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 107.6325 27.0764) (end 108.4325 27.0764) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D08))
  (segment (start 194.5005 71.755) (end 194.5005 70.231) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 126.492 47.3209) (end 126.504 47.3329) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D41))
  (segment (start 116.0145 51.8664) (end 116.0395 51.8414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D44))
  (segment (start 115.5305 54.9264) (end 116.0395 54.4174) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D47))
  (segment (start 115.5305 55.6514) (end 115.5305 54.9264) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D4A))
  (segment (start 116.8395 39.3414) (end 116.8395 40.4414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D4D))
  (segment (start 116.8395 37.6204) (end 116.8395 39.3414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D50))
  (segment (start 117.1455 37.3144) (end 116.8395 37.6204) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D53))
  (segment (start 117.1455 36.4744) (end 117.1455 37.3144) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D56))
  (segment (start 125.3875 46.9414) (end 123.6395 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D59))
  (segment (start 123.6395 46.9414) (end 122.5395 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D5C))
  (segment (start 116.0395 52.9414) (end 116.0395 51.8414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D5F))
  (segment (start 116.0395 54.4174) (end 116.0395 52.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D62))
  (segment (start 116.1135 46.9414) (end 116.0395 47.0154) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D65))
  (segment (start 118.8085 46.9414) (end 116.1135 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D68))
  (segment (start 111.1395 45.3414) (end 115.9105 45.3414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D6B))
  (segment (start 116.0395 45.4704) (end 115.9105 45.3414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D6E))
  (segment (start 116.0395 51.8414) (end 116.0395 47.5234) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D71))
  (segment (start 116.0395 47.5234) (end 116.0395 47.0154) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D74))
  (segment (start 115.9105 45.3414) (end 115.9735 45.3414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D77))
  (segment (start 116.8395 40.4414) (end 116.8395 44.4754) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D7A))
  (segment (start 125.767 47.3209) (end 125.3875 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D7D))
  (segment (start 126.492 47.3209) (end 125.767 47.3209) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D80))
  (segment (start 116.0395 45.9994) (end 116.0395 45.2754) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D83))
  (segment (start 115.9735 45.3414) (end 116.3315 44.9834) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D86))
  (segment (start 116.0395 47.5234) (end 116.0395 45.9994) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D89))
  (segment (start 116.0395 45.9994) (end 116.0395 45.4704) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D8C))
  (segment (start 111.1395 45.3414) (end 108.2445 45.3414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D8F))
  (segment (start 107.8985 44.9954) (end 106.8705 44.9954) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D92))
  (segment (start 108.2445 45.3414) (end 107.8985 44.9954) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D95))
  (segment (start 116.0395 45.2754) (end 116.3315 44.9834) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D98))
  (segment (start 116.3315 44.9834) (end 116.8395 44.4754) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D9B))
  (segment (start 122.5395 46.9414) (end 120.5865 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3D9E))
  (segment (start 120.5865 46.9414) (end 118.8085 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DA1))
  (segment (start 129.056 47.3209) (end 129.2225 47.1544) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DA4))
  (segment (start 126.492 47.3209) (end 129.056 47.3209) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DA7))
  (via (at 80.1878 9.5123) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 80.1363 9.4608) (end 80.1878 9.5123) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 78.3463 9.4608) (end 80.1363 9.4608) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 115.7605 31.7239) (end 117.1455 33.1089) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DAA))
  (segment (start 115.7605 28.5884) (end 115.7605 31.7239) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DAD))
  (segment (start 117.1455 36.4744) (end 117.1455 33.1089) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3DB0))
  (segment (start 138.6256 10.3454) (end 137.6756 10.3454) (width 0.35) (layer F.Cu) (net 7))
  (via (at 180.2384 102.362) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 180.2384 106.3244) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 180.2384 102.362) (end 180.2384 106.3244) (width 0.7) (layer F.Cu) (net 7))
  (segment (start 171.4754 106.3244) (end 171.45 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 180.2384 106.3244) (end 171.4754 106.3244) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 171.45 106.299) (end 160.655 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 160.655 106.299) (end 142.24 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 142.24 106.299) (end 131.445 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 131.445 106.299) (end 113.03 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 113.03 106.299) (end 102.235 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 97.471599) (end 181.7116 102.362) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 181.7116 102.362) (end 180.2384 102.362) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 80.3656) (end 186.602001 97.471599) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 50.158799) (end 186.602001 80.3656) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.576601 80.391) (end 179.959 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 80.3656) (end 186.576601 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 179.959 80.391) (end 167.005 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 167.005 80.391) (end 150.749 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 150.749 80.391) (end 138.049 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 138.049 80.391) (end 128.651 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 128.651 80.391) (end 121.412 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 121.412 80.391) (end 108.585 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 107.45363 80.391) (end 99.8855 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 108.585 80.391) (end 107.45363 80.391) (width 0.7) (layer B.Cu) (net 7))
  (via (at 135.8392 6.8961) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 176.276 26.6192) (end 186.5884 36.9316) (width 0.7) (layer B.Cu) (net 7))
  (via (at 186.5884 44.8056) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 186.5884 36.9316) (end 186.5884 44.8056) (width 0.7) (layer B.Cu) (net 7))
  (via (at 186.602001 50.158799) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 186.5884 50.145198) (end 186.602001 50.158799) (width 0.7) (layer F.Cu) (net 7))
  (segment (start 186.5884 44.8056) (end 186.5884 50.145198) (width 0.7) (layer F.Cu) (net 7))
  (segment (start 137.3632 26.6192) (end 176.276 26.6192) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 137.3632 26.6192) (end 134.9756 26.6192) (width 0.7) (layer B.Cu) (net 7))
  (via (at 128.6891 26.0096) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BCC3B4F))
  (segment (start 134.9248 26.67) (end 134.9756 26.6192) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 135.7884 9.1821) (end 135.7884 6.9469) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 79.4893 8.8138) (end 80.1878 9.5123) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 130.3655 44.6659) (end 130.3655 46.5074) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BCC3B7C))
  (segment (start 138.6256 11.4954) (end 138.6256 10.3454) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 140.1826 13.0524) (end 138.6256 11.4954) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 138.05112 16.57488) (end 139.8016 16.57488) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 140.1826 16.19388) (end 140.1826 13.0524) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.8016 16.57488) (end 140.1826 16.19388) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 135.0391 19.5869) (end 138.05112 16.57488) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 135.0391 20.2869) (end 135.0391 19.5869) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 116.4855 28.5884) (end 116.4989 28.575) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BEE))
  (segment (start 115.7605 28.5884) (end 116.4855 28.5884) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3CA8))
  (segment (start 126.1237 28.575) (end 128.6891 26.0096) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3B1F))
  (segment (start 116.4989 28.575) (end 126.1237 28.575) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3B28))
  (segment (start 79.6036 16.4338) (end 79.6036 17.3228) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 79.6036 11.2903) (end 79.6036 16.4338) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 80.1878 10.7061) (end 79.6036 11.2903) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 80.1878 9.5123) (end 80.1878 10.7061) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 125.476 54.705898) (end 125.476 55.765) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3B9D))
  (segment (start 117.711502 46.9414) (end 125.476 54.705898) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BA0))
  (segment (start 116.1135 46.9414) (end 117.711502 46.9414) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BAF))
  (segment (start 126.9111 55.765) (end 126.9238 55.7523) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BA6))
  (segment (start 125.476 55.765) (end 126.9111 55.765) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BBB))
  (segment (start 106.9855 37.9349) (end 108.585 37.9349) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3B6D))
  (segment (start 108.585 37.9349) (end 113.2586 42.6085) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BD0))
  (segment (start 113.2586 42.6085) (end 113.4999 42.6085) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC3BCA))
  (segment (start 133.5405 8.152) (end 133.5405 6.8961) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 133.5532 8.1647) (end 133.5405 8.152) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 133.5532 8.9147) (end 133.5532 8.1647) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 143.1163 26.3525) (end 130.937 26.3525) (width 0.7) (layer B.Cu) (net 7) (tstamp 5BCC3B55))
  (segment (start 145.415 26.3525) (end 143.1163 26.3525) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 112.014 76.962) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE3) (status 30))
  (segment (start 108.839 78.232) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC95) (status 30))
  (segment (start 112.014 80.137) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD3A) (status 30))
  (segment (start 141.224 79.883) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC98) (status 30))
  (segment (start 138.049 78.232) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC92) (status 30))
  (segment (start 141.224 79.883) (end 141.224 78.867) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD79) (status 10))
  (segment (start 112.014 79.883) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA6) (status 10))
  (segment (start 167.259 78.232) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD28) (status 30))
  (segment (start 170.434 78.232) (end 170.434 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE9) (status 30))
  (segment (start 157.859 78.232) (end 157.859 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA3) (status 30))
  (segment (start 128.649 76.962) (end 128.649 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD1C) (status 30))
  (segment (start 141.224 80.137) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDF7) (status 30))
  (segment (start 114.3 97.63) (end 113.03 97.63) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 112.014 80.137) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9A) (status 10))
  (segment (start 141.224 77.597) (end 141.224 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD34) (status 20))
  (segment (start 141.224 78.867) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCFE) (status 20))
  (segment (start 216.384 30.7481) (end 216.154 30.5181) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFE9))
  (segment (start 216.384 32.4231) (end 216.384 30.7481) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFEC))
  (via (at 218.059 30.5181) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC4B001))
  (segment (start 216.154 30.5181) (end 218.059 30.5181) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFEF))
  (segment (start 218.059 28.9281) (end 218.059 30.5181) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFF2))
  (segment (start 116.8395 55.5764) (end 116.7645 55.6514) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DD1))
  (segment (start 117.0305 54.6354) (end 117.0305 55.6514) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DD4))
  (segment (start 116.8395 54.4444) (end 117.0305 54.6354) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DD7))
  (segment (start 116.8395 51.8414) (end 116.8395 54.4444) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DE0))
  (segment (start 116.0395 37.4784) (end 116.0395 39.3414) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DE3))
  (segment (start 116.0395 39.3414) (end 116.0395 40.4414) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DE6))
  (segment (start 115.7605 37.1994) (end 116.0395 37.4784) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DE9))
  (segment (start 115.7605 36.4744) (end 115.7605 37.1994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DEC))
  (segment (start 126.492 45.8209) (end 125.6545 45.8209) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DF2))
  (segment (start 125.334 46.1414) (end 122.5395 46.1414) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DF5))
  (segment (start 125.6545 45.8209) (end 125.334 46.1414) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DF8))
  (segment (start 80.5815 5.3834) (end 80.5815 3.4812) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 105.5645 46.4954) (end 105.4735 46.4044) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DFB))
  (segment (start 106.8705 46.4954) (end 105.5645 46.4954) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3DFE))
  (segment (start 131.0894 114.4665) (end 132.4864 114.4665) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E01))
  (segment (start 132.4864 114.4665) (end 133.8834 114.4665) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3BF1))
  (segment (start 135.2684 114.4665) (end 135.2804 114.4785) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3C24))
  (segment (start 133.8834 114.4665) (end 135.2684 114.4665) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3C2A))
  (segment (start 179.959 78.232) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD61))
  (segment (start 181.991 78.891) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC9B))
  (segment (start 170.422 80.391) (end 170.422 79.006) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8E))
  (segment (start 170.422 79.006) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD10))
  (segment (start 170.434 78.994) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9D))
  (segment (start 170.434 80.137) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD55))
  (segment (start 141.224 80.391) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD46))
  (segment (start 141.224 77.851) (end 141.224 77.597) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD64))
  (segment (start 141.224 78.232) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8B))
  (segment (start 112.014 80.391) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD5B))
  (segment (start 112.014 79.375) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD82))
  (segment (start 112.014 79.883) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDCD))
  (via (at 140.335 82.296) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1E1))
  (segment (start 141.224 80.391) (end 141.224 80.645) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD67))
  (via (at 169.418 82.042) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1DE))
  (segment (start 170.422 80.391) (end 170.422 80.657) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD40))
  (segment (start 141.224 80.391) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDAC))
  (segment (start 141.224 81.116) (end 141.224 81.28) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6A))
  (segment (start 140.870999 81.469001) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDB5))
  (segment (start 140.399999 81.469001) (end 140.870999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE7E))
  (segment (start 139.7 82.169) (end 140.399999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDC1))
  (segment (start 152.781 78.232) (end 152.781 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE00))
  (segment (start 150.749 78.232) (end 152.781 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD91))
  (segment (start 123.444 78.486) (end 123.444 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE30))
  (segment (start 123.444 78.232) (end 123.444 78.486) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE75))
  (segment (start 121.414 78.232) (end 123.444 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE48))
  (via (at 140.335 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 142.24 95.25) (end 140.335 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 129.54 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 131.445 95.25) (end 129.54 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 158.75 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3E595))
  (segment (start 160.54 95.25) (end 158.75 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 169.545 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 171.22 95.25) (end 169.545 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 95.25) (end 100.33 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 103.505 97.63) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 97.515) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 95.25) (end 102.12 97.515) (width 0.35) (layer F.Cu) (net 8))
  (via (at 123.825 97.79) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 8))
  (segment (start 124.095 97.52) (end 123.825 97.79) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 125.415 97.52) (end 124.095 97.52) (width 0.35) (layer B.Cu) (net 8))
  (via (at 111.125 94.869) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 112.8 95.25) (end 111.125 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 129.945 104.775) (end 129.54 104.775) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 129.945 104.775) (end 129.195 104.775) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 156.271 83.852) (end 156.271 83.5) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 155.805 83.096) (end 155.805 82.296) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 156.209 83.5) (end 155.805 83.096) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 156.271 83.5) (end 156.209 83.5) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 112.014 80.391) (end 112.014 81.153) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE39))
  (segment (start 112.014 81.153) (end 110.998 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BF53))
  (segment (start 110.998 82.169) (end 110.49 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6D))
  (segment (start 108.3795 46.1414) (end 108.0255 46.4954) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E1F))
  (segment (start 108.0255 46.4954) (end 106.8705 46.4954) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E22))
  (segment (start 111.1395 46.1414) (end 108.3795 46.1414) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E25))
  (segment (start 99.439 78.232) (end 99.314 78.232) (width 0.35) (layer F.Cu) (net 8))
  (via (at 98.044 80.01) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 97.663 79.883) (end 97.663 80.391) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 99.314 78.232) (end 97.663 79.883) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 136.6654 114.4785) (end 136.6774 114.4665) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E28))
  (segment (start 135.2804 114.4785) (end 136.6654 114.4785) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E2B))
  (segment (start 138.0624 114.4665) (end 138.0744 114.4785) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E2E))
  (segment (start 136.6774 114.4665) (end 138.0624 114.4665) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E31))
  (segment (start 90.817 62.8765) (end 90.869 62.9285) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.869 62.9285) (end 90.869 68.6785) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.869 72.0235) (end 90.9005 72.055) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.869 68.6785) (end 90.869 72.0235) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.9005 73.78) (end 90.9005 77.805) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.9005 72.055) (end 90.9005 73.78) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 90.9005 81.1355) (end 90.9005 77.805) (width 0.35) (layer F.Cu) (net 8))
  (via (at 102.2985 46.3804) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BCC4011))
  (segment (start 102.3225 46.4044) (end 102.2985 46.3804) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E37))
  (segment (start 105.4735 46.4044) (end 102.3225 46.4044) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E3A))
  (segment (start 115.6455 36.4744) (end 115.6455 35.7004) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E3D))
  (segment (start 127.696729 14.3434) (end 127.68161 14.358519) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB68))
  (segment (start 129.3876 14.3434) (end 127.696729 14.3434) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB6B))
  (segment (start 126.881611 13.55852) (end 127.68161 14.358519) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB6E))
  (segment (start 124.6976 13.2879) (end 126.610991 13.2879) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB71))
  (segment (start 126.610991 13.2879) (end 126.881611 13.55852) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB74))
  (segment (start 115.6455 36.4744) (end 115.6455 35.7494) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E40))
  (via (at 124.6886 16.0909) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC5AB7A))
  (segment (start 124.6976 16.0819) (end 124.6886 16.0909) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 124.6976 13.2879) (end 124.6976 16.0819) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC5AB77))
  (via (at 115.7605 33.9344) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BCC4005))
  (segment (start 115.6455 34.0494) (end 115.7605 33.9344) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E43))
  (segment (start 115.6455 35.7494) (end 115.6455 34.0494) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E46))
  (segment (start 117.0305 55.6514) (end 117.0305 57.421717) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3E49))
  (segment (start 117.0305 57.421717) (end 116.74551 57.706707) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3C1B))
  (via (at 116.4463 57.4548) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BCC401D))
  (segment (start 117.0305 55.6514) (end 117.0305 58.3184) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3BDF))
  (via (at 84.6836 15.1638) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 84.6836 17.3228) (end 84.6836 15.1638) (width 0.35) (layer B.Cu) (net 8))
  (via (at 108.458 32.4739) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BCC3FF9))
  (segment (start 110.2995 32.5374) (end 108.5215 32.5374) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3D14))
  (segment (start 108.5215 32.5374) (end 108.458 32.4739) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3C0F))
  (via (at 111.0615 82.271021) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (via (at 184.9628 11.938) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 185.2422 11.4554) (end 184.9374 11.7602) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 187.5282 11.4554) (end 185.2422 11.4554) (width 0.35) (layer F.Cu) (net 8))
  (via (at 212.3186 21.8821) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 213.2584 22.8219) (end 212.3186 21.8821) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 213.384 22.8219) (end 213.2584 22.8219) (width 0.35) (layer F.Cu) (net 8))
  (via (at 126.1872 78.232) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 128.649 78.232) (end 126.1872 78.232) (width 0.35) (layer F.Cu) (net 8))
  (via (at 155.3464 78.2574) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 155.3718 78.232) (end 155.3464 78.2574) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 157.859 78.232) (end 155.3718 78.232) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 181.4322 78.232) (end 182.5752 77.089) (width 0.35) (layer F.Cu) (net 8))
  (via (at 182.5752 77.089) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 179.959 78.232) (end 181.4322 78.232) (width 0.35) (layer F.Cu) (net 8))
  (via (at 110.4138 65.6336) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 115.062 66.802) (end 115.2144 66.6496) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 112.014 66.802) (end 115.062 66.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 143.637 66.802) (end 144.1196 66.3194) (width 0.35) (layer F.Cu) (net 8))
  (via (at 139.6746 66.2432) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 141.349 66.802) (end 143.637 66.802) (width 0.35) (layer F.Cu) (net 8))
  (via (at 168.9608 66.2432) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 169.3926 66.802) (end 168.9608 66.3702) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 170.559 66.802) (end 169.3926 66.802) (width 0.35) (layer F.Cu) (net 8))
  (via (at 154.2034 66.3194) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 153.7208 66.802) (end 154.2034 66.3194) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 150.749 66.802) (end 153.7208 66.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 82.5183 8.1273) (end 83.1018 7.5438) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 76.7461 8.1273) (end 82.5183 8.1273) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 126.492 45.8209) (end 127.6223 45.8209) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3BC4))
  (segment (start 83.1018 7.5438) (end 85.2018 7.5438) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 127.6223 45.8209) (end 127.8255 45.8209) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC3BD3))
  (segment (start 99.439 66.802) (end 100.114 66.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.325252 64.590748) (end 102.325252 64.543833) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 100.114 66.802) (end 102.325252 64.590748) (width 0.35) (layer F.Cu) (net 8))
  (via (at 102.325252 64.543833) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 142.24 95.25) (end 142.24 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 131.445 95.25) (end 131.445 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 171.958 74.422) (end 170.434 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 75.438) (end 171.958 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 80.5434) (end 172.974 75.438) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.1927 83.3247) (end 172.974 80.5434) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.1927 83.9724) (end 170.1927 83.3247) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 171.6017 83.3724) (end 171.6621 83.312) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 171.6017 83.9724) (end 171.6017 83.3724) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.0215 73.152) (end 170.434 73.152) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 74.7395) (end 172.0215 73.152) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 81.3651) (end 173.609 74.7395) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 171.6017 83.3724) (end 173.609 81.3651) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.9987 83.3724) (end 173.0591 83.312) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.9987 83.9724) (end 172.9987 83.3724) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.0215 71.882) (end 170.434 71.882) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 82.1271) (end 174.244 74.1045) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 74.1045) (end 172.0215 71.882) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.9987 83.3724) (end 174.244 82.1271) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.879 73.533) (end 171.958 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.879 82.8294) (end 174.879 73.533) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 171.958 70.612) (end 170.434 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.3247) (end 174.879 82.8294) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.9724) (end 174.3837 83.3247) (width 0.35) (layer F.Cu) (net 12))
  (via (at 104.0765 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (via (at 116.6495 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 104.0765 72.009) (end 116.6495 72.009) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 113.9825 69.342) (end 112.014 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 116.6495 72.009) (end 113.9825 69.342) (width 0.35) (layer F.Cu) (net 13))
  (via (at 133.223 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 116.6495 72.009) (end 133.223 72.009) (width 0.35) (layer B.Cu) (net 13))
  (via (at 145.9865 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 133.223 72.009) (end 145.9865 72.009) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 143.3195 69.342) (end 141.349 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 145.9865 72.009) (end 143.3195 69.342) (width 0.35) (layer F.Cu) (net 13))
  (via (at 162.4965 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 145.9865 72.009) (end 162.4965 72.009) (width 0.35) (layer B.Cu) (net 13))
  (via (at 175.3235 72.009) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 162.4965 72.009) (end 175.3235 72.009) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 172.6565 69.342) (end 170.559 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 175.3235 72.009) (end 172.6565 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 159.8295 69.342) (end 157.859 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 162.4965 72.009) (end 159.8295 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 130.556 69.342) (end 128.649 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 133.223 72.009) (end 130.556 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 103.505 72.009) (end 104.0765 72.009) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 100.838 69.342) (end 103.505 72.009) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 99.439 69.342) (end 100.838 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 72.009) (end 104.0765 70.485) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 70.485) (end 104.0765 70.231) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 67.437) (end 104.0765 67.2465) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 70.485) (end 104.0765 67.437) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 67.437) (end 104.0765 66.9925) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 104.0765 66.8655) (end 104.0765 67.437) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 118.4275 60.0964) (end 117.8941 60.6298) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BCC3B82))
  (segment (start 118.4275 57.2784) (end 118.4275 60.0964) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BCC3B85))
  (segment (start 107.4547 60.8965) (end 101.8286 66.5226) (width 0.35) (layer F.Cu) (net 13) (tstamp 5BCC3B79))
  (segment (start 175.514 73.66) (end 178.562 70.612) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 178.562 70.612) (end 179.959 70.612) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.514 83.058) (end 175.514 73.66) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.7807 83.3247) (end 175.514 83.058) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.7807 83.9724) (end 175.7807 83.3247) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 178.562 71.882) (end 179.834 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 74.295) (end 178.562 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 82.296) (end 176.149 74.295) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.3247) (end 176.149 82.296) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.9724) (end 177.1777 83.3247) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 178.562 73.152) (end 179.834 73.152) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 74.93) (end 178.562 73.152) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.312) (end 176.784 81.534) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.3597) (end 178.562 83.312) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.5747 83.3724) (end 178.562 83.3597) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 81.534) (end 176.784 74.93) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.5747 83.9724) (end 178.5747 83.3724) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 74.422) (end 179.834 74.422) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 75.565) (end 178.562 74.422) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 80.8863) (end 177.419 75.565) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.9717 83.439) (end 177.419 80.8863) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.9717 83.9724) (end 179.9717 83.439) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 165.9255 74.422) (end 167.259 74.422) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 76.2635) (end 165.9255 74.422) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 80.045) (end 164.084 76.2635) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 167.386 83.347) (end 164.084 80.045) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 167.386 83.947) (end 167.386 83.347) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 165.9255 73.152) (end 167.259 73.152) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 163.449 75.6285) (end 165.9255 73.152) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 163.449 80.807) (end 163.449 75.6285) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.347) (end 163.449 80.807) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.947) (end 165.989 83.347) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.862 71.882) (end 167.259 71.882) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 81.569) (end 162.814 74.93) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.592 83.347) (end 162.814 81.569) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 74.93) (end 165.862 71.882) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.592 83.947) (end 164.592 83.347) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 165.7985 70.612) (end 167.259 70.612) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 74.2315) (end 165.7985 70.612) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 82.331) (end 162.179 74.2315) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 163.195 83.347) (end 162.179 82.331) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 163.195 83.947) (end 163.195 83.347) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 161.544 83.093) (end 161.798 83.347) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 83.093) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.798 83.347) (end 161.798 83.947) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.927) (end 161.544 81.534) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 159.258 70.612) (end 157.859 70.612) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 72.898) (end 159.258 70.612) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 72.898) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 160.401 83.347) (end 160.401 83.947) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 82.804011) (end 160.401 83.347) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.804011) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.596989) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 159.1945 71.882) (end 157.859 71.882) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 73.631489) (end 159.1945 71.882) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 73.631489) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 159.004 83.947) (end 159.004 83.347) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 82.159011) (end 160.191989 74.159989) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 74.159989) (end 159.184 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.004 83.347) (end 160.191989 82.159011) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 73.152) (end 157.859 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 74.422) (end 159.524 74.762) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BEED))
  (segment (start 157.859 74.422) (end 159.184 74.422) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BF23) (status 10))
  (segment (start 157.607 83.347) (end 159.524 81.43) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 81.43) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 157.607 83.947) (end 157.607 83.347) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 74.762) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 143.764 80.553) (end 143.764 75.5015) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 143.764 75.5015) (end 142.6845 74.422) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.97 83.347) (end 143.764 80.553) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 142.6845 74.422) (end 141.224 74.422) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.97 83.947) (end 140.97 83.347) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 144.354011 74.758011) (end 142.748 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.748 73.152) (end 141.224 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 144.354011 81.359989) (end 144.354011 74.758011) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.347) (end 144.354011 81.359989) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.947) (end 142.367 83.347) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 141.224 71.882) (end 142.549 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 142.748 71.882) (end 141.224 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 74.168) (end 142.748 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 82.077) (end 145.034 74.168) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.347) (end 145.034 82.077) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.947) (end 143.764 83.347) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.669 82.839) (end 145.669 81.788) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.947) (end 145.161 83.347) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.347) (end 145.669 82.839) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 81.788) (end 145.669 81.927) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 142.748 70.612) (end 141.224 70.612) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 73.533) (end 142.748 70.612) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 81.788) (end 145.669 73.533) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 149.4155 70.612) (end 150.624 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.304 73.7235) (end 149.4155 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.304 83.093) (end 146.304 73.7235) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.347) (end 146.304 83.093) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.947) (end 146.558 83.347) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 149.352 71.882) (end 150.624 71.882) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 74.295) (end 149.352 71.882) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 82.296) (end 146.939 74.295) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 147.955 83.312) (end 146.939 82.296) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 147.955 83.947) (end 147.955 83.312) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 149.4155 73.152) (end 150.624 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 74.9935) (end 149.4155 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 81.534) (end 147.574 74.9935) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.312) (end 147.574 81.534) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.947) (end 149.352 83.312) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 74.422) (end 150.624 74.422) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.209 75.565) (end 149.352 74.422) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.209 80.899) (end 148.209 75.565) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.2375 80.899) (end 148.209 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 150.6855 83.347) (end 148.2375 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 150.6855 83.947) (end 150.6855 83.347) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 138.176 83.347) (end 138.176 83.947) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 76.272) (end 134.874 80.045) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 80.045) (end 138.176 83.347) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 136.724 74.422) (end 134.874 76.272) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 138.049 74.422) (end 136.724 74.422) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 136.779 83.312) (end 136.779 83.947) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 75.637) (end 134.239 80.772) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 136.724 73.152) (end 134.239 75.637) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 80.772) (end 136.779 83.312) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 138.049 73.152) (end 136.724 73.152) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 135.382 83.347) (end 135.382 83.947) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 137.374 71.882) (end 136.724 72.532) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 81.534) (end 135.382 83.312) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 135.382 83.312) (end 135.382 83.347) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 138.049 71.882) (end 137.374 71.882) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.724 72.532) (end 136.2884 72.532) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.2884 72.532) (end 133.604 75.2164) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 75.2164) (end 133.604 81.534) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.985 83.347) (end 133.95 83.312) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 133.985 83.947) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 75.017) (end 132.969 82.331) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 138.049 70.612) (end 137.374 70.612) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 82.331) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 137.374 70.612) (end 132.969 75.017) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.588 83.347) (end 132.588 83.947) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 83.093) (end 132.588 83.347) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 129.974 70.612) (end 132.334 72.972) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 72.972) (end 132.334 83.093) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 128.649 70.612) (end 129.974 70.612) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 131.191 83.347) (end 131.191 83.947) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 73.607) (end 131.699 82.839) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 82.839) (end 131.191 83.347) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 129.974 71.882) (end 131.699 73.607) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 128.649 71.882) (end 129.974 71.882) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 129.794 83.347) (end 129.794 83.947) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 131.064 82.077) (end 129.794 83.347) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 131.064 74.242) (end 131.064 82.077) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 129.974 73.152) (end 131.064 74.242) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 128.649 73.152) (end 129.974 73.152) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 128.397 83.947) (end 128.397 83.347) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 128.397 83.347) (end 130.413989 81.330011) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 129.974 74.422) (end 128.649 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFEF) (status 20))
  (segment (start 130.413989 81.330011) (end 130.413989 80.772) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 80.772) (end 130.413989 74.861989) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 74.861989) (end 129.974 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFBF))
  (segment (start 114.554 80.518) (end 111.76 83.312) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 111.76 83.312) (end 111.76 83.947) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 114.554 75.057) (end 114.554 80.518) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.919 74.422) (end 114.554 75.057) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 112.014 74.422) (end 113.919 74.422) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.6015 73.152) (end 112.014 73.152) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.189 74.7395) (end 113.6015 73.152) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.189 81.28) (end 115.189 74.7395) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.157 83.312) (end 115.189 81.28) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.157 83.947) (end 113.157 83.312) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.3475 71.882) (end 112.014 71.882) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 74.3585) (end 113.3475 71.882) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 82.042) (end 115.824 74.3585) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 114.554 83.312) (end 115.824 82.042) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 114.554 83.947) (end 114.554 83.312) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 113.339 70.612) (end 112.014 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 82.839) (end 116.459 73.732) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 73.732) (end 113.339 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.347) (end 116.459 82.839) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.947) (end 115.951 83.347) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 120.015 70.612) (end 121.414 70.612) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 73.533) (end 120.015 70.612) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 82.562) (end 117.094 73.533) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.348 82.816) (end 117.094 82.562) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.348 83.947) (end 117.348 82.816) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 120.0785 71.882) (end 121.414 71.882) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 74.2315) (end 120.0785 71.882) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 82.331) (end 117.729 74.2315) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.745 83.347) (end 117.729 82.331) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.745 83.947) (end 118.745 83.347) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 120.142 73.152) (end 121.414 73.152) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 74.93) (end 120.142 73.152) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 81.569) (end 118.364 74.93) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.142 83.347) (end 118.364 81.569) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.142 83.947) (end 120.142 83.347) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 121.539 83.947) (end 121.539 83.347) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 121.539 83.347) (end 118.999 80.807) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 119.7064 74.422) (end 120.089 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 80.807) (end 118.999 75.1294) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 75.1294) (end 119.7064 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 120.089 74.422) (end 121.414 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 107.5055 74.422) (end 108.839 74.422) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 105.664 76.2635) (end 107.5055 74.422) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 105.664 80.045) (end 105.664 76.2635) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 108.966 83.347) (end 105.664 80.045) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 108.966 83.947) (end 108.966 83.347) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 107.5055 73.152) (end 108.839 73.152) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 75.6285) (end 107.5055 73.152) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 80.807) (end 105.029 75.6285) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.569 83.347) (end 105.029 80.807) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.569 83.947) (end 107.569 83.347) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.442 71.882) (end 108.839 71.882) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 74.93) (end 107.442 71.882) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 81.581) (end 104.394 74.93) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 106.172 83.359) (end 104.394 81.581) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 106.172 83.959) (end 106.172 83.359) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 103.759 74.422) (end 107.569 70.612) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 107.569 70.612) (end 108.839 70.612) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 103.759 82.296) (end 103.759 74.422) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 104.775 83.312) (end 103.759 82.296) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 104.775 83.947) (end 104.775 83.312) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 103.124 72.898) (end 100.838 70.612) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 100.838 70.612) (end 99.439 70.612) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.124 83.093) (end 103.124 72.898) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.378 83.347) (end 103.124 83.093) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.378 83.947) (end 103.378 83.347) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 100.584 71.882) (end 99.439 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 102.489 73.66) (end 100.711 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 102.489 82.839) (end 102.489 73.66) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.981 83.347) (end 102.489 82.839) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 100.711 71.882) (end 100.584 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.981 83.947) (end 101.981 83.347) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.854 74.242) (end 100.764 73.152) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 101.854 82.077) (end 101.854 74.242) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.764 73.152) (end 99.439 73.152) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 83.347) (end 101.854 82.077) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 83.947) (end 100.584 83.347) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 74.422) (end 99.439 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BF29) (status 20))
  (segment (start 101.219 75.057) (end 100.584 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3C0AC))
  (segment (start 101.219 81.327) (end 101.219 79.502) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC77))
  (segment (start 99.187 83.959) (end 99.187 83.359) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC6B))
  (segment (start 101.219 79.502) (end 101.219 75.057) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC5F))
  (segment (start 99.187 83.359) (end 101.219 81.327) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC7D))
  (segment (start 170.1927 90.813115) (end 171.466915 92.08733) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.1927 85.4724) (end 170.1927 90.813115) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.823172 89.638927) (end 171.466915 90.28267) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 170.823172 86.850928) (end 170.823172 89.638927) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 86.0724) (end 170.823172 86.850928) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 85.4724) (end 171.6017 86.0724) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 172.9987 86.0724) (end 172.5841 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.9987 85.4724) (end 172.9987 86.0724) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.5841 86.487) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.527667 88.82267) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 174.3837 88.1253) (end 174.244 88.265) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 174.3837 85.4724) (end 174.3837 88.1253) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 175.7807 88.643037) (end 175.960333 88.82267) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 175.7807 85.4724) (end 175.7807 88.643037) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 177.1777 90.126055) (end 177.021085 90.28267) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 177.1777 85.4724) (end 177.1777 90.126055) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 178.5747 90.533715) (end 177.021085 92.08733) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 178.5747 85.4724) (end 178.5747 90.533715) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 176.769882 93.54733) (end 175.960333 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 177.310383 93.54733) (end 176.769882 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 90.886013) (end 177.310383 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 85.4724) (end 179.9717 90.886013) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 167.196 93.535) (end 165.974882 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.275 92.456) (end 167.196 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.275 87.376) (end 168.275 92.456) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 86.487) (end 168.275 87.376) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 165.974882 93.535) (end 165.165333 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 85.447) (end 167.386 86.487) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.459838 87.703838) (end 165.989 86.233) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.478494 89.773451) (end 167.459838 89.754795) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 165.989 86.233) (end 165.989 85.447) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.459838 89.754795) (end 167.459838 87.703838) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.478494 90.612721) (end 167.478494 89.773451) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 91.86513) (end 167.478494 90.612721) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 92.075) (end 166.226085 91.86513) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.869828 89.626597) (end 166.226085 90.27034) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 166.869828 88.324828) (end 166.869828 89.626597) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 86.047) (end 166.869828 88.324828) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 85.447) (end 164.592 86.047) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 165.165333 88.017333) (end 165.165333 88.81034) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 86.047) (end 165.165333 88.017333) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 85.447) (end 163.195 86.047) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.449 88.00267) (end 163.449 88.25267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 86.35167) (end 163.449 88.00267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 85.447) (end 161.798 86.35167) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 160.401 87.478673) (end 161.732667 88.81034) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 160.401 85.447) (end 160.401 87.478673) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 159.004 85.447) (end 159.004 86.106) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 89.110425) (end 160.063575 89.662) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 86.614) (end 159.512 89.110425) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 160.063575 89.662) (end 160.671915 90.27034) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 86.614) (end 159.004 86.106) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 157.607 85.447) (end 157.607 86.106) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 159.004 90.407085) (end 160.671915 92.075) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 90.153085) (end 159.004 90.407085) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 87.249) (end 158.75 90.153085) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 87.249) (end 157.607 86.106) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 141.61733 92.08733) (end 142.256915 92.08733) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.716 91.186) (end 141.61733 92.08733) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.716 86.614) (end 140.716 91.186) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.97 86.36) (end 140.716 86.614) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.97 85.447) (end 140.97 86.36) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 141.613172 89.638927) (end 142.256915 90.28267) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 141.613172 86.800828) (end 141.613172 89.638927) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 86.047) (end 141.613172 86.800828) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 85.447) (end 142.367 86.047) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 143.764 85.447) (end 143.764 85.979) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.317667 86.425333) (end 143.317667 88.82267) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.764 85.979) (end 143.317667 86.425333) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 145.161 88.138) (end 145.034 88.265) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 145.161 85.447) (end 145.161 88.138) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 146.558 88.630337) (end 146.750333 88.82267) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 146.558 85.447) (end 146.558 88.630337) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 147.955 90.138755) (end 147.811085 90.28267) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 147.955 85.447) (end 147.955 90.138755) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 149.352 90.546415) (end 149.352 85.447) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 149.352 91.476899) (end 149.352 90.546415) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 148.741569 92.08733) (end 149.352 91.476899) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 147.811085 92.08733) (end 148.741569 92.08733) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 147.559882 93.54733) (end 146.750333 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.100383 93.54733) (end 147.559882 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.100383 93.54733) (end 149.14967 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 90.297) (end 150.6855 92.0115) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.114 92.583) (end 150.241 92.456) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 149.14967 93.54733) (end 150.114 92.583) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 85.447) (end 150.6855 90.297) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 92.0115) (end 150.114 92.583) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 138.938 86.995) (end 138.176 86.233) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.176 86.233) (end 138.176 85.447) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.938 92.837) (end 138.938 86.995) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.22767 93.54733) (end 138.938 92.837) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 135.955333 93.54733) (end 138.22767 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.268494 87.536494) (end 138.268494 90.834921) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 86.047) (end 138.268494 87.536494) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 85.447) (end 136.779 86.047) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.016085 92.08733) (end 138.268494 90.834921) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.659828 89.638927) (end 137.016085 90.28267) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 86.047) (end 137.659828 88.324828) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 137.659828 88.324828) (end 137.659828 89.638927) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 85.447) (end 135.382 86.047) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.955333 88.017333) (end 135.955333 88.82267) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 86.047) (end 135.955333 88.017333) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 85.447) (end 133.985 86.047) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 132.588 86.364) (end 132.588 85.447) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.015) (end 132.588 86.364) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.265) (end 134.239 88.015) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 131.191 87.491003) (end 132.522667 88.82267) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 131.191 85.447) (end 131.191 87.491003) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 130.429 89.249755) (end 130.429 86.741) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 129.794 85.447) (end 129.794 86.106) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 130.429 86.741) (end 129.794 86.106) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 130.429 89.249755) (end 131.461915 90.28267) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 128.397 86.233) (end 128.397 85.447) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 129.798585 87.634585) (end 128.397 86.233) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 129.798585 90.424) (end 129.798585 87.634585) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 131.461915 92.08733) (end 129.798585 90.424) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 111.76 90.800415) (end 113.046915 92.08733) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 111.76 85.447) (end 111.76 90.800415) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 112.403172 89.638927) (end 113.046915 90.28267) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 112.403172 86.800828) (end 112.403172 89.638927) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 86.047) (end 112.403172 86.800828) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 85.447) (end 113.157 86.047) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 114.554 85.979) (end 114.554 85.447) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 86.425333) (end 114.554 85.979) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 88.82267) (end 114.107667 86.425333) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 115.951 88.138) (end 115.824 88.265) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 115.951 85.447) (end 115.951 88.138) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 117.348 88.630337) (end 117.540333 88.82267) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 117.348 85.447) (end 117.348 88.630337) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 118.745 90.138755) (end 118.601085 90.28267) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 118.745 85.447) (end 118.745 90.138755) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 120.142 90.546415) (end 118.601085 92.08733) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.142 85.447) (end 120.142 90.546415) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.777 87.376) (end 121.539 86.614) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 120.777 92.456) (end 120.777 87.376) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 119.68567 93.54733) (end 120.777 92.456) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 121.539 86.614) (end 121.539 85.447) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 117.540333 93.54733) (end 119.68567 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 109.855 92.164534) (end 108.458 93.561534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.855 86.936) (end 109.855 92.164534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.458 93.561534) (end 106.673633 93.561534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.966 86.047) (end 109.855 86.936) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.966 85.447) (end 108.966 86.047) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 107.569 86.047) (end 109.22 87.698) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 107.569 85.447) (end 107.569 86.047) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 90.615919) (end 107.734385 92.101534) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 87.698) (end 109.22 90.615919) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 108.378128 89.653131) (end 107.734385 90.296874) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 108.378128 88.265128) (end 108.378128 89.653131) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 86.059) (end 108.378128 88.265128) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 85.459) (end 106.172 86.059) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.673633 87.945633) (end 106.673633 87.95306) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 106.673633 87.95306) (end 106.673633 88.836874) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 86.047) (end 106.673633 87.945633) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 85.447) (end 104.775 86.047) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.9573 88.029204) (end 104.9573 88.279204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 86.449904) (end 104.9573 88.029204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 85.447) (end 103.378 86.449904) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 101.981 87.576907) (end 103.240967 88.836874) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 101.981 85.447) (end 101.981 87.576907) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 100.584 88.700659) (end 102.180215 90.296874) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 100.584 85.447) (end 100.584 88.700659) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 99.187 89.108319) (end 102.180215 92.101534) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 99.187 85.459) (end 99.187 89.108319) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 170.434 75.692) (end 167.259 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0BB) (status 30))
  (segment (start 167.259 75.692) (end 166.584 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0C4) (status 30))
  (segment (start 141.224 75.692) (end 138.049 75.692) (width 0.35) (layer F.Cu) (net 107) (tstamp 5BC3C0C1) (status 30))
  (segment (start 150.624 75.692) (end 157.859 75.692) (width 0.35) (layer F.Cu) (net 108) (tstamp 5BC3C0BE) (status 30))
  (segment (start 121.414 75.692) (end 128.649 75.692) (width 0.35) (layer F.Cu) (net 109) (tstamp 5BC3C0C7) (status 30))
  (segment (start 108.839 75.692) (end 112.014 75.692) (width 0.35) (layer F.Cu) (net 110) (tstamp 5BC3C0CA) (status 30))
  (segment (start 112.2145 40.4414) (end 112.8395 40.4414) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC3CC0))
  (segment (start 110.0455 38.2724) (end 112.2145 40.4414) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC3FD2))
  (segment (start 110.0455 36.6014) (end 110.0455 38.2724) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC3FCF))
  (segment (start 125.5395 37.8714) (end 125.5395 36.6028) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC3FCC))
  (segment (start 122.5395 40.8714) (end 125.5395 37.8714) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC3FC9))
  (segment (start 122.5395 42.1414) (end 122.5395 40.8714) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC3FC6))
  (segment (start 114.4395 51.8414) (end 114.4395 52.9084) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC3FC3))
  (segment (start 112.7125 55.7784) (end 112.7125 55.1434) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC3FC0))
  (segment (start 114.4395 53.4164) (end 114.4395 51.8414) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC3FBD))
  (segment (start 112.7125 55.1434) (end 114.4395 53.4164) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC3FD8))
  (segment (start 124.1425 37.2014) (end 124.1425 36.6014) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC3FD5))
  (segment (start 124.1425 37.7634) (end 124.1425 37.2014) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC3FB4))
  (segment (start 121.4645 40.4414) (end 124.1425 37.7634) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC3FB1))
  (segment (start 120.8395 40.4414) (end 121.4645 40.4414) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC3FAE))
  (segment (start 123.6395 47.7414) (end 122.5395 47.7414) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC3FAB))
  (segment (start 124.84 47.7414) (end 123.6395 47.7414) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC3FA8))
  (segment (start 125.765 48.6664) (end 124.84 47.7414) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC3FA5))
  (segment (start 126.365 48.6664) (end 125.765 48.6664) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC3FA2))
  (segment (start 114.2365 37.2364) (end 114.2365 36.5894) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC3F9F))
  (segment (start 115.2395 38.2394) (end 114.2365 37.2364) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC3F9C))
  (segment (start 115.2395 40.4414) (end 115.2395 38.2394) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC3F99))
  (segment (start 112.8515 36.5894) (end 112.8515 37.2244) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC3F96))
  (segment (start 114.4395 38.8124) (end 114.4395 40.4414) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC3F93))
  (segment (start 112.8515 37.2244) (end 114.4395 38.8124) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC3F90))
  (segment (start 118.5545 36.6014) (end 118.5545 37.2364) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC3F8D))
  (segment (start 117.6395 38.1514) (end 117.6395 40.4414) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC3F8A))
  (segment (start 118.5545 37.2364) (end 117.6395 38.1514) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC3F87))
  (segment (start 118.4395 38.7134) (end 118.4395 39.3414) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC3F84))
  (segment (start 119.9515 37.2014) (end 118.4395 38.7134) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC3F81))
  (segment (start 118.4395 39.3414) (end 118.4395 40.4414) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC3FBA))
  (segment (start 119.9515 36.6014) (end 119.9515 37.2014) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC3FB7))
  (segment (start 119.2395 38.9644) (end 121.3485 36.8554) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC3F7B))
  (segment (start 121.3485 36.8554) (end 121.3485 36.6014) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC3F78))
  (segment (start 119.2395 40.4414) (end 119.2395 38.9644) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC3F75))
  (segment (start 111.3155 55.2654) (end 111.3155 55.6514) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC3F72))
  (segment (start 113.6395 52.9414) (end 111.3155 55.2654) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC3F6F))
  (segment (start 113.6395 51.8414) (end 113.6395 52.9414) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC3F6C))
  (segment (start 111.3155 55.6514) (end 111.3155 55.7784) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC3F69))
  (via (at 83.4136 12.3698) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 83.4136 18.5928) (end 83.4136 17.1958) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 82.1436 19.8628) (end 83.4136 18.5928) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 83.4136 12.3698) (end 83.4136 17.1958) (width 0.35) (layer B.Cu) (net 122))
  (via (at 106.553 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (via (at 118.0465 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 118.237 68.072) (end 118.0465 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 121.414 68.072) (end 118.237 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 134.874 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 135.0645 68.072) (end 134.874 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 138.049 68.072) (end 135.0645 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 147.447 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 134.874 67.8815) (end 147.447 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 147.6375 68.072) (end 147.447 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 150.749 68.072) (end 147.6375 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 163.957 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 147.447 67.8815) (end 163.957 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 164.1475 68.072) (end 163.957 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 167.259 68.072) (end 164.1475 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 176.7205 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 163.957 67.8815) (end 176.7205 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 176.911 68.072) (end 176.7205 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 179.959 68.072) (end 176.911 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 126.1237 67.8561) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 124.841 67.8815) (end 134.874 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 118.0465 67.8815) (end 124.841 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 106.6165 68.072) (end 106.553 68.0085) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 107.6325 68.072) (end 106.6165 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 108.839 68.072) (end 107.6325 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 106.7435 68.072) (end 106.553 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 108.839 68.072) (end 106.7435 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 118.0465 67.8815) (end 106.553 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 127.865 50.0634) (end 129.3749 50.0634) (width 0.35) (layer F.Cu) (net 122) (tstamp 5BCC3B64))
  (segment (start 129.3749 50.0634) (end 129.0588 50.0634) (width 0.35) (layer F.Cu) (net 122) (tstamp 5BCC3B70))
  (segment (start 83.4136 12.3698) (end 78.4987 12.3698) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 86.0933 9.6901) (end 83.4136 12.3698) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 86.0933 6.9163) (end 86.0933 9.6901) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 83.439 20.3454) (end 83.4136 20.32) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 83.4136 12.3698) (end 83.4136 20.32) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 126.365 50.0634) (end 125.7935 50.0634) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC3F4E))
  (segment (start 124.2715 48.5414) (end 122.5395 48.5414) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC3F4B))
  (segment (start 125.7935 50.0634) (end 124.2715 48.5414) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC3F48))
  (segment (start 126.365 51.4604) (end 125.7935 51.4604) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC3F45))
  (segment (start 123.6745 49.3414) (end 122.5395 49.3414) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC3F42))
  (segment (start 125.7935 51.4604) (end 123.6745 49.3414) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC3F3C))
  (via (at 80.8736 13.7668) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 125))
  (segment (start 80.8736 13.7668) (end 80.8736 17.6403) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 80.8736 17.6403) (end 80.8736 17.8943) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 79.6036 19.7358) (end 79.6036 19.8628) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 80.8736 18.4658) (end 79.6036 19.7358) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 80.8736 17.8943) (end 80.8736 18.4658) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 127.865 51.4604) (end 128.465 51.4604) (width 0.35) (layer F.Cu) (net 125) (tstamp 5BCC3B91))
  (segment (start 129.5273 51.4604) (end 129.0588 51.4604) (width 0.35) (layer F.Cu) (net 125) (tstamp 5BCC3BB8))
  (segment (start 128.465 51.4604) (end 129.5273 51.4604) (width 0.35) (layer F.Cu) (net 125) (tstamp 5BCC3BAC))
  (segment (start 80.8736 13.7668) (end 78.6511 13.7668) (width 0.35) (layer F.Cu) (net 125))
  (segment (start 80.8736 11.9253) (end 80.8736 13.7668) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 81.7118 11.0871) (end 80.8736 11.9253) (width 0.35) (layer B.Cu) (net 125))
  (segment (start 81.7118 6.9723) (end 81.7118 11.0871) (width 0.35) (layer B.Cu) (net 125))
  (via (at 82.1436 15.1638) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 126))
  (segment (start 82.1436 15.1638) (end 80.868601 16.438799) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 80.8736 19.867799) (end 80.868601 19.8628) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 80.868601 16.438799) (end 80.868601 19.8628) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 82.1436 17.3228) (end 82.1436 15.1638) (width 0.35) (layer B.Cu) (net 126))
  (segment (start 80.868601 20.9296) (end 80.868601 21.2344) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 80.868601 19.8628) (end 80.868601 20.9296) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 128.465 52.8574) (end 129.5019 52.8574) (width 0.35) (layer F.Cu) (net 126) (tstamp 5BCC3BD6))
  (segment (start 127.865 52.8574) (end 128.465 52.8574) (width 0.35) (layer F.Cu) (net 126) (tstamp 5BCC3BC7))
  (segment (start 78.6257 15.1638) (end 82.1436 15.1638) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 129.0588 52.8574) (end 129.5019 52.8574) (width 0.35) (layer F.Cu) (net 126) (tstamp 5BCC3BC1))
  (segment (start 82.1436 11.6713) (end 82.1436 15.1638) (width 0.35) (layer B.Cu) (net 126))
  (segment (start 83.8708 9.9441) (end 82.1436 11.6713) (width 0.35) (layer B.Cu) (net 126))
  (segment (start 83.8708 6.9088) (end 83.8708 9.9441) (width 0.35) (layer B.Cu) (net 126))
  (segment (start 122.5395 50.7664) (end 124.6305 52.8574) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC3F27))
  (segment (start 122.5395 50.1414) (end 122.5395 50.7664) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC3F24))
  (segment (start 124.6305 52.8574) (end 126.0475 52.8574) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC3F21))
  (segment (start 126.0475 52.8574) (end 125.6665 52.8574) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC3F1E))
  (segment (start 126.365 52.8574) (end 126.0475 52.8574) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC3F1B))
  (segment (start 109.0185 39.3954) (end 107.5975 39.3954) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC3F18))
  (segment (start 111.1395 41.5164) (end 109.0185 39.3954) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC3F2D))
  (segment (start 107.5975 39.3954) (end 106.9975 39.3954) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC3F2A))
  (segment (start 111.1395 42.1414) (end 111.1395 41.5164) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC3F15))
  (segment (start 106.6165 58.0644) (end 106.6165 56.7944) (width 0.35) (layer B.Cu) (net 129) (tstamp 5BCC3F0C))
  (segment (start 155.749 101.6) (end 156.349 101.6) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 153.924 101.6) (end 155.749 101.6) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 151.204001 98.880001) (end 153.924 101.6) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 99.134001 98.880001) (end 151.204001 98.880001) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 137.0584 110.6805) (end 136.6774 111.0615) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3ED0))
  (segment (start 136.6774 111.0615) (end 136.6774 112.9665) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3ED3))
  (segment (start 108.6485 56.8084) (end 108.6485 56.7944) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EDC))
  (segment (start 109.9185 57.2784) (end 109.1185 57.2784) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EDF))
  (segment (start 109.1185 57.2784) (end 108.6485 56.8084) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EE2))
  (segment (start 107.1245 55.2704) (end 106.8705 55.2704) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EE5))
  (segment (start 105.2195 55.2704) (end 106.8705 55.2704) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EE8))
  (segment (start 105.2195 55.2704) (end 102.8065 55.2704) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EF4))
  (segment (start 108.6485 56.7944) (end 107.1245 55.2704) (width 0.35) (layer F.Cu) (net 130) (tstamp 5BCC3EF7))
  (segment (start 156.349 102.997) (end 154.178 102.997) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 154.178 102.997) (end 150.73399 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 98.82101 99.55299) (end 98.806 99.568) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 150.73399 99.55299) (end 98.82101 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 103.5805 53.5044) (end 103.5685 53.4924) (width 0.35) (layer F.Cu) (net 131) (tstamp 5BCC3ECD))
  (segment (start 100.5085 53.4924) (end 103.9495 53.4924) (width 0.35) (layer F.Cu) (net 131) (tstamp 5BCC3EC4))
  (segment (start 105.4855 53.5044) (end 103.9615 53.5044) (width 0.35) (layer F.Cu) (net 131) (tstamp 5BCC3EC7))
  (segment (start 103.9615 53.5044) (end 103.9495 53.4924) (width 0.35) (layer F.Cu) (net 131) (tstamp 5BCC3ECA))
  (segment (start 122.047 100.203) (end 99.090252 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 122.20402 100.36002) (end 122.047 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 99.075244 100.218008) (end 98.724032 100.218008) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 99.090252 100.203) (end 99.075244 100.218008) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 127.139 101.6) (end 123.444 101.6) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 123.444 101.6) (end 122.20402 100.36002) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 105.4975 52.0954) (end 102.2985 52.0954) (width 0.35) (layer F.Cu) (net 132) (tstamp 5BCC3ED6))
  (segment (start 133.8834 112.9665) (end 133.8834 111.1885) (width 0.35) (layer F.Cu) (net 132) (tstamp 5BCC3ED9))
  (segment (start 127.151 102.9335) (end 126.551 102.9335) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 126.551 102.9335) (end 123.7615 102.9335) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 123.7615 102.9335) (end 121.83803 101.01003) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 121.83803 101.01003) (end 121.68101 100.85301) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 121.68101 100.85301) (end 100.122012 100.85301) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 99.344486 100.868018) (end 97.312018 100.868018) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 99.359494 100.85301) (end 99.344486 100.868018) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 100.122012 100.85301) (end 99.359494 100.85301) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 100.5205 50.6984) (end 103.9495 50.6984) (width 0.35) (layer F.Cu) (net 133) (tstamp 5BCC3EAC))
  (segment (start 105.4975 50.6984) (end 103.9495 50.6984) (width 0.35) (layer F.Cu) (net 133) (tstamp 5BCC3EAF))
  (segment (start 131.0894 111.1885) (end 131.0894 112.9665) (width 0.35) (layer F.Cu) (net 134) (tstamp 5BCC3EBB))
  (segment (start 105.4975 49.3014) (end 103.886 49.3014) (width 0.35) (layer F.Cu) (net 134))
  (via (at 103.886 49.3014) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 134))
  (segment (start 103.886 49.3014) (end 102.2985 49.3014) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 122.5395 45.3414) (end 125.0545 45.3414) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC3DB3))
  (segment (start 126.4285 43.9674) (end 128.8415 43.9674) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC3DB6))
  (segment (start 125.0545 45.3414) (end 126.4285 43.9674) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC3DBC))
  (segment (start 129.4511 44.577) (end 128.8415 43.9674) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC3F33))
  (segment (start 80.5815 6.8834) (end 78.5749 6.8834) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 123.6345 44.5414) (end 123.9495 44.5414) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3DB9))
  (segment (start 122.5395 44.5414) (end 123.6345 44.5414) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3F57))
  (segment (start 127.2915 40.2674) (end 128.8415 40.2674) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3F54))
  (segment (start 125.9205 41.6384) (end 127.2915 40.2674) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3CA5))
  (segment (start 125.9205 43.5254) (end 125.9205 41.6384) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3C27))
  (segment (start 124.9045 44.5414) (end 125.9205 43.5254) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3C72))
  (segment (start 123.6345 44.5414) (end 124.9045 44.5414) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3CCF))
  (segment (start 129.4341 39.6748) (end 128.8415 40.2674) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3C33))
  (segment (start 131.4577 39.6748) (end 129.4341 39.6748) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC3BE5))
  (segment (start 107.7595 47.9044) (end 105.4735 47.9044) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC3CDB))
  (segment (start 108.7225 46.9414) (end 107.7595 47.9044) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC3C15))
  (segment (start 111.1395 46.9414) (end 108.7225 46.9414) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC3F51))
  (segment (start 123.6445 42.9414) (end 122.5395 42.9414) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC3F30))
  (segment (start 124.2695 42.3164) (end 123.6445 42.9414) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC3F3F))
  (segment (start 124.2695 40.2844) (end 124.2695 42.3164) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC3F36))
  (segment (start 126.9365 37.6174) (end 124.2695 40.2844) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC3F60))
  (segment (start 126.9365 36.6148) (end 126.9365 37.6174) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC3F5D))
  (segment (start 120.0395 39.3074) (end 121.7295 37.6174) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC3F5A))
  (segment (start 121.7295 37.6174) (end 122.7455 36.6014) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC3C7B))
  (segment (start 120.0395 40.4414) (end 120.0395 39.3074) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC3E94))
  (segment (start 128.3335 37.4904) (end 128.3335 36.6148) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BCC3BEB))
  (segment (start 125.0315 40.7924) (end 128.3335 37.4904) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BCC3CAB))
  (segment (start 124.4955 43.7414) (end 125.0315 43.2054) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BCC3BDC))
  (segment (start 125.0315 43.2054) (end 125.0315 40.7924) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BCC3C36))
  (segment (start 122.5395 43.7414) (end 124.4955 43.7414) (width 0.35) (layer F.Cu) (net 140) (tstamp 5BCC3D05))
  (segment (start 114.1095 55.1784) (end 114.1095 55.7784) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC3C00))
  (segment (start 114.1095 55.1434) (end 114.1095 55.1784) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC3C06))
  (segment (start 115.2395 54.0134) (end 114.1095 55.1434) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC3D0E))
  (segment (start 115.2395 51.8414) (end 115.2395 54.0134) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC3CF9))
  (segment (start 114.1095 33.8074) (end 114.1095 32.5374) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C3F))
  (segment (start 114.2365 33.9344) (end 114.1095 33.8074) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3BD9))
  (segment (start 114.2365 35.0894) (end 114.2365 33.9344) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C1E))
  (segment (start 114.1095 31.1404) (end 114.1095 32.5374) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C4E))
  (segment (start 112.3315 29.3624) (end 114.1095 31.1404) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C81))
  (segment (start 109.2185 29.3624) (end 112.3315 29.3624) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C03))
  (segment (start 108.4325 28.5764) (end 109.2185 29.3624) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3BF4))
  (segment (start 107.6325 28.5764) (end 108.4325 28.5764) (width 0.35) (layer F.Cu) (net 142) (tstamp 5BCC3C2D))
  (segment (start 112.8515 33.6924) (end 112.8395 33.6804) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3CDE))
  (segment (start 112.8515 35.0894) (end 112.8515 33.6924) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3CF6))
  (segment (start 112.8395 35.0774) (end 112.8515 35.0894) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3C99))
  (segment (start 112.8395 32.5374) (end 112.8395 35.0774) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3C3C))
  (segment (start 112.8395 31.3944) (end 112.8395 32.5374) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3C7E))
  (segment (start 111.5225 30.0774) (end 112.8395 31.3944) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3BFA))
  (segment (start 106.9975 30.0774) (end 111.5225 30.0774) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3E97))
  (segment (start 106.1085 29.1884) (end 106.9975 30.0774) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3C93))
  (segment (start 106.1085 28.5884) (end 106.1085 29.1884) (width 0.35) (layer F.Cu) (net 143) (tstamp 5BCC3C09))
  (segment (start 130.6576 20.8684) (end 131.0871 21.2979) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB56))
  (segment (start 130.6576 19.7434) (end 130.6576 20.8684) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB53))
  (segment (start 136.2006 21.2979) (end 134.5946 21.2979) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB50))
  (segment (start 134.5946 21.2979) (end 135.6106 21.2979) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC3A70C))
  (segment (start 131.0871 21.2979) (end 134.5946 21.2979) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB4D))
  (segment (start 130.6576 18.6184) (end 130.6576 19.7434) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB4A))
  (segment (start 129.9081 17.8689) (end 130.6576 18.6184) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB47))
  (segment (start 127.7246 17.8689) (end 129.9081 17.8689) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BC5AB44))
  (segment (start 214.884 23.1521) (end 214.884 25.1181) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 246.517 22.880887) (end 247.269 22.128887) (width 1) (layer B.Cu) (net 147))
  (segment (start 246.517 24.2951) (end 246.517 22.880887) (width 1) (layer B.Cu) (net 147))
  (segment (start 247.269 22.128887) (end 247.269 14.6431) (width 1) (layer B.Cu) (net 147))
  (segment (start 175.133 35.306) (end 175.133 30.988) (width 1) (layer B.Cu) (net 147))
  (segment (start 175.133 30.988) (end 175.133 30.734) (width 1) (layer B.Cu) (net 147))
  (via (at 166.3065 28.1305) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 147))
  (segment (start 175.133 30.734) (end 172.5295 28.1305) (width 1) (layer B.Cu) (net 147))
  (segment (start 172.5295 28.1305) (end 169.037 28.1305) (width 1) (layer B.Cu) (net 147))
  (segment (start 169.037 28.1305) (end 166.3065 28.1305) (width 1) (layer B.Cu) (net 147))
  (segment (start 169.037 28.1305) (end 166.624 28.1305) (width 1) (layer B.Cu) (net 147))
  (segment (start 191.1731 -0.6858) (end 191.2366 -0.7493) (width 1) (layer F.Cu) (net 147))
  (segment (start 184.3456 -0.6858) (end 191.1731 -0.6858) (width 1) (layer F.Cu) (net 147))
  (segment (start 198.0946 -0.7493) (end 202.4761 -0.7493) (width 1) (layer F.Cu) (net 147))
  (segment (start 177.0126 -0.6858) (end 184.3456 -0.6858) (width 1) (layer F.Cu) (net 147))
  (segment (start 141.3256 8.8519) (end 141.7066 8.4709) (width 1) (layer F.Cu) (net 147))
  (segment (start 140.0556 17.9324) (end 141.3256 16.6624) (width 1) (layer F.Cu) (net 147))
  (segment (start 137.8966 18.9484) (end 138.9126 17.9324) (width 1) (layer F.Cu) (net 147))
  (segment (start 138.9126 17.9324) (end 140.0556 17.9324) (width 1) (layer F.Cu) (net 147))
  (segment (start 140.8176 19.6469) (end 137.8966 19.6469) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 137.8966 19.6469) (end 137.8966 18.9484) (width 1) (layer F.Cu) (net 147))
  (segment (start 137.8966 21.2979) (end 137.8966 19.6469) (width 1) (layer F.Cu) (net 147))
  (segment (start 195.1736 -0.5715) (end 195.3514 -0.7493) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 195.3514 -0.7493) (end 198.0946 -0.7493) (width 1) (layer F.Cu) (net 147))
  (segment (start 191.2366 -0.7493) (end 195.3514 -0.7493) (width 1) (layer F.Cu) (net 147))
  (segment (start 140.5128 19.6469) (end 137.8966 19.6469) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 142.367 14.7193) (end 141.3764 14.7193) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 141.3256 14.6685) (end 141.3256 8.8519) (width 1) (layer F.Cu) (net 147))
  (segment (start 141.3256 16.6624) (end 141.3256 14.6685) (width 1) (layer F.Cu) (net 147))
  (segment (start 141.4667 16.5213) (end 141.3256 16.6624) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 142.3416 16.5213) (end 141.4667 16.5213) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 141.4787 16.5093) (end 141.3256 16.6624) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 171.9453 12.3056) (end 170.7776 12.3056) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 170.6753 10.5156) (end 171.9453 10.5156) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 141.3256 14.6685) (end 141.3764 14.7193) (width 0.35) (layer F.Cu) (net 147))
  (segment (start 133.2306 14.3764) (end 133.1976 14.3434) (width 0.35) (layer F.Cu) (net 148) (tstamp 5BC5AB41) (status 30))
  (segment (start 134.4676 14.3764) (end 133.2306 14.3764) (width 0.35) (layer F.Cu) (net 148) (tstamp 5BC5AB3E) (status 20))
  (segment (start 133.1976 19.7434) (end 133.1976 14.3434) (width 0.7) (layer F.Cu) (net 148) (tstamp 5BC5AB3B))
  (segment (start 133.1976 14.3434) (end 134.3076 14.3434) (width 0.7) (layer F.Cu) (net 148) (tstamp 5BC5AB38))
  (segment (start 133.1976 19.7434) (end 131.9276 19.7434) (width 0.7) (layer F.Cu) (net 148) (tstamp 5BC5AB35))
  (segment (start 137.3961 14.3434) (end 138.1506 15.0979) (width 0.7) (layer F.Cu) (net 148) (tstamp 5BC5AB32))
  (segment (start 133.1976 14.3434) (end 137.3961 14.3434) (width 0.7) (layer F.Cu) (net 148) (tstamp 5BC5AB2F))
  (segment (start 128.4746 16.2814) (end 127.7246 16.2814) (width 0.35) (layer F.Cu) (net 149) (tstamp 5BC5AB17))
  (segment (start 130.6576 14.8184) (end 129.1946 16.2814) (width 0.35) (layer F.Cu) (net 149) (tstamp 5BC5AB1D))
  (segment (start 129.1946 16.2814) (end 128.4746 16.2814) (width 0.35) (layer F.Cu) (net 149) (tstamp 5BC5AB0E))
  (segment (start 130.6576 14.3434) (end 130.6576 14.8184) (width 0.35) (layer F.Cu) (net 149) (tstamp 5BC5AB14))
  (segment (start 129.3571 19.7739) (end 129.3876 19.7434) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB2C))
  (segment (start 127.5461 19.7739) (end 129.3571 19.7739) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB29))
  (segment (start 85.8393 3.0888) (end 85.8393 2.5908) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB26))
  (segment (start 129.9006 22.1819) (end 129.3876 21.6689) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB23))
  (segment (start 129.3876 19.7434) (end 129.3876 21.1709) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB20))
  (segment (start 133.0756 22.1869) (end 133.0706 22.1819) (width 0.35) (layer F.Cu) (net 150))
  (segment (start 135.3566 22.1869) (end 133.0756 22.1869) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB1A))
  (segment (start 133.0706 22.1819) (end 129.9006 22.1819) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC5AB11))
  (segment (start 135.1026 22.1819) (end 133.0706 22.1819) (width 0.35) (layer F.Cu) (net 150))
  (segment (start 188.4886 16.2687) (end 188.4816 16.2757) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 190.2206 16.2687) (end 188.4886 16.2687) (width 0.35) (layer F.Cu) (net 151))
  (segment (start 190.2136 13.9757) (end 190.2231 13.9852) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 188.4816 13.9757) (end 190.2136 13.9757) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 214.884 32.4231) (end 214.884 30.5181) (width 0.35) (layer F.Cu) (net 153) (tstamp 5BC4AFB3))
  (segment (start 183.9816 7.493) (end 184.023 7.5344) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 181.2462 7.493) (end 183.9816 7.493) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 176.3801 14.4932) (end 175.8569 14.4932) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 182.7302 9.5402) (end 181.4576 9.5402) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 175.4505 14.4932) (end 173.4091 14.4932) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 182.7404 9.5504) (end 182.7302 9.5402) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 175.8569 14.4932) (end 175.4505 14.4932) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 175.4563 14.4874) (end 175.4505 14.4932) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 183.073 9.5344) (end 181.4634 9.5344) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 183.244 10.5054) (end 187.5536 10.5054) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 183.073 9.5344) (end 183.073 10.3344) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 183.073 10.3344) (end 183.244 10.5054) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 172.7335 13.8176) (end 171.6405 13.8176) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 173.4091 14.4932) (end 172.7335 13.8176) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 172.7215 13.8056) (end 173.4091 14.4932) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 171.9453 13.8056) (end 172.7215 13.8056) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 189.5282 10.5054) (end 187.3758 10.5054) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 187.3758 10.5054) (end 186.7814 10.5054) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 187.5536 10.5054) (end 187.3758 10.5054) (width 0.35) (layer F.Cu) (net 156))
  (segment (start 172.4117 15.4432) (end 175.4091 15.4432) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 171.7117 15.4432) (end 172.4117 15.4432) (width 0.35) (layer F.Cu) (net 157))
  (segment (start 187.5536 9.53) (end 187.5282 9.5554) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 187.5536 7.9502) (end 187.5536 9.53) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 190.9268 9.5554) (end 190.9318 9.5504) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 187.5282 9.5554) (end 190.9268 9.5554) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 190.9438 9.5384) (end 190.9318 9.5504) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 190.9438 8.001) (end 190.9438 9.5384) (width 0.35) (layer F.Cu) (net 158))
  (segment (start 173.1659 12.4192) (end 173.1391 12.446) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 173.4453 12.4192) (end 173.4185 12.446) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 173.4453 10.5156) (end 173.4453 12.4192) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 181.1015 34.925) (end 179.5145 36.512) (width 1) (layer F.Cu) (net 160))
  (segment (start 183.642 34.925) (end 181.1015 34.925) (width 1) (layer F.Cu) (net 160))
  (via (at 183.642 37.6555) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 183.642 34.925) (end 183.642 37.6555) (width 1) (layer F.Cu) (net 160))
  (segment (start 183.642 37.6555) (end 181.6835 37.6555) (width 1) (layer B.Cu) (net 160))
  (segment (start 176.911 42.428) (end 181.6835 37.6555) (width 1) (layer B.Cu) (net 160))
  (segment (start 249.047 24.2951) (end 249.047 21.7651) (width 1) (layer B.Cu) (net 160) (tstamp 5BC76F31))
  (segment (start 246.7805 19.2151) (end 247.4595 18.5361) (width 1) (layer F.Cu) (net 161))
  (segment (start 244.0305 19.2151) (end 246.7805 19.2151) (width 1) (layer F.Cu) (net 161))
  (segment (start 175.3235 32.953) (end 179.5145 28.762) (width 1) (layer F.Cu) (net 161))
  (segment (start 179.5145 28.762) (end 179.5145 28.512) (width 1) (layer F.Cu) (net 161))
  (segment (start 175.3235 39.199) (end 175.3235 32.953) (width 1) (layer F.Cu) (net 161))
  (segment (start 115.443 68.072) (end 116.6495 69.2785) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 112.014 68.072) (end 115.443 68.072) (width 0.35) (layer F.Cu) (net 163))
  (via (at 116.6495 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (via (at 133.223 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (segment (start 116.6495 69.2785) (end 133.223 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 132.0165 68.072) (end 128.649 68.072) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 133.223 69.2785) (end 132.0165 68.072) (width 0.35) (layer F.Cu) (net 163))
  (via (at 145.9865 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (segment (start 133.223 69.2785) (end 145.9865 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 144.78 68.072) (end 141.349 68.072) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 145.9865 69.2785) (end 144.78 68.072) (width 0.35) (layer F.Cu) (net 163))
  (via (at 162.4965 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (segment (start 145.9865 69.2785) (end 162.4965 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 161.29 68.072) (end 157.859 68.072) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 162.4965 69.2785) (end 161.29 68.072) (width 0.35) (layer F.Cu) (net 163))
  (via (at 175.3235 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (segment (start 162.4965 69.2785) (end 175.3235 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 174.117 68.072) (end 170.559 68.072) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 175.3235 69.2785) (end 174.117 68.072) (width 0.35) (layer F.Cu) (net 163))
  (segment (start 103.5685 69.2785) (end 104.8385 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 104.8385 69.2785) (end 116.6495 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (via (at 101.854 68.072) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163))
  (segment (start 104.521 69.2785) (end 103.886 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 104.8385 69.2785) (end 104.521 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 103.0605 69.2785) (end 101.854 68.072) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 103.886 69.2785) (end 103.0605 69.2785) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 99.439 68.072) (end 101.854 68.072) (width 0.35) (layer F.Cu) (net 163))
  (via (at 105.537 70.612) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 106.807 69.342) (end 105.537 70.612) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 108.839 69.342) (end 106.807 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 117.983 70.612) (end 118.0465 70.6755) (width 0.35) (layer B.Cu) (net 164))
  (via (at 118.0465 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 105.537 70.612) (end 117.983 70.612) (width 0.35) (layer B.Cu) (net 164))
  (segment (start 119.38 69.342) (end 121.414 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 118.0465 70.6755) (end 119.38 69.342) (width 0.35) (layer F.Cu) (net 164))
  (via (at 134.874 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 118.0465 70.6755) (end 134.874 70.6755) (width 0.35) (layer B.Cu) (net 164))
  (segment (start 136.2075 69.342) (end 138.049 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 134.874 70.6755) (end 136.2075 69.342) (width 0.35) (layer F.Cu) (net 164))
  (via (at 147.447 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 134.874 70.6755) (end 147.447 70.6755) (width 0.35) (layer B.Cu) (net 164))
  (segment (start 148.7805 69.342) (end 150.749 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 147.447 70.6755) (end 148.7805 69.342) (width 0.35) (layer F.Cu) (net 164))
  (via (at 163.957 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 147.447 70.6755) (end 163.957 70.6755) (width 0.35) (layer B.Cu) (net 164))
  (segment (start 165.2905 69.342) (end 167.259 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 163.957 70.6755) (end 165.2905 69.342) (width 0.35) (layer F.Cu) (net 164))
  (via (at 176.7205 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 164))
  (segment (start 163.957 70.6755) (end 176.7205 70.6755) (width 0.35) (layer B.Cu) (net 164))
  (segment (start 178.054 69.342) (end 179.959 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 176.7205 70.6755) (end 178.054 69.342) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 104.902 68.84563) (end 104.902 66.9925) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 105.537 70.612) (end 105.537 69.48063) (width 0.35) (layer F.Cu) (net 164))
  (segment (start 105.537 69.48063) (end 104.902 68.84563) (width 0.35) (layer F.Cu) (net 164))
  (via (at 122.7455 33.6804) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171) (tstamp 5BCC4020))
  (segment (start 122.7455 33.6804) (end 122.7455 35.1014) (width 0.35) (layer F.Cu) (net 171) (tstamp 5BCC3E8E))
  (segment (start 122.7455 30.6084) (end 122.7455 33.6804) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BCC3E88))
  (segment (start 122.7455 35.1014) (end 122.7455 33.6804) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BCC3E8B))
  (via (at 124.1425 32.2834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 174) (tstamp 5BCC4014))
  (segment (start 124.1425 32.2834) (end 124.1425 35.1014) (width 0.35) (layer F.Cu) (net 174) (tstamp 5BCC3E4C))
  (segment (start 124.1425 30.6324) (end 124.1425 32.2834) (width 0.35) (layer B.Cu) (net 174) (tstamp 5BCC3E55))
  (segment (start 124.1425 35.0774) (end 124.1425 32.2834) (width 0.35) (layer B.Cu) (net 174) (tstamp 5BCC3E58))
  (segment (start 125.5395 35.1028) (end 125.5395 33.6804) (width 0.35) (layer F.Cu) (net 175) (tstamp 5BCC3E4F))
  (via (at 125.5395 33.6804) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 175) (tstamp 5BCC3FF6))
  (segment (start 125.5395 30.6204) (end 125.5395 33.6804) (width 0.35) (layer B.Cu) (net 175) (tstamp 5BCC3E52))
  (segment (start 125.5395 35.0894) (end 125.5395 33.6804) (width 0.35) (layer B.Cu) (net 175) (tstamp 5BCC3E5B))
  (segment (start 126.365 85.82) (end 126.365 91.186) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 125.415 83.82) (end 125.415 83.02) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 125.4125 83.0175) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 125.415 83.02) (end 125.4125 83.0175) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 152.8445 81.8515) (end 153.0985 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (via (at 103.886 43.6499) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 177) (tstamp 5BCC3FDE))
  (segment (start 100.5205 43.6499) (end 103.886 43.6499) (width 0.35) (layer F.Cu) (net 177) (tstamp 5BCC3E5E))
  (segment (start 154.305 83.786) (end 154.371 83.852) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 154.305 82.4865) (end 154.305 83.786) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 153.67 81.8515) (end 154.305 82.4865) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 152.8445 81.8515) (end 153.67 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 103.9495 43.5864) (end 103.886 43.6499) (width 0.35) (layer F.Cu) (net 177) (tstamp 5BCC3E61))
  (segment (start 105.4975 43.5864) (end 103.9495 43.5864) (width 0.35) (layer F.Cu) (net 177) (tstamp 5BCC3E64))
  (segment (start 141.7955 81.8515) (end 141.100011 81.156011) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 152.8445 81.8515) (end 141.7955 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 141.100011 81.156011) (end 139.569989 81.156011) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 139.569989 81.156011) (end 138.8745 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 138.8745 81.8515) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 108.091848 47.855748) (end 108.091848 59.746252) (width 0.35) (layer B.Cu) (net 177) (tstamp 5BCC3E67))
  (segment (start 94.06998 66.18622) (end 94.06998 82.250981) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 112.017011 81.156011) (end 112.7125 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 94.06998 82.250981) (end 94.742 82.923001) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 94.742 82.923001) (end 108.338999 82.923001) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 108.338999 82.923001) (end 110.105989 81.156011) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 110.105989 81.156011) (end 112.017011 81.156011) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 103.886 43.6499) (end 108.091848 47.855748) (width 0.35) (layer B.Cu) (net 177) (tstamp 5BCC3E6D))
  (segment (start 112.7125 81.8515) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 155.321 91.186) (end 155.321 85.852) (width 0.35) (layer B.Cu) (net 178))
  (segment (start 123.825 91.186) (end 123.825 90.17) (width 0.35) (layer F.Cu) (net 179) (status 10))
  (segment (start 123.825 88.38) (end 123.825 91.186) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 123.825 82.538) (end 123.825 83.566) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 123.825 83.566) (end 123.825 83.82) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 123.825 83.82) (end 123.825 88.38) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 123.825 83.046) (end 123.825 83.82) (width 0.35) (layer B.Cu) (net 179))
  (segment (start 152.654 91.059) (end 152.781 91.186) (width 0.35) (layer F.Cu) (net 180) (status 30))
  (segment (start 152.781 89.662) (end 152.781 88.38) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 152.781 91.186) (end 152.781 89.662) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 152.781 82.6015) (end 152.781 83.5025) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 152.781 83.5025) (end 152.781 89.662) (width 0.35) (layer B.Cu) (net 180))
  (segment (start 152.781 83.046) (end 152.781 83.5025) (width 0.35) (layer B.Cu) (net 180))
  (via (at 119.9515 33.6804) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 181) (tstamp 5BCC3FF3))
  (segment (start 119.9515 35.1014) (end 119.9515 33.6804) (width 0.35) (layer F.Cu) (net 181) (tstamp 5BCC3FDB))
  (segment (start 95.631 77.978) (end 95.631 78.74) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 95.631 77.978) (end 95.631 81.915) (width 0.35) (layer B.Cu) (net 181))
  (via (at 128.3335 33.6804) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 182) (tstamp 5BCC401A))
  (segment (start 128.3335 35.1148) (end 128.3335 33.6804) (width 0.35) (layer F.Cu) (net 182) (tstamp 5BCC3DC5))
  (segment (start 129.133499 34.480399) (end 129.133499 35.369399) (width 0.35) (layer B.Cu) (net 182) (tstamp 5BCC3DC2))
  (segment (start 128.3335 33.6804) (end 129.133499 34.480399) (width 0.35) (layer B.Cu) (net 182) (tstamp 5BCC3DBF))
  (via (at 127.127 104.775) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 118.42 103.03) (end 118.745 103.355) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 115.57 103.03) (end 118.42 103.03) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 136.835 103.03) (end 137.16 103.355) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 133.985 103.03) (end 136.835 103.03) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 144.94 103.03) (end 147.63 103.03) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 163.195 103.03) (end 165.97 103.03) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 176.765 103.03) (end 177.165 103.43) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 173.99 103.03) (end 176.765 103.03) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (via (at 107.95 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (via (at 177.165 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 119.38 104.610001) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 118.745 104.775) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 109.22 104.610001) (end 108.749999 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 165.97 103.03) (end 166.37 103.43) (width 0.35) (layer F.Cu) (net 183) (status 30))
  (segment (start 118.745 104.648) (end 118.745 103.355) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 107.95 104.648) (end 107.95 103.43) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 109.817001 104.648) (end 109.855 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 109.855 104.610001) (end 109.22 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 107.95 104.648) (end 109.817001 104.648) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 119.38 104.610001) (end 109.855 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 137.16 104.648) (end 137.16 103.355) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 148.082 103.482) (end 148.03 103.43) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 148.082 104.648) (end 148.082 103.482) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 166.37 104.648) (end 166.37 103.43) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 177.165 104.648) (end 177.165 103.43) (width 0.7) (layer F.Cu) (net 183))
  (segment (start 177.165 104.648) (end 107.95 104.648) (width 1) (layer B.Cu) (net 183))
  (segment (start 107.55 103.03) (end 107.95 103.43) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 104.775 103.03) (end 107.55 103.03) (width 0.35) (layer F.Cu) (net 183))
  (via (at 137.16 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 147.955 104.610001) (end 138.43 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (via (at 148.082 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (via (at 166.37 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (via (at 118.745 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 165.570001 104.610001) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 148.754999 104.610001) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 166.37 104.610001) (end 176.365001 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 137.16 104.610001) (end 126.8095 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 148.754999 104.610001) (end 165.570001 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 138.43 104.610001) (end 137.16 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 126.8095 104.610001) (end 119.38 104.610001) (width 0.7) (layer B.Cu) (net 183))
  (segment (start 243.459 33.7036) (end 245.0995 35.3441) (width 1) (layer F.Cu) (net 183))
  (segment (start 243.459 30.5816) (end 243.459 33.7036) (width 1) (layer F.Cu) (net 183))
  (segment (start 246.9795 35.3441) (end 245.0995 35.3441) (width 1) (layer F.Cu) (net 183))
  (segment (start 243.459 28.2956) (end 241.935 26.7716) (width 1) (layer F.Cu) (net 183))
  (segment (start 243.459 30.5816) (end 243.459 28.2956) (width 1) (layer F.Cu) (net 183))
  (segment (start 241.935 26.7716) (end 241.8969 26.7716) (width 1) (layer F.Cu) (net 183))
  (via (at 241.1984 26.0223) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 241.1984 26.0731) (end 241.1984 26.0223) (width 1) (layer F.Cu) (net 183))
  (segment (start 241.8969 26.7716) (end 241.1984 26.0731) (width 1) (layer F.Cu) (net 183))
  (segment (start 241.046 25.8699) (end 241.1984 26.0223) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 241.046 24.0919) (end 241.046 25.8699) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 228.6237 26.0223) (end 228.2681 25.6667) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 228.087 25.4856) (end 228.2681 25.6667) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 184.8104 46.6852) (end 169.0624 46.6852) (width 1) (layer B.Cu) (net 183))
  (segment (start 177.165 104.648) (end 181.525908 104.648) (width 1) (layer B.Cu) (net 183))
  (segment (start 188.142002 48.543602) (end 186.2836 46.6852) (width 1) (layer B.Cu) (net 183))
  (segment (start 188.142002 98.031906) (end 188.142002 48.543602) (width 1) (layer B.Cu) (net 183))
  (segment (start 181.525908 104.648) (end 188.142002 98.031906) (width 1) (layer B.Cu) (net 183))
  (segment (start 186.2836 46.6852) (end 184.8104 46.6852) (width 1) (layer B.Cu) (net 183))
  (segment (start 228.6237 26.0223) (end 229.9716 26.0223) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 228.087 25.4856) (end 228.6237 26.0223) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 192.1206 16.2687) (end 192.1206 17.2687) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 241.1984 26.0223) (end 229.9716 26.0223) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 182.9816 16.2687) (end 182.9816 15.1257) (width 0.35) (layer F.Cu) (net 185))
  (segment (start 182.3491 16.9012) (end 182.9816 16.2687) (width 0.35) (layer F.Cu) (net 185))
  (segment (start 173.4091 16.3932) (end 173.4091 17.8468) (width 0.35) (layer F.Cu) (net 185))
  (segment (start 213.614 32.7431) (end 213.614 30.5181) (width 0.35) (layer F.Cu) (net 186) (tstamp 5BC4AF47))
  (segment (start 214.884 27.0281) (end 218.059 27.0281) (width 0.35) (layer F.Cu) (net 186) (tstamp 5BC4AF44))
  (segment (start 213.614 28.2981) (end 214.884 27.0281) (width 0.35) (layer F.Cu) (net 186) (tstamp 5BC4AF41))
  (segment (start 213.614 30.5181) (end 213.614 28.2981) (width 0.35) (layer F.Cu) (net 186) (tstamp 5BC4AF3E))
  (segment (start 120.175713 30.2004) (end 128.7615 30.2004) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3E7F))
  (via (at 106.8705 31.4198) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 187) (tstamp 5BCC3FEA))
  (segment (start 111.5695 31.4124) (end 111.0435 30.8864) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3E82))
  (segment (start 111.5695 32.5374) (end 111.5695 31.4124) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3E85))
  (segment (start 128.6855 30.1244) (end 117.729 30.1244) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3BE2))
  (segment (start 128.7615 30.2004) (end 128.6855 30.1244) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3C21))
  (segment (start 118.11 30.1244) (end 128.11 30.1244) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3BE8))
  (segment (start 116.695787 30.1244) (end 116.3955 30.1244) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3C12))
  (segment (start 118.11 30.1244) (end 116.695787 30.1244) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3DC8))
  (segment (start 117.729 30.1244) (end 116.3955 30.1244) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3BFD))
  (segment (start 107.4039 30.8864) (end 106.8705 31.4198) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3B8B))
  (segment (start 111.0435 30.8864) (end 108.5469 30.8864) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3B9A))
  (segment (start 108.5469 30.8864) (end 107.4039 30.8864) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC3BA9))
  (segment (start 108.1659 30.1244) (end 106.8705 31.4198) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3B40))
  (segment (start 109.7915 30.1244) (end 108.1659 30.1244) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3B10))
  (segment (start 116.3955 30.1244) (end 109.7915 30.1244) (width 0.35) (layer B.Cu) (net 187) (tstamp 5BCC3B43))
  (segment (start 243.3955 36.5401) (end 242.1995 35.3441) (width 1) (layer F.Cu) (net 188))
  (segment (start 243.3955 40.2336) (end 243.3955 36.5401) (width 1) (layer F.Cu) (net 188))
  (segment (start 243.3955 40.2336) (end 240.7285 40.2336) (width 1) (layer F.Cu) (net 188))
  (segment (start 238.7545 38.2596) (end 240.7285 40.2336) (width 1) (layer F.Cu) (net 188))
  (segment (start 238.7545 34.8361) (end 238.7545 38.2596) (width 1) (layer F.Cu) (net 188))
  (segment (start 238.7545 34.8361) (end 235.842 34.8361) (width 1) (layer F.Cu) (net 188))
  (segment (start 238.7545 34.8361) (end 238.7545 41.4456) (width 1) (layer F.Cu) (net 188))
  (segment (start 241.1095 40.6146) (end 240.7285 40.2336) (width 0.5) (layer F.Cu) (net 188))
  (segment (start 241.1095 43.1546) (end 241.1095 41.3131) (width 0.5) (layer F.Cu) (net 188))
  (segment (start 241.1095 41.3131) (end 241.1095 40.6146) (width 0.5) (layer F.Cu) (net 188))
  (segment (start 241.1095 42.8371) (end 241.1095 41.3131) (width 0.5) (layer F.Cu) (net 188))
  (segment (start 127.877 48.6544) (end 127.865 48.6664) (width 0.35) (layer F.Cu) (net 189) (tstamp 5BCC3DDD))
  (segment (start 129.2225 48.6544) (end 127.877 48.6544) (width 0.35) (layer F.Cu) (net 189) (tstamp 5BCC3DDA))
  (segment (start 85.9536 13.952301) (end 85.948601 13.9573) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 85.9536 14.841301) (end 85.948601 14.8463) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 85.948601 13.9573) (end 85.948601 14.8463) (width 0.35) (layer B.Cu) (net 189))
  (via (at 85.9536 13.7668) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 189))
  (segment (start 85.9536 13.7668) (end 85.9536 14.841301) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 83.08517 10.9608) (end 82.7278 10.9608) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 85.948601 17.5133) (end 85.948601 18.597799) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 85.948601 14.8463) (end 85.948601 17.5133) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 85.948601 18.597799) (end 84.6836 19.8628) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 84.6836 19.8628) (end 82.3976 22.1488) (width 0.35) (layer B.Cu) (net 189))
  (segment (start 84.27897 10.9608) (end 85.9536 12.63543) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 85.9536 12.63543) (end 85.9536 13.7668) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 78.3463 10.9608) (end 83.4771 10.9608) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 83.4771 10.9608) (end 84.27897 10.9608) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 82.7278 10.9608) (end 83.4771 10.9608) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 109.9185 55.2374) (end 109.9185 55.7784) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC3C9F))
  (segment (start 112.8395 51.8414) (end 112.2045 51.8414) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC3EB8))
  (segment (start 109.9185 54.1274) (end 109.9185 55.2374) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC3CF3))
  (segment (start 112.2045 51.8414) (end 109.9185 54.1274) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC3CC3))
  (segment (start 121.89821 111.85349) (end 121.89821 112.45349) (width 0.35) (layer F.Cu) (net 192) (tstamp 5BCC3C4B))
  (segment (start 108.4015 53.5044) (end 107.5855 53.5044) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BCC3C39))
  (segment (start 107.5855 53.5044) (end 106.9855 53.5044) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BCC3D11))
  (segment (start 111.1395 50.7664) (end 108.4015 53.5044) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BCC3CD5))
  (segment (start 111.1395 50.1414) (end 111.1395 50.7664) (width 0.35) (layer F.Cu) (net 194) (tstamp 5BCC3C30))
  (segment (start 107.5975 52.0954) (end 110.3515 49.3414) (width 0.35) (layer F.Cu) (net 195) (tstamp 5BCC3C6F))
  (segment (start 110.3515 49.3414) (end 111.1395 49.3414) (width 0.35) (layer F.Cu) (net 195) (tstamp 5BCC3C54))
  (segment (start 106.9975 52.0954) (end 107.5975 52.0954) (width 0.35) (layer F.Cu) (net 195) (tstamp 5BCC3C9C))
  (segment (start 111.1395 48.5414) (end 109.7895 48.5414) (width 0.35) (layer F.Cu) (net 197) (tstamp 5BCC3CD8))
  (segment (start 107.6325 50.6984) (end 106.9975 50.6984) (width 0.35) (layer F.Cu) (net 197) (tstamp 5BCC3CEA))
  (segment (start 109.7895 48.5414) (end 107.6325 50.6984) (width 0.35) (layer F.Cu) (net 197) (tstamp 5BCC3D0B))
  (segment (start 111.1395 47.7414) (end 109.3195 47.7414) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC3C75))
  (segment (start 107.7595 49.3014) (end 106.9975 49.3014) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC3C84))
  (segment (start 109.3195 47.7414) (end 107.7595 49.3014) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC3E91))
  (segment (start 211.7115 32.7406) (end 211.714 32.7431) (width 0.35) (layer F.Cu) (net 201))
  (segment (start 210.353 32.7406) (end 211.7115 32.7406) (width 0.35) (layer F.Cu) (net 201))
  (segment (start 210.353 34.0106) (end 210.353 35.2906) (width 0.35) (layer F.Cu) (net 202))
  (segment (start 210.353 35.2906) (end 210.353 36.5606) (width 0.35) (layer F.Cu) (net 202))
  (segment (start 216.2075 35.2906) (end 216.281 35.2171) (width 0.35) (layer F.Cu) (net 202))
  (segment (start 210.353 35.2906) (end 216.2075 35.2906) (width 0.35) (layer F.Cu) (net 202))
  (segment (start 208.534 30.5181) (end 212.344 30.5181) (width 0.7) (layer F.Cu) (net 203) (tstamp 5BC4AF35))
  (segment (start 212.344 30.5181) (end 212.344 25.1181) (width 0.7) (layer F.Cu) (net 203) (tstamp 5BC4AF32))
  (segment (start 212.344 25.1181) (end 213.614 25.1181) (width 0.7) (layer F.Cu) (net 203) (tstamp 5BC4AF2F))
  (segment (start 111.1395 44.5414) (end 108.7145 44.5414) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC3CC9))
  (segment (start 107.7595 43.5864) (end 106.9975 43.5864) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC3C63))
  (segment (start 108.7145 44.5414) (end 107.7595 43.5864) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC3CB1))
  (segment (start 106.9975 42.1894) (end 107.6325 42.1894) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC3CE4))
  (segment (start 109.1845 43.7414) (end 111.1395 43.7414) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC3CE1))
  (segment (start 107.6325 42.1894) (end 109.1845 43.7414) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC3CA2))
  (segment (start 107.5975 40.7924) (end 106.9975 40.7924) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC3CFC))
  (segment (start 109.7465 42.9414) (end 107.5975 40.7924) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC3C42))
  (segment (start 111.1395 42.9414) (end 109.7465 42.9414) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC3C66))
  (segment (start 113.6395 39.3414) (end 111.4425 37.1444) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC3CB7))
  (segment (start 113.6395 40.4414) (end 113.6395 39.3414) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC3C90))
  (segment (start 111.4425 37.1444) (end 111.4425 36.6014) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC3E04))
  (segment (start 124.0155 55.1784) (end 124.0155 55.7784) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC3E19))
  (segment (start 124.0155 54.3924) (end 124.0155 55.1784) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC3E16))
  (segment (start 121.4645 51.8414) (end 124.0155 54.3924) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC3E13))
  (segment (start 120.8395 51.8414) (end 121.4645 51.8414) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC3E10))
  (segment (start 122.6185 55.2704) (end 122.6185 55.5244) (width 0.35) (layer F.Cu) (net 209) (tstamp 5BCC3E0A))
  (segment (start 122.6185 55.5244) (end 122.6185 55.7784) (width 0.35) (layer F.Cu) (net 209) (tstamp 5BCC3E1C))
  (segment (start 120.0395 52.7304) (end 120.0785 52.7304) (width 0.35) (layer F.Cu) (net 209) (tstamp 5BCC3E07))
  (segment (start 120.0785 52.7304) (end 122.6185 55.2704) (width 0.35) (layer F.Cu) (net 209) (tstamp 5BCC3E0D))
  (segment (start 120.0395 51.8414) (end 120.0395 52.7304) (width 0.35) (layer F.Cu) (net 209) (tstamp 5BCC3DCB))
  (segment (start 121.2215 55.1784) (end 121.2215 55.7784) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BCC3DCE))
  (segment (start 119.2395 53.1964) (end 121.2215 55.1784) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BCC3D2F))
  (segment (start 119.2395 51.8414) (end 119.2395 53.1964) (width 0.35) (layer F.Cu) (net 210) (tstamp 5BCC3D2C))
  (segment (start 119.8245 55.1904) (end 119.8245 55.7904) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3D26))
  (segment (start 118.4395 53.8054) (end 119.8245 55.1904) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3D23))
  (segment (start 118.4395 51.8414) (end 118.4395 53.8054) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3C69))
  (segment (start 118.4275 55.0164) (end 118.4275 55.7784) (width 0.35) (layer F.Cu) (net 212) (tstamp 5BCC3C51))
  (segment (start 117.6395 54.2284) (end 118.4275 55.0164) (width 0.35) (layer F.Cu) (net 212) (tstamp 5BCC3C87))
  (segment (start 117.6395 51.8414) (end 117.6395 54.2284) (width 0.35) (layer F.Cu) (net 212) (tstamp 5BCC3F63))
  (via (at 121.3485 32.2834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 163) (tstamp 5BCC4017))
  (segment (start 121.3485 35.1014) (end 121.3485 32.2834) (width 0.35) (layer F.Cu) (net 163) (tstamp 5BCC3F7E))
  (segment (start 121.3485 34.3027) (end 121.3485 34.544) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B1C))
  (segment (start 121.3485 32.2834) (end 121.3485 34.3027) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B49))
  (segment (start 101.054001 67.272001) (end 101.854 68.072) (width 0.35) (layer B.Cu) (net 163))
  (segment (start 121.3485 35.3822) (end 121.2977 35.433) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B58))
  (segment (start 110.5027 49.6951) (end 110.5027 61.0743) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B7F))
  (segment (start 121.2977 38.9001) (end 110.5027 49.6951) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B67))
  (segment (start 98.806101 62.610899) (end 98.806101 66.929101) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 121.2977 35.433) (end 121.2977 38.9001) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B6A))
  (segment (start 99.6823 61.7347) (end 98.806101 62.610899) (width 0.35) (layer B.Cu) (net 181) (tstamp 5BCC3B76))
  (segment (start 99.6823 61.722) (end 99.6823 61.7347) (width 0.35) (layer B.Cu) (net 181) (tstamp 5BCC3B73))
  (segment (start 121.3485 34.3027) (end 121.3485 35.3822) (width 0.35) (layer B.Cu) (net 163) (tstamp 5BCC3B52))
  (segment (start 119.8245 59.6519) (end 119.7229 59.7535) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BCC3B8E))
  (segment (start 119.8245 57.2904) (end 119.8245 59.6519) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BCC3BB2))
  (segment (start 113.0935 66.3829) (end 119.7229 59.7535) (width 0.35) (layer F.Cu) (net 164) (tstamp 5BCC3B94))
  (segment (start 122.7455 33.6804) (end 122.7455 34.798) (width 0.35) (layer B.Cu) (net 171) (tstamp 5BCC3BB5))
  (segment (start 246.750458 42.974642) (end 253.492 36.2331) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 246.451469 42.384631) (end 253.619 35.2171) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 98.679 64.389) (end 98.679 74.93) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 109.912689 49.396111) (end 109.912689 60.737211) (width 0.35) (layer B.Cu) (net 181) (tstamp 5BCC3B3A))
  (segment (start 98.679 74.93) (end 95.631 77.978) (width 0.35) (layer B.Cu) (net 181))
  (segment (start 119.9515 39.3573) (end 109.912689 49.396111) (width 0.35) (layer B.Cu) (net 181) (tstamp 5BCC3B4C))
  (segment (start 119.9515 33.6804) (end 119.9515 39.3573) (width 0.35) (layer B.Cu) (net 181) (tstamp 5BCC3B2E))
  (segment (start 129.0955 32.2834) (end 129.9845 33.1724) (width 0.35) (layer B.Cu) (net 184) (tstamp 5BCC3E70))
  (segment (start 129.9845 33.1724) (end 129.9845 35.2044) (width 0.35) (layer B.Cu) (net 184) (tstamp 5BCC3E73))
  (segment (start 128.06787 32.2834) (end 129.0955 32.2834) (width 0.35) (layer B.Cu) (net 184) (tstamp 5BCC3E76))
  (segment (start 126.9365 35.1148) (end 126.9365 32.2834) (width 0.35) (layer F.Cu) (net 184) (tstamp 5BCC3E79))
  (segment (start 126.9365 32.2834) (end 128.06787 32.2834) (width 0.35) (layer B.Cu) (net 184) (tstamp 5BCC3E7C))
  (via (at 126.9365 32.2834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 184) (tstamp 5BCC4023))
  (segment (start 111.11 103.03) (end 111.76 103.03) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 109.82201 101.74201) (end 111.11 103.03) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 100.15299 101.74201) (end 100.838 101.74201) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 100.041 101.854) (end 100.15299 101.74201) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 99.441 101.854) (end 100.041 101.854) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 100.838 101.74201) (end 109.82201 101.74201) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 170.18 102.555) (end 170.18 103.03) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 169.225 101.6) (end 170.18 102.555) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 157.849 101.6) (end 169.225 101.6) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 157.849 102.997) (end 159.512 102.997) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 159.352 102.997) (end 159.385 103.03) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 157.849 102.997) (end 159.352 102.997) (width 0.35) (layer F.Cu) (net 193))
  (segment (start 99.429 103.251) (end 100.029 103.251) (width 0.35) (layer F.Cu) (net 196))
  (segment (start 100.094 103.251) (end 100.029 103.251) (width 0.35) (layer F.Cu) (net 196))
  (segment (start 100.315 103.03) (end 100.094 103.251) (width 0.35) (layer F.Cu) (net 196))
  (segment (start 100.965 103.03) (end 100.315 103.03) (width 0.35) (layer F.Cu) (net 196))
  (segment (start 140.97 102.555) (end 140.97 103.03) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 140.015 101.6) (end 140.97 102.555) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 128.639 101.6) (end 140.015 101.6) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 130.0785 102.9335) (end 130.175 103.03) (width 0.35) (layer F.Cu) (net 199))
  (segment (start 128.651 102.9335) (end 130.0785 102.9335) (width 0.35) (layer F.Cu) (net 199))
  (via (at 118.5545 32.2834) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 213) (tstamp 5BCC3FFC))
  (segment (start 118.5545 35.1014) (end 118.5545 32.2834) (width 0.35) (layer F.Cu) (net 213) (tstamp 5BCC3E9D))
  (segment (start 100.2513 35.8673) (end 99.9871 36.1315) (width 0.35) (layer F.Cu) (net 214) (tstamp 5BCC3B2B))
  (segment (start 101.1773 36.1315) (end 101.7082 35.6006) (width 0.35) (layer F.Cu) (net 214) (tstamp 5BCC3B5B))
  (segment (start 99.9871 36.1315) (end 101.1773 36.1315) (width 0.35) (layer F.Cu) (net 214) (tstamp 5BCC3B61))
  (segment (start 100.9371 38.3315) (end 101.3337 37.9349) (width 0.35) (layer F.Cu) (net 215) (tstamp 5BCC3B0D))
  (segment (start 101.3337 37.9349) (end 101.3841 37.9349) (width 0.35) (layer F.Cu) (net 215) (tstamp 5BCC3B31))
  (segment (start 99.9871 38.3315) (end 100.9371 38.3315) (width 0.35) (layer F.Cu) (net 215) (tstamp 5BCC3B22))
  (segment (start 105.4855 37.9349) (end 101.3841 37.9349) (width 0.35) (layer F.Cu) (net 215) (tstamp 5BCC3B46))
  (via (at 116.928503 91.12853) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 116.185973 90.386) (end 116.928503 91.12853) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 115.824 90.386) (end 116.185973 90.386) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 116.928503 91.12853) (end 116.38947 91.12853) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 116.38947 91.12853) (end 114.173 93.345) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 114.173 93.345) (end 114.173 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 114.173 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 216))
  (via (at 135.382 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 134.582 90.386) (end 135.382 91.186) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 134.239 90.386) (end 134.582 90.386) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 134.533472 91.186) (end 132.842 92.877472) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 135.382 91.186) (end 134.533472 91.186) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 132.842 92.877472) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 132.842 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 216))
  (via (at 146.177 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 145.377 90.386) (end 146.177 91.186) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 144.996 90.386) (end 145.377 90.386) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 145.328472 91.186) (end 143.637 92.877472) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 146.177 91.186) (end 145.328472 91.186) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 143.637 92.877472) (end 143.637 96.52) (width 0.35) (layer B.Cu) (net 216))
  (via (at 164.592 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 163.792 90.386) (end 164.592 91.186) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 163.28 90.386) (end 163.792 90.386) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 163.743472 91.186) (end 162.052 92.877472) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 164.592 91.186) (end 163.743472 91.186) (width 0.35) (layer B.Cu) (net 216))
  (via (at 175.387 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 174.587 90.386) (end 175.387 91.186) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 174.075 90.386) (end 174.587 90.386) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 143.256 96.52) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 162.052 92.877472) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 143.637 96.52) (end 143.256 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 143.256 96.52) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 102.997 96.52) (end 104.267 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 104.267 96.52) (end 103.886 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 114.173 96.52) (end 104.267 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 105.372 90.386) (end 106.172 91.186) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 104.902 90.386) (end 105.372 90.386) (width 0.35) (layer F.Cu) (net 216))
  (via (at 106.172 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 216))
  (segment (start 101.6 94.996) (end 101.6 95.123) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 101.6 95.123) (end 102.997 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 99.314 92.837) (end 101.6 95.123) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 101.6 94.909472) (end 101.6 94.996) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 105.323472 91.186) (end 101.6 94.909472) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 106.172 91.186) (end 105.323472 91.186) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 171.577 96.52) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 172.847 95.25) (end 171.577 96.52) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 172.847 92.837) (end 172.847 95.25) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 174.498 91.186) (end 172.847 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 175.387 91.186) (end 174.498 91.186) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 99.314 92.837) (end 98.171 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.799 83.947) (end 95.831 83.915) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.831 83.915) (end 96.581 83.915) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.504 92.837) (end 94.234 91.567) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 96.52 92.837) (end 95.504 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 98.171 92.837) (end 96.52 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 96.52 92.837) (end 95.758 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.123 83.947) (end 94.996 83.947) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.123 83.947) (end 95.799 83.947) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.123 83.947) (end 94.488 83.947) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 94.488 83.947) (end 94.107 84.328) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.504 92.837) (end 94.107 91.44) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 95.758 92.837) (end 95.504 92.837) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 94.107 84.328) (end 94.107 91.44) (width 0.35) (layer B.Cu) (net 216))
  (segment (start 163.28 91.99) (end 163.28 91.986) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 161.671 93.599) (end 163.28 91.99) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 157.793 87.63) (end 157.793 91.499) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 156.21 86.047) (end 157.793 87.63) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 159.893 93.599) (end 161.671 93.599) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 157.793 91.499) (end 159.893 93.599) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 156.21 85.447) (end 156.21 86.047) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 115.786 91.986) (end 115.824 91.986) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 114.3 93.472) (end 115.786 91.986) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 112.141 93.472) (end 114.3 93.472) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 110.871 92.202) (end 112.141 93.472) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 110.363 86.233) (end 110.871 86.741) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 110.871 86.741) (end 110.871 92.202) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 110.363 85.447) (end 110.363 86.233) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 169.164 86.614) (end 168.783 86.233) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 168.783 86.233) (end 168.783 85.447) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 169.164 92.202) (end 169.164 86.614) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 170.561 93.599) (end 169.164 92.202) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 174.075 91.986) (end 174.075 91.99) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 172.466 93.599) (end 170.561 93.599) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 174.075 91.99) (end 172.466 93.599) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 139.573 85.447) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 139.954 92.964) (end 140.335 93.345) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 139.954 86.614) (end 139.954 92.964) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 139.954 86.614) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 143.383 93.599) (end 140.589 93.599) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 144.996 91.986) (end 143.383 93.599) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 140.335 93.345) (end 140.589 93.599) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 104.864 91.986) (end 104.902 91.986) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 97.79 85.447) (end 97.79 90.17) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 103.378 93.472) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 97.79 90.17) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 103.378 93.472) (end 104.864 91.986) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 127 85.471) (end 127 86.071) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 127 86.233) (end 127 85.471) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 128.778 88.011) (end 127 86.233) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 134.201 91.986) (end 132.588 93.599) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 130.048 93.599) (end 128.778 92.329) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 132.588 93.599) (end 130.048 93.599) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 128.778 92.329) (end 128.778 88.011) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 134.239 91.986) (end 134.201 91.986) (width 0.35) (layer F.Cu) (net 222))
  (via (at 102.2985 39.3954) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 223) (tstamp 5BCC400B))
  (segment (start 105.4975 39.3954) (end 102.2985 39.3954) (width 0.35) (layer F.Cu) (net 223) (tstamp 5BCC3CBA))
  (segment (start 94.9005 82.8605) (end 94.9005 86.8855) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 94.9005 81.1355) (end 94.9005 82.8605) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 93.472 87.464) (end 94.0505 86.8855) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 94.0505 86.8855) (end 94.9005 86.8855) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 93.472 89.789) (end 93.472 87.464) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 95.631 80.518) (end 95.518 80.518) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 95.518 80.518) (end 94.9005 81.1355) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 97.155 78.994) (end 95.631 80.518) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 97.155 76.811) (end 97.155 78.994) (width 0.35) (layer F.Cu) (net 224))
  (via (at 97.155 73.787) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 225))
  (segment (start 97.155 73.787) (end 97.155 75.311) (width 0.35) (layer F.Cu) (net 225))
  (segment (start 102.2985 42.3164) (end 100.5205 42.3164) (width 0.35) (layer F.Cu) (net 225) (tstamp 5BCC3CBD))
  (via (at 102.2985 42.3164) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 225) (tstamp 5BCC3FFF))
  (segment (start 105.4975 42.1894) (end 102.4255 42.1894) (width 0.35) (layer F.Cu) (net 225) (tstamp 5BCC3C57))
  (segment (start 102.4255 42.1894) (end 102.2985 42.3164) (width 0.35) (layer F.Cu) (net 225) (tstamp 5BCC3CFF))
  (segment (start 108.681859 46.359159) (end 104.6391 42.3164) (width 0.35) (layer B.Cu) (net 225) (tstamp 5BCC3C5A))
  (segment (start 95.885 72.517) (end 95.885 65.2056) (width 0.35) (layer B.Cu) (net 225))
  (segment (start 104.0765 64.596) (end 108.681859 59.990641) (width 0.35) (layer B.Cu) (net 225) (tstamp 5BCC3C8A))
  (segment (start 104.6391 42.3164) (end 102.2985 42.3164) (width 0.35) (layer B.Cu) (net 225) (tstamp 5BCC3C45))
  (segment (start 108.681859 59.990641) (end 108.681859 46.359159) (width 0.35) (layer B.Cu) (net 225) (tstamp 5BCC3C6C))
  (segment (start 97.155 73.787) (end 95.885 72.517) (width 0.35) (layer B.Cu) (net 225))
  (via (at 103.8225 40.7924) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 226) (tstamp 5BCC4008))
  (segment (start 105.4975 40.7924) (end 103.8225 40.7924) (width 0.35) (layer F.Cu) (net 226) (tstamp 5BCC3CF0))
  (segment (start 103.6955 40.6654) (end 103.8225 40.7924) (width 0.35) (layer F.Cu) (net 226) (tstamp 5BCC3C78))
  (segment (start 103.759 40.7289) (end 103.8225 40.7924) (width 0.35) (layer F.Cu) (net 226) (tstamp 5BCC3CE7))
  (segment (start 100.5085 40.7289) (end 103.759 40.7289) (width 0.35) (layer F.Cu) (net 226) (tstamp 5BCC3CAE))
  (via (at 97.417249 69.015042) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 226))
  (segment (start 97.155 70.509) (end 97.155 69.277291) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 97.155 69.277291) (end 97.417249 69.015042) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 97.417249 69.015042) (end 97.417249 64.761751) (width 0.35) (layer B.Cu) (net 226))
  (segment (start 104.95387 40.7924) (end 103.8225 40.7924) (width 0.35) (layer B.Cu) (net 226) (tstamp 5BCC3CB4))
  (segment (start 109.27187 60.48903) (end 109.27187 45.1104) (width 0.35) (layer B.Cu) (net 226) (tstamp 5BCC3C96))
  (segment (start 109.27187 45.1104) (end 104.95387 40.7924) (width 0.35) (layer B.Cu) (net 226) (tstamp 5BCC3CD2))
  (segment (start 94.9005 77.805) (end 94.9005 72.055) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 94.9465 72.009) (end 94.9005 72.055) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 97.155 72.009) (end 94.9465 72.009) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 94.0505 77.805) (end 94.9005 77.805) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 93.599 85.852) (end 92.075 87.376) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 93.599 78.2565) (end 93.599 85.852) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 92.075 89.801) (end 92.075 87.376) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 93.599 78.2565) (end 94.0505 77.805) (width 0.35) (layer F.Cu) (net 227))
  (segment (start 251.8665 29.4146) (end 252.6665 29.4146) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 239.8268 41.204609) (end 245.167691 41.204609) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 251.968 34.4043) (end 251.968 28.9963) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 245.167691 41.204609) (end 251.968 34.4043) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 251.2568 33.8963) (end 244.6655 40.4876) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 251.2568 30.8991) (end 251.2568 33.8963) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 248.8692 28.5115) (end 251.2568 30.8991) (width 0.35) (layer B.Cu) (net 229))
  (via (at 192.4304 11.176) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 229))
  (segment (start 192.4318 11.1746) (end 192.4304 11.176) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 192.4318 9.5504) (end 192.4318 11.1746) (width 0.35) (layer F.Cu) (net 229))
  (segment (start 237.5154 28.5115) (end 240.9444 28.5115) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 192.4304 11.176) (end 201.549 20.2946) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 240.9444 28.5115) (end 248.8692 28.5115) (width 0.35) (layer B.Cu) (net 229))
  (segment (start 111.4425 34.5014) (end 111.4425 35.1014) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B97))
  (segment (start 111.0787 34.1376) (end 111.4425 34.5014) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3BA3))
  (segment (start 103.7082 36.5506) (end 105.2322 36.5506) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B88))
  (segment (start 106.0322 36.5506) (end 106.3498 36.233) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B13))
  (segment (start 105.2322 36.5506) (end 106.0322 36.5506) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B25))
  (segment (start 106.3498 35.052) (end 107.2642 34.1376) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B34))
  (segment (start 106.3498 36.233) (end 106.3498 35.052) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B19))
  (segment (start 107.2642 34.1376) (end 111.0787 34.1376) (width 0.35) (layer F.Cu) (net 233) (tstamp 5BCC3B37))
  (segment (start 72.8406 52.1938) (end 72.8406 52.9438) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 71.7906 50.1552) (end 72.8406 51.2052) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 72.8406 51.2052) (end 72.8406 52.1938) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 70.8406 50.1552) (end 71.7906 50.1552) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 70.8279 52.0065) (end 70.8406 51.9938) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 66.9544 48.479802) (end 67.572798 49.0982) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 66.9544 46.5596) (end 66.9544 48.479802) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 67.572798 49.0982) (end 69.4055 49.0982) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 69.7357 49.4284) (end 69.7357 52.0065) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 69.7357 52.0065) (end 70.8279 52.0065) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 69.4055 49.0982) (end 69.7357 49.4284) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 69.1642 52.0065) (end 69.7357 52.0065) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 65.6591 51.955) (end 65.675 51.9709) (width 0.35) (layer F.Cu) (net 236))
  (segment (start 64.1858 51.955) (end 65.6591 51.955) (width 0.35) (layer F.Cu) (net 236))
  (segment (start 64.1604 51.9296) (end 64.1858 51.955) (width 0.35) (layer F.Cu) (net 236))
  (segment (start 64.1604 46.5596) (end 64.1604 51.9296) (width 0.35) (layer F.Cu) (net 236))
  (segment (start 67.675 50.984) (end 68.4403 50.2187) (width 0.35) (layer F.Cu) (net 237))
  (segment (start 67.675 52.9209) (end 67.675 50.984) (width 0.35) (layer F.Cu) (net 237))
  (segment (start 125.5014 57.2904) (end 125.476 57.265) (width 0.35) (layer F.Cu) (net 238) (tstamp 5BCC3B3D))
  (segment (start 68.4403 48.0187) (end 68.4403 46.5716) (width 0.35) (layer F.Cu) (net 238))
  (segment (start 70.8406 47.5114) (end 69.8627 46.5335) (width 0.35) (layer F.Cu) (net 239))
  (segment (start 70.8406 47.9552) (end 70.8406 47.5114) (width 0.35) (layer F.Cu) (net 239))
  (segment (start 108.7769 35.1014) (end 107.9754 35.9029) (width 0.35) (layer F.Cu) (net 242) (tstamp 5BCC3BBE))
  (via (at 107.9754 35.9029) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 242) (tstamp 5BCC400E))
  (segment (start 110.0455 35.1014) (end 108.7769 35.1014) (width 0.35) (layer F.Cu) (net 242) (tstamp 5BCC3BCD))

  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BC5A961) (hatch full 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 140.8176 6.3119) (xy 140.8176 11.2649) (xy 140.8811 15.6464) (xy 134.2771 15.6464) (xy 133.0706 13.6144)
        (xy 133.0706 6.3754) (xy 133.7056 6.3119)
      )
    )
  )
  (zone (net 154) (net_name "/5V PSU /SwE") (layer F.Cu) (tstamp 5BC5A95E) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 132.4991 6.3119) (xy 132.6261 15.2654) (xy 126.9111 15.2654) (xy 126.8476 11.0744) (xy 121.6406 11.0744)
        (xy 121.5771 6.3119)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (tstamp 5BC3B7FA) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.154 25.781) (xy 188.849 25.781) (xy 188.849 109.093) (xy 89.154 109.093)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (tstamp 5BC3B7F7) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.190634 25.908) (xy 188.885634 25.908) (xy 188.758634 109.093) (xy 89.063634 109.093)
      )
    )
  )
  (zone (net 202) (net_name "/3_3V PSU/HC_Plain") (layer F.Cu) (tstamp 5BC4ABC3) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 209.169 33.6931) (xy 216.789 33.6931) (xy 219.329 31.1531) (xy 219.202 27.4701) (xy 226.187 27.4701)
        (xy 226.441 40.1701) (xy 209.296 40.1701)
      )
    )
  )
  (zone (net 188) (net_name "/3_3V PSU/MC34063_HC_A") (layer F.Cu) (tstamp 5BC4ABC0) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 231.14 27.3431) (xy 231.14 42.2021) (xy 245.364 42.0751) (xy 245.3005 38.8366) (xy 241.173 38.9001)
        (xy 241.1095 27.2161)
      )
    )
  )
  (zone (net 203) (net_name "/3_3V PSU/HC_Plain_b") (layer F.Cu) (tstamp 5BC4ABBD) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 203.835 28.2321) (xy 212.852 28.2321) (xy 212.852 31.6611) (xy 215.9 31.5341) (xy 215.9 40.1701)
        (xy 203.708 40.1066) (xy 203.708 30.7086)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BCC30F3) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 120.3325 50.3174) (xy 112.7125 50.3174) (xy 112.7125 41.9354) (xy 121.0945 41.9354) (xy 121.0945 50.3174)
      )
    )
  )
)
