(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")

  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 1826)
    (zones 0)
    (modules 261)
    (nets 242)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 1)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.9)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (user_via 1.4 0.9)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.9 2.9)
    (pad_drill 1.9)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_fffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "../../../Desktop/"))
  )

  (net 0 "")
  (net 1 "Net-(C802-Pad1)")
  (net 2 "Net-(C702-Pad1)")
  (net 3 "Net-(C602-Pad1)")
  (net 4 "Net-(C502-Pad1)")
  (net 5 "Net-(C402-Pad1)")
  (net 6 "Net-(C302-Pad1)")
  (net 7 VCC)
  (net 8 GND)
  (net 9 "Net-(R808-Pad2)")
  (net 10 "Net-(R807-Pad2)")
  (net 11 "Net-(R806-Pad2)")
  (net 12 "Net-(R805-Pad2)")
  (net 13 ~enable_Shiftregister)
  (net 14 "Net-(R804-Pad2)")
  (net 15 "Net-(R803-Pad2)")
  (net 16 "Net-(R802-Pad2)")
  (net 17 "Net-(R801-Pad2)")
  (net 18 "Net-(R701-Pad2)")
  (net 19 "Net-(R702-Pad2)")
  (net 20 "Net-(R703-Pad2)")
  (net 21 "Net-(R704-Pad2)")
  (net 22 "Net-(R705-Pad2)")
  (net 23 "Net-(R706-Pad2)")
  (net 24 "Net-(R707-Pad2)")
  (net 25 "Net-(R708-Pad2)")
  (net 26 "Net-(R608-Pad2)")
  (net 27 "Net-(R607-Pad2)")
  (net 28 "Net-(R606-Pad2)")
  (net 29 "Net-(R605-Pad2)")
  (net 30 "Net-(R604-Pad2)")
  (net 31 "Net-(R603-Pad2)")
  (net 32 "Net-(R602-Pad2)")
  (net 33 "Net-(R601-Pad2)")
  (net 34 "Net-(R501-Pad2)")
  (net 35 "Net-(R502-Pad2)")
  (net 36 "Net-(R503-Pad2)")
  (net 37 "Net-(R504-Pad2)")
  (net 38 "Net-(R505-Pad2)")
  (net 39 "Net-(R506-Pad2)")
  (net 40 "Net-(R507-Pad2)")
  (net 41 "Net-(R508-Pad2)")
  (net 42 "Net-(R408-Pad2)")
  (net 43 "Net-(R407-Pad2)")
  (net 44 "Net-(R406-Pad2)")
  (net 45 "Net-(R405-Pad2)")
  (net 46 "Net-(R404-Pad2)")
  (net 47 "Net-(R403-Pad2)")
  (net 48 "Net-(R402-Pad2)")
  (net 49 "Net-(R401-Pad2)")
  (net 50 "Net-(R301-Pad2)")
  (net 51 "Net-(R302-Pad2)")
  (net 52 "Net-(R303-Pad2)")
  (net 53 "Net-(R304-Pad2)")
  (net 54 "Net-(R305-Pad2)")
  (net 55 "Net-(R306-Pad2)")
  (net 56 "Net-(R307-Pad2)")
  (net 57 "Net-(R308-Pad2)")
  (net 58 /Tubes/sheet5BB3E86D/e)
  (net 59 /Tubes/sheet5BB3E86D/d)
  (net 60 /Tubes/sheet5BB3E86D/g)
  (net 61 /Tubes/sheet5BB3E86D/f)
  (net 62 /Tubes/sheet5BB3E86D/a)
  (net 63 /Tubes/sheet5BB3E86D/c)
  (net 64 /Tubes/sheet5BB3E86D/b)
  (net 65 /Tubes/sheet5BB3E86D/Dot)
  (net 66 /Tubes/sheet5BB3E86C/Dot)
  (net 67 /Tubes/sheet5BB3E86C/b)
  (net 68 /Tubes/sheet5BB3E86C/c)
  (net 69 /Tubes/sheet5BB3E86C/a)
  (net 70 /Tubes/sheet5BB3E86C/f)
  (net 71 /Tubes/sheet5BB3E86C/g)
  (net 72 /Tubes/sheet5BB3E86C/d)
  (net 73 /Tubes/sheet5BB3E86C/e)
  (net 74 /Tubes/sheet5BB3BB93/e)
  (net 75 /Tubes/sheet5BB3BB93/d)
  (net 76 /Tubes/sheet5BB3BB93/g)
  (net 77 /Tubes/sheet5BB3BB93/f)
  (net 78 /Tubes/sheet5BB3BB93/a)
  (net 79 /Tubes/sheet5BB3BB93/c)
  (net 80 /Tubes/sheet5BB3BB93/b)
  (net 81 /Tubes/sheet5BB3BB93/Dot)
  (net 82 /Tubes/sheet5BB36ADE/Dot)
  (net 83 /Tubes/sheet5BB36ADE/b)
  (net 84 /Tubes/sheet5BB36ADE/c)
  (net 85 /Tubes/sheet5BB36ADE/a)
  (net 86 /Tubes/sheet5BB36ADE/f)
  (net 87 /Tubes/sheet5BB36ADE/g)
  (net 88 /Tubes/sheet5BB36ADE/d)
  (net 89 /Tubes/sheet5BB36ADE/e)
  (net 90 /Tubes/sheet5BB32DC8/e)
  (net 91 /Tubes/sheet5BB32DC8/d)
  (net 92 /Tubes/sheet5BB32DC8/g)
  (net 93 /Tubes/sheet5BB32DC8/f)
  (net 94 /Tubes/sheet5BB32DC8/a)
  (net 95 /Tubes/sheet5BB32DC8/c)
  (net 96 /Tubes/sheet5BB32DC8/b)
  (net 97 /Tubes/sheet5BB32DC8/Dot)
  (net 98 /Tubes/IV-9_Tube/Dot)
  (net 99 /Tubes/IV-9_Tube/b)
  (net 100 /Tubes/IV-9_Tube/c)
  (net 101 /Tubes/IV-9_Tube/a)
  (net 102 /Tubes/IV-9_Tube/f)
  (net 103 /Tubes/IV-9_Tube/g)
  (net 104 /Tubes/IV-9_Tube/d)
  (net 105 /Tubes/IV-9_Tube/e)
  (net 106 /Tubes/sheet5BB3E86C/Data_in)
  (net 107 /Tubes/sheet5BB36ADE/Data_in)
  (net 108 /Tubes/sheet5BB3BB93/Data_in)
  (net 109 /Tubes/sheet5BB32DC8/Data_in)
  (net 110 /Tubes/IV-9_Tube/Data_in)
  (net 111 "Net-(R902-Pad2)")
  (net 112 "Net-(R914-Pad2)")
  (net 113 "Net-(R916-Pad2)")
  (net 114 "Net-(R915-Pad2)")
  (net 115 "Net-(R913-Pad2)")
  (net 116 "Net-(R912-Pad2)")
  (net 117 "Net-(R911-Pad2)")
  (net 118 "Net-(R910-Pad2)")
  (net 119 "Net-(R909-Pad2)")
  (net 120 "Net-(R908-Pad2)")
  (net 121 "Net-(R907-Pad2)")
  (net 122 clk)
  (net 123 "Net-(R906-Pad2)")
  (net 124 "Net-(R905-Pad2)")
  (net 125 MISO)
  (net 126 MOSI)
  (net 127 "Net-(R904-Pad2)")
  (net 128 "Net-(R903-Pad2)")
  (net 129 Currentsensing_Tube_6)
  (net 130 Currentsensing_Tube_5)
  (net 131 Currentsensing_Tube_4)
  (net 132 Currentsensing_Tube_3)
  (net 133 Currentsensing_Tube_2)
  (net 134 Currentsensing_Tube_1)
  (net 135 /uC/XTAL2)
  (net 136 /uC/XTAL1)
  (net 137 "Net-(C901-Pad1)")
  (net 138 "Net-(R921-Pad2)")
  (net 139 "Net-(R918-Pad2)")
  (net 140 "Net-(R920-Pad2)")
  (net 141 "Net-(R919-Pad2)")
  (net 142 SCL)
  (net 143 SDA)
  (net 144 +12V)
  (net 145 "Net-(R1201-Pad1)")
  (net 146 "Net-(C1203-Pad1)")
  (net 147 "Net-(R1202-Pad2)")
  (net 148 "Net-(R1302-Pad2)")
  (net 149 "Net-(R1303-Pad1)")
  (net 150 "Net-(C1303-Pad1)")
  (net 151 "/5V PSU /SwE")
  (net 152 "Net-(D1303-Pad1)")
  (net 153 "Net-(Q1301-Pad3)")
  (net 154 "Net-(Q1302-Pad3)")
  (net 155 "Net-(C1306-Pad1)")
  (net 156 "Net-(D1401-Pad1)")
  (net 157 "Net-(F1401-Pad2)")
  (net 158 /Tubes/IV-9_Tube/Data_out)
  (net 159 reset_Shiftregister)
  (net 160 ~latch_Shiftregister)
  (net 161 "Net-(U503-Pad4)")
  (net 162 "Net-(U803-Pad4)")
  (net 163 "Net-(U703-Pad4)")
  (net 164 "Net-(U303-Pad4)")
  (net 165 "Net-(U603-Pad4)")
  (net 166 "Net-(U403-Pad4)")
  (net 167 Encoder_B)
  (net 168 "Net-(R1501-Pad1)")
  (net 169 "Net-(R1502-Pad1)")
  (net 170 Encoder_A)
  (net 171 Encoder_push)
  (net 172 "Net-(D202-Pad1)")
  (net 173 Dot)
  (net 174 "Net-(D201-Pad1)")
  (net 175 "Net-(D202-Pad2)")
  (net 176 "Net-(D201-Pad2)")
  (net 177 Tube_LED)
  (net 178 Rx)
  (net 179 +3V3)
  (net 180 Tx)
  (net 181 "/3_3V PSU/MC34063_Feedback")
  (net 182 "/3_3V PSU/SwE")
  (net 183 V_Bat)
  (net 184 "/3_3V PSU/MC34063_HC_A")
  (net 185 /uC/~Reset_ISP)
  (net 186 "Net-(R411-Pad2)")
  (net 187 "Net-(R933-Pad2)")
  (net 188 "Net-(R711-Pad2)")
  (net 189 "Net-(R811-Pad2)")
  (net 190 "Net-(R934-Pad2)")
  (net 191 "Net-(R935-Pad2)")
  (net 192 "Net-(R311-Pad2)")
  (net 193 "Net-(R936-Pad2)")
  (net 194 "Net-(R611-Pad2)")
  (net 195 "Net-(R511-Pad2)")
  (net 196 "Net-(R937-Pad2)")
  (net 197 "Net-(Q1201-Pad4)")
  (net 198 "/3_3V PSU/HC_Plain")
  (net 199 "/3_3V PSU/HC_Plain_b")
  (net 200 "Net-(R946-Pad2)")
  (net 201 "Net-(R945-Pad2)")
  (net 202 "Net-(R944-Pad2)")
  (net 203 "Net-(R943-Pad2)")
  (net 204 "Net-(R942-Pad2)")
  (net 205 "Net-(R941-Pad2)")
  (net 206 "Net-(R940-Pad2)")
  (net 207 "Net-(R939-Pad2)")
  (net 208 "Net-(R938-Pad2)")
  (net 209 "Net-(R908-Pad1)")
  (net 210 "Net-(R910-Pad1)")
  (net 211 "Net-(D1603-Pad1)")
  (net 212 "Net-(D1603-Pad2)")
  (net 213 /Tubes/IV-9_Tube/Tube_LED)
  (net 214 "Net-(D801-Pad2)")
  (net 215 "Net-(D401-Pad2)")
  (net 216 "Net-(D701-Pad2)")
  (net 217 "Net-(D601-Pad2)")
  (net 218 "Net-(D301-Pad2)")
  (net 219 "Net-(D501-Pad2)")
  (net 220 "Net-(R903-Pad1)")
  (net 221 "Net-(R1402-Pad2)")
  (net 222 Button_B)
  (net 223 Button_A)
  (net 224 "Net-(R1401-Pad2)")
  (net 225 feedback_Tube_PSU)
  (net 226 enable_Tube_PSU)
  (net 227 "Net-(R916-Pad1)")
  (net 228 "Net-(R1405-Pad2)")
  (net 229 Status_LED_a)
  (net 230 "Net-(D1502-Pad1)")
  (net 231 Status_LED_c)
  (net 232 Status_LED_b)
  (net 233 "Net-(D1501-Pad1)")
  (net 234 "Net-(D1501-Pad2)")
  (net 235 "Net-(D1502-Pad2)")
  (net 236 "Net-(U1001-Pad4)")
  (net 237 "Net-(U1001-Pad3)")
  (net 238 "Net-(U1001-Pad1)")
  (net 239 "Net-(R938-Pad1)")
  (net 240 "Net-(SW1401-Pad3)")
  (net 241 "Net-(Q1303-Pad3)")

  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net "/3_3V PSU/HC_Plain")
    (add_net "/3_3V PSU/HC_Plain_b")
    (add_net "/3_3V PSU/MC34063_Feedback")
    (add_net "/3_3V PSU/MC34063_HC_A")
    (add_net "/3_3V PSU/SwE")
    (add_net "/5V PSU /SwE")
    (add_net /Tubes/IV-9_Tube/Data_in)
    (add_net /Tubes/IV-9_Tube/Data_out)
    (add_net /Tubes/IV-9_Tube/Dot)
    (add_net /Tubes/IV-9_Tube/Tube_LED)
    (add_net /Tubes/IV-9_Tube/a)
    (add_net /Tubes/IV-9_Tube/b)
    (add_net /Tubes/IV-9_Tube/c)
    (add_net /Tubes/IV-9_Tube/d)
    (add_net /Tubes/IV-9_Tube/e)
    (add_net /Tubes/IV-9_Tube/f)
    (add_net /Tubes/IV-9_Tube/g)
    (add_net /Tubes/sheet5BB32DC8/Data_in)
    (add_net /Tubes/sheet5BB32DC8/Dot)
    (add_net /Tubes/sheet5BB32DC8/a)
    (add_net /Tubes/sheet5BB32DC8/b)
    (add_net /Tubes/sheet5BB32DC8/c)
    (add_net /Tubes/sheet5BB32DC8/d)
    (add_net /Tubes/sheet5BB32DC8/e)
    (add_net /Tubes/sheet5BB32DC8/f)
    (add_net /Tubes/sheet5BB32DC8/g)
    (add_net /Tubes/sheet5BB36ADE/Data_in)
    (add_net /Tubes/sheet5BB36ADE/Dot)
    (add_net /Tubes/sheet5BB36ADE/a)
    (add_net /Tubes/sheet5BB36ADE/b)
    (add_net /Tubes/sheet5BB36ADE/c)
    (add_net /Tubes/sheet5BB36ADE/d)
    (add_net /Tubes/sheet5BB36ADE/e)
    (add_net /Tubes/sheet5BB36ADE/f)
    (add_net /Tubes/sheet5BB36ADE/g)
    (add_net /Tubes/sheet5BB3BB93/Data_in)
    (add_net /Tubes/sheet5BB3BB93/Dot)
    (add_net /Tubes/sheet5BB3BB93/a)
    (add_net /Tubes/sheet5BB3BB93/b)
    (add_net /Tubes/sheet5BB3BB93/c)
    (add_net /Tubes/sheet5BB3BB93/d)
    (add_net /Tubes/sheet5BB3BB93/e)
    (add_net /Tubes/sheet5BB3BB93/f)
    (add_net /Tubes/sheet5BB3BB93/g)
    (add_net /Tubes/sheet5BB3E86C/Data_in)
    (add_net /Tubes/sheet5BB3E86C/Dot)
    (add_net /Tubes/sheet5BB3E86C/a)
    (add_net /Tubes/sheet5BB3E86C/b)
    (add_net /Tubes/sheet5BB3E86C/c)
    (add_net /Tubes/sheet5BB3E86C/d)
    (add_net /Tubes/sheet5BB3E86C/e)
    (add_net /Tubes/sheet5BB3E86C/f)
    (add_net /Tubes/sheet5BB3E86C/g)
    (add_net /Tubes/sheet5BB3E86D/Dot)
    (add_net /Tubes/sheet5BB3E86D/a)
    (add_net /Tubes/sheet5BB3E86D/b)
    (add_net /Tubes/sheet5BB3E86D/c)
    (add_net /Tubes/sheet5BB3E86D/d)
    (add_net /Tubes/sheet5BB3E86D/e)
    (add_net /Tubes/sheet5BB3E86D/f)
    (add_net /Tubes/sheet5BB3E86D/g)
    (add_net /uC/XTAL1)
    (add_net /uC/XTAL2)
    (add_net /uC/~Reset_ISP)
    (add_net Button_A)
    (add_net Button_B)
    (add_net Currentsensing_Tube_1)
    (add_net Currentsensing_Tube_2)
    (add_net Currentsensing_Tube_3)
    (add_net Currentsensing_Tube_4)
    (add_net Currentsensing_Tube_5)
    (add_net Currentsensing_Tube_6)
    (add_net Dot)
    (add_net Encoder_A)
    (add_net Encoder_B)
    (add_net Encoder_push)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1203-Pad1)")
    (add_net "Net-(C1303-Pad1)")
    (add_net "Net-(C1306-Pad1)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C602-Pad1)")
    (add_net "Net-(C702-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C901-Pad1)")
    (add_net "Net-(D1303-Pad1)")
    (add_net "Net-(D1401-Pad1)")
    (add_net "Net-(D1501-Pad1)")
    (add_net "Net-(D1501-Pad2)")
    (add_net "Net-(D1502-Pad1)")
    (add_net "Net-(D1502-Pad2)")
    (add_net "Net-(D1603-Pad1)")
    (add_net "Net-(D1603-Pad2)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad1)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D401-Pad2)")
    (add_net "Net-(D501-Pad2)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D701-Pad2)")
    (add_net "Net-(D801-Pad2)")
    (add_net "Net-(F1401-Pad2)")
    (add_net "Net-(Q1201-Pad4)")
    (add_net "Net-(Q1301-Pad3)")
    (add_net "Net-(Q1302-Pad3)")
    (add_net "Net-(Q1303-Pad3)")
    (add_net "Net-(R1201-Pad1)")
    (add_net "Net-(R1202-Pad2)")
    (add_net "Net-(R1302-Pad2)")
    (add_net "Net-(R1303-Pad1)")
    (add_net "Net-(R1401-Pad2)")
    (add_net "Net-(R1402-Pad2)")
    (add_net "Net-(R1405-Pad2)")
    (add_net "Net-(R1501-Pad1)")
    (add_net "Net-(R1502-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad2)")
    (add_net "Net-(R306-Pad2)")
    (add_net "Net-(R307-Pad2)")
    (add_net "Net-(R308-Pad2)")
    (add_net "Net-(R311-Pad2)")
    (add_net "Net-(R401-Pad2)")
    (add_net "Net-(R402-Pad2)")
    (add_net "Net-(R403-Pad2)")
    (add_net "Net-(R404-Pad2)")
    (add_net "Net-(R405-Pad2)")
    (add_net "Net-(R406-Pad2)")
    (add_net "Net-(R407-Pad2)")
    (add_net "Net-(R408-Pad2)")
    (add_net "Net-(R411-Pad2)")
    (add_net "Net-(R501-Pad2)")
    (add_net "Net-(R502-Pad2)")
    (add_net "Net-(R503-Pad2)")
    (add_net "Net-(R504-Pad2)")
    (add_net "Net-(R505-Pad2)")
    (add_net "Net-(R506-Pad2)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R508-Pad2)")
    (add_net "Net-(R511-Pad2)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad2)")
    (add_net "Net-(R605-Pad2)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R607-Pad2)")
    (add_net "Net-(R608-Pad2)")
    (add_net "Net-(R611-Pad2)")
    (add_net "Net-(R701-Pad2)")
    (add_net "Net-(R702-Pad2)")
    (add_net "Net-(R703-Pad2)")
    (add_net "Net-(R704-Pad2)")
    (add_net "Net-(R705-Pad2)")
    (add_net "Net-(R706-Pad2)")
    (add_net "Net-(R707-Pad2)")
    (add_net "Net-(R708-Pad2)")
    (add_net "Net-(R711-Pad2)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad2)")
    (add_net "Net-(R805-Pad2)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R807-Pad2)")
    (add_net "Net-(R808-Pad2)")
    (add_net "Net-(R811-Pad2)")
    (add_net "Net-(R902-Pad2)")
    (add_net "Net-(R903-Pad1)")
    (add_net "Net-(R903-Pad2)")
    (add_net "Net-(R904-Pad2)")
    (add_net "Net-(R905-Pad2)")
    (add_net "Net-(R906-Pad2)")
    (add_net "Net-(R907-Pad2)")
    (add_net "Net-(R908-Pad1)")
    (add_net "Net-(R908-Pad2)")
    (add_net "Net-(R909-Pad2)")
    (add_net "Net-(R910-Pad1)")
    (add_net "Net-(R910-Pad2)")
    (add_net "Net-(R911-Pad2)")
    (add_net "Net-(R912-Pad2)")
    (add_net "Net-(R913-Pad2)")
    (add_net "Net-(R914-Pad2)")
    (add_net "Net-(R915-Pad2)")
    (add_net "Net-(R916-Pad1)")
    (add_net "Net-(R916-Pad2)")
    (add_net "Net-(R918-Pad2)")
    (add_net "Net-(R919-Pad2)")
    (add_net "Net-(R920-Pad2)")
    (add_net "Net-(R921-Pad2)")
    (add_net "Net-(R933-Pad2)")
    (add_net "Net-(R934-Pad2)")
    (add_net "Net-(R935-Pad2)")
    (add_net "Net-(R936-Pad2)")
    (add_net "Net-(R937-Pad2)")
    (add_net "Net-(R938-Pad1)")
    (add_net "Net-(R938-Pad2)")
    (add_net "Net-(R939-Pad2)")
    (add_net "Net-(R940-Pad2)")
    (add_net "Net-(R941-Pad2)")
    (add_net "Net-(R942-Pad2)")
    (add_net "Net-(R943-Pad2)")
    (add_net "Net-(R944-Pad2)")
    (add_net "Net-(R945-Pad2)")
    (add_net "Net-(R946-Pad2)")
    (add_net "Net-(SW1401-Pad3)")
    (add_net "Net-(U1001-Pad1)")
    (add_net "Net-(U1001-Pad3)")
    (add_net "Net-(U1001-Pad4)")
    (add_net "Net-(U303-Pad4)")
    (add_net "Net-(U403-Pad4)")
    (add_net "Net-(U503-Pad4)")
    (add_net "Net-(U603-Pad4)")
    (add_net "Net-(U703-Pad4)")
    (add_net "Net-(U803-Pad4)")
    (add_net Rx)
    (add_net SCL)
    (add_net SDA)
    (add_net Status_LED_a)
    (add_net Status_LED_b)
    (add_net Status_LED_c)
    (add_net Tube_LED)
    (add_net Tx)
    (add_net VCC)
    (add_net V_Bat)
    (add_net clk)
    (add_net enable_Tube_PSU)
    (add_net feedback_Tube_PSU)
    (add_net reset_Shiftregister)
    (add_net ~enable_Shiftregister)
    (add_net ~latch_Shiftregister)
  )

  (net_class Antenna ""
    (clearance 0.3)
    (trace_width 1.40626)
    (via_dia 1.6)
    (via_drill 0.9)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BD1E001)
    (at 163.437 41.6814 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB71DFD)
    (attr smd)
    (fp_text reference R1308 (at 0 -1.65 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(Q1303-Pad3)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D1303-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BD13E8C)
    (at 163.51 38.0746 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB5A81D)
    (attr smd)
    (fp_text reference R1306 (at 0 -1.65 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(Q1301-Pad3)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5BB5DBAF) (tstamp 5BC3B6F2)
    (at 172.6184 38.5445 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5BB7D616/5BB7D6F8)
    (fp_text reference J1401 (at 2.794 -0.507 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.8 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 157 "Net-(F1401-Pad2)"))
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC3A49B)
    (at 151.229 33.0454)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB73C46/5BB4952F)
    (attr smd)
    (fp_text reference D1202 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_Vishay_IHLP-6767 (layer F.Cu) (tedit 5990349D) (tstamp 5BC4AF06)
    (at 167.767 55.2196 180)
    (descr "Inductor, Vishay, IHLP series, 17.0mmx17.0mm")
    (tags "inductor vishay ihlp smd")
    (path /5BB8D2EE/59D4542E)
    (attr smd)
    (fp_text reference L1301 (at 0 -9.509 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 10.009 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 10.3 -8.8) (end -10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.3 8.8) (end 10.3 -8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 8.8) (end 10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.3 -8.8) (end -10.3 8.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.609 8.609) (end 8.609 6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 8.609) (end 8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 6.46) (end -8.609 8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.609 -8.609) (end 8.609 -6.46) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -8.609) (end 8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start -8.609 -6.46) (end -8.609 -8.609) (layer F.SilkS) (width 0.15))
    (fp_line (start 8.509 -8.509) (end -8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start 8.509 8.509) (end 8.509 -8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 8.509) (end 8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_line (start -8.509 -8.509) (end -8.509 8.509) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 198 "/3_3V PSU/HC_Plain"))
    (pad 1 smd rect (at -8.1225 0 180) (size 3.825 12.32) (layers F.Cu F.Paste F.Mask)
      (net 184 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Vishay_IHLP-6767.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FBD) (tstamp 5BCC818F)
    (at 97.3455 47.8155 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CFEE)
    (attr smd)
    (fp_text reference R926 (at 2.667 -0.254 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 1.294 -0.762 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BCE025F)
    (at 92.1385 37.8765 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB6494F/5BC5953E)
    (attr smd)
    (fp_text reference U1001 (at 0 -3.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DS3231MZ (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 183 V_Bat))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(U1001-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(U1001-Pad3)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(U1001-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "GPS:NEO-6M Breakout" (layer F.Cu) (tedit 5BC38E9A) (tstamp 5BCDB1F2)
    (at 111.252 26.543 90)
    (path /5BB48B05/5BC4C86E)
    (fp_text reference J902 (at 0 4.31 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 3.31 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 -13) (end 1.27 13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 13) (end -34.29 13) (layer F.SilkS) (width 0.15))
    (fp_line (start -34.29 -13) (end 1.27 -13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 -7.62) (end 1.27 -6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -34.29 13) (end -34.29 -13) (layer F.SilkS) (width 0.15))
    (pad 4 thru_hole circle (at 0 3.81 90) (size 2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole circle (at 0 1.27 90) (size 2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 178 Rx))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 180 Tx))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 5 thru_hole circle (at -31.75 -10.16 90) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -31.75 10.16 90) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4E0EE) (tstamp 5BCE701A)
    (at 98.806 46.3035 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB6CF46)
    (attr smd)
    (fp_text reference R925 (at 3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC815F)
    (at 93.5235 33.274 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB6494F/5BB64C0D)
    (attr smd)
    (fp_text reference C1101 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCD2A96)
    (at 83.5152 29.1592 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4B0C4)
    (attr smd)
    (fp_text reference R1509 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(D1502-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC86F6)
    (at 84.963 29.1465 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4AE47)
    (attr smd)
    (fp_text reference R1508 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D1501-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B110)
    (at 162.559 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BB249C1)
    (attr smd)
    (fp_text reference U701 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC3ABC)
    (at 77.2287 31.1651 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D21)
    (attr smd)
    (fp_text reference R1603 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 229 Status_LED_a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BCC31F4)
    (at 71.9836 32.596 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BCA1CF3)
    (attr smd)
    (fp_text reference D1603 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D1603-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BC38ABF) (tstamp 5BCC3187)
    (at 74.7047 30.9651 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BCA1CEC)
    (attr smd)
    (fp_text reference Q1601 (at 0 -2.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 -90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D1603-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 229 Status_LED_a))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Encoder:STEC11B01 (layer F.Cu) (tedit 5BC4D20F) (tstamp 5BCC6F1B)
    (at 93.98 68.58 90)
    (path /5BBCA088/5BBCA305)
    (fp_text reference SW1501 (at 1.048 11.564999 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Rotary_Encoder_Switch (at 0 7.119999 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -18) (end 1 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -18) (end 1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start -1 -29) (end -1 -18) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3 -29) (end 3 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -29) (end 3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -28) (end -3 -29) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3 -11) (end -3 -28) (layer Dwgs.User) (width 0.15))
    (fp_line (start -3.5 -11) (end -3.5 -4) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -11) (end -3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start 3.5 -4) (end 3.5 -11) (layer Dwgs.User) (width 0.15))
    (fp_line (start -6 -4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 4) (end 6 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 4) (end 6 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -6 -4) (end -6 4) (layer F.SilkS) (width 0.15))
    (pad B thru_hole circle (at -2.54 -1.27 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 169 "Net-(R1502-Pad1)"))
    (pad C thru_hole circle (at 0 -1.27 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad A thru_hole circle (at 2.54 -1.27 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 168 "Net-(R1501-Pad1)"))
    (pad S2 thru_hole circle (at 2.54 1.27 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad S1 thru_hole circle (at -2.54 1.27 90) (size 1.75 1.75) (drill 1.1) (layers *.Cu *.Mask)
      (net 228 "Net-(R1405-Pad2)"))
    (pad "" thru_hole circle (at -5.842 0 225) (size 2.9 2.9) (drill 1.9) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.842 0 90) (size 2.9 2.9) (drill 1.9) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643BD)
    (at 85.725 73.394 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC55AEB)
    (attr smd)
    (fp_text reference R1404 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 Button_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BCA440F)
    (at 75.216 64.1525 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BB48B05/5BB3C67E)
    (attr smd)
    (fp_text reference SW901 (at -5.034 1.175 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 185 /uC/~Reset_ISP))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 185 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BC665EA)
    (at 75.2475 73.279 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BBCA088/5BC50C98)
    (attr smd)
    (fp_text reference SW1402 (at 0 -4.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1401-Pad2)"))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1401-Pad2)"))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 58724122) (tstamp 5BC665D0)
    (at 75.2475 82.3595 270)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (path /5BBCA088/5BC55ACC)
    (attr smd)
    (fp_text reference SW1403 (at 0 -4.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at 0 4.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.1 3.25) (end -3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 3.25) (end -3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.1 -3.25) (end 3.1 3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.1 -3.25) (end 3.1 -3.25) (layer F.Fab) (width 0.1))
    (fp_line (start -3.25 -1.25) (end -3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -1.25) (end 3.25 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 -3.4) (end -3.25 -2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -3.4) (end -3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 -2.75) (end 3.25 -3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.25 3.4) (end -3.25 2.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 3.4) (end -3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.25 2.75) (end 3.25 3.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 -3.65) (end -4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.65) (end -4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.65) (end 4.5 -3.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.5 3.65) (end 4.5 3.65) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 1.25 0) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at -2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.875 2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at 2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -2.875 -2 270) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R1402-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3SL-1002P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643F0)
    (at 74.422 88.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC52136)
    (attr smd)
    (fp_text reference R1401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643DF)
    (at 75.819 88.888 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC55ADB)
    (attr smd)
    (fp_text reference R1402 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(R1402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC36CC)
    (at 157.099 102.997)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC2388D)
    (attr smd)
    (fp_text reference R811 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R811-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC322E)
    (at 94.107 58.5844 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B465E)
    (attr smd)
    (fp_text reference R1501 (at 0 1.45 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 168 "Net-(R1501-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 167 Encoder_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC8A67E)
    (at 69.1642 52.7565 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4B0D2)
    (attr smd)
    (fp_text reference R1507 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 231 Status_LED_c))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC8A66E)
    (at 64.1858 52.705 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BC4AE55)
    (attr smd)
    (fp_text reference R1506 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 232 Status_LED_b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BC8618F)
    (at 70.8406 49.0552 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BC4B0BD)
    (attr smd)
    (fp_text reference D1502 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(D1502-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(D1502-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803) (tstamp 5BC86179)
    (at 68.4403 49.1187 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BCA1C95/5BC4AE40)
    (attr smd)
    (fp_text reference D1501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_error_red (at 0 1.55 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_line (start -1.95 -0.85) (end 1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 0.85) (end -1.95 -0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 0.85) (end -1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.95 -0.85) (end 1.95 0.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -0.7) (end 1 -0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 0.7) (end 1 0.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 0.6) (end -1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.6) (end 1 -0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.6) (end 1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.6) (end -1 0.6) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.8 -0.7) (end -1.8 0.7) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(D1501-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D1501-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BCA0D47)
    (at 66.675 52.9209)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BC4AE39)
    (attr smd)
    (fp_text reference Q1501 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 232 Status_LED_b))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(D1501-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BC84F27)
    (at 71.8406 52.9438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BCA1C95/5BC4B0B6)
    (attr smd)
    (fp_text reference Q1502 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(D1502-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 231 Status_LED_c))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB61104) (tstamp 5BC4AC69)
    (at 162.4424 35.3924)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB6719E)
    (attr smd)
    (fp_text reference Q1303 (at -2.286 0.127 90) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(Q1303-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(Q1301-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC7A14E)
    (at 260.858 28.448 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BB967B8)
    (attr smd)
    (fp_text reference R1309 (at 0 1.85 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.95 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 2.15 -1.1) (end -2.15 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.15 -1.1) (end 2.15 1.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.15 1.11) (end -2.15 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.15 1.11) (end 2.15 1.11) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1 1.07) (end 1 1.07) (layer B.SilkS) (width 0.12))
    (fp_line (start 1 -1.07) (end -1 -1.07) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end 1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end -1.6 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.7 0.7) (thickness 0.105)) (justify mirror))
    )
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 179 +3V3))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 225 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BC08)
    (at 104.139 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BB249C1)
    (attr smd)
    (fp_text reference U301 (at 0 7.366 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 158 /Tubes/IV-9_Tube/Data_out))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC6239E)
    (at 152.1638 12.2682 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB7D616/5BB7F33C)
    (attr smd)
    (fp_text reference C1401 (at 0 4.43 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BD20C2C)
    (at 164.3126 29.2278 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB7D616/5BB7DD24)
    (attr smd)
    (fp_text reference C1402 (at 0 4.43 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (fp_text user + (at -1.73 -0.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 4.43 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC62317)
    (at 139.6492 45.1866 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BB80A8D)
    (attr smd)
    (fp_text reference C1302 (at 0 4.43 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (fp_text user + (at -1.73 -0.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 4.43 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BD09DC5)
    (at 152.8572 37.5412)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49533)
    (attr smd)
    (fp_text reference C1202 (at 0 4.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5BCC7933)
    (at 129.3622 37.0586)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (path /5BB48B05/5BB4F230)
    (fp_text reference J901 (at 1.27 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 6.85) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 6.85) (end 4.35 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 6.41) (end 3.87 6.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 6.35) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 6.35) (end -1.27 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 185 /uC/~Reset_ISP))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 MOSI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 clk))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC9B64A)
    (at 93.2815 78.22 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F47F)
    (attr smd)
    (fp_text reference R1505 (at 0.647 5.334 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 228 "Net-(R1405-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC14464)
    (at 90.4875 78.244 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3C9)
    (attr smd)
    (fp_text reference R1504 (at 0.647 4.318 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 168 "Net-(R1501-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCB5CCC)
    (at 91.8845 78.22 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/59F6F3FA)
    (attr smd)
    (fp_text reference R1503 (at 0.647 4.826 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 169 "Net-(R1502-Pad1)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC3366)
    (at 95.504 58.5604 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5A0B4628)
    (attr smd)
    (fp_text reference R1502 (at 0 1.45 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 170 Encoder_A))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 169 "Net-(R1502-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BCC3336)
    (at 96.901 58.5724 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC36391)
    (attr smd)
    (fp_text reference R1405 (at 0 1.45 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 228 "Net-(R1405-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 171 Encoder_push))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module BatteryHolder:Battery_Holder (layer F.Cu) (tedit 5BC35560) (tstamp 5BCBEDAC)
    (at 93.04 51.2445 270)
    (path /5BB6494F/5BB6519B)
    (fp_text reference BT1101 (at -9 4.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Battery_Cell (at -2.75 -4.25 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.6 -3.5) (end -6.6 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.6 3.5) (end -6.6 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.5 -3.5) (end 6.5 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 3.5) (end 11 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.5 -3.5) (end 10.5 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 3.5) (end 11 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 -3.5) (end 10.5 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.5 -3.5) (end -6.5 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.5 3.5) (end -11 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 3.5) (end -11 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -11 -3.5) (end -6.5 -3.5) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -5 1.6 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 183 V_Bat))
    (pad 1 thru_hole circle (at 5 1.6 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 183 V_Bat))
    (pad 2 thru_hole circle (at 0 -1.6 270) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 GND))
  )

  (module Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL (layer F.Cu) (tedit 58826B0B) (tstamp 5BC574A7)
    (at 157.8932 43.434)
    (descr "Spindle Trimmer Potentiometer, Vishay TS53YL, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Vishay TS53YL")
    (path /5BB8D2EE/5BB85821)
    (attr smd)
    (fp_text reference RV1301 (at -4.87 1.016 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at -0.18 3.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 1.21 0) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 3.67 -2.75) (end -4.03 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.67 2.75) (end 3.67 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 2.75) (end 3.67 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.03 -2.75) (end -4.03 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.56 1.98) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -0.32) (end 2.56 0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.56 -2.56) (end 2.56 -1.98) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 0.83) (end -2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end -2.56 -0.83) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 2.56) (end 2.56 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.56 -2.56) (end 2.56 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.92 0.06) (end -0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.06) (end -0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 0.92) (end -0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.92) (end -0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 0.06) (end 0.06 0.92) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 0.06) (end 0.06 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.92 -0.06) (end 0.92 0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.06) (end 0.92 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 0.06 -0.92) (end 0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.92) (end 0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.06 -0.06) (end -0.06 -0.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.92 -0.06) (end -0.06 -0.06) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
    (pad 3 smd rect (at 2.75 1.15) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 149 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at -2.75 0) (size 2 1.3) (layers F.Cu F.Mask)
      (net 181 "/3_3V PSU/MC34063_Feedback"))
    (pad 1 smd rect (at 2.75 -1.15) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 148 "Net-(R1302-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Vishay_TS53YL.wrl
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BC4AEBA)
    (at 151.384 48.2016 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB8D2EE/5BB49532)
    (attr smd)
    (fp_text reference U1301 (at 0 -3.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 181 "/3_3V PSU/MC34063_Feedback"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C1303-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 182 "/3_3V PSU/SwE"))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer B.Cu) (tedit 5905D8F5) (tstamp 5BCC32F6)
    (at 85.852 54.328 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5BB9689B)
    (attr smd)
    (fp_text reference D1304 (at 0 2 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DZ_5.1V (at 0 -1.75 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -2.65 -1.1) (end -2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end -2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end 2.65 -1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end 2.65 1.1) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end 0.25 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end -0.35 0) (layer B.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end 1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end -1.65 0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end -1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end 1.65 -0.8) (layer B.Fab) (width 0.1))
    (fp_line (start -2.55 -1) (end 1.75 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end -2.55 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.75 1) (end -2.55 1) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 2 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 225 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC4AE7E)
    (at 152.0444 42.5316 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB81889)
    (attr smd)
    (fp_text reference C1301 (at 1.0915 -1.7145 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC7C948)
    (at 186.5884 34.6736 90)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB7D616/5BB7D945)
    (attr smd)
    (fp_text reference D1401 (at 0 -2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value D_Schottky (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 90) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(D1401-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Fuse Holder:Nano Fuse Holder" (layer F.Cu) (tedit 5BB4B4A4) (tstamp 5BC4C751)
    (at 179.9844 31.242 90)
    (path /5BB7D616/5BB7D87A)
    (fp_text reference F1401 (at -3.25 -3.25 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Fuse (at 0.5 3.25 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.5 -2.5) (end 5.5 -2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 -2.5) (end 5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 2.5) (end -5.5 2.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.5 2.5) (end -5.5 -2.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4 0 180) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(D1401-Pad1)"))
    (pad 2 smd rect (at 4 0 180) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(F1401-Pad2)"))
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC32BE)
    (at 68.834 74.1299 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5BC52E3C)
    (attr smd)
    (fp_text reference C1404 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 223 Button_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC328E)
    (at 68.846 75.7174 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5BC55AF2)
    (attr smd)
    (fp_text reference C1405 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 222 Button_B))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC643CE)
    (at 85.852 70.092 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BBCA088/5BC52D73)
    (attr smd)
    (fp_text reference R1403 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 Button_A))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(R1401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC55271)
    (at 116.326886 19.651202 270)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BC3F0BE)
    (attr smd)
    (fp_text reference D904 (at 0 -2 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0 270) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5BC359F7) (tstamp 5BC3C5BE)
    (at 101.473 98.806)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BCE9EA1)
    (attr smd)
    (fp_text reference Q203 (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 177 Tube_LED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC7C46C)
    (at 101.346 100.965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BCF2CFF)
    (attr smd)
    (fp_text reference R203 (at 0 1.45) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 10k (at 0 -1.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 177 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB40647)
    (at 145.034 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3BB9E/5BB249BA)
    (fp_text reference U602 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B218)
    (at 159.004 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249EB)
    (attr smd)
    (fp_text reference R707 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R707-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B248)
    (at 160.401 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F2)
    (attr smd)
    (fp_text reference R706 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R706-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B278)
    (at 161.798 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249F9)
    (attr smd)
    (fp_text reference R705 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R705-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2A8)
    (at 163.195 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249C8)
    (attr smd)
    (fp_text reference R704 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R704-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B2D8)
    (at 164.592 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249CF)
    (attr smd)
    (fp_text reference R703 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R703-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B308)
    (at 165.989 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249D6)
    (attr smd)
    (fp_text reference R702 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R702-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B338)
    (at 157.607 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249E4)
    (attr smd)
    (fp_text reference R708 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R708-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B368)
    (at 140.97 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249E4)
    (attr smd)
    (fp_text reference R608 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /Tubes/sheet5BB3BB93/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B398)
    (at 142.367 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249EB)
    (attr smd)
    (fp_text reference R607 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /Tubes/sheet5BB3BB93/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3C8)
    (at 143.764 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F2)
    (attr smd)
    (fp_text reference R606 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /Tubes/sheet5BB3BB93/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B3F8)
    (at 145.161 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249F9)
    (attr smd)
    (fp_text reference R605 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 /Tubes/sheet5BB3BB93/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B428)
    (at 146.558 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249C8)
    (attr smd)
    (fp_text reference R604 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /Tubes/sheet5BB3BB93/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D171)
    (at 147.955 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249CF)
    (attr smd)
    (fp_text reference R603 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /Tubes/sheet5BB3BB93/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D0DE)
    (at 149.352 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249D6)
    (attr smd)
    (fp_text reference R602 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 /Tubes/sheet5BB3BB93/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4B8)
    (at 128.397 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249E4)
    (attr smd)
    (fp_text reference R508 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B4E8)
    (at 129.794 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249EB)
    (attr smd)
    (fp_text reference R507 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B518)
    (at 131.191 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F2)
    (attr smd)
    (fp_text reference R506 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B548)
    (at 132.588 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249F9)
    (attr smd)
    (fp_text reference R505 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B578)
    (at 133.985 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249C8)
    (attr smd)
    (fp_text reference R504 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5A8)
    (at 135.382 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249CF)
    (attr smd)
    (fp_text reference R503 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B5D8)
    (at 136.779 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249D6)
    (attr smd)
    (fp_text reference R502 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B608)
    (at 111.76 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249E4)
    (attr smd)
    (fp_text reference R408 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B638)
    (at 113.157 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249EB)
    (attr smd)
    (fp_text reference R407 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B668)
    (at 114.554 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F2)
    (attr smd)
    (fp_text reference R406 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B698)
    (at 115.951 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249F9)
    (attr smd)
    (fp_text reference R405 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6C8)
    (at 117.348 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249C8)
    (attr smd)
    (fp_text reference R404 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B6F8)
    (at 118.745 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249CF)
    (attr smd)
    (fp_text reference R403 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.627 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B728)
    (at 120.142 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249D6)
    (attr smd)
    (fp_text reference R402 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B758)
    (at 99.187 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249E4)
    (attr smd)
    (fp_text reference R308 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R308-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B788)
    (at 100.584 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249EB)
    (attr smd)
    (fp_text reference R307 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R307-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7B8)
    (at 101.981 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F2)
    (attr smd)
    (fp_text reference R306 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R306-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B7E8)
    (at 103.378 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249F9)
    (attr smd)
    (fp_text reference R305 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R305-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B818)
    (at 104.775 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249C8)
    (attr smd)
    (fp_text reference R304 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R304-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B848)
    (at 106.172 84.709 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249CF)
    (attr smd)
    (fp_text reference R303 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R303-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B878)
    (at 107.569 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249D6)
    (attr smd)
    (fp_text reference R302 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R302-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8A8)
    (at 178.5747 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249D6)
    (attr smd)
    (fp_text reference R802 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B908)
    (at 177.1777 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249CF)
    (attr smd)
    (fp_text reference R803 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B938)
    (at 175.7807 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249C8)
    (attr smd)
    (fp_text reference R804 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B968)
    (at 174.3837 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F9)
    (attr smd)
    (fp_text reference R805 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B998)
    (at 172.9987 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249F2)
    (attr smd)
    (fp_text reference R806 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B9C8)
    (at 171.6017 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249EB)
    (attr smd)
    (fp_text reference R807 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B8D8)
    (at 170.1927 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249E4)
    (attr smd)
    (fp_text reference R808 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8544)
    (at 104.902 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB247DF/5BB7D8C2)
    (attr smd)
    (fp_text reference D301 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D301-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8530)
    (at 115.824 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB32DD3/5BB7D8C2)
    (attr smd)
    (fp_text reference D401 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF851C)
    (at 134.239 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB36AE9/5BB7D8C2)
    (attr smd)
    (fp_text reference D501 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF8508)
    (at 144.996 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3BB9E/5BB7D8C2)
    (attr smd)
    (fp_text reference D601 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84F4)
    (at 174.075 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E89F/5BB7D8C2)
    (attr smd)
    (fp_text reference D701 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(D701-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5) (tstamp 5BCF84E0)
    (at 163.28 91.186 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (path /5BB1F5A4/5BB3E878/5BB7D8C2)
    (attr smd)
    (fp_text reference D801 (at 0 -1.25 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_blue (at 0 1.35 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.65) (end 1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.65) (end -1.45 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 0.65) (end -1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.65) (end 1.45 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.5) (end 0.8 -0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 0.5) (end 0.8 0.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 -0.2) (end 0.15 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 0.2) (end -0.15 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 0) (end 0.15 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.2 -0.2) (end -0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -1.3 -0.5) (end -1.3 0.5) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 213 /Tubes/IV-9_Tube/Tube_LED))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D801-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B9FF)
    (at 127 84.721 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC38F55)
    (attr smd)
    (fp_text reference R510 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D501-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8240)
    (at 76.466 37.973 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BCA1C95/5BCA1D07)
    (attr smd)
    (fp_text reference R1609 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D1603-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Crystals:Crystal_SMD_5032-2pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C) (tstamp 5BCC81FC)
    (at 107.3319 33.274)
    (descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (path /5BB48B05/5BB3A603)
    (attr smd)
    (fp_text reference Y901 (at 0 -2.8) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Crystal (at 0 2.8) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.093333 0) (layer F.Adhes) (width 0.186667))
    (fp_circle (center 0 0) (end 0.213333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.333333 0) (layer F.Adhes) (width 0.133333))
    (fp_circle (center 0 0) (end 0.4 0) (layer F.Adhes) (width 0.1))
    (fp_line (start 3.1 -1.9) (end -3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.1 1.9) (end 3.1 -1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 1.9) (end 3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.1 -1.9) (end -3.1 1.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.05 1.8) (end 2.7 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.05 -1.8) (end -3.05 1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.7 -1.8) (end -3.05 -1.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 0.6) (end -1.5 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 -1.4) (end -2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -2.5 1.4) (end -2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 1.6) (end -2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 1.6) (end -2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 1.4) (end 2.3 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.5 -1.4) (end 2.5 1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -1.6) (end 2.5 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 -1.6) (end 2.3 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.85 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (pad 1 smd rect (at -1.85 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_5032-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC81C2)
    (at 101.0659 50.673)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC662F3)
    (attr smd)
    (fp_text reference R943 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(R943-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC32321) (tstamp 5BCC8516)
    (at 101.6889 45.72 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B3DE)
    (attr smd)
    (fp_text reference C906 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC1B200) (tstamp 5BCC84E6)
    (at 120.8659 45.835 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BC6B34B)
    (attr smd)
    (fp_text reference C907 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48) (tstamp 5BCC8452)
    (at 111.3559 45.276 270)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (path /5BB48B05/5BC060C8)
    (attr smd)
    (fp_text reference U902 (at 0 -7.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ATmega32-16AU (at 0 7.45 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.175 -4.6) (end -6.45 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.175 -5.175) (end -5.175 -4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 -4) (end -4 -5) (layer F.Fab) (width 0.15))
    (fp_line (start -5 5) (end -5 -4) (layer F.Fab) (width 0.15))
    (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.15))
    (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.15))
    (fp_line (start -4 -5) (end 5 -5) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 44 smd rect (at -4 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R942-Pad2)"))
    (pad 43 smd rect (at -3.2 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R941-Pad2)"))
    (pad 42 smd rect (at -2.4 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R940-Pad2)"))
    (pad 41 smd rect (at -1.6 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R939-Pad2)"))
    (pad 40 smd rect (at -0.8 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R938-Pad2)"))
    (pad 39 smd rect (at 0 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at 0.8 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 37 smd rect (at 1.6 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R919-Pad2)"))
    (pad 36 smd rect (at 2.4 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (pad 35 smd rect (at 3.2 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R907-Pad2)"))
    (pad 34 smd rect (at 4 -5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R933-Pad2)"))
    (pad 33 smd rect (at 5.7 -4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R934-Pad2)"))
    (pad 32 smd rect (at 5.7 -3.2 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R935-Pad2)"))
    (pad 31 smd rect (at 5.7 -2.4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R936-Pad2)"))
    (pad 30 smd rect (at 5.7 -1.6 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R937-Pad2)"))
    (pad 29 smd rect (at 5.7 -0.8 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C901-Pad1)"))
    (pad 28 smd rect (at 5.7 0 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 27 smd rect (at 5.7 0.8 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 26 smd rect (at 5.7 1.6 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(R946-Pad2)"))
    (pad 25 smd rect (at 5.7 2.4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R945-Pad2)"))
    (pad 24 smd rect (at 5.7 3.2 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(R944-Pad2)"))
    (pad 23 smd rect (at 5.7 4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R903-Pad2)"))
    (pad 22 smd rect (at 4 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 21 smd rect (at 3.2 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(R943-Pad2)"))
    (pad 20 smd rect (at 2.4 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R911-Pad2)"))
    (pad 19 smd rect (at 1.6 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R912-Pad2)"))
    (pad 18 smd rect (at 0.8 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at 0 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 16 smd rect (at -0.8 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R910-Pad2)"))
    (pad 15 smd rect (at -1.6 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R909-Pad2)"))
    (pad 14 smd rect (at -2.4 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R908-Pad2)"))
    (pad 13 smd rect (at -3.2 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R918-Pad2)"))
    (pad 12 smd rect (at -4 5.7) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 11 smd rect (at -5.7 4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (pad 10 smd rect (at -5.7 3.2 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R921-Pad2)"))
    (pad 9 smd rect (at -5.7 2.4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R920-Pad2)"))
    (pad 8 smd rect (at -5.7 1.6 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (pad 7 smd rect (at -5.7 0.8 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (pad 6 smd rect (at -5.7 0 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -5.7 -0.8 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at -5.7 -1.6 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R913-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R906-Pad2)"))
    (pad 2 smd rect (at -5.7 -3.2 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -5.7 -4 270) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4D506) (tstamp 5BCC83F0)
    (at 121.7429 43.688 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5FA00)
    (attr smd)
    (fp_text reference R938 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R938-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(R938-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC83C0)
    (at 121.7549 42.291 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F9F9)
    (attr smd)
    (fp_text reference R939 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R939-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8390)
    (at 121.7429 40.894 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D25)
    (attr smd)
    (fp_text reference R940 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R940-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 232 Status_LED_b))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8360)
    (at 121.7429 39.497 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC61D1E)
    (attr smd)
    (fp_text reference R941 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 enable_Tube_PSU))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R941-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8330)
    (at 121.7429 38.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC64046)
    (attr smd)
    (fp_text reference R942 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R942-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 231 Status_LED_c))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8300)
    (at 106.0069 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC685A2)
    (attr smd)
    (fp_text reference R944 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(R944-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 Button_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC82D0)
    (at 107.4039 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D766)
    (attr smd)
    (fp_text reference R945 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 Button_B))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R945-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC82A0)
    (at 108.8009 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5D75F)
    (attr smd)
    (fp_text reference R946 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(R946-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BD0A773)
    (at 135.2956 38.6715 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D469D9)
    (attr smd)
    (fp_text reference R1203 (at 0.828 3.429 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R1202-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463) (tstamp 5BC4791C)
    (at 198.501 48.784 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (path /5BB8D2EE/5BC34D02)
    (attr smd)
    (fp_text reference C1206 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 0.87) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 0.87) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end -1.75 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -0.88) (end 1.75 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-669_LFPAK_ThermalVias-2 (layer F.Cu) (tedit 59217BD0) (tstamp 5BC4AB42)
    (at 144.653 55.0341 180)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT669 Thermical Vias Power-SO8")
    (path /5BB8D2EE/5BC31987)
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference Q1201 (at 1.085 -5.26 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PHPT60406NY (at 1.085 5.58 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.66 4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.66 4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end -3.66 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.75 -4.75) (end 5.75 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.855 2.5) (end 1.855 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 2.5) (end 1.855 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -2.5) (end -2.245 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.855 -2.5) (end -2.245 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 1.855 -2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 2.2) (end 1.855 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start 3.155 -2.2) (end 3.155 2.2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -1.65) (end -2.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -2.245 -2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -2.15) (end -3.245 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.4) (end -2.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 -0.85) (end -3.245 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 -0.85) (end -3.245 -0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.85) (end -2.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 0.4) (end -3.245 0.85) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 0.4) (end -3.245 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 2.15) (end -2.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.245 1.7) (end -3.245 2.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.245 1.7) (end -3.245 1.7) (layer F.Fab) (width 0.1))
    (fp_line (start -2.345 -2.6) (end -2.345 -2.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.345 2.4) (end -2.345 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 2.6) (end -1.155 2.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.355 -2.6) (end -1.205 -2.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 thru_hole rect (at 4.745 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 4 smd rect (at -2.835 1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(Q1201-Pad4)") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 0.445 0 90) (size 4.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 2.645 0 90) (size 4.7 1.55) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.835 0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 198 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.835 -1.91 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 198 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 2 smd rect (at -2.835 -0.64 90) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask)
      (net 198 "/3_3V PSU/HC_Plain") (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.895 -0.6 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.895 -1.88 90) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 0 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 1.045 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at -0.655 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 0.195 -1.15 180) (size 0.6 0.9) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 -1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 4.745 1.75 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at -0.005 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 1.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 thru_hole rect (at 3.995 -3.5 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (pad 5 smd rect (at 2.245 0 90) (size 9 6.5) (layers B.Cu B.Paste B.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC39110)
    (at 121.8845 30.9245)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E24)
    (attr smd)
    (fp_text reference D902 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC390F7)
    (at 121.892 26.3525)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54DD6)
    (attr smd)
    (fp_text reference D903 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_6.3x6.3_H3 (layer F.Cu) (tedit 5990349C) (tstamp 5BD0A7AB)
    (at 139.5916 28.5115 180)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (path /5BB73C46/5BB49522)
    (attr smd)
    (fp_text reference L1201 (at 0 -4.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uH (at 0 4.45 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0 0) (end 1.91 1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_arc (start 0 0) (end -1.91 -1.91) (angle 90) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -3.15) (end -3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 3.15) (end -3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -3.15) (end 3.15 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -3.4) (end -3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.4) (end 3.75 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.4) (end 3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.4) (end -3.75 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.3 -3.2) (end 3.3 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -3.2) (end 3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -1.5) (end -3.3 -3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 3.2) (end -3.3 1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.2) (end -3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 1.5) (end 3.3 3.2) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.75 0 180) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 151 "/5V PSU /SwE"))
    (pad 1 smd rect (at -2.75 0 180) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC341FE) (tstamp 5BC4AAE5)
    (at 152.769 52.8066)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/59D455EA)
    (attr smd)
    (fp_text reference C1303 (at 3.81 1.016) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330pF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(C1303-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMC (layer F.Cu) (tedit 5864295D) (tstamp 5BC4AAA7)
    (at 153.416 59.0006 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (path /5BB8D2EE/5BB49523)
    (attr smd)
    (fp_text reference D1301 (at 0 -4.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value VSSC8L45-M3/9AT (at 0 4.2 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.8 -3.25) (end 3.6 -3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.8 3.25) (end 3.6 3.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -4.9 3.35) (end -4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 3.35) (end -4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.9 -3.35) (end 4.9 3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.9 -3.35) (end 4.9 -3.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 -3.1) (end 3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 3.1) (end -3.55 -3.1) (layer F.Fab) (width 0.1))
    (fp_line (start 3.55 3.1) (end -3.55 3.1) (layer F.Fab) (width 0.1))
    (fp_line (start -4.8 3.25) (end -4.8 -3.25) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 198 "/3_3V PSU/HC_Plain"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC86C6)
    (at 104.6099 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F7)
    (attr smd)
    (fp_text reference R903 (at 0 9.853 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R903-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(R903-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8696)
    (at 118.0719 35.0005 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6F0)
    (attr smd)
    (fp_text reference R904 (at 0 9.853 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R904-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8666)
    (at 116.6749 35.0005 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E9)
    (attr smd)
    (fp_text reference R905 (at 0 9.853 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R905-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8636)
    (at 101.0659 52.07)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6FE)
    (attr smd)
    (fp_text reference R902 (at 0 9.853) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(R902-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC477AA)
    (at 183.294 50.9651)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/5BC3EDF8)
    (attr smd)
    (fp_text reference C1307 (at 0 4.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC4CD6D) (tstamp 5BCC393C)
    (at 127.127 105.513 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC237F5)
    (attr smd)
    (fp_text reference C504 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC4CCAA) (tstamp 5BCC390C)
    (at 128.524 105.525 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC237F5)
    (attr smd)
    (fp_text reference C604 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC38DC)
    (at 157.734 105.525 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC237F5)
    (attr smd)
    (fp_text reference C704 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC38AC)
    (at 156.337 105.525 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BC237F5)
    (attr smd)
    (fp_text reference C804 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC4CD4A) (tstamp 5BCC387C)
    (at 99.314 105.525 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC237F5)
    (attr smd)
    (fp_text reference C404 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC384C)
    (at 97.917 105.525 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BC237F5)
    (attr smd)
    (fp_text reference C304 (at 0 -1.5 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Inductors_SMD:L_1206 (layer F.Cu) (tedit 58307BE8) (tstamp 5BC4776F)
    (at 180.7845 55.7276)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (path /5BB8D2EE/5BC1CECA)
    (attr smd)
    (fp_text reference L1202 (at 0 -2.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BLM31KN601SN1L (at 0 2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.07) (end 1 -1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 1.07) (end -1 1.07) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.2 -1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end -2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 1.2) (end 2.2 1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -1.2) (end 2.2 -1.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 184 "/3_3V PSU/MC34063_HC_A"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8606)
    (at 114.5159 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5F151)
    (attr smd)
    (fp_text reference R937 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R937-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC37EC)
    (at 127.901 102.9335)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BC2388D)
    (attr smd)
    (fp_text reference R511 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R511-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC37BC)
    (at 127.889 101.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC2388D)
    (attr smd)
    (fp_text reference R611 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R611-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC85D6)
    (at 115.9129 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5CD4F)
    (attr smd)
    (fp_text reference R936 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R936-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC375C)
    (at 98.679 103.251)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC2388D)
    (attr smd)
    (fp_text reference R311 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 Currentsensing_Tube_1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R311-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCF0B13)
    (at 117.3099 55.868 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC5AA8D)
    (attr smd)
    (fp_text reference R935 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R935-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 Currentsensing_Tube_3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8576)
    (at 121.7295 53.6575 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC58906)
    (attr smd)
    (fp_text reference R934 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 Currentsensing_Tube_4))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R934-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC369C)
    (at 157.099 101.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC2388D)
    (attr smd)
    (fp_text reference R711 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R711-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8546)
    (at 121.7429 52.197 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC568B6)
    (attr smd)
    (fp_text reference R933 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R933-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 Currentsensing_Tube_5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC363C)
    (at 98.691 101.854)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC2388D)
    (attr smd)
    (fp_text reference R411 (at 0 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R411-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 Currentsensing_Tube_2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AA70)
    (at 149.799 53.1266)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC25F71)
    (attr smd)
    (fp_text reference R1311 (at 0 -1.65) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(Q1201-Pad4)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 182 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AA40)
    (at 155.194 48.3616 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BC1FD35)
    (attr smd)
    (fp_text reference R1310 (at 0 -1.65 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 182 "/3_3V PSU/SwE"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB60FC6) (tstamp 5BCC8726)
    (at 113.1189 32.893)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BE4C)
    (attr smd)
    (fp_text reference R917 (at 0.9405 -2.159 -270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 /uC/~Reset_ISP))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC8756)
    (at 113.8809 35.0005 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3BA78)
    (attr smd)
    (fp_text reference R913 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R913-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 185 /uC/~Reset_ISP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB8C91E)
    (at 97.79 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BC38F55)
    (attr smd)
    (fp_text reference R310 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D301-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AF48)
    (at 108.966 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB247DF/5BB249DD)
    (attr smd)
    (fp_text reference R301 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R301-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B068)
    (at 121.539 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB249DD)
    (attr smd)
    (fp_text reference R401 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC2EA1B) (tstamp 5BC3AF78)
    (at 110.363 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB32DD3/5BC38F55)
    (attr smd)
    (fp_text reference R410 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D401-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B008)
    (at 138.176 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB249DD)
    (attr smd)
    (fp_text reference R501 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BB02)
    (at 156.21 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BC38F55)
    (attr smd)
    (fp_text reference R810 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D801-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3AFD8)
    (at 179.9717 84.7224 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB249DD)
    (attr smd)
    (fp_text reference R801 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7BA70)
    (at 168.783 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E89F/5BC38F55)
    (attr smd)
    (fp_text reference R710 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(D701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3D07E)
    (at 150.6855 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB249DD)
    (attr smd)
    (fp_text reference R601 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /Tubes/sheet5BB3BB93/Dot))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BB7B8ED)
    (at 139.573 84.697 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BC38F55)
    (attr smd)
    (fp_text reference R610 (at 0 -1.45 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D601-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC3B038)
    (at 167.386 84.697 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BB3E878/5BB249DD)
    (attr smd)
    (fp_text reference R701 (at 0 -1.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 25R (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R701-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC3E015)
    (at 155.321 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBD4644)
    (fp_text reference D201 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 174 "Net-(D201-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 176 "Net-(D201-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B) (tstamp 5BC23268)
    (at 126.365 91.186 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (path /5BB1F5A4/5BBEEFA5)
    (fp_text reference D202 (at 1.27 -2.96 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_Dot_red (at 1.27 2.96 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.7 -2.25) (end -1.15 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.25) (end 3.7 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2.25) (end 3.7 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 -2.25) (end -1.15 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.29 1.08) (end -0.29 1.236) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.29 -1.236) (end -0.29 -1.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.23 -1.16619) (end -0.23 1.16619) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 2.77 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end 0.229039 1.08) (angle -87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end 0.229039 -1.08) (angle 87.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 1.235516) (angle -108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.29 -1.235516) (angle 108.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -0.23 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 175 "Net-(D202-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 172 "Net-(D202-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC2C5E)
    (at 68.846 77.0509 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBE40CE)
    (attr smd)
    (fp_text reference R201 (at 0.012 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 Dot))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804) (tstamp 5BC23018)
    (at 152.781 81.8515 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBD471C)
    (attr smd)
    (fp_text reference R202 (at 0 -1.397 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 176 "Net-(D201-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5BC3033A) (tstamp 5BC22FD6)
    (at 123.825 81.788 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB1F5A4/5BBEEFB2)
    (attr smd)
    (fp_text reference R204 (at 0 -1.27 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 1k (at 0 -1.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.25 -0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.25 -0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end -1.25 -0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.25 0.7) (end 1.25 0.7) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.68) (end 0.5 0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.68) (end -0.5 -0.68) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer B.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 175 "Net-(D202-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22B05)
    (at 155.321 84.852 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBDEA3D)
    (attr smd)
    (fp_text reference Q201 (at 0 2.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 173 Dot))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 174 "Net-(D201-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E) (tstamp 5BC22AF0)
    (at 126.365 84.82 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB1F5A4/5BBEEFBB)
    (attr smd)
    (fp_text reference Q202 (at 0 2.5 270) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BSS138 (at 0 -2.5 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -1.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end -1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end -1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end 1.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end 1.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 172 "Net-(D202-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 173 Dot))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB75445) (tstamp 5BCC2CBE)
    (at 80.3275 46.6859 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46FC)
    (attr smd)
    (fp_text reference C1501 (at -0.115 -3.302 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 167 Encoder_B))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5BB7544A) (tstamp 5BCC2C8E)
    (at 81.7245 46.7099 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0B46B9)
    (attr smd)
    (fp_text reference C1502 (at -0.115 -2.921 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 170 Encoder_A))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7) (tstamp 5BCC2CEE)
    (at 83.1215 46.6979 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BBCA088/5A0DEE19)
    (attr smd)
    (fp_text reference C1503 (at 0 1.5 90) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 100nF (at 0 -1.5 90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 90) (layer B.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start -0.8 -0.4) (end -0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end -0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end 0.8 0.4) (layer B.Fab) (width 0.1))
    (fp_line (start -0.35 0.6) (end 0.35 0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.35 -0.6) (end -0.35 -0.6) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end 1.4 0.65) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.65) (end -1.4 -0.65) (layer B.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 171 Encoder_push))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC7DDB)
    (at 101.0659 42.164)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D785)
    (attr smd)
    (fp_text reference R909 (at -3.06 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R909-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 177 Tube_LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BBE7DB5)
    (at 104.9573 94.119204 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB247DF/5BB249BA)
    (fp_text reference U302 (at 7.124204 -4.3733 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 /Tubes/IV-9_Tube/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /Tubes/IV-9_Tube/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /Tubes/IV-9_Tube/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /Tubes/IV-9_Tube/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 /Tubes/IV-9_Tube/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 /Tubes/IV-9_Tube/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 /Tubes/IV-9_Tube/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 98 /Tubes/IV-9_Tube/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EAE)
    (at 107.95 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB247DF/5BB24A0E)
    (attr smd)
    (fp_text reference R309 (at -4.6355 -0.0635 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E8E)
    (at 137.16 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB36AE9/5BB24A0E)
    (attr smd)
    (fp_text reference R509 (at -4.7105 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EEE)
    (at 148.03 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3BB9E/5BB24A0E)
    (attr smd)
    (fp_text reference R609 (at -4.6355 -0.0115 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6EDE)
    (at 177.165 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E89F/5BB24A0E)
    (attr smd)
    (fp_text reference R809 (at -4.6355 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BC301D8) (tstamp 5BBD6ECE)
    (at 118.745 100.255 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB32DD3/5BB24A0E)
    (attr smd)
    (fp_text reference R409 (at -4.647 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BBD6E9E)
    (at 166.37 100.33 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB1F5A4/5BB3E878/5BB24A0E)
    (attr smd)
    (fp_text reference R709 (at -4.6355 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1.2R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD3416)
    (at 112.28 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BBBEA7E)
    (attr smd)
    (fp_text reference C403 (at -0.012 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD33E5)
    (at 113.55 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB26FB6)
    (attr smd)
    (fp_text reference C402 (at 2.044 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF88)
    (at 113.665 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BBB5EFE)
    (attr smd)
    (fp_text reference U403 (at 0 3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U403-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(R411-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEF6C)
    (at 142.875 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BBB5EFE)
    (attr smd)
    (fp_text reference U603 (at 0 3.2385 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R611-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U603-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BB97560)
    (at 102.87 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB247DF/5BBB5EFE)
    (attr smd)
    (fp_text reference U303 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U303-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R311-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEC4)
    (at 172.085 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BBB5EFE)
    (attr smd)
    (fp_text reference U703 (at -0.0635 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R711-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U703-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEEA8)
    (at 161.29 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E878/5BBB5EFE)
    (attr smd)
    (fp_text reference U803 (at 0 3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U803-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R811-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BBCEE1C)
    (at 132.08 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BBB5EFE)
    (attr smd)
    (fp_text reference U503 (at 0 3.2385 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD8418 (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R511-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U503-Pad4)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BD0A5CE)
    (at 148.8694 28.6004)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB73C46/5BB49527)
    (attr smd)
    (fp_text reference C1204 (at 5.4915 1.143 -270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Kippschalter:B12AV (layer F.Cu) (tedit 5BB5DE12) (tstamp 5BC76F0B)
    (at 177.038 41.7576 180)
    (path /5BB7D616/5BB7EDAF)
    (fp_text reference SW1401 (at -7.8105 -4.826 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_SPDT (at -9.5 5.25 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7 -4) (end 7 1) (layer F.SilkS) (width 0.15))
    (fp_line (start 7 -4) (end -11.75 -4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -4) (end -11.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 4) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (fp_line (start -11.75 -1.25) (end -21.75 -1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 -1.25) (end -21.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start -21.75 1.25) (end -11.75 1.25) (layer Dwgs.User) (width 0.15))
    (fp_line (start 7 1) (end -0.75 1) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.75 1) (end -0.75 4) (layer F.SilkS) (width 0.15))
    (pad "" thru_hole rect (at -5.08 1.27 180) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad "" thru_hole rect (at -5.08 -1.27 180) (size 3 2) (drill 0.95) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 240 "Net-(SW1401-Pad3)"))
    (pad 2 thru_hole circle (at 2.53 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 156 "Net-(D1401-Pad1)"))
    (pad 1 thru_hole circle (at 5.08 -1.27 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 144 +12V))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E14) (tstamp 5BCD58C1)
    (at 91.948 27.686 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB8682A)
    (fp_text reference MH1401 (at 0 -3.048 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 270) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E06) (tstamp 5BB7BA9E)
    (at 186.055 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB86916)
    (fp_text reference MH1402 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60F0C) (tstamp 5BC63C85)
    (at 93.472 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868BC)
    (fp_text reference MH1403 (at 0 -3.048 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Connectors:1pin (layer F.Cu) (tedit 5BB60E19) (tstamp 5BCFF4F0)
    (at 185.3565 27.7495)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5BB7D616/5BB868ED)
    (fp_text reference MH1404 (at 0 -3.048) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC382CF) (tstamp 5BC4AE4E)
    (at 159.4492 31.1912)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB5DF23)
    (attr smd)
    (fp_text reference C1306 (at -1.131 -1.3462) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4) (tstamp 5BD2034F)
    (at 167.8686 44.8142)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (path /5BB8D2EE/5BB6A6ED)
    (attr smd)
    (fp_text reference D1303 (at -1.3675 1.397 -180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LED_2.5VPSU_off_red (at 0 1.7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.6 -0.8) (end 1 -0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 0.8) (end 1 0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.65) (end 1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.65) (end 1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.65) (end -1 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.65) (end -1 -0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.2) (end -0.1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end 0.2 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.2) (end 0.2 -0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 -0.2) (end -0.1 0.2) (layer F.Fab) (width 0.1))
    (fp_line (start -0.1 0) (end -0.3 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0) (end 0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -0.88) (end 1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -0.88) (end 1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 0.88) (end -1.7 0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 0.88) (end -1.7 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 -0.8) (end -1.6 0.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -1.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D1303-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB61283) (tstamp 5BC4ADD9)
    (at 156.7688 32.6524 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5CFDD)
    (attr smd)
    (fp_text reference R1304 (at 2.4758 -1.2032 -90) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 226 enable_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB612A8) (tstamp 5BC4ADA9)
    (at 159.4492 32.6644)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB8D2EE/5BB5D0B6)
    (attr smd)
    (fp_text reference R1305 (at 2.171 1.651) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 10k (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AD19)
    (at 163.4998 39.9034 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB57E62)
    (attr smd)
    (fp_text reference R1307 (at -2.601 -4.572 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 200R (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(Q1302-Pad3)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E) (tstamp 5BD0AD59)
    (at 158.734 35.4076 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB59C86)
    (attr smd)
    (fp_text reference Q1301 (at 2.286 0.447 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(C1306-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BB610FE) (tstamp 5BC7D234)
    (at 159.496 38.9788)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (path /5BB8D2EE/5BB57D85)
    (attr smd)
    (fp_text reference Q1302 (at -2.286 -0.066 90) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value BC850 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 -1.75) (end 1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1.75) (end 1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1.75) (end -1.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1.75) (end -1.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -1.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(Q1301-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 181 "/3_3V PSU/MC34063_Feedback"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(Q1302-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 58AA8B76) (tstamp 5BC47AEC)
    (at 183.2305 60.6171)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (path /5BB8D2EE/59D46505)
    (attr smd)
    (fp_text reference C1304 (at 5.6185 0 -270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 470uF (at 0 -4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.7 3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end -4.7 3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.7 -3.4) (end 4.7 -3.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.54 -3.3) (end 3.3 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -2.54 -3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.54 3.3) (end -3.3 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end -2.54 3.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 -2.54) (end -3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 -3.3) (end 3.3 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 3.3) (end 3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 2.54) (end -3.3 1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.15 -3.15) (end -2.48 -3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 -3.15) (end -3.15 -2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 -2.48) (end -3.15 2.48) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 2.48) (end -2.48 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start -2.48 3.15) (end 3.15 3.15) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 3.15) (end 3.15 -3.15) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 4.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -4.28 2.91) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user + (at -1.73 -0.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 0.5 3) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 184 "/3_3V PSU/MC34063_HC_A"))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC47A60)
    (at 177.4945 63.5381 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB8D2EE/5BB49531)
    (attr smd)
    (fp_text reference C1305 (at 1.9805 -1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 184 "/3_3V PSU/MC34063_HC_A"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BC47A20)
    (at 185.8645 55.7276)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB8D2EE/5AAD3380)
    (attr smd)
    (fp_text reference D1302 (at 1.425 -1.778) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_2.7V (at 0.889 -2.568) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BC4AC35)
    (at 163.4338 45.3898)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB4952A)
    (attr smd)
    (fp_text reference R1303 (at 3.6855 -7.8105) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4.7k (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R1303-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BB6113F) (tstamp 5BC4AC05)
    (at 163.449 43.5356 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB8D2EE/5BB49529)
    (attr smd)
    (fp_text reference R1302 (at -3.1115 0.6985 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 27k (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R1302-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 179 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 5BB611A5) (tstamp 5BC4ABD5)
    (at 146.304 46.3816 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB8D2EE/59D44D00)
    (attr smd)
    (fp_text reference R1301 (at 3.3135 -2.667 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 199 "/3_3V PSU/HC_Plain_b"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BD0A73D)
    (at 135.3566 35.179 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49524)
    (attr smd)
    (fp_text reference C1203 (at 0.8255 1.4605 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 83pF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1203-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3) (tstamp 5BD0A6FF)
    (at 133.0796 30.0355 270)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (path /5BB73C46/59D454FD)
    (attr smd)
    (fp_text reference D1201 (at -1.397 2.9845 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SB350 (at 0 3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.55 -2.15) (end 2.15 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.55 2.15) (end 2.15 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112) (layer F.Fab) (width 0.1))
    (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102) (layer F.Fab) (width 0.1))
    (fp_line (start -3.65 2.25) (end -3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 2.25) (end -3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -2.25) (end 3.65 2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -2.25) (end 3.65 -2.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.3 -2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 -2) (end 2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -2.3 2) (end -2.3 -2) (layer F.Fab) (width 0.1))
    (fp_line (start 2.3 2) (end -2.3 2) (layer F.Fab) (width 0.1))
    (fp_line (start -3.55 -2.15) (end -3.55 2.15) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 151 "/5V PSU /SwE"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804) (tstamp 5BD0A6C8)
    (at 146.2786 37.0955 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (path /5BB73C46/5BB49521)
    (attr smd)
    (fp_text reference R1201 (at 0 -2.413 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.33R (at 0 2.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.85 1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.85 1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end -3.85 1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.85 -1.85) (end 3.85 -1.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.6 -1.82) (end 2.6 -1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.6 1.82) (end -2.6 1.82) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.15 -1.6) (end 3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 -1.6) (end 3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start 3.15 1.6) (end -3.15 1.6) (layer F.Fab) (width 0.1))
    (fp_line (start -3.15 1.6) (end -3.15 -1.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA) (tstamp 5BD0A680)
    (at 139.6746 35.941 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB73C46/5BB74814)
    (attr smd)
    (fp_text reference U1201 (at 0 -3.302 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MC34063AD (at 0 3.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.73 -2.7) (end -3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.73 -2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 -2.7) (end 3.73 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.73 2.7) (end 3.73 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.075 -2.575) (end -2.075 -2.525) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -2.525) (end -3.475 -2.525) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R1201-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 151 "/5V PSU /SwE"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1203-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R1202-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R1201-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R1201-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BD0A644)
    (at 135.3566 36.7665 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB49534)
    (attr smd)
    (fp_text reference C1201 (at -0.496 -2.794 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 144 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC44171)
    (at 132.842 -5.83 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB73C46/5BB47F9D)
    (attr smd)
    (fp_text reference C1205 (at 0 -1.5 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value C (at 0 1.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804) (tstamp 5BD0A614)
    (at 143.4211 40.1345 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (path /5BB73C46/59D46945)
    (attr smd)
    (fp_text reference R1202 (at 0.254 -3.3655 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 3k (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.55 0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.55 0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end -1.55 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 -0.9) (end 1.55 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R1202-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC80DB)
    (at 121.7429 48.006 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60B72)
    (attr smd)
    (fp_text reference R919 (at -3.1235 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R919-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 feedback_Tube_PSU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC80AB)
    (at 103.378 31.2293 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63D55)
    (attr smd)
    (fp_text reference R920 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 Rx))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R920-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC807B)
    (at 101.0659 39.37)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB60C0B)
    (attr smd)
    (fp_text reference R918 (at -3.2505 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 167 Encoder_B))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R918-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC804B)
    (at 101.981 31.2293 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB63CF7)
    (attr smd)
    (fp_text reference R921 (at -3.06 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R921-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 Tx))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC801B)
    (at 112.3689 56.642 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A35B)
    (attr smd)
    (fp_text reference C901 (at 3.187 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C901-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC19AE4) (tstamp 5BCC7FEB)
    (at 111.7854 35.6235 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A26C)
    (attr smd)
    (fp_text reference C902 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BCC7FBB)
    (at 110.9599 55.245 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB39CC9)
    (attr smd)
    (fp_text reference C903 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BC3DD04)
    (at 105.652 30.607 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A69F)
    (attr smd)
    (fp_text reference C904 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 136 /uC/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BC4E5F7) (tstamp 5BB891B4)
    (at 109.728 30.607 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB48B05/5BB3A72A)
    (attr smd)
    (fp_text reference C905 (at 0 -1.5 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22pF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 135 /uC/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_SMD:D_MiniMELF (layer F.Cu) (tedit 5905D8F5) (tstamp 5BB397FA)
    (at 121.892 28.6385)
    (descr "Diode Mini-MELF")
    (tags "Diode Mini-MELF")
    (path /5BB48B05/5BB54E76)
    (attr smd)
    (fp_text reference D901 (at 0 -2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DZ_5.1V (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 1.1) (end -2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 1.1) (end -2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.65 -1.1) (end 2.65 1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.65 -1.1) (end 2.65 -1.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.75 0) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0.25 0) (end 0.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 -0.8) (end 1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -1.65 0.8) (end -1.65 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 0.8) (end -1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 1.65 -0.8) (end 1.65 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -2.55 1) (end 1.75 1) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.55 -1) (end -2.55 1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.75 -1) (end -2.55 -1) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 -2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.75 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 125 MISO))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC33ABB) (tstamp 5BCC7F8B)
    (at 115.2779 35.0005 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3F6E2)
    (attr smd)
    (fp_text reference R906 (at -3.2505 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R906-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4D4FB) (tstamp 5BCC7F5B)
    (at 121.7429 50.8 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BC50B36)
    (attr smd)
    (fp_text reference R907 (at -3.1235 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R907-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 Currentsensing_Tube_6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4E04A) (tstamp 5BCC7F2B)
    (at 101.0659 40.767)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D7AF)
    (attr smd)
    (fp_text reference R908 (at -3.1235 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R908-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R908-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC7EFB)
    (at 101.0659 43.561)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D75D)
    (attr smd)
    (fp_text reference R910 (at -3.06 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R910-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R910-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC7ECB)
    (at 101.0539 49.264)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D737)
    (attr smd)
    (fp_text reference R911 (at -3.06 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R911-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 143 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4D760) (tstamp 5BCC7E9B)
    (at 101.0539 47.879)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3D711)
    (attr smd)
    (fp_text reference R912 (at -3.06 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 142 SCL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R912-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC4E050) (tstamp 5BCC7E6B)
    (at 101.0659 37.973)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E7E0)
    (attr smd)
    (fp_text reference R915 (at 0.0254 -1.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(R915-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 171 Encoder_push))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BC1B239) (tstamp 5BCC7E3B)
    (at 121.7429 49.403 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB4E3C2)
    (attr smd)
    (fp_text reference R916 (at 0 -1.45 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(R916-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(R916-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804) (tstamp 5BCC7E0B)
    (at 101.0673 36.576)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (path /5BB48B05/5BB3E361)
    (attr smd)
    (fp_text reference R914 (at -3.048 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0R (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 0.68) (end -0.5 0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -0.68) (end 0.5 -0.68) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end 1.25 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.25 0.7) (end -1.25 0.7) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 170 Encoder_A))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(R914-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3B188)
    (at 175.259 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3E89F/5BB249C1)
    (attr smd)
    (fp_text reference U801 (at -0.001 7.62 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /Tubes/sheet5BB3E86C/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R808-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R807-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R806-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R805-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R804-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R803-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R802-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 126 MOSI))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B5BB)
    (at 142.99 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB26FB6)
    (attr smd)
    (fp_text reference C602 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C602-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B4CB)
    (at 102.87 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB26FB6)
    (attr smd)
    (fp_text reference C302 (at 2.159 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C302-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B49B)
    (at 101.485 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BBBEA7E)
    (attr smd)
    (fp_text reference C303 (at -0.012 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608EF) (tstamp 5BC3B0C8)
    (at 123.444 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB32DD3/5BB2618D)
    (attr smd)
    (fp_text reference C401 (at -0.242 -1.3335 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60CBD) (tstamp 5BC3B098)
    (at 140.474 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB2618D)
    (attr smd)
    (fp_text reference C501 (at -0.242 -1.2065 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7B3DB)
    (at 132.195 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BB26FB6)
    (attr smd)
    (fp_text reference C502 (at 2.274 0.889 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA2D)
    (at 130.695 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB36AE9/5BBBEA7E)
    (attr smd)
    (fp_text reference C503 (at 0.0515 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60E26) (tstamp 5BC3B1E8)
    (at 152.781 79.641 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BB2618D)
    (attr smd)
    (fp_text reference C601 (at -0.3055 -1.2065 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABB6)
    (at 141.49 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3BB9E/5BBBEA7E)
    (attr smd)
    (fp_text reference C603 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DA1) (tstamp 5BC3BA58)
    (at 169.672 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB2618D)
    (attr smd)
    (fp_text reference C701 (at -0.242 -1.27 180) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BBD8FE6)
    (at 161.29 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BB26FB6)
    (attr smd)
    (fp_text reference C702 (at 2.159 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7AA96)
    (at 159.905 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BBBEA7E)
    (attr smd)
    (fp_text reference C703 (at 0 1.4605) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB60DE8) (tstamp 5BC3BA28)
    (at 181.991 79.629 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB2618D)
    (attr smd)
    (fp_text reference C801 (at -0.3055 -1.27 270) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BB608D4) (tstamp 5BC3B9F8)
    (at 111.264 80.391 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB247DF/5BB2618D)
    (attr smd)
    (fp_text reference C301 (at -0.369 -1.27) (layer F.SilkS)
      (effects (font (size 0.7 0.7) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB7ABE6)
    (at 171.97 95.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E89F/5BB26FB6)
    (attr smd)
    (fp_text reference C802 (at 2.044 0.9525 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7) (tstamp 5BB39C36)
    (at 170.7 104.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5BB1F5A4/5BB3E878/5BBBEA7E)
    (attr smd)
    (fp_text reference C803 (at 0 1.524) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 0 1.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.4 0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end -1.4 0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.65) (end 1.4 -0.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    )
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB90)
    (at 116.714 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB32DD3/5BB249C1)
    (attr smd)
    (fp_text reference U401 (at 0.763 7.493 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /Tubes/IV-9_Tube/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R408-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R407-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R406-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R405-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R404-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R403-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R402-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R401-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BB18)
    (at 133.349 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB36AE9/5BB249C1)
    (attr smd)
    (fp_text reference U501 (at -0.0645 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R501-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R502-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R503-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R504-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R505-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R506-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R507-Pad2)"))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R508-Pad2)"))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 /Tubes/sheet5BB32DC8/Data_in))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64) (tstamp 5BC3BAA0)
    (at 146.049 72.517 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5BB1F5A4/5BB3BB9E/5BB249C1)
    (attr smd)
    (fp_text reference U601 (at 0 7.5565 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.875 -6.325) (end -5.675 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end 3.875 6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end 3.875 -6.575) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 6.575) (end -3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 6.575) (end 3.875 6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.875 -6.575) (end 3.875 -6.24) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.875 -6.575) (end -3.875 -6.325) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.95 6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end 5.95 -6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.95 -6.75) (end 5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.95 -6.75) (end -5.95 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -5.4) (end -2.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -3.75 6.4) (end -3.75 -5.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 6.4) (end -3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start 3.75 -6.4) (end 3.75 6.4) (layer F.Fab) (width 0.15))
    (fp_line (start -2.75 -6.4) (end 3.75 -6.4) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 /Tubes/sheet5BB36ADE/Data_in))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R608-Pad2)"))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R607-Pad2)"))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R606-Pad2)"))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R605-Pad2)"))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~enable_Shiftregister))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 reset_Shiftregister))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 clk))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 160 ~latch_Shiftregister))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R604-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R603-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R602-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 /Tubes/sheet5BB3BB93/Data_in))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB29692)
    (at 115.824 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB32DD3/5BB249BA)
    (fp_text reference U402 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 90 /Tubes/sheet5BB32DC8/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 91 /Tubes/sheet5BB32DC8/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 92 /Tubes/sheet5BB32DC8/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 /Tubes/sheet5BB32DC8/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 /Tubes/sheet5BB32DC8/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 95 /Tubes/sheet5BB32DC8/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 96 /Tubes/sheet5BB32DC8/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 97 /Tubes/sheet5BB32DC8/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C402-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E57)
    (at 134.239 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB36AE9/5BB249BA)
    (fp_text reference U502 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C502-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 82 /Tubes/sheet5BB36ADE/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 /Tubes/sheet5BB36ADE/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 /Tubes/sheet5BB36ADE/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 85 /Tubes/sheet5BB36ADE/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 86 /Tubes/sheet5BB36ADE/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 87 /Tubes/sheet5BB36ADE/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 88 /Tubes/sheet5BB36ADE/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 89 /Tubes/sheet5BB36ADE/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E2D)
    (at 163.449 94.09267 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E878/5BB249BA)
    (fp_text reference U702 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C702-Pad1)"))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 /Tubes/sheet5BB3E86C/Dot))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 /Tubes/sheet5BB3E86C/b))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 /Tubes/sheet5BB3E86C/c))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 /Tubes/sheet5BB3E86C/a))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 /Tubes/sheet5BB3E86C/f))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 /Tubes/sheet5BB3E86C/g))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 /Tubes/sheet5BB3E86C/d))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 /Tubes/sheet5BB3E86C/e))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module cFootprints:IV-9-tube (layer F.Cu) (tedit 5BB225C8) (tstamp 5BB24E18)
    (at 174.244 94.105 90)
    (descr TO-100-10)
    (tags TO-100-10)
    (path /5BB1F5A4/5BB3E89F/5BB249BA)
    (fp_text reference U802 (at 2.92 -5.82 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value IV-9_Tube (at 2.92 5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.92 -5.82 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 7.87 -4.95) (end -2.04 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.87 4.95) (end 7.87 -4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 4.95) (end 7.87 4.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.04 -4.95) (end -2.04 4.95) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.92 0) (end 7.17 0) (layer F.Fab) (width 0.1))
    (fp_arc (start 2.92 0) (end -0.077084 -3.774902) (angle 360) (layer F.SilkS) (width 0.12))
    (fp_arc (start 2.92 0) (end -0.085408 -3.61352) (angle 360) (layer F.Fab) (width 0.1))
    (pad 9 thru_hole oval (at 2.01767 -2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /Tubes/sheet5BB3E86D/e))
    (pad 8 thru_hole oval (at 3.82233 -2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /Tubes/sheet5BB3E86D/d))
    (pad 7 thru_hole oval (at 5.28233 -1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Tubes/sheet5BB3E86D/g))
    (pad 6 thru_hole oval (at 5.84 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 /Tubes/sheet5BB3E86D/f))
    (pad 5 thru_hole oval (at 5.28233 1.716333 234) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /Tubes/sheet5BB3E86D/a))
    (pad 4 thru_hole oval (at 3.82233 2.777085 198) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /Tubes/sheet5BB3E86D/c))
    (pad 3 thru_hole oval (at 2.01767 2.777085 162) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /Tubes/sheet5BB3E86D/b))
    (pad 2 thru_hole oval (at 0.55767 1.716333 126) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /Tubes/sheet5BB3E86D/Dot))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C802-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-100-10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text 9-24VDC (at 100.838 10.16 180) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "IV-9 Clock  Max Nowka  10.2018 V1.0 " (at 114.173 108.331) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.25)))
  )

  (segment (start 172.72 95.25) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 173.99 95.25) (end 173.99 94.359) (width 0.35) (layer F.Cu) (net 1) (status 20))
  (segment (start 173.99 97.63) (end 173.99 95.25) (width 0.35) (layer F.Cu) (net 1) (status 10))
  (segment (start 176.765 97.63) (end 177.165 97.23) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 173.99 97.63) (end 176.765 97.63) (width 0.35) (layer F.Cu) (net 1) (status 30))
  (segment (start 165.97 97.63) (end 166.37 97.23) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 163.195 97.63) (end 165.97 97.63) (width 0.35) (layer F.Cu) (net 2) (status 30))
  (segment (start 162.04 95.25) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 163.195 95.25) (end 163.195 94.34667) (width 0.35) (layer F.Cu) (net 2) (status 20))
  (segment (start 163.195 97.63) (end 163.195 95.25) (width 0.35) (layer F.Cu) (net 2) (status 10))
  (segment (start 144.94 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 143.74 95.25) (end 144.78 95.25) (width 0.35) (layer F.Cu) (net 3) (status 10))
  (segment (start 144.78 95.25) (end 144.78 97.63) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 147.63 97.63) (end 148.03 97.23) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 97.63) (end 147.63 97.63) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 94.359) (end 145.034 94.105) (width 0.35) (layer F.Cu) (net 3) (status 30))
  (segment (start 144.78 95.25) (end 144.78 94.359) (width 0.35) (layer F.Cu) (net 3) (status 20))
  (segment (start 133.985 97.63) (end 136.365 97.63) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.84 97.155) (end 137.16 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 136.365 97.63) (end 136.84 97.155) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 133.985 94.359) (end 134.239 94.105) (width 0.35) (layer F.Cu) (net 4) (status 30))
  (segment (start 132.945 95.25) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 133.985 95.25) (end 133.985 94.359) (width 0.35) (layer F.Cu) (net 4) (status 20))
  (segment (start 133.985 97.63) (end 133.985 95.25) (width 0.35) (layer F.Cu) (net 4) (status 10))
  (segment (start 118.27 97.63) (end 118.745 97.155) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 115.57 97.63) (end 118.27 97.63) (width 0.35) (layer F.Cu) (net 5) (status 30))
  (segment (start 114.3 95.25) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 97.63) (end 115.57 95.25) (width 0.35) (layer F.Cu) (net 5) (status 10))
  (segment (start 115.57 94.359) (end 115.824 94.105) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 115.57 95.25) (end 115.57 94.359) (width 0.35) (layer F.Cu) (net 5))
  (segment (start 107.55 97.63) (end 107.95 97.23) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 97.63) (end 107.55 97.63) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 104.775 94.359) (end 105.029 94.105) (width 0.35) (layer F.Cu) (net 6) (status 30))
  (segment (start 103.62 95.25) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 104.775 95.25) (end 104.775 94.359) (width 0.35) (layer F.Cu) (net 6) (status 20))
  (segment (start 104.775 97.63) (end 104.775 95.25) (width 0.35) (layer F.Cu) (net 6) (status 10))
  (segment (start 123.825 80.391) (end 126.365 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 157.861 80.391) (end 167.005 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 171.45 104.775) (end 171.45 106.299) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 122.555 80.391) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 139.573 83.947) (end 139.573 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 127 83.971) (end 127 83.439) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 106.934 78.74) (end 106.934 79.87137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC62))
  (segment (start 106.934 79.87137) (end 108.966 81.90337) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC6E))
  (segment (start 108.966 81.90337) (end 110.363 83.30037) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC71))
  (segment (start 136.144 77.597) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 136.144 79.918) (end 136.144 79.121) (width 0.35) (layer F.Cu) (net 7))
  (via (at 157.861 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 138.049 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 167.005 80.391) (end 166.913 80.391) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.347) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.913 80.391) (end 166.37 80.934) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 127 83.439) (end 127 83.312) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 166.37 80.934) (end 165.354 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 113.03 106.68) (end 113.03 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 110.514 80.391) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BC9E))
  (segment (start 113.03 104.775) (end 113.03 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 150.749 80.391) (end 149.606 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA1))
  (segment (start 160.655 104.775) (end 160.655 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 119.634 77.417) (end 119.634 79.756) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCA7))
  (segment (start 150.749 80.391) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAA))
  (segment (start 120.089 76.962) (end 119.634 77.417) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCAD))
  (segment (start 123.444 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB0))
  (segment (start 149.606 80.391) (end 148.844 79.629) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB3))
  (segment (start 107.514 76.962) (end 106.934 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB6))
  (segment (start 171.45 103.03) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 179.959 80.391) (end 178.713 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCB9))
  (segment (start 178.713 80.391) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBC))
  (segment (start 179.959 76.962) (end 178.634 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCBF) (status 10))
  (segment (start 178.054 77.542) (end 178.054 79.732) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC2))
  (segment (start 121.414 76.962) (end 120.089 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC5))
  (segment (start 120.269 80.391) (end 121.412 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCC8))
  (segment (start 139.724 80.391) (end 138.049 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCB))
  (segment (start 108.839 76.962) (end 107.514 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCCE) (status 10))
  (segment (start 165.354 79.502) (end 165.354 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD1))
  (segment (start 102.235 105.41) (end 102.235 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 106.934 77.542) (end 106.934 78.74) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCD4))
  (segment (start 102.235 106.68) (end 102.235 105.41) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.844 79.629) (end 148.844 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCDA))
  (segment (start 148.844 77.542) (end 149.424 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCE0))
  (segment (start 102.235 104.775) (end 102.235 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 120.904 80.391) (end 122.555 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCEC))
  (segment (start 136.779 76.962) (end 138.049 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCEF) (status 20))
  (segment (start 171.45 106.68) (end 171.45 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 108.839 80.137) (end 108.585 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCF5))
  (segment (start 122.555 80.391) (end 122.174 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BCF8))
  (segment (start 149.424 76.962) (end 150.749 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BCFB))
  (segment (start 131.445 106.68) (end 131.445 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 126.365 80.391) (end 128.27 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD01))
  (segment (start 108.585 80.391) (end 120.904 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD07))
  (segment (start 178.054 79.732) (end 178.459 80.137) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD0A) (status 20))
  (segment (start 181.991 80.391) (end 179.959 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD1F))
  (segment (start 165.354 77.542) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3BD31))
  (segment (start 150.749 80.391) (end 151.88037 80.391) (width 0.35) (layer B.Cu) (net 7) (tstamp 5BC3BD94))
  (via (at 179.959 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1ED))
  (via (at 150.749 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F0))
  (via (at 171.45 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 160.655 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 142.24 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 131.445 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 102.235 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 113.03 106.299) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 167.005 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F3))
  (via (at 108.585 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1F6))
  (via (at 121.412 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7) (tstamp 5BC3C1FC))
  (segment (start 167.259 80.137) (end 167.005 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C22C))
  (segment (start 178.634 76.962) (end 178.054 77.542) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C232))
  (segment (start 131.445 104.775) (end 131.445 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 160.655 106.68) (end 160.655 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 167.005 80.391) (end 168.922 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23B))
  (segment (start 142.24 106.68) (end 142.24 104.775) (width 0.35) (layer F.Cu) (net 7) (status 20))
  (segment (start 136.779 76.962) (end 136.144 77.597) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C23E))
  (segment (start 119.634 79.756) (end 120.269 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C241))
  (segment (start 167.259 76.962) (end 165.934 76.962) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C244) (status 10))
  (segment (start 152.654 80.518) (end 152.781 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24A))
  (segment (start 142.24 104.775) (end 142.24 103.03) (width 0.35) (layer F.Cu) (net 7) (status 30))
  (segment (start 110.363 83.347) (end 110.363 83.947) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C24D))
  (segment (start 157.861 81.696) (end 156.21 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 165.354 79.918) (end 165.354 79.502) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 168.783 83.947) (end 168.783 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 128.651 81.661) (end 127 83.312) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 128.651 80.391) (end 128.651 81.661) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 151.88037 80.391) (end 152.781 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 128.27 80.391) (end 128.651 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 139.573 83.347) (end 139.065 82.839) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 110.363 83.30037) (end 110.363 83.347) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C277))
  (segment (start 156.21 83.947) (end 156.21 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 152.781 80.391) (end 157.861 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 157.861 80.391) (end 157.861 81.696) (width 0.35) (layer F.Cu) (net 7))
  (via (at 128.651 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 108.46963 80.391) (end 107.96163 80.899) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C280))
  (segment (start 179.971 80.379) (end 179.959 80.391) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 177.927 106.299) (end 171.45 106.299) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 138.049 80.391) (end 137.449001 80.990999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.449001 81.152999) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 108.585 80.391) (end 108.46963 80.391) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BC3C28C))
  (segment (start 181.991 80.379) (end 179.971 80.379) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 137.414 81.188) (end 136.144 79.918) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 139.573 83.347) (end 137.414 81.188) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 178.562 106.299) (end 177.927 106.299) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 137.449001 80.990999) (end 137.449001 81.152999) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 123.825 80.946) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 80.438) (end 123.825 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 123.825 81.038) (end 123.825 80.438) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7645 80.4545) (end 152.781 80.4545) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7175 80.5015) (end 152.7645 80.4545) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.781 80.4545) (end 152.781 80.391) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 152.7175 81.1015) (end 152.7175 80.5015) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 108.585 80.391) (end 99.441 80.391) (width 0.35) (layer B.Cu) (net 7))
  (via (at 99.8855 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 97.79 83.947) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 83.058) (end 97.79 83.347) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 98.73087 82.677) (end 98.171 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.8855 81.52237) (end 98.73087 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 99.8855 80.391) (end 99.8855 81.52237) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 83.058) (end 97.79 82.677) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.79 82.677) (end 98.171 82.677) (width 0.35) (layer F.Cu) (net 7))
  (via (at 180.2384 102.362) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (via (at 180.2384 106.3244) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 180.2384 102.362) (end 180.2384 106.3244) (width 0.7) (layer F.Cu) (net 7))
  (segment (start 171.4754 106.3244) (end 171.45 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 180.2384 106.3244) (end 171.4754 106.3244) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 171.45 106.299) (end 160.655 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 160.655 106.299) (end 142.24 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 142.24 106.299) (end 131.445 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 131.445 106.299) (end 113.03 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 113.03 106.299) (end 102.235 106.299) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 97.471599) (end 181.7116 102.362) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 181.7116 102.362) (end 180.2384 102.362) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 80.3656) (end 186.602001 97.471599) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 50.158799) (end 186.602001 80.3656) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.576601 80.391) (end 179.959 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 186.602001 80.3656) (end 186.576601 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 179.959 80.391) (end 167.005 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 167.005 80.391) (end 150.749 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 150.749 80.391) (end 138.049 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 138.049 80.391) (end 128.651 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 128.651 80.391) (end 121.412 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 121.412 80.391) (end 108.585 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 107.45363 80.391) (end 99.8855 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 108.585 80.391) (end 107.45363 80.391) (width 0.7) (layer B.Cu) (net 7))
  (segment (start 83.5279 29.8965) (end 83.5152 29.9092) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC87B6))
  (segment (start 77.621 89.638) (end 77.089 89.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 78.867 88.392) (end 77.621 89.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 78.867 81.407) (end 78.867 88.392) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 79.248 81.026) (end 78.867 81.407) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 77.089 89.638) (end 75.819 89.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 75.807 89.65) (end 75.819 89.638) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 74.422 89.65) (end 75.807 89.65) (width 0.35) (layer F.Cu) (net 7))
  (via (at 90.4875 80.391) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 7))
  (segment (start 99.8855 80.391) (end 90.4875 80.391) (width 0.7) (layer F.Cu) (net 7))
  (segment (start 90.4875 80.391) (end 90.4875 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 91.8605 78.994) (end 91.8845 78.97) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 90.4875 78.994) (end 91.8605 78.994) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 91.8845 78.97) (end 93.2815 78.97) (width 0.35) (layer B.Cu) (net 7))
  (segment (start 84.963 29.8965) (end 83.5279 29.8965) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC87BC))
  (segment (start 112.5354 35.6235) (end 112.5474 35.6115) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88D3))
  (segment (start 117.0809 46.101) (end 117.0559 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88D6))
  (segment (start 120.1409 46.585) (end 119.6319 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88D9))
  (segment (start 120.8659 46.585) (end 120.1409 46.585) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88DC))
  (segment (start 104.5559 45.276) (end 105.6559 45.276) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88DF))
  (segment (start 102.8349 45.276) (end 104.5559 45.276) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88E2))
  (segment (start 102.5289 44.97) (end 102.8349 45.276) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88E5))
  (segment (start 101.6889 44.97) (end 102.5289 44.97) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88E8))
  (segment (start 112.1559 36.728) (end 112.1559 38.476) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88EB))
  (segment (start 112.1559 38.476) (end 112.1559 39.576) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88EE))
  (segment (start 118.1559 46.076) (end 117.0559 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88F1))
  (segment (start 119.6319 46.076) (end 118.1559 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88F4))
  (segment (start 112.1559 46.002) (end 112.2299 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88F7))
  (segment (start 112.1559 43.307) (end 112.1559 46.002) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88FA))
  (segment (start 110.5559 50.976) (end 110.5559 46.205) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC88FD))
  (segment (start 110.6849 46.076) (end 110.5559 46.205) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8900))
  (segment (start 117.0559 46.076) (end 112.7379 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8903))
  (segment (start 112.7379 46.076) (end 112.2299 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8906))
  (segment (start 110.5559 46.205) (end 110.5559 46.142) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8909))
  (segment (start 105.6559 45.276) (end 109.6899 45.276) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC890C))
  (segment (start 112.5354 36.3485) (end 112.1559 36.728) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC890F))
  (segment (start 112.5354 35.6235) (end 112.5354 36.3485) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8912))
  (segment (start 111.2139 46.076) (end 110.4899 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8915))
  (segment (start 110.5559 46.142) (end 110.1979 45.784) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8918))
  (segment (start 112.7379 46.076) (end 111.2139 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC891B))
  (segment (start 111.2139 46.076) (end 110.6849 46.076) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC891E))
  (segment (start 110.5559 50.976) (end 110.5559 53.871) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8921))
  (segment (start 110.2099 54.217) (end 110.2099 55.245) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8924))
  (segment (start 110.5559 53.871) (end 110.2099 54.217) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8927))
  (segment (start 110.4899 46.076) (end 110.1979 45.784) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC892A))
  (segment (start 110.1979 45.784) (end 109.6899 45.276) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC892D))
  (segment (start 112.1559 39.576) (end 112.1559 41.529) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8930))
  (segment (start 112.1559 41.529) (end 112.1559 43.307) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8933))
  (segment (start 112.5354 33.0595) (end 112.3689 32.893) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8936))
  (segment (start 112.5354 35.6235) (end 112.5354 33.0595) (width 0.35) (layer F.Cu) (net 7) (tstamp 5BCC8939))
  (segment (start 99.3895 44.97) (end 98.806 45.5535) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 101.6889 44.97) (end 99.3895 44.97) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.3455 45.5295) (end 97.3695 45.5535) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.3695 45.5535) (end 98.806 45.5535) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 97.3455 47.0655) (end 97.3455 45.5295) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 95.504 44.6405) (end 96.393 45.5295) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 95.504 39.3065) (end 95.504 44.6405) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 92.7735 36.576) (end 95.504 39.3065) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 96.393 45.5295) (end 97.3455 45.5295) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 92.7735 35.1765) (end 92.7735 36.576) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 92.7735 33.274) (end 92.7735 35.1765) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 146.0805 28.5115) (end 146.1694 28.6004) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 142.3416 28.5115) (end 146.0805 28.5115) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 147.1194 28.6004) (end 146.1694 28.6004) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.479 30.96) (end 147.1194 28.6004) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.479 33.2232) (end 149.479 30.96) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 149.479 34.4232) (end 149.479 33.2232) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 143.4211 39.1845) (end 143.4211 37.4015) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 143.4211 37.4015) (end 145.3072 35.5154) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 145.3072 35.5154) (end 148.3868 35.5154) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 148.3868 35.5154) (end 149.479 34.4232) (width 0.35) (layer F.Cu) (net 7))
  (segment (start 112.014 76.962) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE3) (status 30))
  (segment (start 108.839 78.232) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC95) (status 30))
  (segment (start 112.014 80.137) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD3A) (status 30))
  (segment (start 141.224 79.883) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC98) (status 30))
  (segment (start 138.049 78.232) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC92) (status 30))
  (segment (start 141.224 79.883) (end 141.224 78.867) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD79) (status 10))
  (segment (start 112.014 79.883) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA6) (status 10))
  (segment (start 167.259 78.232) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD28) (status 30))
  (segment (start 170.434 78.232) (end 170.434 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCE9) (status 30))
  (segment (start 157.859 78.232) (end 157.859 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDA3) (status 30))
  (segment (start 128.649 76.962) (end 128.649 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD1C) (status 30))
  (segment (start 141.224 80.137) (end 141.224 80.264) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDF7) (status 30))
  (segment (start 114.3 97.63) (end 113.03 97.63) (width 0.35) (layer F.Cu) (net 8) (status 30))
  (segment (start 112.014 80.137) (end 112.014 80.518) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9A) (status 10))
  (segment (start 141.224 77.597) (end 141.224 76.962) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD34) (status 20))
  (segment (start 141.224 78.867) (end 141.224 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BCFE) (status 20))
  (segment (start 153.519 51.1316) (end 153.289 50.9016) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFE9))
  (segment (start 153.519 52.8066) (end 153.519 51.1316) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFEC))
  (via (at 155.194 50.9016) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC4B001))
  (segment (start 153.289 50.9016) (end 155.194 50.9016) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFEF))
  (segment (start 155.194 49.3116) (end 155.194 50.9016) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC4AFF2))
  (segment (start 120.7909 45.276) (end 120.8659 45.351) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8960))
  (segment (start 119.8499 45.085) (end 120.8659 45.085) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8963))
  (segment (start 119.6589 45.276) (end 119.8499 45.085) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8966))
  (segment (start 117.0559 45.276) (end 119.6589 45.276) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC896F))
  (segment (start 111.0354 35.6235) (end 111.0354 36.461) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC897E))
  (segment (start 111.3559 36.7815) (end 111.3559 39.576) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8981))
  (segment (start 111.0354 36.461) (end 111.3559 36.7815) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8984))
  (segment (start 111.7099 56.551) (end 111.6189 56.642) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8987))
  (segment (start 111.7099 55.245) (end 111.7099 56.551) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC898A))
  (segment (start 179.959 78.232) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD61))
  (segment (start 181.991 78.891) (end 181.332 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BC9B))
  (segment (start 170.422 80.391) (end 170.422 79.006) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8E))
  (segment (start 170.422 79.006) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD10))
  (segment (start 170.434 78.994) (end 170.434 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD9D))
  (segment (start 170.434 80.137) (end 170.434 78.994) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD55))
  (segment (start 141.224 80.391) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD46))
  (segment (start 141.224 77.851) (end 141.224 77.597) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD64))
  (segment (start 141.224 78.232) (end 141.224 77.851) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD8B))
  (segment (start 112.014 80.391) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD5B))
  (segment (start 112.014 79.375) (end 112.014 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD82))
  (segment (start 112.014 79.883) (end 112.014 79.375) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDCD))
  (via (at 140.335 82.296) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1E1))
  (segment (start 141.224 80.391) (end 141.224 80.645) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD67))
  (via (at 169.418 82.042) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3C1DE))
  (segment (start 170.422 80.391) (end 170.422 80.657) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD40))
  (segment (start 141.224 80.391) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDAC))
  (segment (start 141.224 81.116) (end 141.224 81.28) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6A))
  (segment (start 140.870999 81.469001) (end 141.224 81.116) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDB5))
  (segment (start 140.399999 81.469001) (end 140.870999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE7E))
  (segment (start 139.7 82.169) (end 140.399999 81.469001) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BDC1))
  (segment (start 152.781 78.232) (end 152.781 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE00))
  (segment (start 150.749 78.232) (end 152.781 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD91))
  (segment (start 123.444 78.486) (end 123.444 78.891) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE30))
  (segment (start 123.444 78.232) (end 123.444 78.486) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE75))
  (segment (start 121.414 78.232) (end 123.444 78.232) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE48))
  (via (at 140.335 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 142.24 95.25) (end 140.335 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 129.54 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 131.445 95.25) (end 129.54 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 158.75 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BC3E595))
  (segment (start 160.54 95.25) (end 158.75 95.25) (width 0.35) (layer F.Cu) (net 8))
  (via (at 169.545 94.996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 171.22 95.25) (end 169.545 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 95.25) (end 100.33 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 103.505 97.63) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 97.515) (end 102.235 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.12 95.25) (end 102.12 97.515) (width 0.35) (layer F.Cu) (net 8))
  (via (at 123.825 97.79) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 8))
  (segment (start 124.095 97.52) (end 123.825 97.79) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 125.415 97.52) (end 124.095 97.52) (width 0.35) (layer B.Cu) (net 8))
  (via (at 111.125 94.869) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 112.8 95.25) (end 111.125 95.25) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 156.271 83.852) (end 156.271 83.5) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 155.805 83.096) (end 155.805 82.296) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 156.209 83.5) (end 155.805 83.096) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 156.271 83.5) (end 156.209 83.5) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 112.014 80.391) (end 112.014 81.153) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BE39))
  (segment (start 112.014 81.153) (end 110.998 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BF53))
  (segment (start 110.998 82.169) (end 110.49 82.169) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BC3BD6D))
  (segment (start 111.3559 53.736) (end 111.7099 54.09) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC89A8))
  (segment (start 111.7099 54.09) (end 111.7099 55.245) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC89AB))
  (segment (start 111.3559 50.976) (end 111.3559 53.736) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC89AE))
  (segment (start 136.078729 33.241) (end 136.06361 33.256119) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A824))
  (segment (start 137.7696 33.241) (end 136.078729 33.241) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A827))
  (segment (start 135.263611 32.45612) (end 136.06361 33.256119) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A82A))
  (segment (start 133.0796 32.1855) (end 134.992991 32.1855) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A82D))
  (segment (start 134.992991 32.1855) (end 135.263611 32.45612) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A830))
  (via (at 133.0706 34.9885) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8) (tstamp 5BD0A863))
  (segment (start 133.0796 34.9795) (end 133.0706 34.9885) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A833))
  (segment (start 133.0796 32.1855) (end 133.0796 34.9795) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BD0A836))
  (via (at 111.0615 82.271021) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 181.4322 78.232) (end 182.5752 77.089) (width 0.35) (layer F.Cu) (net 8))
  (via (at 182.5752 77.089) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 179.959 78.232) (end 181.4322 78.232) (width 0.35) (layer F.Cu) (net 8))
  (via (at 110.4138 65.6336) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 115.062 66.802) (end 115.2144 66.6496) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 112.014 66.802) (end 115.062 66.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 143.637 66.802) (end 144.1196 66.3194) (width 0.35) (layer F.Cu) (net 8))
  (via (at 139.6746 66.2432) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 141.349 66.802) (end 143.637 66.802) (width 0.35) (layer F.Cu) (net 8))
  (via (at 168.9608 66.2432) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 169.3926 66.802) (end 168.9608 66.3702) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 170.559 66.802) (end 169.3926 66.802) (width 0.35) (layer F.Cu) (net 8))
  (via (at 154.2034 66.3194) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 153.7208 66.802) (end 154.2034 66.3194) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 150.749 66.802) (end 153.7208 66.802) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 142.24 95.25) (end 142.24 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 131.445 95.25) (end 131.445 97.63) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.164 61.2255) (end 73.216 61.2775) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.216 61.2775) (end 73.216 67.0275) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.216 70.3725) (end 73.2475 70.404) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.216 67.0275) (end 73.216 70.3725) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.2475 72.129) (end 73.2475 76.154) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.2475 70.404) (end 73.2475 72.129) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 73.2475 79.4845) (end 73.2475 76.154) (width 0.35) (layer F.Cu) (net 8))
  (via (at 95.25 68.58) (size 1.4) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 95.25 68.58) (end 95.25 66.04) (width 0.35) (layer B.Cu) (net 8))
  (segment (start 92.71 68.58) (end 95.25 68.58) (width 0.35) (layer B.Cu) (net 8))
  (via (at 154.809692 77.78249) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 157.859 78.232) (end 155.259202 78.232) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 155.259202 78.232) (end 154.809692 77.78249) (width 0.35) (layer F.Cu) (net 8))
  (via (at 125.920792 77.78249) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 128.649 78.232) (end 126.370302 78.232) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 126.370302 78.232) (end 125.920792 77.78249) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 102.6929 46.076) (end 104.5559 46.076) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8972))
  (segment (start 104.5559 46.076) (end 105.6559 46.076) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8975))
  (segment (start 102.4139 46.355) (end 102.6929 46.076) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC8978))
  (segment (start 101.6889 46.355) (end 102.4139 46.355) (width 0.35) (layer F.Cu) (net 8) (tstamp 5BCC897B))
  (via (at 100.2665 46.2915) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 8))
  (segment (start 100.687504 46.47) (end 100.546502 46.328998) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 101.6889 46.47) (end 100.687504 46.47) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 100.4055 46.47) (end 100.3935 46.482) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 101.6889 46.47) (end 100.4055 46.47) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 171.958 74.422) (end 170.434 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 75.438) (end 171.958 74.422) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 172.974 80.5434) (end 172.974 75.438) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.1927 83.3247) (end 172.974 80.5434) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 170.1927 83.9724) (end 170.1927 83.3247) (width 0.35) (layer F.Cu) (net 9))
  (segment (start 171.6017 83.3724) (end 171.6621 83.312) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 171.6017 83.9724) (end 171.6017 83.3724) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.0215 73.152) (end 170.434 73.152) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 74.7395) (end 172.0215 73.152) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 173.609 81.3651) (end 173.609 74.7395) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 171.6017 83.3724) (end 173.609 81.3651) (width 0.35) (layer F.Cu) (net 10))
  (segment (start 172.9987 83.3724) (end 173.0591 83.312) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.9987 83.9724) (end 172.9987 83.3724) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.0215 71.882) (end 170.434 71.882) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 82.1271) (end 174.244 74.1045) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.244 74.1045) (end 172.0215 71.882) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 172.9987 83.3724) (end 174.244 82.1271) (width 0.35) (layer F.Cu) (net 11))
  (segment (start 174.879 73.533) (end 171.958 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.879 82.8294) (end 174.879 73.533) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 171.958 70.612) (end 170.434 70.612) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.3247) (end 174.879 82.8294) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 174.3837 83.9724) (end 174.3837 83.3247) (width 0.35) (layer F.Cu) (net 12))
  (segment (start 132.423001 71.203991) (end 133.223 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 145.9865 72.00399) (end 144.85513 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (via (at 175.3235 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 103.27633 71.203991) (end 104.076329 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 128.649 69.342) (end 130.56101 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 162.4965 72.00399) (end 161.36513 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (via (at 145.9865 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 170.559 69.342) (end 172.66151 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 174.523501 71.203991) (end 175.3235 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 144.85513 72.00399) (end 133.223 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 143.32451 69.342) (end 145.186501 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (via (at 104.076329 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 157.859 69.342) (end 159.83451 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 161.696501 71.203991) (end 162.4965 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (via (at 133.223 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (via (at 162.4965 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 130.56101 69.342) (end 132.423001 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 172.66151 69.342) (end 174.523501 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 141.349 69.342) (end 143.32451 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 145.186501 71.203991) (end 145.9865 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (via (at 116.6495 72.00399) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 13))
  (segment (start 161.36513 72.00399) (end 145.9865 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 113.98751 69.342) (end 115.849501 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 132.09163 72.00399) (end 116.6495 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 112.014 69.342) (end 113.98751 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 159.83451 69.342) (end 161.696501 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 174.19213 72.00399) (end 162.4965 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 115.849501 71.203991) (end 116.6495 72.00399) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 116.6495 72.00399) (end 104.076329 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 101.414339 69.342) (end 103.27633 71.203991) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 175.3235 72.00399) (end 174.19213 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 133.223 72.00399) (end 132.09163 72.00399) (width 0.35) (layer B.Cu) (net 13))
  (segment (start 99.439 69.342) (end 101.414339 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 175.514 73.66) (end 178.562 70.612) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 178.562 70.612) (end 179.959 70.612) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.514 83.058) (end 175.514 73.66) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.7807 83.3247) (end 175.514 83.058) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 175.7807 83.9724) (end 175.7807 83.3247) (width 0.35) (layer F.Cu) (net 14))
  (segment (start 178.562 71.882) (end 179.834 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 74.295) (end 178.562 71.882) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 176.149 82.296) (end 176.149 74.295) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.3247) (end 176.149 82.296) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 177.1777 83.9724) (end 177.1777 83.3247) (width 0.35) (layer F.Cu) (net 15))
  (segment (start 178.562 73.152) (end 179.834 73.152) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 74.93) (end 178.562 73.152) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.312) (end 176.784 81.534) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 83.3597) (end 178.562 83.312) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.5747 83.3724) (end 178.562 83.3597) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 176.784 81.534) (end 176.784 74.93) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.5747 83.9724) (end 178.5747 83.3724) (width 0.35) (layer F.Cu) (net 16))
  (segment (start 178.562 74.422) (end 179.834 74.422) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 75.565) (end 178.562 74.422) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 177.419 80.8863) (end 177.419 75.565) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.9717 83.439) (end 177.419 80.8863) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 179.9717 83.9724) (end 179.9717 83.439) (width 0.35) (layer F.Cu) (net 17))
  (segment (start 165.9255 74.422) (end 167.259 74.422) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 76.2635) (end 165.9255 74.422) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 164.084 80.045) (end 164.084 76.2635) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 167.386 83.347) (end 164.084 80.045) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 167.386 83.947) (end 167.386 83.347) (width 0.35) (layer F.Cu) (net 18))
  (segment (start 165.9255 73.152) (end 167.259 73.152) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 163.449 75.6285) (end 165.9255 73.152) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 163.449 80.807) (end 163.449 75.6285) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.347) (end 163.449 80.807) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.989 83.947) (end 165.989 83.347) (width 0.35) (layer F.Cu) (net 19))
  (segment (start 165.862 71.882) (end 167.259 71.882) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 81.569) (end 162.814 74.93) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.592 83.347) (end 162.814 81.569) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 162.814 74.93) (end 165.862 71.882) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 164.592 83.947) (end 164.592 83.347) (width 0.35) (layer F.Cu) (net 20))
  (segment (start 165.7985 70.612) (end 167.259 70.612) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 74.2315) (end 165.7985 70.612) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 162.179 82.331) (end 162.179 74.2315) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 163.195 83.347) (end 162.179 82.331) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 163.195 83.947) (end 163.195 83.347) (width 0.35) (layer F.Cu) (net 21))
  (segment (start 161.544 83.093) (end 161.798 83.347) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 83.093) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.798 83.347) (end 161.798 83.947) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.927) (end 161.544 81.534) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 159.258 70.612) (end 157.859 70.612) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 72.898) (end 159.258 70.612) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 161.544 81.534) (end 161.544 72.898) (width 0.35) (layer F.Cu) (net 22))
  (segment (start 160.401 83.347) (end 160.401 83.947) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 82.804011) (end 160.401 83.347) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.804011) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 82.596989) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 159.1945 71.882) (end 157.859 71.882) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 73.631489) (end 159.1945 71.882) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 160.943989 81.534) (end 160.943989 73.631489) (width 0.35) (layer F.Cu) (net 23))
  (segment (start 159.004 83.947) (end 159.004 83.347) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 82.159011) (end 160.191989 74.159989) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 160.191989 74.159989) (end 159.184 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.004 83.347) (end 160.191989 82.159011) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 73.152) (end 157.859 73.152) (width 0.35) (layer F.Cu) (net 24))
  (segment (start 159.184 74.422) (end 159.524 74.762) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BEED))
  (segment (start 157.859 74.422) (end 159.184 74.422) (width 0.35) (layer F.Cu) (net 25) (tstamp 5BC3BF23) (status 10))
  (segment (start 157.607 83.347) (end 159.524 81.43) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 81.43) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 157.607 83.947) (end 157.607 83.347) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 159.524 74.762) (end 159.524 80.137) (width 0.35) (layer F.Cu) (net 25))
  (segment (start 143.764 80.553) (end 143.764 75.5015) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 143.764 75.5015) (end 142.6845 74.422) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.97 83.347) (end 143.764 80.553) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 142.6845 74.422) (end 141.224 74.422) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 140.97 83.947) (end 140.97 83.347) (width 0.35) (layer F.Cu) (net 26))
  (segment (start 144.354011 74.758011) (end 142.748 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.748 73.152) (end 141.224 73.152) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 144.354011 81.359989) (end 144.354011 74.758011) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.347) (end 144.354011 81.359989) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 142.367 83.947) (end 142.367 83.347) (width 0.35) (layer F.Cu) (net 27))
  (segment (start 141.224 71.882) (end 142.549 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 142.748 71.882) (end 141.224 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 74.168) (end 142.748 71.882) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.034 82.077) (end 145.034 74.168) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.347) (end 145.034 82.077) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 143.764 83.947) (end 143.764 83.347) (width 0.35) (layer F.Cu) (net 28))
  (segment (start 145.669 82.839) (end 145.669 81.788) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.947) (end 145.161 83.347) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.161 83.347) (end 145.669 82.839) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 81.788) (end 145.669 81.927) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 142.748 70.612) (end 141.224 70.612) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 73.533) (end 142.748 70.612) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 145.669 81.788) (end 145.669 73.533) (width 0.35) (layer F.Cu) (net 29))
  (segment (start 149.4155 70.612) (end 150.624 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.304 73.7235) (end 149.4155 70.612) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.304 83.093) (end 146.304 73.7235) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.347) (end 146.304 83.093) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 146.558 83.947) (end 146.558 83.347) (width 0.35) (layer F.Cu) (net 30))
  (segment (start 149.352 71.882) (end 150.624 71.882) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 74.295) (end 149.352 71.882) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 146.939 82.296) (end 146.939 74.295) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 147.955 83.312) (end 146.939 82.296) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 147.955 83.947) (end 147.955 83.312) (width 0.35) (layer F.Cu) (net 31))
  (segment (start 149.4155 73.152) (end 150.624 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 74.9935) (end 149.4155 73.152) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 147.574 81.534) (end 147.574 74.9935) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.312) (end 147.574 81.534) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 83.947) (end 149.352 83.312) (width 0.35) (layer F.Cu) (net 32))
  (segment (start 149.352 74.422) (end 150.624 74.422) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.209 75.565) (end 149.352 74.422) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.209 80.899) (end 148.209 75.565) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 148.2375 80.899) (end 148.209 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 150.6855 83.347) (end 148.2375 80.899) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 150.6855 83.947) (end 150.6855 83.347) (width 0.35) (layer F.Cu) (net 33))
  (segment (start 138.176 83.347) (end 138.176 83.947) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 76.272) (end 134.874 80.045) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 134.874 80.045) (end 138.176 83.347) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 136.724 74.422) (end 134.874 76.272) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 138.049 74.422) (end 136.724 74.422) (width 0.35) (layer F.Cu) (net 34))
  (segment (start 136.779 83.312) (end 136.779 83.947) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 75.637) (end 134.239 80.772) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 136.724 73.152) (end 134.239 75.637) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 134.239 80.772) (end 136.779 83.312) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 138.049 73.152) (end 136.724 73.152) (width 0.35) (layer F.Cu) (net 35))
  (segment (start 135.382 83.347) (end 135.382 83.947) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 137.374 71.882) (end 136.724 72.532) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 81.534) (end 135.382 83.312) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 135.382 83.312) (end 135.382 83.347) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 138.049 71.882) (end 137.374 71.882) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.724 72.532) (end 136.2884 72.532) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 136.2884 72.532) (end 133.604 75.2164) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.604 75.2164) (end 133.604 81.534) (width 0.35) (layer F.Cu) (net 36))
  (segment (start 133.985 83.347) (end 133.95 83.312) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 133.985 83.947) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 75.017) (end 132.969 82.331) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 138.049 70.612) (end 137.374 70.612) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.969 82.331) (end 133.985 83.347) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 137.374 70.612) (end 132.969 75.017) (width 0.35) (layer F.Cu) (net 37))
  (segment (start 132.588 83.347) (end 132.588 83.947) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 83.093) (end 132.588 83.347) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 129.974 70.612) (end 132.334 72.972) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 132.334 72.972) (end 132.334 83.093) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 128.649 70.612) (end 129.974 70.612) (width 0.35) (layer F.Cu) (net 38))
  (segment (start 131.191 83.347) (end 131.191 83.947) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 73.607) (end 131.699 82.839) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 131.699 82.839) (end 131.191 83.347) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 129.974 71.882) (end 131.699 73.607) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 128.649 71.882) (end 129.974 71.882) (width 0.35) (layer F.Cu) (net 39))
  (segment (start 129.794 83.347) (end 129.794 83.947) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 131.064 82.077) (end 129.794 83.347) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 131.064 74.242) (end 131.064 82.077) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 129.974 73.152) (end 131.064 74.242) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 128.649 73.152) (end 129.974 73.152) (width 0.35) (layer F.Cu) (net 40))
  (segment (start 128.397 83.947) (end 128.397 83.347) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 128.397 83.347) (end 130.413989 81.330011) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 129.974 74.422) (end 128.649 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFEF) (status 20))
  (segment (start 130.413989 81.330011) (end 130.413989 80.772) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 80.772) (end 130.413989 74.861989) (width 0.35) (layer F.Cu) (net 41))
  (segment (start 130.413989 74.861989) (end 129.974 74.422) (width 0.35) (layer F.Cu) (net 41) (tstamp 5BC3BFBF))
  (segment (start 114.554 80.518) (end 111.76 83.312) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 111.76 83.312) (end 111.76 83.947) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 114.554 75.057) (end 114.554 80.518) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.919 74.422) (end 114.554 75.057) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 112.014 74.422) (end 113.919 74.422) (width 0.35) (layer F.Cu) (net 42))
  (segment (start 113.6015 73.152) (end 112.014 73.152) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.189 74.7395) (end 113.6015 73.152) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 115.189 81.28) (end 115.189 74.7395) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.157 83.312) (end 115.189 81.28) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.157 83.947) (end 113.157 83.312) (width 0.35) (layer F.Cu) (net 43))
  (segment (start 113.3475 71.882) (end 112.014 71.882) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 74.3585) (end 113.3475 71.882) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 115.824 82.042) (end 115.824 74.3585) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 114.554 83.312) (end 115.824 82.042) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 114.554 83.947) (end 114.554 83.312) (width 0.35) (layer F.Cu) (net 44))
  (segment (start 113.339 70.612) (end 112.014 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 82.839) (end 116.459 73.732) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 116.459 73.732) (end 113.339 70.612) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.347) (end 116.459 82.839) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 115.951 83.947) (end 115.951 83.347) (width 0.35) (layer F.Cu) (net 45))
  (segment (start 120.015 70.612) (end 121.414 70.612) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 73.533) (end 120.015 70.612) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.094 82.562) (end 117.094 73.533) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.348 82.816) (end 117.094 82.562) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 117.348 83.947) (end 117.348 82.816) (width 0.35) (layer F.Cu) (net 46))
  (segment (start 120.0785 71.882) (end 121.414 71.882) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 74.2315) (end 120.0785 71.882) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 117.729 82.331) (end 117.729 74.2315) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.745 83.347) (end 117.729 82.331) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 118.745 83.947) (end 118.745 83.347) (width 0.35) (layer F.Cu) (net 47))
  (segment (start 120.142 73.152) (end 121.414 73.152) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 74.93) (end 120.142 73.152) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 118.364 81.569) (end 118.364 74.93) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.142 83.347) (end 118.364 81.569) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 120.142 83.947) (end 120.142 83.347) (width 0.35) (layer F.Cu) (net 48))
  (segment (start 121.539 83.947) (end 121.539 83.347) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 121.539 83.347) (end 118.999 80.807) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 119.7064 74.422) (end 120.089 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 80.807) (end 118.999 75.1294) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 118.999 75.1294) (end 119.7064 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 120.089 74.422) (end 121.414 74.422) (width 0.35) (layer F.Cu) (net 49))
  (segment (start 107.5055 74.422) (end 108.839 74.422) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 105.664 76.2635) (end 107.5055 74.422) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 105.664 80.045) (end 105.664 76.2635) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 108.966 83.347) (end 105.664 80.045) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 108.966 83.947) (end 108.966 83.347) (width 0.35) (layer F.Cu) (net 50))
  (segment (start 107.5055 73.152) (end 108.839 73.152) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 75.6285) (end 107.5055 73.152) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 105.029 80.807) (end 105.029 75.6285) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.569 83.347) (end 105.029 80.807) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.569 83.947) (end 107.569 83.347) (width 0.35) (layer F.Cu) (net 51))
  (segment (start 107.442 71.882) (end 108.839 71.882) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 74.93) (end 107.442 71.882) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 104.394 81.581) (end 104.394 74.93) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 106.172 83.359) (end 104.394 81.581) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 106.172 83.959) (end 106.172 83.359) (width 0.35) (layer F.Cu) (net 52))
  (segment (start 103.759 74.422) (end 107.569 70.612) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 107.569 70.612) (end 108.839 70.612) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 103.759 82.296) (end 103.759 74.422) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 104.775 83.312) (end 103.759 82.296) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 104.775 83.947) (end 104.775 83.312) (width 0.35) (layer F.Cu) (net 53))
  (segment (start 103.124 72.898) (end 100.838 70.612) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 100.838 70.612) (end 99.439 70.612) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.124 83.093) (end 103.124 72.898) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.378 83.347) (end 103.124 83.093) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 103.378 83.947) (end 103.378 83.347) (width 0.35) (layer F.Cu) (net 54))
  (segment (start 100.584 71.882) (end 99.439 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 102.489 73.66) (end 100.711 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 102.489 82.839) (end 102.489 73.66) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.981 83.347) (end 102.489 82.839) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 100.711 71.882) (end 100.584 71.882) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.981 83.947) (end 101.981 83.347) (width 0.35) (layer F.Cu) (net 55))
  (segment (start 101.854 74.242) (end 100.764 73.152) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 101.854 82.077) (end 101.854 74.242) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.764 73.152) (end 99.439 73.152) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 83.347) (end 101.854 82.077) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 83.947) (end 100.584 83.347) (width 0.35) (layer F.Cu) (net 56))
  (segment (start 100.584 74.422) (end 99.439 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BF29) (status 20))
  (segment (start 101.219 75.057) (end 100.584 74.422) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3C0AC))
  (segment (start 101.219 81.327) (end 101.219 79.502) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC77))
  (segment (start 99.187 83.959) (end 99.187 83.359) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC6B))
  (segment (start 101.219 79.502) (end 101.219 75.057) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC5F))
  (segment (start 99.187 83.359) (end 101.219 81.327) (width 0.35) (layer F.Cu) (net 57) (tstamp 5BC3BC7D))
  (segment (start 170.1927 90.813115) (end 171.466915 92.08733) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.1927 85.4724) (end 170.1927 90.813115) (width 0.35) (layer F.Cu) (net 58))
  (segment (start 170.823172 89.638927) (end 171.466915 90.28267) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 170.823172 86.850928) (end 170.823172 89.638927) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 86.0724) (end 170.823172 86.850928) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 171.6017 85.4724) (end 171.6017 86.0724) (width 0.35) (layer F.Cu) (net 59))
  (segment (start 172.9987 86.0724) (end 172.5841 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.9987 85.4724) (end 172.9987 86.0724) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.5841 86.487) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 172.527667 88.82267) (end 172.527667 86.487) (width 0.35) (layer F.Cu) (net 60))
  (segment (start 174.3837 88.1253) (end 174.244 88.265) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 174.3837 85.4724) (end 174.3837 88.1253) (width 0.35) (layer F.Cu) (net 61))
  (segment (start 175.7807 88.643037) (end 175.960333 88.82267) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 175.7807 85.4724) (end 175.7807 88.643037) (width 0.35) (layer F.Cu) (net 62))
  (segment (start 177.1777 90.126055) (end 177.021085 90.28267) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 177.1777 85.4724) (end 177.1777 90.126055) (width 0.35) (layer F.Cu) (net 63))
  (segment (start 178.5747 90.533715) (end 177.021085 92.08733) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 178.5747 85.4724) (end 178.5747 90.533715) (width 0.35) (layer F.Cu) (net 64))
  (segment (start 176.769882 93.54733) (end 175.960333 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 177.310383 93.54733) (end 176.769882 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 90.886013) (end 177.310383 93.54733) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 179.9717 85.4724) (end 179.9717 90.886013) (width 0.35) (layer F.Cu) (net 65))
  (segment (start 167.196 93.535) (end 165.974882 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.275 92.456) (end 167.196 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 168.275 87.376) (end 168.275 92.456) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 86.487) (end 168.275 87.376) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 165.974882 93.535) (end 165.165333 93.535) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.386 85.447) (end 167.386 86.487) (width 0.35) (layer F.Cu) (net 66))
  (segment (start 167.459838 87.703838) (end 165.989 86.233) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.478494 89.773451) (end 167.459838 89.754795) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 165.989 86.233) (end 165.989 85.447) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.459838 89.754795) (end 167.459838 87.703838) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 167.478494 90.612721) (end 167.478494 89.773451) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 91.86513) (end 167.478494 90.612721) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.226085 92.075) (end 166.226085 91.86513) (width 0.35) (layer F.Cu) (net 67))
  (segment (start 166.869828 89.626597) (end 166.226085 90.27034) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 166.869828 88.324828) (end 166.869828 89.626597) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 86.047) (end 166.869828 88.324828) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 164.592 85.447) (end 164.592 86.047) (width 0.35) (layer F.Cu) (net 68))
  (segment (start 165.165333 88.017333) (end 165.165333 88.81034) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 86.047) (end 165.165333 88.017333) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.195 85.447) (end 163.195 86.047) (width 0.35) (layer F.Cu) (net 69))
  (segment (start 163.449 88.00267) (end 163.449 88.25267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 86.35167) (end 163.449 88.00267) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 161.798 85.447) (end 161.798 86.35167) (width 0.35) (layer F.Cu) (net 70))
  (segment (start 160.401 87.478673) (end 161.732667 88.81034) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 160.401 85.447) (end 160.401 87.478673) (width 0.35) (layer F.Cu) (net 71))
  (segment (start 159.004 85.447) (end 159.004 86.106) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 89.110425) (end 160.063575 89.662) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 86.614) (end 159.512 89.110425) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 160.063575 89.662) (end 160.671915 90.27034) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 159.512 86.614) (end 159.004 86.106) (width 0.35) (layer F.Cu) (net 72))
  (segment (start 157.607 85.447) (end 157.607 86.106) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 159.004 90.407085) (end 160.671915 92.075) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 90.153085) (end 159.004 90.407085) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 87.249) (end 158.75 90.153085) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 158.75 87.249) (end 157.607 86.106) (width 0.35) (layer F.Cu) (net 73))
  (segment (start 141.61733 92.08733) (end 142.256915 92.08733) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.716 91.186) (end 141.61733 92.08733) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.716 86.614) (end 140.716 91.186) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.97 86.36) (end 140.716 86.614) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 140.97 85.447) (end 140.97 86.36) (width 0.35) (layer F.Cu) (net 74))
  (segment (start 141.613172 89.638927) (end 142.256915 90.28267) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 141.613172 86.800828) (end 141.613172 89.638927) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 86.047) (end 141.613172 86.800828) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 142.367 85.447) (end 142.367 86.047) (width 0.35) (layer F.Cu) (net 75))
  (segment (start 143.764 85.447) (end 143.764 85.979) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.317667 86.425333) (end 143.317667 88.82267) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 143.764 85.979) (end 143.317667 86.425333) (width 0.35) (layer F.Cu) (net 76))
  (segment (start 145.161 88.138) (end 145.034 88.265) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 145.161 85.447) (end 145.161 88.138) (width 0.35) (layer F.Cu) (net 77))
  (segment (start 146.558 88.630337) (end 146.750333 88.82267) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 146.558 85.447) (end 146.558 88.630337) (width 0.35) (layer F.Cu) (net 78))
  (segment (start 147.955 90.138755) (end 147.811085 90.28267) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 147.955 85.447) (end 147.955 90.138755) (width 0.35) (layer F.Cu) (net 79))
  (segment (start 149.352 90.546415) (end 149.352 85.447) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 149.352 91.476899) (end 149.352 90.546415) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 148.741569 92.08733) (end 149.352 91.476899) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 147.811085 92.08733) (end 148.741569 92.08733) (width 0.35) (layer F.Cu) (net 80))
  (segment (start 147.559882 93.54733) (end 146.750333 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.100383 93.54733) (end 147.559882 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 148.100383 93.54733) (end 149.14967 93.54733) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 90.297) (end 150.6855 92.0115) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.114 92.583) (end 150.241 92.456) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 149.14967 93.54733) (end 150.114 92.583) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 85.447) (end 150.6855 90.297) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 150.6855 92.0115) (end 150.114 92.583) (width 0.35) (layer F.Cu) (net 81))
  (segment (start 138.938 86.995) (end 138.176 86.233) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.176 86.233) (end 138.176 85.447) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.938 92.837) (end 138.938 86.995) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.22767 93.54733) (end 138.938 92.837) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 135.955333 93.54733) (end 138.22767 93.54733) (width 0.35) (layer F.Cu) (net 82))
  (segment (start 138.268494 87.536494) (end 138.268494 90.834921) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 86.047) (end 138.268494 87.536494) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 136.779 85.447) (end 136.779 86.047) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.016085 92.08733) (end 138.268494 90.834921) (width 0.35) (layer F.Cu) (net 83))
  (segment (start 137.659828 89.638927) (end 137.016085 90.28267) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 86.047) (end 137.659828 88.324828) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 137.659828 88.324828) (end 137.659828 89.638927) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.382 85.447) (end 135.382 86.047) (width 0.35) (layer F.Cu) (net 84))
  (segment (start 135.955333 88.017333) (end 135.955333 88.82267) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 86.047) (end 135.955333 88.017333) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 133.985 85.447) (end 133.985 86.047) (width 0.35) (layer F.Cu) (net 85))
  (segment (start 132.588 86.364) (end 132.588 85.447) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.015) (end 132.588 86.364) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 134.239 88.265) (end 134.239 88.015) (width 0.35) (layer F.Cu) (net 86))
  (segment (start 131.191 87.491003) (end 132.522667 88.82267) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 131.191 85.447) (end 131.191 87.491003) (width 0.35) (layer F.Cu) (net 87))
  (segment (start 130.429 89.249755) (end 130.429 86.741) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 129.794 85.447) (end 129.794 86.106) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 130.429 86.741) (end 129.794 86.106) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 130.429 89.249755) (end 131.461915 90.28267) (width 0.35) (layer F.Cu) (net 88))
  (segment (start 128.397 86.233) (end 128.397 85.447) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 129.798585 87.634585) (end 128.397 86.233) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 129.798585 90.424) (end 129.798585 87.634585) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 131.461915 92.08733) (end 129.798585 90.424) (width 0.35) (layer F.Cu) (net 89))
  (segment (start 111.76 90.800415) (end 113.046915 92.08733) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 111.76 85.447) (end 111.76 90.800415) (width 0.35) (layer F.Cu) (net 90))
  (segment (start 112.403172 89.638927) (end 113.046915 90.28267) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 112.403172 86.800828) (end 112.403172 89.638927) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 86.047) (end 112.403172 86.800828) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 113.157 85.447) (end 113.157 86.047) (width 0.35) (layer F.Cu) (net 91))
  (segment (start 114.554 85.979) (end 114.554 85.447) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 86.425333) (end 114.554 85.979) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 114.107667 88.82267) (end 114.107667 86.425333) (width 0.35) (layer F.Cu) (net 92))
  (segment (start 115.951 88.138) (end 115.824 88.265) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 115.951 85.447) (end 115.951 88.138) (width 0.35) (layer F.Cu) (net 93))
  (segment (start 117.348 88.630337) (end 117.540333 88.82267) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 117.348 85.447) (end 117.348 88.630337) (width 0.35) (layer F.Cu) (net 94))
  (segment (start 118.745 90.138755) (end 118.601085 90.28267) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 118.745 85.447) (end 118.745 90.138755) (width 0.35) (layer F.Cu) (net 95))
  (segment (start 120.142 90.546415) (end 118.601085 92.08733) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.142 85.447) (end 120.142 90.546415) (width 0.35) (layer F.Cu) (net 96))
  (segment (start 120.777 87.376) (end 121.539 86.614) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 120.777 92.456) (end 120.777 87.376) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 119.68567 93.54733) (end 120.777 92.456) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 121.539 86.614) (end 121.539 85.447) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 117.540333 93.54733) (end 119.68567 93.54733) (width 0.35) (layer F.Cu) (net 97))
  (segment (start 109.855 92.164534) (end 108.458 93.561534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 109.855 86.936) (end 109.855 92.164534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.458 93.561534) (end 106.673633 93.561534) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.966 86.047) (end 109.855 86.936) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 108.966 85.447) (end 108.966 86.047) (width 0.35) (layer F.Cu) (net 98))
  (segment (start 107.569 86.047) (end 109.22 87.698) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 107.569 85.447) (end 107.569 86.047) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 90.615919) (end 107.734385 92.101534) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 109.22 87.698) (end 109.22 90.615919) (width 0.35) (layer F.Cu) (net 99))
  (segment (start 108.378128 89.653131) (end 107.734385 90.296874) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 108.378128 88.265128) (end 108.378128 89.653131) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 86.059) (end 108.378128 88.265128) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.172 85.459) (end 106.172 86.059) (width 0.35) (layer F.Cu) (net 100))
  (segment (start 106.673633 87.945633) (end 106.673633 87.95306) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 106.673633 87.95306) (end 106.673633 88.836874) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 86.047) (end 106.673633 87.945633) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.775 85.447) (end 104.775 86.047) (width 0.35) (layer F.Cu) (net 101))
  (segment (start 104.9573 88.029204) (end 104.9573 88.279204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 86.449904) (end 104.9573 88.029204) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 103.378 85.447) (end 103.378 86.449904) (width 0.35) (layer F.Cu) (net 102))
  (segment (start 101.981 87.576907) (end 103.240967 88.836874) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 101.981 85.447) (end 101.981 87.576907) (width 0.35) (layer F.Cu) (net 103))
  (segment (start 100.584 88.700659) (end 102.180215 90.296874) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 100.584 85.447) (end 100.584 88.700659) (width 0.35) (layer F.Cu) (net 104))
  (segment (start 99.187 89.108319) (end 102.180215 92.101534) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 99.187 85.459) (end 99.187 89.108319) (width 0.35) (layer F.Cu) (net 105))
  (segment (start 170.434 75.692) (end 167.259 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0BB) (status 30))
  (segment (start 167.259 75.692) (end 166.584 75.692) (width 0.35) (layer F.Cu) (net 106) (tstamp 5BC3C0C4) (status 30))
  (segment (start 141.224 75.692) (end 138.049 75.692) (width 0.35) (layer F.Cu) (net 107) (tstamp 5BC3C0C1) (status 30))
  (segment (start 150.624 75.692) (end 157.859 75.692) (width 0.35) (layer F.Cu) (net 108) (tstamp 5BC3C0BE) (status 30))
  (segment (start 121.414 75.692) (end 128.649 75.692) (width 0.35) (layer F.Cu) (net 109) (tstamp 5BC3C0C7) (status 30))
  (segment (start 108.839 75.692) (end 112.014 75.692) (width 0.35) (layer F.Cu) (net 110) (tstamp 5BC3C0CA) (status 30))
  (segment (start 105.6559 49.901) (end 105.6559 49.276) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC8867))
  (segment (start 103.4869 52.07) (end 105.6559 49.901) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC8A9E))
  (segment (start 101.8159 52.07) (end 103.4869 52.07) (width 0.35) (layer F.Cu) (net 111) (tstamp 5BCC8A9B))
  (segment (start 103.0859 36.576) (end 101.8173 36.576) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC8A98))
  (segment (start 106.0859 39.576) (end 103.0859 36.576) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC8A95))
  (segment (start 107.3559 39.576) (end 106.0859 39.576) (width 0.35) (layer F.Cu) (net 112) (tstamp 5BCC8A92))
  (segment (start 117.0559 47.676) (end 118.1229 47.676) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC8A8F))
  (segment (start 120.9929 49.403) (end 120.3579 49.403) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC8A8C))
  (segment (start 118.6309 47.676) (end 117.0559 47.676) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC8A89))
  (segment (start 120.3579 49.403) (end 118.6309 47.676) (width 0.35) (layer F.Cu) (net 113) (tstamp 5BCC8AA4))
  (segment (start 102.4159 37.973) (end 101.8159 37.973) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC8AA1))
  (segment (start 102.9779 37.973) (end 102.4159 37.973) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC8A80))
  (segment (start 105.6559 40.651) (end 102.9779 37.973) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC8A7D))
  (segment (start 105.6559 41.276) (end 105.6559 40.651) (width 0.35) (layer F.Cu) (net 114) (tstamp 5BCC8A7A))
  (segment (start 112.9559 38.476) (end 112.9559 39.576) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC8A77))
  (segment (start 112.9559 37.2755) (end 112.9559 38.476) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC8A74))
  (segment (start 113.8809 36.3505) (end 112.9559 37.2755) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC8A71))
  (segment (start 113.8809 35.7505) (end 113.8809 36.3505) (width 0.35) (layer F.Cu) (net 115) (tstamp 5BCC8A6E))
  (segment (start 102.4509 47.879) (end 101.8039 47.879) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC8A6B))
  (segment (start 103.4539 46.876) (end 102.4509 47.879) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC8A68))
  (segment (start 105.6559 46.876) (end 103.4539 46.876) (width 0.35) (layer F.Cu) (net 116) (tstamp 5BCC8A65))
  (segment (start 101.8039 49.264) (end 102.4389 49.264) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC8A62))
  (segment (start 104.0269 47.676) (end 105.6559 47.676) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC8A5F))
  (segment (start 102.4389 49.264) (end 104.0269 47.676) (width 0.35) (layer F.Cu) (net 117) (tstamp 5BCC8A5C))
  (segment (start 101.8159 43.561) (end 102.4509 43.561) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC8A59))
  (segment (start 103.3659 44.476) (end 105.6559 44.476) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC8A56))
  (segment (start 102.4509 43.561) (end 103.3659 44.476) (width 0.35) (layer F.Cu) (net 118) (tstamp 5BCC8A53))
  (segment (start 103.9279 43.676) (end 104.5559 43.676) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC8A50))
  (segment (start 102.4159 42.164) (end 103.9279 43.676) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC8A4D))
  (segment (start 104.5559 43.676) (end 105.6559 43.676) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC8A86))
  (segment (start 101.8159 42.164) (end 102.4159 42.164) (width 0.35) (layer F.Cu) (net 119) (tstamp 5BCC8A83))
  (segment (start 104.1789 42.876) (end 102.0699 40.767) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC8A47))
  (segment (start 102.0699 40.767) (end 101.8159 40.767) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC8A44))
  (segment (start 105.6559 42.876) (end 104.1789 42.876) (width 0.35) (layer F.Cu) (net 120) (tstamp 5BCC8A41))
  (segment (start 120.4799 50.8) (end 120.8659 50.8) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC8A3E))
  (segment (start 118.1559 48.476) (end 120.4799 50.8) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC8A3B))
  (segment (start 117.0559 48.476) (end 118.1559 48.476) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC8A38))
  (segment (start 120.8659 50.8) (end 120.9929 50.8) (width 0.35) (layer F.Cu) (net 121) (tstamp 5BCC8A35))
  (via (at 106.553 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (via (at 118.0465 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 118.237 68.072) (end 118.0465 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 121.414 68.072) (end 118.237 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 134.874 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 135.0645 68.072) (end 134.874 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 138.049 68.072) (end 135.0645 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 147.447 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 134.874 67.8815) (end 147.447 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 147.6375 68.072) (end 147.447 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 150.749 68.072) (end 147.6375 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 163.957 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 147.447 67.8815) (end 163.957 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 164.1475 68.072) (end 163.957 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 167.259 68.072) (end 164.1475 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 176.7205 67.8815) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 163.957 67.8815) (end 176.7205 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 176.911 68.072) (end 176.7205 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 179.959 68.072) (end 176.911 68.072) (width 0.35) (layer F.Cu) (net 122))
  (via (at 126.1237 67.8561) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 124.841 67.8815) (end 134.874 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 118.0465 67.8815) (end 124.841 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 106.6165 68.072) (end 106.553 68.0085) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 107.6325 68.072) (end 106.6165 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 108.839 68.072) (end 107.6325 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 106.7435 68.072) (end 106.553 67.8815) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 108.839 68.072) (end 106.7435 68.072) (width 0.35) (layer F.Cu) (net 122))
  (segment (start 118.0465 67.8815) (end 106.553 67.8815) (width 0.35) (layer B.Cu) (net 122))
  (segment (start 115.2779 35.7505) (end 115.2779 36.322) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC8A1D))
  (segment (start 113.7559 37.844) (end 113.7559 39.576) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC8A1A))
  (segment (start 115.2779 36.322) (end 113.7559 37.844) (width 0.35) (layer F.Cu) (net 123) (tstamp 5BCC8A17))
  (segment (start 116.6749 35.7505) (end 116.6749 36.322) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC8A14))
  (segment (start 114.5559 38.441) (end 114.5559 39.576) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC8A11))
  (segment (start 116.6749 36.322) (end 114.5559 38.441) (width 0.35) (layer F.Cu) (net 124) (tstamp 5BCC8A0B))
  (via (at 182.4355 73.279) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 126))
  (segment (start 181.284 75.692) (end 182.4355 74.5405) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 182.4355 74.5405) (end 182.4355 73.279) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 179.959 75.692) (end 181.284 75.692) (width 0.35) (layer F.Cu) (net 126))
  (segment (start 182.4355 73.279) (end 103.505 73.279) (width 0.35) (layer B.Cu) (net 126))
  (segment (start 115.9809 39.576) (end 118.0719 37.485) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC89F9))
  (segment (start 115.3559 39.576) (end 115.9809 39.576) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC89F6))
  (segment (start 118.0719 37.485) (end 118.0719 36.068) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC89F3))
  (segment (start 118.0719 36.068) (end 118.0719 36.449) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC89F0))
  (segment (start 118.0719 35.7505) (end 118.0719 36.068) (width 0.35) (layer F.Cu) (net 127) (tstamp 5BCC89ED))
  (segment (start 104.6099 53.097) (end 104.6099 54.518) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC89EA))
  (segment (start 106.7309 50.976) (end 104.6099 53.097) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC89FF))
  (segment (start 104.6099 54.518) (end 104.6099 55.118) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC89FC))
  (segment (start 107.3559 50.976) (end 106.7309 50.976) (width 0.35) (layer F.Cu) (net 128) (tstamp 5BCC89E7))
  (segment (start 156.337 101.588) (end 156.349 101.6) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 157.734 104.437002) (end 157.734 104.775) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 157.123999 103.827001) (end 157.734 104.437002) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 157.123999 101.774999) (end 157.123999 103.827001) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 156.949 101.6) (end 157.123999 101.774999) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 156.349 101.6) (end 156.949 101.6) (width 0.35) (layer F.Cu) (net 129))
  (via (at 98.044 98.044) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 129))
  (segment (start 156.349 101.6) (end 152.198999 101.6) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 152.198999 101.6) (end 149.479 98.880001) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 98.880001 98.880001) (end 98.044 98.044) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 149.479 98.880001) (end 98.880001 98.880001) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 97.55101 78.37401) (end 101.31252 74.6125) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 94.615 83.656756) (end 97.55101 80.720746) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 98.044 93.472) (end 94.615 90.043) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 97.55101 80.720746) (end 97.55101 78.37401) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 94.615 90.043) (end 94.615 83.656756) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 98.044 98.044) (end 98.044 93.472) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 156.349 102.997) (end 154.432 102.997) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 154.432 102.997) (end 152.654 102.997) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 149.20999 99.55299) (end 148.463 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 148.463 99.55299) (end 98.82101 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 152.654 102.997) (end 149.20999 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 156.337 103.009) (end 156.349 102.997) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 156.337 104.775) (end 156.337 103.009) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 98.82101 99.55299) (end 97.581494 99.55299) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 96.52 98.491496) (end 96.52 96.647) (width 0.35) (layer F.Cu) (net 130))
  (via (at 96.52 96.647) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 130))
  (segment (start 97.581494 99.55299) (end 96.52 98.491496) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 96.52 96.647) (end 96.52 93.091) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 96.52 93.091) (end 93.853 90.424) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 93.853 90.424) (end 93.853 83.499504) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 100.66251 74.265508) (end 100.66251 74.2315) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 96.901 80.451504) (end 96.901 78.027018) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 93.853 83.499504) (end 96.901 80.451504) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 96.901 78.027018) (end 100.66251 74.265508) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 127.913999 103.751501) (end 127.913999 101.774999) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 127.739 101.6) (end 127.139 101.6) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 127.913999 101.774999) (end 127.739 101.6) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 128.524 104.361502) (end 127.913999 103.751501) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 128.524 104.775) (end 128.524 104.361502) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 127.139 101.6) (end 123.19 101.6) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 123.19 101.6) (end 121.793 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 97.312252 100.203) (end 95.123 98.013748) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 95.123 98.013748) (end 95.123 95.123) (width 0.35) (layer F.Cu) (net 131))
  (via (at 95.123 95.123) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 131))
  (segment (start 99.949 100.203) (end 99.628736 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 98.521748 100.203) (end 99.628736 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 99.628736 100.203) (end 97.312252 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 121.793 100.203) (end 99.949 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 99.949 100.203) (end 99.695 100.203) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 93.091 90.805) (end 93.091 83.342252) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 95.123 95.123) (end 95.123 92.837) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 93.091 83.342252) (end 96.232752 80.2005) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 95.123 92.837) (end 93.091 90.805) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 100.012499 73.996265) (end 100.0125 73.962256) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 96.232752 77.776012) (end 100.012499 73.996265) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 96.232752 80.2005) (end 96.232752 77.776012) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 127.127 102.9575) (end 127.151 102.9335) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 127.151 104.739) (end 127.127 104.763) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 127.151 102.9335) (end 127.151 104.739) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 127.151 102.9335) (end 123.49249 102.9335) (width 0.35) (layer F.Cu) (net 132))
  (via (at 93.713431 93.738569) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 132))
  (segment (start 93.713431 97.523431) (end 93.713431 94.869939) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 123.49249 102.9335) (end 121.412 100.85301) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 121.412 100.85301) (end 97.04301 100.85301) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 93.713431 94.869939) (end 93.713431 93.738569) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 97.04301 100.85301) (end 93.713431 97.523431) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 98.541 101.854) (end 97.941 101.854) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 98.703999 102.016999) (end 98.541 101.854) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 98.703999 104.164999) (end 98.703999 102.016999) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 99.314 104.775) (end 98.703999 104.164999) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 97.941 101.854) (end 97.028 101.854) (width 0.35) (layer F.Cu) (net 133))
  (via (at 92.202 95.123) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 133))
  (segment (start 92.202 97.028) (end 92.202 95.123) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 97.028 101.854) (end 92.202 97.028) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 92.202 95.123) (end 92.202 93.99163) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 91.567 93.35663) (end 91.567 82.9945) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 92.202 93.99163) (end 91.567 93.35663) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 69.722998) (end 98.69401 69.707988) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 73.491256) (end 98.679 73.025) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 94.869 77.301256) (end 98.679 73.491256) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 94.869 79.6925) (end 94.869 77.301256) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 91.567 82.9945) (end 94.869 79.6925) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 97.929 104.763) (end 97.917 104.775) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 97.929 103.251) (end 97.929 104.763) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 97.929 103.251) (end 97.329 103.251) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 90.805 96.727) (end 90.805 96.647) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 97.329 103.251) (end 90.805 96.727) (width 0.35) (layer F.Cu) (net 134))
  (via (at 90.805 96.647) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 134))
  (segment (start 94.21899 77.032012) (end 98.028989 73.222013) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.028989 73.222013) (end 98.02899 72.755756) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 94.218989 79.423257) (end 94.21899 77.032012) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 90.805 96.647) (end 90.805 82.837246) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 90.805 82.837246) (end 94.218989 79.423257) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 110.5559 39.576) (end 110.5559 37.061) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC8945))
  (segment (start 109.1819 35.687) (end 109.1819 33.274) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC8948))
  (segment (start 110.5559 37.061) (end 109.1819 35.687) (width 0.35) (layer F.Cu) (net 135) (tstamp 5BCC894E))
  (segment (start 109.7559 38.481) (end 109.7559 38.166) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC894B))
  (segment (start 109.7559 39.576) (end 109.7559 38.481) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC8A26))
  (segment (start 105.4819 34.824) (end 105.4819 33.274) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC8A23))
  (segment (start 106.8529 36.195) (end 105.4819 34.824) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC885B))
  (segment (start 108.7399 36.195) (end 106.8529 36.195) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC87FE))
  (segment (start 109.7559 37.211) (end 108.7399 36.195) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC8834))
  (segment (start 109.7559 38.481) (end 109.7559 37.211) (width 0.35) (layer F.Cu) (net 136) (tstamp 5BCC8870))
  (segment (start 113.1189 54.356) (end 113.1189 56.642) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC8879))
  (segment (start 112.1559 53.393) (end 113.1189 54.356) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC87F8))
  (segment (start 112.1559 50.976) (end 112.1559 53.393) (width 0.35) (layer F.Cu) (net 137) (tstamp 5BCC8A20))
  (segment (start 108.1559 38.471) (end 108.1559 39.576) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC8A02))
  (segment (start 107.5309 37.846) (end 108.1559 38.471) (width 0.35) (layer F.Cu) (net 138) (tstamp 5BCC8A0E))
  (segment (start 104.5219 42.076) (end 102.8319 40.386) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC8A29))
  (segment (start 102.8319 40.386) (end 101.8159 39.37) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC883A))
  (segment (start 105.6559 42.076) (end 104.5219 42.076) (width 0.35) (layer F.Cu) (net 139) (tstamp 5BCC89D8))
  (segment (start 120.3929 48.006) (end 120.9929 48.006) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC87E6))
  (segment (start 120.3579 48.006) (end 120.3929 48.006) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC87EC))
  (segment (start 119.2279 46.876) (end 120.3579 48.006) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC88A0))
  (segment (start 117.0559 46.876) (end 119.2279 46.876) (width 0.35) (layer F.Cu) (net 141) (tstamp 5BCC8891))
  (via (at 107.696 30.607) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 108.978 30.607) (end 107.696 30.607) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 106.402 30.607) (end 107.696 30.607) (width 0.35) (layer F.Cu) (net 8))
  (via (at 110.998 58.293) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 111.6189 57.6721) (end 110.998 58.293) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 111.6189 56.642) (end 111.6189 57.6721) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 160.1992 31.1912) (end 160.1992 32.6644) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 160.1992 33.9924) (end 159.734 34.4576) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 160.1992 32.6644) (end 160.1992 33.9924) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 161.4424 36.166) (end 159.734 34.4576) (width 0.35) (layer F.Cu) (net 8))
  (segment (start 161.4424 36.3424) (end 161.4424 36.166) (width 0.35) (layer F.Cu) (net 8))
  (via (at 151.6634 26.1112) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 151.5694 26.2052) (end 151.6634 26.1112) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 151.5694 28.6004) (end 151.5694 26.2052) (width 0.5) (layer F.Cu) (net 8))
  (via (at 168.8846 40.64) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 8))
  (segment (start 167.9184 39.6738) (end 168.8846 40.64) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 167.9184 35.5445) (end 167.9184 39.6738) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 96.774 57.404) (end 96.774 68.002) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 99.314 54.864) (end 96.774 57.404) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 98.114 69.342) (end 99.439 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 96.774 68.002) (end 98.114 69.342) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 99.314 51.0749) (end 99.314 54.864) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 99.7159 50.673) (end 99.314 51.0749) (width 0.35) (layer F.Cu) (net 13))
  (segment (start 100.3159 50.673) (end 99.7159 50.673) (width 0.35) (layer F.Cu) (net 13))
  (via (at 115.2652 32.7914) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 122))
  (segment (start 115.2779 32.8041) (end 115.2652 32.7914) (width 0.5) (layer F.Cu) (net 122))
  (segment (start 115.2779 34.2505) (end 115.2779 32.8041) (width 0.5) (layer F.Cu) (net 122))
  (segment (start 115.2652 30.0793) (end 118.992 26.3525) (width 0.5) (layer F.Cu) (net 122))
  (segment (start 118.992 26.3525) (end 120.142 26.3525) (width 0.5) (layer F.Cu) (net 122))
  (segment (start 115.2652 32.7914) (end 115.2652 30.0793) (width 0.5) (layer F.Cu) (net 122))
  (segment (start 116.6749 31.3436) (end 116.713 31.3055) (width 0.5) (layer F.Cu) (net 125))
  (segment (start 116.6749 34.2505) (end 116.6749 31.3436) (width 0.5) (layer F.Cu) (net 125))
  (via (at 116.713 31.3055) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 125))
  (segment (start 116.713 30.353) (end 116.713 31.3055) (width 0.5) (layer F.Cu) (net 125))
  (segment (start 118.4275 28.6385) (end 116.713 30.353) (width 0.5) (layer F.Cu) (net 125))
  (segment (start 120.142 28.6385) (end 118.4275 28.6385) (width 0.5) (layer F.Cu) (net 125))
  (via (at 118.0465 32.766) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 126))
  (segment (start 118.0719 32.7914) (end 118.0465 32.766) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 118.0719 34.2505) (end 118.0719 32.7914) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 118.0465 31.63463) (end 118.75663 30.9245) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 118.0465 32.766) (end 118.0465 31.63463) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 118.75663 30.9245) (end 119.0625 30.9245) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 120.1345 30.9245) (end 119.0625 30.9245) (width 0.5) (layer F.Cu) (net 126))
  (segment (start 101.31252 74.6125) (end 101.31252 67.119732) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 101.31252 67.119732) (end 105.679242 62.75301) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 105.679242 62.75301) (end 122.8725 62.75301) (width 0.35) (layer B.Cu) (net 129))
  (via (at 128.143 58.8645) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 129))
  (segment (start 124.25449 62.75301) (end 128.143 58.8645) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 122.8725 62.75301) (end 124.25449 62.75301) (width 0.35) (layer B.Cu) (net 129))
  (segment (start 128.143 54.991) (end 128.143 58.8645) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 123.952 50.8) (end 128.143 54.991) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 122.4929 50.8) (end 123.952 50.8) (width 0.35) (layer F.Cu) (net 129))
  (segment (start 100.66251 74.265508) (end 100.66251 67.92999) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 100.66251 67.92999) (end 100.66251 66.85049) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 100.66251 66.85049) (end 105.41 62.103) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 105.41 62.103) (end 123.6345 62.103) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 126.619 57.0865) (end 126.619 59.1185) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 126.619 59.1185) (end 126.1745 59.563) (width 0.35) (layer B.Cu) (net 130))
  (segment (start 123.6345 62.103) (end 126.1745 59.563) (width 0.35) (layer B.Cu) (net 130))
  (via (at 126.619 57.0865) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 130))
  (segment (start 124.079 52.197) (end 122.4929 52.197) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 126.619 54.737) (end 124.079 52.197) (width 0.35) (layer F.Cu) (net 130))
  (segment (start 126.619 57.0865) (end 126.619 54.737) (width 0.35) (layer F.Cu) (net 130))
  (via (at 125.114181 58.820181) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 131))
  (segment (start 124.314182 59.62018) (end 125.114181 58.820181) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 100.012499 73.996265) (end 100.0125 66.581246) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 100.0125 66.581246) (end 105.140757 61.452989) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 105.140757 61.452989) (end 122.481373 61.452989) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 122.481373 61.452989) (end 124.314182 59.62018) (width 0.35) (layer B.Cu) (net 131))
  (segment (start 124.2695 53.6575) (end 122.4795 53.6575) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 125.114181 54.502181) (end 124.2695 53.6575) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 125.114181 58.820181) (end 125.114181 54.502181) (width 0.35) (layer F.Cu) (net 131))
  (segment (start 92.329 83.151752) (end 92.329 92.354138) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 95.582742 79.89801) (end 92.329 83.151752) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 92.329 92.354138) (end 93.713431 93.738569) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 95.582742 77.506768) (end 95.582742 79.89801) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 73.727021) (end 95.582742 77.506768) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 66.055011) (end 99.362489 66.6115) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 66.6115) (end 99.362489 73.727021) (width 0.35) (layer B.Cu) (net 132))
  (via (at 100.1395 64.0715) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 132))
  (segment (start 117.3099 56.618) (end 117.3099 57.218) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 99.339501 65.382012) (end 99.339501 64.871499) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.339501 64.871499) (end 100.1395 64.0715) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 65.405) (end 99.339501 65.382012) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 66.6115) (end 99.362489 65.405) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 99.362489 65.405) (end 99.362489 65.024) (width 0.35) (layer B.Cu) (net 132))
  (segment (start 103.7926 62.9584) (end 102.6795 64.0715) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 111.5695 62.9584) (end 103.7926 62.9584) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 117.3099 57.218) (end 111.5695 62.9584) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 102.6795 64.0715) (end 100.1395 64.0715) (width 0.35) (layer F.Cu) (net 132))
  (segment (start 98.679 73.025) (end 98.679 69.977) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 69.977) (end 98.679 69.722998) (width 0.35) (layer B.Cu) (net 133))
  (via (at 101.7905 62.738) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 133))
  (segment (start 101.7905 62.738) (end 99.2505 62.738) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 63.3095) (end 98.679 64.135) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 64.135) (end 98.679 63.881) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 99.2505 62.738) (end 98.679 63.3095) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 98.679 69.977) (end 98.679 64.135) (width 0.35) (layer B.Cu) (net 133))
  (segment (start 110.9009 62.23) (end 102.2985 62.23) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 115.9129 57.218) (end 110.9009 62.23) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 102.2985 62.23) (end 101.7905 62.738) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 115.9129 56.618) (end 115.9129 57.218) (width 0.35) (layer F.Cu) (net 133))
  (segment (start 98.02899 72.755756) (end 98.02899 65.42001) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 63.119) (end 98.02899 62.81651) (width 0.35) (layer B.Cu) (net 134))
  (via (at 98.8695 61.4045) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 134))
  (segment (start 114.5159 57.218) (end 110.3294 61.4045) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 114.5159 56.618) (end 114.5159 57.218) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 98.02899 63.373) (end 98.02899 63.119) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 65.42001) (end 98.02899 63.373) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 62.24501) (end 98.8695 61.4045) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 62.738) (end 98.02899 62.24501) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 63.373) (end 98.02899 62.738) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 98.02899 62.738) (end 98.02899 62.44714) (width 0.35) (layer B.Cu) (net 134))
  (segment (start 104.14 61.4045) (end 103.1875 61.4045) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 98.8695 61.4045) (end 104.14 61.4045) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 110.3294 61.4045) (end 104.14 61.4045) (width 0.35) (layer F.Cu) (net 134))
  (segment (start 110.478 31.9779) (end 109.1819 33.274) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 110.478 30.607) (end 110.478 31.9779) (width 0.35) (layer F.Cu) (net 135))
  (segment (start 104.902 32.6941) (end 105.4819 33.274) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 104.902 30.607) (end 104.902 32.6941) (width 0.35) (layer F.Cu) (net 136))
  (segment (start 101.981 31.9793) (end 101.981 33.7185) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 101.981 33.7185) (end 106.1085 37.846) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 106.1085 37.846) (end 107.5309 37.846) (width 0.35) (layer F.Cu) (net 138))
  (segment (start 108.4199 37.084) (end 108.9559 37.62) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 103.378 31.9793) (end 103.378 34.196246) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 103.378 34.196246) (end 106.265754 37.084) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 106.265754 37.084) (end 108.4199 37.084) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 108.9559 37.62) (end 108.9559 38.476) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 108.9559 38.476) (end 108.9559 39.576) (width 0.35) (layer F.Cu) (net 140))
  (segment (start 98.806 47.879) (end 100.3039 47.879) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 98.806 47.0535) (end 98.806 47.879) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 94.0435 41.656) (end 94.0435 40.6095) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 94.0435 45.5295) (end 94.0435 41.656) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 96.393 47.879) (end 94.0435 45.5295) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 98.806 47.879) (end 96.393 47.879) (width 0.35) (layer F.Cu) (net 142))
  (segment (start 97.3455 48.5655) (end 97.3455 49.264) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 97.3455 49.264) (end 100.3039 49.264) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 93.218 42.7355) (end 92.7735 42.291) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 92.7735 42.291) (end 92.7735 40.5765) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 93.218 46.228) (end 93.218 42.7355) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 96.254 49.264) (end 93.218 46.228) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 97.3455 49.264) (end 96.254 49.264) (width 0.35) (layer F.Cu) (net 143))
  (segment (start 139.0396 39.766) (end 139.4691 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A818))
  (segment (start 139.0396 38.641) (end 139.0396 39.766) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A81E))
  (segment (start 144.5826 40.1955) (end 142.9766 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A81B))
  (segment (start 139.4691 40.1955) (end 142.9766 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A812))
  (segment (start 139.0396 37.516) (end 139.0396 38.641) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A815))
  (segment (start 138.2901 36.7665) (end 139.0396 37.516) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A80C))
  (segment (start 136.1066 36.7665) (end 138.2901 36.7665) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A80F))
  (segment (start 144.3286 40.1955) (end 143.3068 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A7F1))
  (segment (start 143.3068 40.1955) (end 143.9926 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A7DF))
  (segment (start 146.2786 40.1955) (end 144.3286 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A7E2))
  (segment (start 142.9766 40.1955) (end 143.3068 40.1955) (width 0.35) (layer F.Cu) (net 144) (tstamp 5BD0A7E5))
  (segment (start 146.2786 43.2562) (end 146.304 43.2816) (width 1) (layer F.Cu) (net 144))
  (segment (start 146.2786 40.1955) (end 146.2786 43.2562) (width 1) (layer F.Cu) (net 144))
  (segment (start 151.765 43.2816) (end 152.019 43.5356) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 152.019 43.9928) (end 152.019 43.307) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 152.019 43.5356) (end 152.019 43.9928) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 152.019 43.307) (end 152.0444 43.2816) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 152.019 43.9928) (end 152.019 45.5016) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 151.2316 43.2816) (end 152.0444 43.2816) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 146.304 43.2816) (end 151.2316 43.2816) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 151.2316 43.2816) (end 151.765 43.2816) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 170.543787 43.0276) (end 171.958 43.0276) (width 1) (layer F.Cu) (net 144))
  (segment (start 168.9186 43.0444) (end 168.9354 43.0276) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 168.9186 44.8142) (end 168.9186 43.0444) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 168.9354 43.0276) (end 170.543787 43.0276) (width 1) (layer F.Cu) (net 144))
  (segment (start 168.0718 43.0276) (end 168.9354 43.0276) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.735 40.6908) (end 165.368399 40.324199) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.735 40.6908) (end 168.0718 43.0276) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.16 38.0746) (end 165.3632 38.2778) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 164.46 38.0746) (end 165.16 38.0746) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 165.3632 38.2778) (end 165.368399 38.2778) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 164.4498 39.9034) (end 165.190599 39.9034) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 165.190599 39.9034) (end 165.368399 39.7256) (width 0.35) (layer F.Cu) (net 144))
  (segment (start 165.368399 39.7256) (end 165.368399 38.2778) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.368399 40.324199) (end 165.368399 39.7256) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.368399 38.2778) (end 165.368399 36.3728) (width 1) (layer F.Cu) (net 144))
  (segment (start 165.368399 32.983599) (end 165.368399 36.3728) (width 1) (layer F.Cu) (net 144))
  (segment (start 164.3126 31.9278) (end 165.368399 32.983599) (width 1) (layer F.Cu) (net 144))
  (segment (start 147.6121 40.1955) (end 150.1648 37.6428) (width 1) (layer F.Cu) (net 144))
  (segment (start 146.2786 40.1955) (end 147.6121 40.1955) (width 1) (layer F.Cu) (net 144))
  (segment (start 150.1648 37.6428) (end 150.1648 37.9984) (width 1) (layer F.Cu) (net 144))
  (segment (start 150.1648 37.2364) (end 150.1648 37.6428) (width 1) (layer F.Cu) (net 144))
  (segment (start 151.3332 36.068) (end 150.1648 37.2364) (width 1) (layer F.Cu) (net 144))
  (segment (start 152.4762 30.734) (end 151.3332 31.877) (width 1) (layer F.Cu) (net 144))
  (segment (start 154.051 30.734) (end 152.4762 30.734) (width 1) (layer F.Cu) (net 144))
  (segment (start 161.7828 28.448) (end 156.337 28.448) (width 1) (layer F.Cu) (net 144))
  (segment (start 156.337 28.448) (end 154.051 30.734) (width 1) (layer F.Cu) (net 144))
  (segment (start 151.3332 31.877) (end 151.3332 36.068) (width 1) (layer F.Cu) (net 144))
  (segment (start 164.3126 30.9778) (end 161.7828 28.448) (width 1) (layer F.Cu) (net 144))
  (segment (start 164.3126 31.9278) (end 164.3126 30.9778) (width 1) (layer F.Cu) (net 144))
  (segment (start 144.2542 43.2816) (end 142.3492 45.1866) (width 1) (layer F.Cu) (net 144))
  (segment (start 146.304 43.2816) (end 144.2542 43.2816) (width 1) (layer F.Cu) (net 144))
  (segment (start 141.6126 33.274) (end 141.5796 33.241) (width 0.35) (layer F.Cu) (net 145) (tstamp 5BD0A839) (status 30))
  (segment (start 142.8496 33.274) (end 141.6126 33.274) (width 0.35) (layer F.Cu) (net 145) (tstamp 5BD0A845) (status 20))
  (segment (start 141.5796 38.641) (end 141.5796 33.241) (width 0.7) (layer F.Cu) (net 145) (tstamp 5BD0A83F))
  (segment (start 141.5796 33.241) (end 142.6896 33.241) (width 0.7) (layer F.Cu) (net 145) (tstamp 5BD0A83C))
  (segment (start 141.5796 38.641) (end 140.3096 38.641) (width 0.7) (layer F.Cu) (net 145) (tstamp 5BD0A842))
  (segment (start 145.7781 33.241) (end 146.5326 33.9955) (width 0.7) (layer F.Cu) (net 145) (tstamp 5BD0A848))
  (segment (start 141.5796 33.241) (end 145.7781 33.241) (width 0.7) (layer F.Cu) (net 145) (tstamp 5BD0A851))
  (segment (start 136.8566 35.179) (end 136.1066 35.179) (width 0.35) (layer F.Cu) (net 146) (tstamp 5BD0A84E))
  (segment (start 139.0396 33.716) (end 137.5766 35.179) (width 0.35) (layer F.Cu) (net 146) (tstamp 5BD0A854))
  (segment (start 137.5766 35.179) (end 136.8566 35.179) (width 0.35) (layer F.Cu) (net 146) (tstamp 5BD0A84B))
  (segment (start 139.0396 33.241) (end 139.0396 33.716) (width 0.35) (layer F.Cu) (net 146) (tstamp 5BD0A857))
  (segment (start 141.4576 41.0845) (end 141.4526 41.0795) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A860))
  (segment (start 143.7386 41.0845) (end 141.4576 41.0845) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A85D))
  (segment (start 143.4846 41.0795) (end 141.4526 41.0795) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A85A))
  (segment (start 137.7391 38.6715) (end 137.7696 38.641) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A806))
  (segment (start 136.2456 38.6715) (end 137.7391 38.6715) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A809))
  (segment (start 137.7696 40.0685) (end 137.7696 38.641) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A7E8))
  (segment (start 138.7806 41.0795) (end 137.7696 40.0685) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A7EB))
  (segment (start 141.4526 41.0795) (end 138.7806 41.0795) (width 0.35) (layer F.Cu) (net 147) (tstamp 5BD0A7DC))
  (segment (start 161.8948 43.5356) (end 160.6432 42.284) (width 0.35) (layer F.Cu) (net 148))
  (segment (start 162.499 43.5356) (end 161.8948 43.5356) (width 0.35) (layer F.Cu) (net 148))
  (segment (start 161.449 45.3898) (end 160.6432 44.584) (width 0.35) (layer F.Cu) (net 149))
  (segment (start 162.4838 45.3898) (end 161.449 45.3898) (width 0.35) (layer F.Cu) (net 149))
  (segment (start 152.019 52.8066) (end 152.019 50.9016) (width 0.35) (layer F.Cu) (net 150) (tstamp 5BC4AFB3))
  (segment (start 164.3956 41.6728) (end 164.387 41.6814) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 166.8186 43.413) (end 166.8186 44.0142) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 165.087 41.6814) (end 166.8186 43.413) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 166.8186 44.0142) (end 166.8186 44.8142) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 164.387 41.6814) (end 165.087 41.6814) (width 0.35) (layer F.Cu) (net 152))
  (segment (start 157.734 36.1576) (end 158.496 36.9196) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 157.734 35.4076) (end 157.734 36.1576) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 158.496 36.9196) (end 158.496 37.4396) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 158.496 38.0288) (end 158.496 37.4396) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 161.4924 34.4424) (end 161.4424 34.4424) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 162.4584 35.4084) (end 161.4924 34.4424) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 162.4584 37.9984) (end 162.4584 35.4084) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 159.9184 38.0288) (end 159.9488 37.9984) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 159.9488 37.9984) (end 162.4584 37.9984) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 160.1928 38.0288) (end 159.9184 38.0288) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 159.9184 38.0288) (end 158.496 38.0288) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 158.5264 37.9984) (end 158.496 38.0288) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 162.4584 37.9984) (end 158.5264 37.9984) (width 0.35) (layer F.Cu) (net 153))
  (segment (start 161.4706 39.9034) (end 160.546 38.9788) (width 0.35) (layer F.Cu) (net 154))
  (segment (start 160.546 38.9788) (end 160.496 38.9788) (width 0.35) (layer F.Cu) (net 154))
  (segment (start 162.5498 39.9034) (end 161.4706 39.9034) (width 0.35) (layer F.Cu) (net 154))
  (segment (start 159.684 36.3576) (end 158.6992 35.3728) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 159.734 36.3576) (end 159.684 36.3576) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 158.6992 32.6644) (end 158.6992 34.4424) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 158.6992 34.4424) (end 158.6992 34.0868) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 158.6992 35.3728) (end 158.6992 34.4424) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 158.6872 32.6524) (end 158.6992 32.6644) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 157.5188 32.6524) (end 158.6872 32.6524) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 158.6992 31.1912) (end 158.6992 32.6644) (width 0.35) (layer F.Cu) (net 155))
  (segment (start 182.4477 35.1785) (end 183.6928 36.4236) (width 1) (layer F.Cu) (net 156))
  (segment (start 179.451 35.1785) (end 182.4477 35.1785) (width 1) (layer F.Cu) (net 156))
  (segment (start 186.5884 36.4236) (end 183.6928 36.4236) (width 1) (layer F.Cu) (net 156))
  (segment (start 174.508 42.0524) (end 174.5488 42.0116) (width 1) (layer F.Cu) (net 156))
  (segment (start 174.508 43.0276) (end 174.508 42.0524) (width 1) (layer F.Cu) (net 156))
  (segment (start 174.508 41.613387) (end 174.508 43.0276) (width 1) (layer F.Cu) (net 156))
  (segment (start 179.9844 36.136987) (end 174.508 41.613387) (width 1) (layer F.Cu) (net 156))
  (segment (start 179.9844 35.242) (end 179.9844 36.136987) (width 1) (layer F.Cu) (net 156))
  (segment (start 175.895 28.0814) (end 175.895 37.2491) (width 1) (layer F.Cu) (net 157))
  (segment (start 174.5996 38.5445) (end 172.6184 38.5445) (width 1) (layer F.Cu) (net 157))
  (segment (start 175.895 37.2491) (end 174.5996 38.5445) (width 1) (layer F.Cu) (net 157))
  (segment (start 176.7344 27.242) (end 175.895 28.0814) (width 1) (layer F.Cu) (net 157))
  (segment (start 179.9844 27.242) (end 176.7344 27.242) (width 1) (layer F.Cu) (net 157))
  (segment (start 115.443 68.072) (end 116.6495 69.2785) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 112.014 68.072) (end 115.443 68.072) (width 0.35) (layer F.Cu) (net 159))
  (via (at 116.6495 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (via (at 133.223 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (segment (start 116.6495 69.2785) (end 133.223 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 132.0165 68.072) (end 128.649 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 133.223 69.2785) (end 132.0165 68.072) (width 0.35) (layer F.Cu) (net 159))
  (via (at 145.9865 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (segment (start 133.223 69.2785) (end 145.9865 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 144.78 68.072) (end 141.349 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 145.9865 69.2785) (end 144.78 68.072) (width 0.35) (layer F.Cu) (net 159))
  (via (at 162.4965 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (segment (start 145.9865 69.2785) (end 162.4965 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 161.29 68.072) (end 157.859 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 162.4965 69.2785) (end 161.29 68.072) (width 0.35) (layer F.Cu) (net 159))
  (via (at 175.3235 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (segment (start 162.4965 69.2785) (end 175.3235 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 174.117 68.072) (end 170.559 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 175.3235 69.2785) (end 174.117 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 104.8385 69.2785) (end 104.521 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (via (at 105.537 70.612) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 106.807 69.342) (end 105.537 70.612) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 108.839 69.342) (end 106.807 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 117.983 70.612) (end 118.0465 70.6755) (width 0.35) (layer B.Cu) (net 160))
  (via (at 118.0465 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 105.537 70.612) (end 117.983 70.612) (width 0.35) (layer B.Cu) (net 160))
  (segment (start 119.38 69.342) (end 121.414 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 118.0465 70.6755) (end 119.38 69.342) (width 0.35) (layer F.Cu) (net 160))
  (via (at 134.874 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 118.0465 70.6755) (end 134.874 70.6755) (width 0.35) (layer B.Cu) (net 160))
  (segment (start 136.2075 69.342) (end 138.049 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 134.874 70.6755) (end 136.2075 69.342) (width 0.35) (layer F.Cu) (net 160))
  (via (at 147.447 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 134.874 70.6755) (end 147.447 70.6755) (width 0.35) (layer B.Cu) (net 160))
  (segment (start 148.7805 69.342) (end 150.749 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 147.447 70.6755) (end 148.7805 69.342) (width 0.35) (layer F.Cu) (net 160))
  (via (at 163.957 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 147.447 70.6755) (end 163.957 70.6755) (width 0.35) (layer B.Cu) (net 160))
  (segment (start 165.2905 69.342) (end 167.259 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 163.957 70.6755) (end 165.2905 69.342) (width 0.35) (layer F.Cu) (net 160))
  (via (at 176.7205 70.6755) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 160))
  (segment (start 163.957 70.6755) (end 176.7205 70.6755) (width 0.35) (layer B.Cu) (net 160))
  (segment (start 178.054 69.342) (end 179.959 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 176.7205 70.6755) (end 178.054 69.342) (width 0.35) (layer F.Cu) (net 160))
  (segment (start 126.365 85.82) (end 126.365 91.186) (width 0.35) (layer B.Cu) (net 172))
  (segment (start 125.415 83.82) (end 125.415 83.02) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 125.4125 83.0175) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 125.415 83.02) (end 125.4125 83.0175) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 152.8445 81.8515) (end 153.0985 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 154.305 83.786) (end 154.371 83.852) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 154.305 82.4865) (end 154.305 83.786) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 153.67 81.8515) (end 154.305 82.4865) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 152.8445 81.8515) (end 153.67 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 141.7955 81.8515) (end 141.100011 81.156011) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 152.8445 81.8515) (end 141.7955 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 141.100011 81.156011) (end 139.569989 81.156011) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 139.569989 81.156011) (end 138.8745 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 138.8745 81.8515) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 112.017011 81.156011) (end 112.7125 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 108.338999 82.923001) (end 110.105989 81.156011) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 110.105989 81.156011) (end 112.017011 81.156011) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 112.7125 81.8515) (end 125.4125 81.8515) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 155.321 91.186) (end 155.321 85.852) (width 0.35) (layer B.Cu) (net 174))
  (segment (start 123.825 91.186) (end 123.825 90.17) (width 0.35) (layer F.Cu) (net 175) (status 10))
  (segment (start 123.825 88.38) (end 123.825 91.186) (width 0.35) (layer B.Cu) (net 175))
  (segment (start 123.825 82.538) (end 123.825 83.566) (width 0.35) (layer B.Cu) (net 175))
  (segment (start 123.825 83.566) (end 123.825 83.82) (width 0.35) (layer B.Cu) (net 175))
  (segment (start 123.825 83.82) (end 123.825 88.38) (width 0.35) (layer B.Cu) (net 175))
  (segment (start 123.825 83.046) (end 123.825 83.82) (width 0.35) (layer B.Cu) (net 175))
  (segment (start 152.654 91.059) (end 152.781 91.186) (width 0.35) (layer F.Cu) (net 176) (status 30))
  (segment (start 152.781 89.662) (end 152.781 88.38) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 152.781 91.186) (end 152.781 89.662) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 152.781 82.6015) (end 152.781 83.5025) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 152.781 83.5025) (end 152.781 89.662) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 152.781 83.046) (end 152.781 83.5025) (width 0.35) (layer B.Cu) (net 176))
  (segment (start 118.42 103.03) (end 118.745 103.355) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 115.57 103.03) (end 118.42 103.03) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 136.835 103.03) (end 137.16 103.355) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 133.985 103.03) (end 136.835 103.03) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 144.94 103.03) (end 147.63 103.03) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 163.195 103.03) (end 165.97 103.03) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 176.765 103.03) (end 177.165 103.43) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 173.99 103.03) (end 176.765 103.03) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (via (at 107.95 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (via (at 177.165 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (segment (start 119.38 104.610001) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 118.745 104.775) (end 118.909999 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 109.22 104.610001) (end 108.749999 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 165.97 103.03) (end 166.37 103.43) (width 0.35) (layer F.Cu) (net 179) (status 30))
  (segment (start 118.745 104.648) (end 118.745 103.355) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 107.95 104.648) (end 107.95 103.43) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 109.817001 104.648) (end 109.855 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 109.855 104.610001) (end 109.22 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 107.95 104.648) (end 109.817001 104.648) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 119.38 104.610001) (end 109.855 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 137.16 104.648) (end 137.16 103.355) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 148.082 103.482) (end 148.03 103.43) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 148.082 104.648) (end 148.082 103.482) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 166.37 104.648) (end 166.37 103.43) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 177.165 104.648) (end 177.165 103.43) (width 0.7) (layer F.Cu) (net 179))
  (segment (start 177.165 104.648) (end 107.95 104.648) (width 1) (layer B.Cu) (net 179))
  (segment (start 107.55 103.03) (end 107.95 103.43) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 104.775 103.03) (end 107.55 103.03) (width 0.35) (layer F.Cu) (net 179))
  (via (at 137.16 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (segment (start 147.955 104.610001) (end 138.43 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (via (at 148.082 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (via (at 166.37 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (via (at 118.745 104.648) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (segment (start 165.570001 104.610001) (end 166.37 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 148.754999 104.610001) (end 147.955 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 166.37 104.610001) (end 176.365001 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 137.16 104.610001) (end 126.8095 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 148.754999 104.610001) (end 165.570001 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 138.43 104.610001) (end 137.16 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 126.8095 104.610001) (end 119.38 104.610001) (width 0.7) (layer B.Cu) (net 179))
  (segment (start 180.594 54.0871) (end 182.2345 55.7276) (width 1) (layer F.Cu) (net 179))
  (segment (start 180.594 50.9651) (end 180.594 54.0871) (width 1) (layer F.Cu) (net 179))
  (segment (start 184.1145 55.7276) (end 182.2345 55.7276) (width 1) (layer F.Cu) (net 179))
  (segment (start 180.594 48.6791) (end 179.07 47.1551) (width 1) (layer F.Cu) (net 179))
  (segment (start 180.594 50.9651) (end 180.594 48.6791) (width 1) (layer F.Cu) (net 179))
  (segment (start 179.07 47.1551) (end 179.0319 47.1551) (width 1) (layer F.Cu) (net 179))
  (via (at 178.3334 46.4058) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 179))
  (segment (start 178.3334 46.4566) (end 178.3334 46.4058) (width 1) (layer F.Cu) (net 179))
  (segment (start 179.0319 47.1551) (end 178.3334 46.4566) (width 1) (layer F.Cu) (net 179))
  (segment (start 178.181 46.2534) (end 178.3334 46.4058) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 177.165 104.648) (end 181.525908 104.648) (width 1) (layer B.Cu) (net 179))
  (segment (start 188.142002 98.031906) (end 188.142002 48.543602) (width 1) (layer B.Cu) (net 179))
  (segment (start 181.525908 104.648) (end 188.142002 98.031906) (width 1) (layer B.Cu) (net 179))
  (segment (start 150.749 53.1266) (end 150.749 50.9016) (width 0.35) (layer F.Cu) (net 182) (tstamp 5BC4AF47))
  (segment (start 152.019 47.4116) (end 155.194 47.4116) (width 0.35) (layer F.Cu) (net 182) (tstamp 5BC4AF44))
  (segment (start 150.749 48.6816) (end 152.019 47.4116) (width 0.35) (layer F.Cu) (net 182) (tstamp 5BC4AF41))
  (segment (start 150.749 50.9016) (end 150.749 48.6816) (width 0.35) (layer F.Cu) (net 182) (tstamp 5BC4AF3E))
  (segment (start 180.5305 56.9236) (end 179.3345 55.7276) (width 1) (layer F.Cu) (net 184))
  (segment (start 180.5305 60.6171) (end 180.5305 56.9236) (width 1) (layer F.Cu) (net 184))
  (segment (start 180.5305 60.6171) (end 177.8635 60.6171) (width 1) (layer F.Cu) (net 184))
  (segment (start 175.8895 58.6431) (end 177.8635 60.6171) (width 1) (layer F.Cu) (net 184))
  (segment (start 175.8895 55.2196) (end 175.8895 58.6431) (width 1) (layer F.Cu) (net 184))
  (segment (start 175.8895 55.2196) (end 172.977 55.2196) (width 1) (layer F.Cu) (net 184))
  (segment (start 175.8895 55.2196) (end 175.8895 61.8291) (width 1) (layer F.Cu) (net 184))
  (segment (start 178.2445 60.9981) (end 177.8635 60.6171) (width 0.5) (layer F.Cu) (net 184))
  (segment (start 178.2445 63.5381) (end 178.2445 61.6966) (width 0.5) (layer F.Cu) (net 184))
  (segment (start 178.2445 61.6966) (end 178.2445 60.9981) (width 0.5) (layer F.Cu) (net 184))
  (segment (start 178.2445 63.2206) (end 178.2445 61.6966) (width 0.5) (layer F.Cu) (net 184))
  (segment (start 113.8689 34.2385) (end 113.8809 34.2505) (width 0.35) (layer F.Cu) (net 185) (tstamp 5BCC896C))
  (segment (start 113.8689 32.893) (end 113.8689 34.2385) (width 0.35) (layer F.Cu) (net 185) (tstamp 5BCC8969))
  (segment (start 120.4519 52.197) (end 120.9929 52.197) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC8855))
  (segment (start 117.0559 49.276) (end 117.0559 49.911) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC89E4))
  (segment (start 119.3419 52.197) (end 120.4519 52.197) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC888B))
  (segment (start 117.0559 49.911) (end 119.3419 52.197) (width 0.35) (layer F.Cu) (net 187) (tstamp 5BCC886A))
  (segment (start 115.3559 50.976) (end 115.9809 50.976) (width 0.35) (layer F.Cu) (net 190) (tstamp 5BCC8804))
  (segment (start 117.3099 54.518) (end 114.5559 51.764) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC8831))
  (segment (start 114.5559 51.764) (end 114.5559 50.976) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC8822))
  (segment (start 117.3099 55.118) (end 117.3099 54.518) (width 0.35) (layer F.Cu) (net 191) (tstamp 5BCC8852))
  (segment (start 113.7559 50.976) (end 113.7559 52.326) (width 0.35) (layer F.Cu) (net 193) (tstamp 5BCC8876))
  (segment (start 115.9129 54.483) (end 115.9129 55.118) (width 0.35) (layer F.Cu) (net 193) (tstamp 5BCC8885))
  (segment (start 113.7559 52.326) (end 115.9129 54.483) (width 0.35) (layer F.Cu) (net 193) (tstamp 5BCC889D))
  (segment (start 112.9559 50.976) (end 112.9559 52.796) (width 0.35) (layer F.Cu) (net 196) (tstamp 5BCC8837))
  (segment (start 114.5159 54.356) (end 114.5159 55.118) (width 0.35) (layer F.Cu) (net 196) (tstamp 5BCC8843))
  (segment (start 112.9559 52.796) (end 114.5159 54.356) (width 0.35) (layer F.Cu) (net 196) (tstamp 5BCC89D5))
  (segment (start 148.8465 53.1241) (end 148.849 53.1266) (width 0.35) (layer F.Cu) (net 197))
  (segment (start 147.488 53.1241) (end 148.8465 53.1241) (width 0.35) (layer F.Cu) (net 197))
  (segment (start 147.488 54.3941) (end 147.488 55.6741) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 147.488 55.6741) (end 147.488 56.9441) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 153.3425 55.6741) (end 153.416 55.6006) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 147.488 55.6741) (end 153.3425 55.6741) (width 0.35) (layer F.Cu) (net 198))
  (segment (start 145.669 50.9016) (end 149.479 50.9016) (width 0.7) (layer F.Cu) (net 199) (tstamp 5BC4AF35))
  (segment (start 149.479 50.9016) (end 149.479 45.5016) (width 0.7) (layer F.Cu) (net 199) (tstamp 5BC4AF32))
  (segment (start 149.479 45.5016) (end 150.749 45.5016) (width 0.7) (layer F.Cu) (net 199) (tstamp 5BC4AF2F))
  (segment (start 109.7559 50.976) (end 109.7559 53.401) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC886D))
  (segment (start 108.8009 54.356) (end 108.8009 55.118) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC8828))
  (segment (start 109.7559 53.401) (end 108.8009 54.356) (width 0.35) (layer F.Cu) (net 200) (tstamp 5BCC8861))
  (segment (start 107.4039 55.118) (end 107.4039 54.483) (width 0.35) (layer F.Cu) (net 201) (tstamp 5BCC8882))
  (segment (start 108.9559 52.931) (end 108.9559 50.976) (width 0.35) (layer F.Cu) (net 201) (tstamp 5BCC887F))
  (segment (start 107.4039 54.483) (end 108.9559 52.931) (width 0.35) (layer F.Cu) (net 201) (tstamp 5BCC8858))
  (segment (start 106.0069 54.518) (end 106.0069 55.118) (width 0.35) (layer F.Cu) (net 202) (tstamp 5BCC8894))
  (segment (start 108.1559 52.369) (end 106.0069 54.518) (width 0.35) (layer F.Cu) (net 202) (tstamp 5BCC8816))
  (segment (start 108.1559 50.976) (end 108.1559 52.369) (width 0.35) (layer F.Cu) (net 202) (tstamp 5BCC882B))
  (segment (start 104.5559 48.476) (end 102.3589 50.673) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BCC8864))
  (segment (start 105.6559 48.476) (end 104.5559 48.476) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BCC8849))
  (segment (start 102.3589 50.673) (end 101.8159 50.673) (width 0.35) (layer F.Cu) (net 203) (tstamp 5BCC898D))
  (segment (start 120.3929 38.1) (end 120.9929 38.1) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC89A2))
  (segment (start 119.6069 38.1) (end 120.3929 38.1) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC899F))
  (segment (start 117.0559 40.651) (end 119.6069 38.1) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC899C))
  (segment (start 117.0559 41.276) (end 117.0559 40.651) (width 0.35) (layer F.Cu) (net 204) (tstamp 5BCC8999))
  (segment (start 120.4849 39.497) (end 120.7389 39.497) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC8993))
  (segment (start 120.7389 39.497) (end 120.9929 39.497) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC89A5))
  (segment (start 117.9449 42.076) (end 117.9449 42.037) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC8990))
  (segment (start 117.9449 42.037) (end 120.4849 39.497) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC8996))
  (segment (start 117.0559 42.076) (end 117.9449 42.076) (width 0.35) (layer F.Cu) (net 205) (tstamp 5BCC895A))
  (segment (start 120.3929 40.894) (end 120.9929 40.894) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC895D))
  (segment (start 118.4109 42.876) (end 120.3929 40.894) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC88C1))
  (segment (start 117.0559 42.876) (end 118.4109 42.876) (width 0.35) (layer F.Cu) (net 206) (tstamp 5BCC88BE))
  (segment (start 120.4049 42.291) (end 121.0049 42.291) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC88B8))
  (segment (start 119.0199 43.676) (end 120.4049 42.291) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC88B5))
  (segment (start 117.0559 43.676) (end 119.0199 43.676) (width 0.35) (layer F.Cu) (net 207) (tstamp 5BCC882E))
  (segment (start 120.2309 43.688) (end 120.9929 43.688) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC881F))
  (segment (start 119.4429 44.476) (end 120.2309 43.688) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC8846))
  (segment (start 117.0559 44.476) (end 119.4429 44.476) (width 0.35) (layer F.Cu) (net 208) (tstamp 5BCC8A32))
  (segment (start 105.9815 69.2785) (end 104.2035 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 105.9815 69.2785) (end 116.6495 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 99.439 68.072) (end 101.092 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 101.092 68.072) (end 101.854 68.072) (width 0.35) (layer F.Cu) (net 159))
  (via (at 98.806 40.767) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 209))
  (segment (start 100.3159 40.767) (end 98.806 40.767) (width 0.35) (layer F.Cu) (net 209))
  (via (at 104.013 69.2785) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 159))
  (segment (start 98.114 68.072) (end 97.536 67.494) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 99.439 68.072) (end 98.114 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 100.3159 54.8781) (end 97.536 57.658) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 100.3159 52.07) (end 100.3159 54.8781) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 97.536 67.494) (end 97.536 57.658) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 102.8065 68.072) (end 104.013 69.2785) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 102.108 68.072) (end 102.8065 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 101.092 68.072) (end 102.108 68.072) (width 0.35) (layer F.Cu) (net 159))
  (segment (start 105.41 69.2785) (end 104.013 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 104.8385 69.2785) (end 105.41 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 105.41 69.2785) (end 105.9815 69.2785) (width 0.35) (layer B.Cu) (net 159))
  (segment (start 90.4875 68.2625) (end 92.71 66.04) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 90.4875 77.3035) (end 90.4875 68.2625) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 95.99699 63.9445) (end 95.99699 63.484756) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 95.251491 64.689999) (end 95.99699 63.9445) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 94.060001 64.689999) (end 95.251491 64.689999) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 92.71 66.04) (end 94.060001 64.689999) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 95.99699 61.82439) (end 95.99699 61.9125) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 94.107 59.9344) (end 95.99699 61.82439) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 94.107 59.3344) (end 94.107 59.9344) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 95.99699 63.484756) (end 95.99699 61.9125) (width 0.35) (layer B.Cu) (net 168))
  (segment (start 91.34291 76.13791) (end 91.8845 76.6795) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 91.34291 72.48709) (end 91.34291 76.13791) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 91.8845 76.6795) (end 91.8845 77.2795) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 92.71 71.12) (end 91.34291 72.48709) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 95.838001 69.769999) (end 96.695489 68.912511) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 92.71 71.12) (end 94.060001 69.769999) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 94.060001 69.769999) (end 95.838001 69.769999) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 96.695489 61.386263) (end 96.7105 61.371252) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 96.695489 62.357) (end 96.695489 61.386263) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 96.695489 68.912511) (end 96.695489 62.357) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 95.504 60.101254) (end 96.695489 61.292743) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 95.504 59.3104) (end 95.504 60.101254) (width 0.35) (layer B.Cu) (net 169))
  (segment (start 96.695489 61.292743) (end 96.695489 62.357) (width 0.35) (layer B.Cu) (net 169))
  (via (at 98.806 37.973) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 171))
  (segment (start 100.3159 37.973) (end 98.806 37.973) (width 0.35) (layer F.Cu) (net 171))
  (segment (start 94.107 57.8344) (end 94.107 55.88) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 94.107 55.88) (end 92.1385 53.9115) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 92.1385 53.9115) (end 91.567 53.34) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 91.567 53.34) (end 91.3765 53.1495) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 91.3765 53.1495) (end 91.3765 50.1015) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 91.3765 50.1015) (end 91.3765 49.9745) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 91.3765 49.9745) (end 94.107 47.244) (width 0.35) (layer B.Cu) (net 167))
  (via (at 97.409 39.37) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 167))
  (segment (start 100.3159 39.37) (end 97.409 39.37) (width 0.35) (layer F.Cu) (net 167))
  (segment (start 94.107 47.244) (end 94.107 38.481) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 94.107 38.481) (end 94.107 37.973) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 96.7105 34.925) (end 94.107 37.5285) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 99.314 34.925) (end 96.7105 34.925) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 100.3935 36.0045) (end 99.314 34.925) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 94.107 37.5285) (end 94.107 38.481) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 100.3935 38.481) (end 100.3935 36.0045) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 99.5045 39.37) (end 100.3935 38.481) (width 0.35) (layer B.Cu) (net 167))
  (segment (start 97.409 39.37) (end 99.5045 39.37) (width 0.35) (layer B.Cu) (net 167))
  (via (at 97.409 36.576) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 170))
  (segment (start 100.3173 36.576) (end 97.409 36.576) (width 0.35) (layer F.Cu) (net 170))
  (segment (start 94.8055 47.5615) (end 94.8055 39.1795) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 92.075 50.292) (end 94.8055 47.5615) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 92.075 52.832) (end 92.075 50.292) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 95.504 57.8104) (end 95.504 56.261) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 94.8055 39.1795) (end 97.409 36.576) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 95.504 56.261) (end 92.075 52.832) (width 0.35) (layer B.Cu) (net 170))
  (segment (start 92.7735 52.2605) (end 96.901 56.388) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 92.7735 50.546) (end 92.7735 52.2605) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 95.504 47.8155) (end 92.7735 50.546) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 95.504 41.275) (end 95.504 41.529) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 95.504 41.529) (end 95.504 47.8155) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 95.504 39.400254) (end 96.931254 37.973) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 97.67463 37.973) (end 98.806 37.973) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 95.504 41.529) (end 95.504 39.400254) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 96.931254 37.973) (end 97.67463 37.973) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 96.901 56.642) (end 96.901 56.3245) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 96.901 56.388) (end 96.901 56.642) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 96.901 56.642) (end 96.901 57.8224) (width 0.35) (layer B.Cu) (net 171))
  (segment (start 76.41698 64.53522) (end 76.41698 80.599981) (width 0.35) (layer B.Cu) (net 173))
  (segment (start 76.41698 80.599981) (end 77.089 81.272001) (width 0.35) (layer B.Cu) (net 173))
  (via (at 108.839 58.293) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 173))
  (segment (start 108.8009 58.2549) (end 108.839 58.293) (width 0.35) (layer F.Cu) (net 173))
  (segment (start 108.8009 56.618) (end 108.8009 58.2549) (width 0.35) (layer F.Cu) (net 173))
  (segment (start 77.978 76.327) (end 77.978 80.264) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 77.978 76.327) (end 77.978 77.089) (width 0.35) (layer B.Cu) (net 177))
  (segment (start 100.3159 42.164) (end 97.409 42.164) (width 0.35) (layer F.Cu) (net 177))
  (via (at 97.409 42.164) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 177))
  (via (at 103.378 29.083) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 178))
  (segment (start 103.378 30.4793) (end 103.378 29.083) (width 0.5) (layer F.Cu) (net 178))
  (segment (start 103.378 29.083) (end 109.982 29.083) (width 0.5) (layer B.Cu) (net 178))
  (segment (start 109.982 29.083) (end 112.522 26.543) (width 0.5) (layer B.Cu) (net 178))
  (segment (start 164.399 43.5356) (end 165.099 43.5356) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 165.608 44.0446) (end 165.608 45.7962) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 165.099 43.5356) (end 165.608 44.0446) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 166.2176 46.4058) (end 169.164 46.4058) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 165.608 45.7962) (end 166.2176 46.4058) (width 0.35) (layer F.Cu) (net 179))
  (segment (start 178.3334 46.4058) (end 169.164 46.4058) (width 0.35) (layer F.Cu) (net 179))
  (via (at 101.981 27.559) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 180))
  (segment (start 101.981 30.4793) (end 101.981 27.559) (width 0.5) (layer F.Cu) (net 180))
  (segment (start 105.0925 28.2575) (end 108.2675 28.2575) (width 0.5) (layer B.Cu) (net 180))
  (segment (start 104.394 27.559) (end 105.0925 28.2575) (width 0.5) (layer B.Cu) (net 180))
  (segment (start 108.2675 28.2575) (end 109.982 26.543) (width 0.5) (layer B.Cu) (net 180))
  (segment (start 101.981 27.559) (end 104.394 27.559) (width 0.5) (layer B.Cu) (net 180))
  (segment (start 158.496 39.9288) (end 158.496 42.0878) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 157.1498 43.434) (end 155.1432 43.434) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 158.496 42.0878) (end 157.1498 43.434) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 153.289 44.0436) (end 153.8986 43.434) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 153.8986 43.434) (end 155.1432 43.434) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 153.289 45.5016) (end 153.289 44.0436) (width 0.35) (layer F.Cu) (net 181))
  (segment (start 91.5035 46.181) (end 91.44 46.2445) (width 0.35) (layer F.Cu) (net 183))
  (via (at 91.5035 43.307) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 183))
  (segment (start 91.5035 40.5765) (end 91.5035 43.307) (width 0.35) (layer F.Cu) (net 183))
  (segment (start 91.5035 46.181) (end 91.44 46.2445) (width 0.35) (layer B.Cu) (net 183))
  (segment (start 91.5035 43.307) (end 91.5035 46.181) (width 0.35) (layer B.Cu) (net 183))
  (via (at 113.8428 31.2928) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 185))
  (segment (start 113.8689 31.3189) (end 113.8428 31.2928) (width 0.5) (layer F.Cu) (net 185))
  (segment (start 113.8689 32.893) (end 113.8689 31.3189) (width 0.5) (layer F.Cu) (net 185))
  (segment (start 111.11 103.03) (end 111.76 103.03) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 109.82201 101.74201) (end 111.11 103.03) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 100.15299 101.74201) (end 100.838 101.74201) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 100.041 101.854) (end 100.15299 101.74201) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 99.441 101.854) (end 100.041 101.854) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 100.838 101.74201) (end 109.82201 101.74201) (width 0.35) (layer F.Cu) (net 186))
  (segment (start 170.18 102.555) (end 170.18 103.03) (width 0.35) (layer F.Cu) (net 188))
  (segment (start 169.225 101.6) (end 170.18 102.555) (width 0.35) (layer F.Cu) (net 188))
  (segment (start 157.849 101.6) (end 169.225 101.6) (width 0.35) (layer F.Cu) (net 188))
  (segment (start 157.849 102.997) (end 159.512 102.997) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 159.352 102.997) (end 159.385 103.03) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 157.849 102.997) (end 159.352 102.997) (width 0.35) (layer F.Cu) (net 189))
  (segment (start 120.9795 53.6575) (end 118.6624 53.6575) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 118.6624 53.6575) (end 117.4559 52.451) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 115.9809 50.976) (end 117.4559 52.451) (width 0.35) (layer F.Cu) (net 190))
  (segment (start 99.429 103.251) (end 100.029 103.251) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 100.094 103.251) (end 100.029 103.251) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 100.315 103.03) (end 100.094 103.251) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 100.965 103.03) (end 100.315 103.03) (width 0.35) (layer F.Cu) (net 192))
  (segment (start 140.97 102.555) (end 140.97 103.03) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 140.015 101.6) (end 140.97 102.555) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 128.639 101.6) (end 140.015 101.6) (width 0.35) (layer F.Cu) (net 194))
  (segment (start 130.0785 102.9335) (end 130.175 103.03) (width 0.35) (layer F.Cu) (net 195))
  (segment (start 128.651 102.9335) (end 130.0785 102.9335) (width 0.35) (layer F.Cu) (net 195))
  (via (at 98.806 43.561) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 210))
  (segment (start 100.3159 43.561) (end 98.806 43.561) (width 0.35) (layer F.Cu) (net 210))
  (segment (start 72.2478 31.2318) (end 71.9836 31.496) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3B2B))
  (segment (start 73.1738 31.496) (end 73.7047 30.9651) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3B5B))
  (segment (start 71.9836 31.496) (end 73.1738 31.496) (width 0.35) (layer F.Cu) (net 211) (tstamp 5BCC3B61))
  (via (at 116.928503 91.12853) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 116.185973 90.386) (end 116.928503 91.12853) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 115.824 90.386) (end 116.185973 90.386) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 116.928503 91.12853) (end 116.38947 91.12853) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 116.38947 91.12853) (end 114.173 93.345) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 114.173 93.345) (end 114.173 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 114.173 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 213))
  (via (at 135.382 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 134.582 90.386) (end 135.382 91.186) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 134.239 90.386) (end 134.582 90.386) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 134.533472 91.186) (end 132.842 92.877472) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 135.382 91.186) (end 134.533472 91.186) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 132.842 92.877472) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 132.842 96.52) (end 132.461 96.52) (width 0.35) (layer B.Cu) (net 213))
  (via (at 146.177 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 145.377 90.386) (end 146.177 91.186) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 144.996 90.386) (end 145.377 90.386) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 145.328472 91.186) (end 143.637 92.877472) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 146.177 91.186) (end 145.328472 91.186) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 143.637 92.877472) (end 143.637 96.52) (width 0.35) (layer B.Cu) (net 213))
  (via (at 164.592 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 163.792 90.386) (end 164.592 91.186) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 163.28 90.386) (end 163.792 90.386) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 163.743472 91.186) (end 162.052 92.877472) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 164.592 91.186) (end 163.743472 91.186) (width 0.35) (layer B.Cu) (net 213))
  (via (at 175.387 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 174.587 90.386) (end 175.387 91.186) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 174.075 90.386) (end 174.587 90.386) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 143.256 96.52) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 162.052 92.877472) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 143.637 96.52) (end 143.256 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 143.256 96.52) (end 132.842 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 102.997 96.52) (end 104.267 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 104.267 96.52) (end 103.886 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 114.173 96.52) (end 104.267 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 105.372 90.386) (end 106.172 91.186) (width 0.35) (layer F.Cu) (net 213))
  (segment (start 104.902 90.386) (end 105.372 90.386) (width 0.35) (layer F.Cu) (net 213))
  (via (at 106.172 91.186) (size 1.2) (drill 0.8) (layers F.Cu B.Cu) (net 213))
  (segment (start 101.6 94.996) (end 101.6 95.123) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 101.6 95.123) (end 102.997 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 101.6 94.909472) (end 101.6 94.996) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 105.323472 91.186) (end 101.6 94.909472) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 106.172 91.186) (end 105.323472 91.186) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 171.577 96.52) (end 162.052 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 172.847 95.25) (end 171.577 96.52) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 172.847 92.837) (end 172.847 95.25) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 174.498 91.186) (end 172.847 92.837) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 175.387 91.186) (end 174.498 91.186) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 77.47 82.296) (end 78.146 82.296) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 77.47 82.296) (end 77.343 82.296) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 78.146 82.296) (end 78.178 82.264) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 76.835 82.296) (end 76.454 82.677) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 76.454 82.677) (end 76.454 89.789) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 78.178 82.264) (end 78.928 82.264) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 77.47 82.296) (end 76.835 82.296) (width 0.35) (layer B.Cu) (net 213))
  (segment (start 163.28 91.99) (end 163.28 91.986) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 161.671 93.599) (end 163.28 91.99) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 157.793 87.63) (end 157.793 91.499) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 156.21 86.047) (end 157.793 87.63) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 159.893 93.599) (end 161.671 93.599) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 157.793 91.499) (end 159.893 93.599) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 156.21 85.447) (end 156.21 86.047) (width 0.35) (layer F.Cu) (net 214))
  (segment (start 115.786 91.986) (end 115.824 91.986) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 114.3 93.472) (end 115.786 91.986) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 112.141 93.472) (end 114.3 93.472) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 110.871 92.202) (end 112.141 93.472) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 110.363 86.233) (end 110.871 86.741) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 110.871 86.741) (end 110.871 92.202) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 110.363 85.447) (end 110.363 86.233) (width 0.35) (layer F.Cu) (net 215))
  (segment (start 169.164 86.614) (end 168.783 86.233) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 168.783 86.233) (end 168.783 85.447) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 169.164 92.202) (end 169.164 86.614) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 170.561 93.599) (end 169.164 92.202) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 174.075 91.986) (end 174.075 91.99) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 172.466 93.599) (end 170.561 93.599) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 174.075 91.99) (end 172.466 93.599) (width 0.35) (layer F.Cu) (net 216))
  (segment (start 139.573 85.447) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 139.954 92.964) (end 140.335 93.345) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 139.954 86.614) (end 139.954 92.964) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 139.954 86.614) (end 139.573 86.233) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 143.383 93.599) (end 140.589 93.599) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 144.996 91.986) (end 143.383 93.599) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 140.335 93.345) (end 140.589 93.599) (width 0.35) (layer F.Cu) (net 217))
  (segment (start 104.864 91.986) (end 104.902 91.986) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 97.79 85.447) (end 97.79 90.17) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 103.378 93.472) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 97.79 90.17) (end 101.092 93.472) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 103.378 93.472) (end 104.864 91.986) (width 0.35) (layer F.Cu) (net 218))
  (segment (start 127 85.471) (end 127 86.071) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 127 86.233) (end 127 85.471) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 128.778 88.011) (end 127 86.233) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 134.201 91.986) (end 132.588 93.599) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 130.048 93.599) (end 128.778 92.329) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 132.588 93.599) (end 130.048 93.599) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 128.778 92.329) (end 128.778 88.011) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 134.239 91.986) (end 134.201 91.986) (width 0.35) (layer F.Cu) (net 219))
  (segment (start 104.6099 59.7916) (end 104.5845 59.817) (width 0.35) (layer F.Cu) (net 220))
  (via (at 104.5845 59.817) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 220))
  (segment (start 104.6099 56.618) (end 104.6099 59.7916) (width 0.35) (layer F.Cu) (net 220))
  (segment (start 77.2475 81.2095) (end 77.2475 85.2345) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 75.819 85.813) (end 76.3975 85.2345) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 75.819 88.138) (end 75.819 85.813) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 76.3975 85.2345) (end 77.2475 85.2345) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 77.2475 79.4845) (end 77.2475 81.2095) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 77.978 78.867) (end 77.865 78.867) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 77.865 78.867) (end 77.2475 79.4845) (width 0.35) (layer F.Cu) (net 221))
  (segment (start 78.232 70.866) (end 78.232 63.5546) (width 0.35) (layer B.Cu) (net 222))
  (via (at 107.3785 59.817) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 222))
  (segment (start 107.4039 59.7916) (end 107.3785 59.817) (width 0.35) (layer F.Cu) (net 222))
  (segment (start 107.4039 56.618) (end 107.4039 59.7916) (width 0.35) (layer F.Cu) (net 222))
  (via (at 105.9815 58.293) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 223))
  (segment (start 106.0069 58.2676) (end 105.9815 58.293) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 106.0069 56.618) (end 106.0069 58.2676) (width 0.35) (layer F.Cu) (net 223))
  (segment (start 76.3975 76.154) (end 77.2475 76.154) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 75.946 76.6055) (end 76.3975 76.154) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 77.2475 76.154) (end 77.2475 70.404) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 77.2935 70.358) (end 77.2475 70.404) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 75.946 84.201) (end 74.422 85.725) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 75.946 76.6055) (end 75.946 84.201) (width 0.35) (layer F.Cu) (net 224))
  (segment (start 74.422 88.15) (end 74.422 85.725) (width 0.35) (layer F.Cu) (net 224))
  (via (at 156.0068 34.8996) (size 1.6) (drill 0.9) (layers F.Cu B.Cu) (net 226))
  (segment (start 156.0188 34.5066) (end 155.7274 34.798) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 156.0188 32.6524) (end 156.0188 34.5066) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 156.0068 32.6644) (end 156.0188 32.6524) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 156.0068 34.8996) (end 156.0068 32.6644) (width 0.35) (layer F.Cu) (net 226))
  (segment (start 94.361 72.009) (end 95.25 71.12) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 93.2815 77.2795) (end 93.2815 76.6795) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 92.0115 75.4095) (end 92.0115 73.279) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 92.9005 72.5805) (end 94.361 72.009) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 92.0115 73.279) (end 92.9005 72.5805) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 93.2815 76.6795) (end 92.0115 75.4095) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 95.25 71.12) (end 95.443492 71.12) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 95.443492 71.12) (end 97.360508 69.202984) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.345499 61.023501) (end 97.345499 61.086999) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.360508 61.102008) (end 97.360508 61.640496) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 96.901 60.579002) (end 97.345499 61.023501) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 96.901 59.3224) (end 96.901 60.579002) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.360508 61.102008) (end 97.345499 61.086999) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.360508 62.6745) (end 97.360508 61.102008) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.360508 69.202984) (end 97.360508 62.6745) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 97.360508 62.6745) (end 97.360508 61.640496) (width 0.35) (layer B.Cu) (net 228))
  (segment (start 75.7047 31.9151) (end 77.2287 31.9151) (width 0.35) (layer F.Cu) (net 229) (tstamp 5BCC3B88))
  (segment (start 72.8406 52.1938) (end 72.8406 52.9438) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 71.7906 50.1552) (end 72.8406 51.2052) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 72.8406 51.2052) (end 72.8406 52.1938) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 70.8406 50.1552) (end 71.7906 50.1552) (width 0.35) (layer F.Cu) (net 230))
  (segment (start 70.8279 52.0065) (end 70.8406 51.9938) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 66.9544 48.479802) (end 67.572798 49.0982) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 66.9544 46.5596) (end 66.9544 48.479802) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 67.572798 49.0982) (end 69.4055 49.0982) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 69.7357 49.4284) (end 69.7357 52.0065) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 69.7357 52.0065) (end 70.8279 52.0065) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 69.4055 49.0982) (end 69.7357 49.4284) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 69.1642 52.0065) (end 69.7357 52.0065) (width 0.35) (layer F.Cu) (net 231))
  (segment (start 65.6591 51.955) (end 65.675 51.9709) (width 0.35) (layer F.Cu) (net 232))
  (segment (start 64.1858 51.955) (end 65.6591 51.955) (width 0.35) (layer F.Cu) (net 232))
  (segment (start 64.1604 51.9296) (end 64.1858 51.955) (width 0.35) (layer F.Cu) (net 232))
  (segment (start 64.1604 46.5596) (end 64.1604 51.9296) (width 0.35) (layer F.Cu) (net 232))
  (segment (start 67.675 50.984) (end 68.4403 50.2187) (width 0.35) (layer F.Cu) (net 233))
  (segment (start 67.675 52.9209) (end 67.675 50.984) (width 0.35) (layer F.Cu) (net 233))
  (segment (start 68.4403 48.0187) (end 68.4403 46.5716) (width 0.35) (layer F.Cu) (net 234))
  (segment (start 84.9376 28.3711) (end 84.963 28.3965) (width 0.35) (layer F.Cu) (net 234) (tstamp 5BCC87A7))
  (segment (start 70.8406 47.5114) (end 69.8627 46.5335) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 70.8406 47.9552) (end 70.8406 47.5114) (width 0.35) (layer F.Cu) (net 235))
  (segment (start 163.4424 41.434) (end 163.4424 35.3924) (width 0.35) (layer F.Cu) (net 241))
  (segment (start 163.195 41.6814) (end 163.4424 41.434) (width 0.35) (layer F.Cu) (net 241))
  (segment (start 162.487 41.6814) (end 163.195 41.6814) (width 0.35) (layer F.Cu) (net 241))

  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BD0A761) (hatch full 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 146.1008 25.2476) (xy 150.0632 25.2222) (xy 150.0886 34.4678) (xy 142.6591 34.544) (xy 141.4526 32.512)
        (xy 141.4526 25.273) (xy 145.7452 25.1968)
      )
    )
  )
  (zone (net 151) (net_name "/5V PSU /SwE") (layer F.Cu) (tstamp 5BD0A75E) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 140.8811 25.2095) (xy 141.0081 34.163) (xy 135.2931 34.163) (xy 135.2296 29.972) (xy 130.0226 29.972)
        (xy 129.9591 25.2095)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (tstamp 5BC3B7FA) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.154 24.511) (xy 188.9125 24.511) (xy 188.849 109.093) (xy 89.154 109.093)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (tstamp 5BC3B7F7) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.2175 24.511) (xy 188.9125 24.511) (xy 188.758634 109.093) (xy 89.063634 109.093)
      )
    )
  )
  (zone (net 198) (net_name "/3_3V PSU/HC_Plain") (layer F.Cu) (tstamp 5BC4ABC3) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 146.304 54.0766) (xy 153.924 54.0766) (xy 156.464 51.5366) (xy 156.337 47.8536) (xy 163.322 47.8536)
        (xy 163.576 60.5536) (xy 146.431 60.5536)
      )
    )
  )
  (zone (net 184) (net_name "/3_3V PSU/MC34063_HC_A") (layer F.Cu) (tstamp 5BC4ABC0) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.275 47.7266) (xy 168.275 62.5856) (xy 182.499 62.4586) (xy 182.4355 59.2201) (xy 178.308 59.2836)
        (xy 178.2445 47.5996)
      )
    )
  )
  (zone (net 199) (net_name "/3_3V PSU/HC_Plain_b") (layer F.Cu) (tstamp 5BC4ABBD) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 140.97 48.6156) (xy 149.987 48.6156) (xy 149.987 52.0446) (xy 153.035 51.9176) (xy 153.035 60.5536)
        (xy 140.843 60.4901) (xy 140.843 51.0921)
      )
    )
  )
  (zone (net 7) (net_name VCC) (layer F.Cu) (tstamp 5BCC81B0) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 115.5319 41.783) (xy 115.5319 49.403) (xy 107.1499 49.403) (xy 107.1499 41.021) (xy 115.5319 41.021)
      )
    )
  )
)
