"Source:","/home/ejung/i_karl/nowker_sattelit/temp_sens_pt100/nowker_sattelit.sch"
"Date:","Mi 01 Apr 2020 02:46:04 CEST"
"Tool:","Eeschema 5.0.2+dfsg1-1"
"Generator:","/usr/share/kicad/plugins/bom_csv_grouped_by_value_with_fp.py"
"Component Count:","107"
"Ref","Qnty","Value","Cmp name","Footprint","Description","Vendor"
"C1, ","1","100u","CP","Capacitor_SMD:CP_Elec_6.3x5.3","Polarized capacitor",""
"C2, ","1","100p","C","Capacitor_SMD:C_0603_1608Metric","Unpolarized capacitor",""
"C4, ","1","100u","CP","Capacitor_SMD:CP_Elec_6.3x3.9","Polarized capacitor",""
"C7, C6, C5, C3, C10, C11, C13, C12, ","8","100n","C_Small","Capacitor_SMD:C_0603_1608Metric","Unpolarized capacitor, small symbol",""
"C9, C8, ","2","22p","C_Small","Capacitor_SMD:C_0603_1608Metric","Unpolarized capacitor, small symbol",""
"D1, ","1","D_Schottky","D_Schottky","Diode_SMD:D_SMA","Schottky diode",""
"D2, D4, D3, D5, D6, ","5","LED","LED","LED_SMD:LED_PLCC-2","Light emitting diode",""
"J1, ","1","AVR-PDI-6","AVR-PDI-6-Connector","Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD","",""
"J2, ","1","Screw_Terminal_01x03","Screw_Terminal_01x03","Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical","Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"J3, ","1","Screw_Terminal_01x02","Screw_Terminal_01x02","Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_2-G_1x02_P5.00mm_Vertical","Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)",""
"J4, ","1","Conn_02x09_Odd_Even","Conn_02x09_Odd_Even","Connector_PinSocket_2.54mm:PinSocket_2x09_P2.54mm_Vertical","Generic connector, double row, 02x09, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)",""
"JP1, ","1","Jumper","Jumper","Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal","Jumper, normally closed",""
"JP2, JP3, JP4, JP5, JP6, JP7, JP8, JP9, JP10, ","9","Jumper_NO_Small","Jumper_NO_Small","Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm","Jumper, normally open, small symbol",""
"L1, ","1","220uH","L","Inductor_SMD:L_Bourns-SRN4018","Inductor",""
"L2, ","1","10u","L","Inductor_SMD:L_1206_3216Metric","Inductor",""
"R1, ","1","1R5","R","Resistor_SMD:R_1206_3216Metric","Resistor",""
"R2, ","1","18k","R_Small","Resistor_SMD:R_0603_1608Metric","Resistor, small symbol",""
"R3, ","1","11k","R_Small","Resistor_SMD:R_0603_1608Metric","Resistor, small symbol",""
"R4, R28, R29, ","3","100","R","Resistor_SMD:R_0603_1608Metric","Resistor",""
"R5, R7, R9, R11, R13, R15, R17, R19, R23, ","9","20k","R_Small","Resistor_SMD:R_0603_1608Metric","Resistor, small symbol",""
"R6, R8, R10, R12, R14, R16, R18, R20, R24, ","9","200","R_Small","Resistor_SMD:R_0603_1608Metric","Resistor, small symbol",""
"R21, ","1","120R","R","Resistor_SMD:R_0603_1608Metric","Resistor",""
"R22, ","1","220R","R","Resistor_SMD:R_0603_1608Metric","Resistor",""
"R25, ","1","33k","R","Resistor_SMD:R_0603_1608Metric","Resistor",""
"R26, R27, ","2","1k","R","Resistor_SMD:R_0603_1608Metric","Resistor",""
"SW1, ","1","SW_DIP_x08","SW_DIP_x08","Button_Switch_SMD:SW_DIP_SPSTx08_Slide_Omron_A6S-810x_W8.9mm_P2.54mm","8x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol",""
"TH1, TH2, TH3, TH4, TH5, TH6, TH7, TH8, TH9, ","9","Thermistor_PTC_3wire","Thermistor_PTC_3wire","Connector_Phoenix_MSTB:PhoenixContact_MSTBVA_2,5_3-G_1x03_P5.00mm_Vertical","Temperature dependent resistor, positive temperature coefficient, 3-wire interface",""
"TP_GND1, TP1, TP10, TP2, TP11, TP3, TP12, TP4, TP13, TP5, TP14, TP6, TP15, TP7, TP16, TP8, TP17, TP9, TP18, ","19","TestPoint","TestPoint","TestPoint:TestPoint_Keystone_5000-5004_Miniature","test point",""
"U1, ","1","MC34063AD","MC34063AD","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8",""
"U2, ","1","ATXMEGA32A4-AU","ATXMEGA32A4-AU-MCU_Atmel_ATMEGA","Package_QFP:TQFP-44_10x10mm_P0.8mm","",""
"U3, ","1","RE-053.3S","RE-053.3S","Converter_DCDC:Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT","",""
"U4, ","1","ADM2481","ADM2481","Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm","",""
"U5, U6, U7, U8, U9, U10, U11, U12, U13, ","9","LT3092xST","LT3092xST","Package_TO_SOT_SMD:SOT-223-3_TabPin2","200mA 2-Terminal Programmable Current Source, SOT-223",""
"Y1, ","1","Crystal_Small","Crystal_Small","Crystal:Crystal_SMD_HC49-SD","Two pin crystal, small symbol",""
