(export (version D)
  (design
    (source "/Users/max/Documents/KiCAD/IV-9_Clock V2/IV-9_Clock.sch")
    (date "Saturday, 13 October 2018 at 09:10:10")
    (tool "Eeschema (5.0.0-3-g5ebb6b6)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Clock.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Tubes/) (tstamps /5BB1F5A4/)
      (title_block
        (title Tubes)
        (company "Maximilian Nowka")
        (rev A)
        (date 2018-10-01)
        (source Tubes.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source IV-9_Tube.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /uC/) (tstamps /5BB48B05/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source uC.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 10) (name /RTC/) (tstamps /5BB6494F/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source RTC.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 11) (name "/5V PSU /") (tstamps /5BB73C46/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "5V PSU.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 12) (name "/3_3V PSU/") (tstamps /5BB8D2EE/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "3_3V PSU.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 13) (name "/PWR Input/") (tstamps /5BB7D616/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "PWR Input.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 14) (name /UserInterface/) (tstamps /5BBCA088/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source UserInterface.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 15) (name /WiFi/) (tstamps /5BC18D95/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source WiFi.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref D201)
      (value LED_Dot_red)
      (footprint LEDs:LED_D3.0mm)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBD4644))
    (comp (ref R202)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBD471C))
    (comp (ref Q201)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBDEA3D))
    (comp (ref R201)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBE40CE))
    (comp (ref D202)
      (value LED_Dot_red)
      (footprint LEDs:LED_D3.0mm)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBEEFA5))
    (comp (ref R204)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBEEFB2))
    (comp (ref Q202)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBEEFBB))
    (comp (ref R203)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBEEFC9))
    (comp (ref R205)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/) (tstamps /5BB1F5A4/))
      (tstamp 5BBE22E8))
    (comp (ref U302)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249BA))
    (comp (ref U301)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249C1))
    (comp (ref R304)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249C8))
    (comp (ref R303)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249CF))
    (comp (ref R302)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249D6))
    (comp (ref R301)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249DD))
    (comp (ref R308)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249E4))
    (comp (ref R307)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249EB))
    (comp (ref R306)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249F2))
    (comp (ref R305)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB249F9))
    (comp (ref R309)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB24A0E))
    (comp (ref C301)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB2618D))
    (comp (ref C302)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB26FB6))
    (comp (ref U303)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BBB5EFE))
    (comp (ref C303)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BBBEA7E))
    (comp (ref D301)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB7D8C2))
    (comp (ref R310)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB7D968))
    (comp (ref Q301)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BB7E97A))
    (comp (ref C304)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BC237F5))
    (comp (ref R311)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/IV-9_Tube/) (tstamps /5BB1F5A4/5BB247DF/))
      (tstamp 5BC2388D))
    (comp (ref U402)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249BA))
    (comp (ref U401)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249C1))
    (comp (ref R404)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249C8))
    (comp (ref R403)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249CF))
    (comp (ref R402)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249D6))
    (comp (ref R401)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249DD))
    (comp (ref R408)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249E4))
    (comp (ref R407)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249EB))
    (comp (ref R406)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249F2))
    (comp (ref R405)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB249F9))
    (comp (ref R409)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB24A0E))
    (comp (ref C401)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB2618D))
    (comp (ref C402)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB26FB6))
    (comp (ref U403)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BBB5EFE))
    (comp (ref C403)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BBBEA7E))
    (comp (ref D401)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB7D8C2))
    (comp (ref R410)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB7D968))
    (comp (ref Q401)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BB7E97A))
    (comp (ref C404)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BC237F5))
    (comp (ref R411)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB32DC8/) (tstamps /5BB1F5A4/5BB32DD3/))
      (tstamp 5BC2388D))
    (comp (ref U502)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249BA))
    (comp (ref U501)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249C1))
    (comp (ref R504)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249C8))
    (comp (ref R503)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249CF))
    (comp (ref R502)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249D6))
    (comp (ref R501)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249DD))
    (comp (ref R508)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249E4))
    (comp (ref R507)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249EB))
    (comp (ref R506)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249F2))
    (comp (ref R505)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB249F9))
    (comp (ref R509)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB24A0E))
    (comp (ref C501)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB2618D))
    (comp (ref C502)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB26FB6))
    (comp (ref U503)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BBB5EFE))
    (comp (ref C503)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BBBEA7E))
    (comp (ref D501)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB7D8C2))
    (comp (ref R510)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB7D968))
    (comp (ref Q501)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BB7E97A))
    (comp (ref C504)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BC237F5))
    (comp (ref R511)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB36ADE/) (tstamps /5BB1F5A4/5BB36AE9/))
      (tstamp 5BC2388D))
    (comp (ref U602)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249BA))
    (comp (ref U601)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249C1))
    (comp (ref R604)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249C8))
    (comp (ref R603)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249CF))
    (comp (ref R602)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249D6))
    (comp (ref R601)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249DD))
    (comp (ref R608)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249E4))
    (comp (ref R607)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249EB))
    (comp (ref R606)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249F2))
    (comp (ref R605)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB249F9))
    (comp (ref R609)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB24A0E))
    (comp (ref C601)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB2618D))
    (comp (ref C602)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB26FB6))
    (comp (ref U603)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BBB5EFE))
    (comp (ref C603)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BBBEA7E))
    (comp (ref D601)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB7D8C2))
    (comp (ref R610)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB7D968))
    (comp (ref Q601)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BB7E97A))
    (comp (ref C604)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BC237F5))
    (comp (ref R611)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3BB93/) (tstamps /5BB1F5A4/5BB3BB9E/))
      (tstamp 5BC2388D))
    (comp (ref U802)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249BA))
    (comp (ref U801)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249C1))
    (comp (ref R804)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249C8))
    (comp (ref R803)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249CF))
    (comp (ref R802)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249D6))
    (comp (ref R801)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249DD))
    (comp (ref R808)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249E4))
    (comp (ref R807)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249EB))
    (comp (ref R806)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249F2))
    (comp (ref R805)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB249F9))
    (comp (ref R809)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB24A0E))
    (comp (ref C801)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB2618D))
    (comp (ref C802)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB26FB6))
    (comp (ref U703)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BBB5EFE))
    (comp (ref C703)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BBBEA7E))
    (comp (ref D701)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB7D8C2))
    (comp (ref R710)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB7D968))
    (comp (ref Q701)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BB7E97A))
    (comp (ref C704)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BC237F5))
    (comp (ref R711)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86D/) (tstamps /5BB1F5A4/5BB3E89F/))
      (tstamp 5BC2388D))
    (comp (ref U702)
      (value IV-9_Tube)
      (footprint cFootprints:IV-9-tube)
      (libsource (lib Numitron) (part IV-9_Tube) (description ""))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249BA))
    (comp (ref U701)
      (value TPIC6595)
      (footprint Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (libsource (lib Interface_Expansion) (part TPIC6595) (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249C1))
    (comp (ref R704)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249C8))
    (comp (ref R703)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249CF))
    (comp (ref R702)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249D6))
    (comp (ref R701)
      (value 25R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249DD))
    (comp (ref R708)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249E4))
    (comp (ref R707)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249EB))
    (comp (ref R706)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249F2))
    (comp (ref R705)
      (value 25R)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB249F9))
    (comp (ref R709)
      (value 0.025R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB24A0E))
    (comp (ref C701)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB2618D))
    (comp (ref C702)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB26FB6))
    (comp (ref U803)
      (value AD8418)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.analog.com/media/en/technical-documentation/data-sheets/AD8418.pdf)
      (libsource (lib Amplifier_Current) (part AD8418) (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 20V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BBB5EFE))
    (comp (ref C803)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BBBEA7E))
    (comp (ref D801)
      (value LED_blue)
      (footprint LEDs:LED_0402)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB7D8C2))
    (comp (ref R810)
      (value 47R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB7D968))
    (comp (ref Q801)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BB7E97A))
    (comp (ref C804)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BC237F5))
    (comp (ref R811)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Tubes/sheet5BB3E86C/) (tstamps /5BB1F5A4/5BB3E878/))
      (tstamp 5BC2388D))
    (comp (ref C903)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB39CC9))
    (comp (ref C902)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3A26C))
    (comp (ref C901)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3A35B))
    (comp (ref Y901)
      (value Crystal)
      (footprint Crystals:Crystal_SMD_HC49-SD)
      (datasheet ~)
      (libsource (lib device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3A603))
    (comp (ref C904)
      (value 22pF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3A69F))
    (comp (ref C905)
      (value 22pF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3A72A))
    (comp (ref R913)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3BA78))
    (comp (ref R917)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3BE4C))
    (comp (ref SW901)
      (value SW_Push)
      (footprint Buttons_Switches_SMD:SW_SPST_B3SL-1002P)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3C67E))
    (comp (ref R912)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3D711))
    (comp (ref R911)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3D737))
    (comp (ref R910)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3D75D))
    (comp (ref R909)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3D785))
    (comp (ref R908)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3D7AF))
    (comp (ref R914)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3E361))
    (comp (ref R915)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3E7E0))
    (comp (ref R906)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3F6E2))
    (comp (ref R905)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3F6E9))
    (comp (ref R904)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3F6F0))
    (comp (ref R903)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3F6F7))
    (comp (ref R902)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB3F6FE))
    (comp (ref R901)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB43320))
    (comp (ref R916)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB4E3C2))
    (comp (ref J901)
      (value AVR-ISP-6)
      (footprint Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD)
      (datasheet " ~")
      (libsource (lib Connector) (part AVR-ISP-6) (description "Atmel 6-pin ISP connector"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB4F230))
    (comp (ref D903)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (datasheet ~)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB54DD6))
    (comp (ref D902)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (datasheet ~)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB54E24))
    (comp (ref D901)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (datasheet ~)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB54E76))
    (comp (ref R919)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB60B72))
    (comp (ref R918)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB60C0B))
    (comp (ref R922)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB62DF5))
    (comp (ref R923)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB62DFC))
    (comp (ref R924)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB63CA3))
    (comp (ref R921)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB63CF7))
    (comp (ref R920)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB63D55))
    (comp (ref R925)
      (value 4.7k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB6CF46))
    (comp (ref R926)
      (value 4.7k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BB6CFEE))
    (comp (ref Q901)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBEE4A1))
    (comp (ref D904)
      (value LED_error_red)
      (footprint LEDs:LED_0805)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBEE58A))
    (comp (ref R928)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBEE970))
    (comp (ref R929)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBF0215))
    (comp (ref D905)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (datasheet ~)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBF0332))
    (comp (ref R927)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BBF7914))
    (comp (ref R930)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC12BB4))
    (comp (ref R931)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC14A1B))
    (comp (ref R932)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC1BD67))
    (comp (ref U902)
      (value ATmega32-16AU)
      (footprint Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf)
      (libsource (lib MCU_Microchip_ATmega) (part ATmega32-16AU) (description "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC060C8))
    (comp (ref U901)
      (value ADR292)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (libsource (lib voltage_ref) (part ADR292) (description ""))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC39713))
    (comp (ref R907)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC50B36))
    (comp (ref R933)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC568B6))
    (comp (ref R934)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC58906))
    (comp (ref R935)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC5AA8D))
    (comp (ref R936)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC5CD4F))
    (comp (ref R937)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /uC/) (tstamps /5BB48B05/))
      (tstamp 5BC5F151))
    (comp (ref U1101)
      (value DS3231MZ)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://datasheets.maximintegrated.com/en/ds/DS3231M.pdf)
      (libsource (lib Timer_RTC) (part DS3231MZ) (description "±5ppm, I2C Real-Time Clock SOIC-8"))
      (sheetpath (names /RTC/) (tstamps /5BB6494F/))
      (tstamp 5BB64ADA))
    (comp (ref C1101)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RTC/) (tstamps /5BB6494F/))
      (tstamp 5BB64C0D))
    (comp (ref BT1101)
      (value Battery_Cell)
      (footprint Battery_Holders:BatteryHolder_CoinCell_Keystone_3000)
      (datasheet ~)
      (libsource (lib device) (part Battery_Cell) (description "single battery cell"))
      (sheetpath (names /RTC/) (tstamps /5BB6494F/))
      (tstamp 5BB6519B))
    (comp (ref R1201)
      (value 0.33R)
      (footprint Resistors_SMD:R_2512)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49521))
    (comp (ref L1201)
      (value 100uH)
      (footprint Inductors_SMD:L_Wuerth_MAPI-4020)
      (libsource (lib device) (part L) (description Inductor))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49522))
    (comp (ref C1203)
      (value 83pF)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49524))
    (comp (ref C1204)
      (value 470uF)
      (footprint Capacitors_SMD:CP_Elec_6.3x7.7)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49527))
    (comp (ref R1202)
      (value 22k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 59D46945))
    (comp (ref R1203)
      (value 4.7k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 59D469D9))
    (comp (ref D1201)
      (value SB350)
      (footprint Diodes_SMD:D_SMB)
      (libsource (lib device) (part D) (description Diode))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 59D454FD))
    (comp (ref D1202)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB4952F))
    (comp (ref U1201)
      (value MC34063AD)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF)
      (libsource (lib Regulator_Switching) (part MC34063AD) (description "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB74814))
    (comp (ref C1202)
      (value 220uF)
      (footprint Capacitors_SMD:CP_Elec_8x10.5)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49533))
    (comp (ref C1201)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49534))
    (comp (ref RV1201)
      (value 10k)
      (footprint Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL)
      (datasheet ~)
      (libsource (lib device) (part R_POT_TRIM) (description Trim-Potentiometer))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB49537))
    (comp (ref C1205)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/5V PSU /") (tstamps /5BB73C46/))
      (tstamp 5BB47F9D))
    (comp (ref R1301)
      (value 0.33R)
      (footprint Resistors_SMD:R_2512)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 59D44D00))
    (comp (ref L1301)
      (value 100uH)
      (footprint Inductors_SMD:L_Wuerth_MAPI-4020)
      (libsource (lib device) (part L) (description Inductor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 59D4542E))
    (comp (ref C1303)
      (value 330pF)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 59D455EA))
    (comp (ref C1304)
      (value 470uF)
      (footprint Capacitors_SMD:CP_Elec_6.3x7.7)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 59D46505))
    (comp (ref R1302)
      (value 27k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB49529))
    (comp (ref R1303)
      (value 4.7k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB4952A))
    (comp (ref D1301)
      (value VSSC8L45-M3/9AT)
      (footprint Diodes_SMD:D_SMC)
      (libsource (lib device) (part D) (description Diode))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB49523))
    (comp (ref U1301)
      (value MC34063AD)
      (footprint Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm)
      (datasheet http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF)
      (libsource (lib Regulator_Switching) (part MC34063AD) (description "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB49532))
    (comp (ref C1302)
      (value 220uF)
      (footprint Capacitors_SMD:CP_Elec_8x10.5)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB80A8D))
    (comp (ref C1301)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB81889))
    (comp (ref RV1301)
      (value 10k)
      (footprint Potentiometers:Potentiometer_Trimmer_Vishay_TS53YL)
      (datasheet ~)
      (libsource (lib device) (part R_POT_TRIM) (description Trim-Potentiometer))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB85821))
    (comp (ref C1305)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB49531))
    (comp (ref Q1302)
      (value BC850)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657)
      (libsource (lib Transistor_BJT) (part BC850) (description "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB57D85))
    (comp (ref R1307)
      (value 200R)
      (footprint Resistors_SMD:R_0805)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB57E62))
    (comp (ref Q1301)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB59C86))
    (comp (ref R1306)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB5A81D))
    (comp (ref R1304)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB5CFDD))
    (comp (ref R1305)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB5D0B6))
    (comp (ref C1306)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB5DF23))
    (comp (ref Q1303)
      (value BSS138)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (libsource (lib Transistor_FET) (part BSS138) (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB6719E))
    (comp (ref D1303)
      (value LED_2.5VPSU_off_red)
      (footprint Diodes_SMD:D_0805)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB6A6ED))
    (comp (ref R1308)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB71DFD))
    (comp (ref R1309)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB967B8))
    (comp (ref D1302)
      (value DZ_2.7V)
      (footprint Diodes_SMD:D_MiniMELF)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5AAD3380))
    (comp (ref D1304)
      (value DZ_5.1V)
      (footprint Diodes_SMD:D_MiniMELF)
      (libsource (lib device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BB9689B))
    (comp (ref Q1304)
      (value PHPT60406NY)
      (footprint TO_SOT_Packages_SMD:SOT-669_LFPAK_ThermalVias-2)
      (datasheet ~)
      (libsource (lib device) (part Q_NPN_BCE) (description "Transistor NPN (general)"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC1E52E))
    (comp (ref R1310)
      (value 3.3k)
      (footprint Resistors_SMD:R_0805)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC1FD35))
    (comp (ref R1311)
      (value 0R)
      (footprint Resistors_SMD:R_0805)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC25F71))
    (comp (ref C1307)
      (value 470uF)
      (footprint Capacitors_SMD:CP_Elec_6.3x7.7)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC3EDF8))
    (comp (ref L1202)
      (value BLM31KN601SN1L)
      (footprint Inductors_SMD:L_1206)
      (datasheet ~)
      (libsource (lib device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC1CECA))
    (comp (ref C1206)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/3_3V PSU/") (tstamps /5BB8D2EE/))
      (tstamp 5BC34D02))
    (comp (ref J1401)
      (value Barrel_Jack_Switch)
      (footprint Connectors:BARREL_JACK)
      (datasheet ~)
      (libsource (lib Connector) (part Barrel_Jack_Switch) (description "DC Barrel Jack with an internal switch"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7D6F8))
    (comp (ref F1401)
      (value Fuse)
      (footprint "Fuse Holder:Nano Fuse Holder")
      (datasheet ~)
      (libsource (lib device) (part Fuse) (description "Fuse, generic"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7D87A))
    (comp (ref D1401)
      (value D_Schottky)
      (footprint Diodes_SMD:D_SMB)
      (datasheet ~)
      (libsource (lib device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7D945))
    (comp (ref C1402)
      (value 220uF)
      (footprint Capacitors_SMD:CP_Elec_8x10.5)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7DD24))
    (comp (ref C1403)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7DDC7))
    (comp (ref SW1401)
      (value SW_SPDT)
      (footprint Kippschalter:B12AV)
      (libsource (lib switch) (part SW_SPDT) (description ""))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7EDAF))
    (comp (ref C1401)
      (value 220uF)
      (footprint Capacitors_SMD:CP_Elec_8x10.5)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB7F33C))
    (comp (ref MH1401)
      (value MountingHole)
      (footprint Connectors:1pin)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB8682A))
    (comp (ref MH1403)
      (value MountingHole)
      (footprint Connectors:1pin)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB868BC))
    (comp (ref MH1404)
      (value MountingHole)
      (footprint Connectors:1pin)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB868ED))
    (comp (ref MH1402)
      (value MountingHole)
      (footprint Connectors:1pin)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names "/PWR Input/") (tstamps /5BB7D616/))
      (tstamp 5BB86916))
    (comp (ref R1504)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 59F6F3C9))
    (comp (ref R1503)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 59F6F3FA))
    (comp (ref R1505)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 59F6F47F))
    (comp (ref R1502)
      (value 1k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5A0B4628))
    (comp (ref R1501)
      (value 1k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5A0B465E))
    (comp (ref C1502)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5A0B46B9))
    (comp (ref C1501)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5A0B46FC))
    (comp (ref C1503)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5A0DEE19))
    (comp (ref SW1501)
      (value Rotary_Encoder_Switch)
      (footprint Encoder:STEC11B01)
      (datasheet ~)
      (libsource (lib device) (part Rotary_Encoder_Switch) (description "Rotary encoder, dual channel, incremental quadrate outputs, with switch"))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5BBCA305))
    (comp (ref SW1503)
      (value SW_DIP_x03)
      (footprint Buttons_Switches_SMD:SW_DIP_x3_W5.9mm_Slide_Copal_CVS)
      (libsource (lib Switch) (part SW_DIP_x03) (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5BC054E9))
    (comp (ref R1506)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5BC06246))
    (comp (ref R1507)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5BC0636F))
    (comp (ref R1508)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /UserInterface/) (tstamps /5BBCA088/))
      (tstamp 5BC0639A))
    (comp (ref R1602)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BC4266E))
    (comp (ref U1601)
      (value "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)")
      (footprint NEO-6M_24P-16X12.2MM_:GPS24P-SMD-1.1-16X12.2MM)
      (datasheet None)
      (fields
        (field (name Field4) "SMD GPS Module;")
        (field (name Field5) NEO-6M-GPS)
        (field (name Field6) None)
        (field (name Field7) u-blox)
        (field (name Field8) Unavailable))
      (libsource (lib NEO-6M_24P-16X12.2MM_) (part "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)") (description ""))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB887E8))
    (comp (ref R1601)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB8A952))
    (comp (ref D1601)
      (value LED)
      (footprint LEDs:LED_0805)
      (datasheet ~)
      (libsource (lib device) (part LED) (description "LED generic"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB8AC9C))
    (comp (ref C1602)
      (value 10uF)
      (footprint Capacitors_SMD:C_1206)
      (datasheet ~)
      (libsource (lib device) (part CP) (description "Polarised capacitor"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB9F9F1))
    (comp (ref C1603)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBA0467))
    (comp (ref C1605)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBA3100))
    (comp (ref C1604)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBA317C))
    (comp (ref R1607)
      (value 22R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBA78F0))
    (comp (ref L1601)
      (value 27uH)
      (footprint Inductors_SMD:L_0603)
      (datasheet ~)
      (libsource (lib device) (part L) (description Inductor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBA9401))
    (comp (ref D1602)
      (value D)
      (footprint Diodes_SMD:D_0603)
      (datasheet ~)
      (libsource (lib device) (part D) (description Diode))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBAE28A))
    (comp (ref J1602)
      (value Antenna_Conc)
      (footprint "Axial Connector SMD:U.FL Coaxial Connector")
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBCE948))
    (comp (ref R1603)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBDEE86))
    (comp (ref R1604)
      (value 0R)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBDFF6A))
    (comp (ref C1601)
      (value 100nF)
      (footprint Capacitors_SMD:C_0603)
      (datasheet ~)
      (libsource (lib device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBE487C))
    (comp (ref U1602)
      (value TXB0102DCT)
      (footprint Housings_SSOP:VSSOP-8_2.3x2mm_Pitch0.5mm)
      (datasheet http://www.ti.com/lit/ds/symlink/txb0102.pdf)
      (libsource (lib Logic_LevelTranslator) (part TXB0102DCT) (description "2-Bit Bidirectional Voltage-Level Translator in TSSOP Package With Auto Direction Sensing and ±15-kV ESD Protection"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB99F1D))
    (comp (ref R1605)
      (value 0R)
      (footprint Resistors_SMD:R_2512)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBF012F))
    (comp (ref J1601)
      (value Conn_01x01_Female)
      (footprint "Axial Connector SMD:Ceramic_GPS_Antenna_SMD")
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x01_Female) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BC0A07F))
    (comp (ref U1603)
      (value 24AA32A)
      (footprint Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm)
      (libsource (lib 24AA32A) (part 24AA32A) (description ""))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BBF235B))
    (comp (ref R1606)
      (value "10k (wenns nicht läuft anpassen! siehe datenblatt)")
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BB9A675))
    (comp (ref R1608)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (datasheet ~)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /WiFi/) (tstamps /5BC18D95/))
      (tstamp 5BC191B1)))
  (libparts
    (libpart (lib 24AA32A) (part 24AA32A)
      (footprints
        (fp TSSOP))
      (fields
        (field (name Reference) U)
        (field (name Value) 24AA32A))
      (pins
        (pin (num 1) (name WP) (type input))
        (pin (num 2) (name VCC) (type input))
        (pin (num 3) (name A0) (type input))
        (pin (num 4) (name A1) (type input))
        (pin (num 5) (name A2) (type input))
        (pin (num 6) (name GND) (type input))
        (pin (num 7) (name SDA) (type input))
        (pin (num 8) (name SCL) (type input))))
    (libpart (lib Amplifier_Current) (part AD8417)
      (aliases
        (alias AD8418))
      (description "70V Bidirectional, Zero Drift, Current Sense Amplifier, 60V/V gain, bandwidth 250kHz, VS=2.7V~5.5V, SOIC-8/MSOP-8")
      (docs http://www.analog.com/media/en/technical-documentation/data-sheets/AD8417.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*)
        (fp MSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) AD8417))
      (pins
        (pin (num 1) (name IN-) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name REF2) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name OUT) (type output))
        (pin (num 6) (name VS) (type power_in))
        (pin (num 7) (name REF1) (type input))
        (pin (num 8) (name IN+) (type input))))
    (libpart (lib Connector) (part AVR-ISP-6)
      (description "Atmel 6-pin ISP connector")
      (docs " ~")
      (footprints
        (fp IDC?Header*2x03*)
        (fp Pin?Header*2x03*))
      (fields
        (field (name Reference) J)
        (field (name Value) AVR-ISP-6))
      (pins
        (pin (num 1) (name MISO) (type passive))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name SCK) (type passive))
        (pin (num 4) (name MOSI) (type passive))
        (pin (num 5) (name ~RST) (type passive))
        (pin (num 6) (name GND) (type power_in))))
    (libpart (lib Connector) (part Barrel_Jack_Switch)
      (description "DC Barrel Jack with an internal switch")
      (docs ~)
      (footprints
        (fp BarrelJack*))
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack_Switch))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib Connector) (part Conn_01x01_Female)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Female)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Interface_Expansion) (part TPIC6595)
      (description "Power Logic 8-bit Shift Register, DIP-8/SOIC-8")
      (docs http://www.ti.com/lit/ds/symlink/tpic6595.pdf)
      (footprints
        (fp SOIC*7.5x12.8mm*P1.27mm*)
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPIC6595))
      (pins
        (pin (num 1) (name PGND) (type power_in))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name SER_IN) (type input))
        (pin (num 4) (name DRAIN0) (type openCol))
        (pin (num 5) (name DRAIN1) (type openCol))
        (pin (num 6) (name DRAIN2) (type openCol))
        (pin (num 7) (name DRAIN3) (type openCol))
        (pin (num 8) (name ~SRCLR) (type input))
        (pin (num 9) (name ~G) (type input))
        (pin (num 10) (name PGND) (type passive))
        (pin (num 11) (name PGND) (type passive))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name SRCK) (type input))
        (pin (num 14) (name DRAIN4) (type openCol))
        (pin (num 15) (name DRAIN5) (type openCol))
        (pin (num 16) (name DRAIN6) (type openCol))
        (pin (num 17) (name DRAIN7) (type openCol))
        (pin (num 18) (name SER_OUT) (type output))
        (pin (num 19) (name LGND) (type power_in))
        (pin (num 20) (name PGND) (type passive))))
    (libpart (lib Logic_LevelTranslator) (part TXB0102DCT)
      (description "2-Bit Bidirectional Voltage-Level Translator in TSSOP Package With Auto Direction Sensing and ±15-kV ESD Protection")
      (docs http://www.ti.com/lit/ds/symlink/txb0102.pdf)
      (footprints
        (fp TSSOP*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TXB0102DCT)
        (field (name Footprint) Package_SO:TSSOP-8_3x3mm_P0.65mm))
      (pins
        (pin (num 1) (name B2) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VCCA) (type power_in))
        (pin (num 4) (name A2) (type BiDi))
        (pin (num 5) (name A1) (type BiDi))
        (pin (num 6) (name OE) (type input))
        (pin (num 7) (name VCCB) (type power_in))
        (pin (num 8) (name B1) (type BiDi))))
    (libpart (lib MCU_Microchip_ATmega) (part ATmega16L-8AU)
      (aliases
        (alias ATmega16-16AU)
        (alias ATmega16A-AU)
        (alias ATmega32L-8AU)
        (alias ATmega32-16AU)
        (alias ATmega32A-AU))
      (description "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf)
      (footprints
        (fp TQFP*10x10mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATmega16L-8AU)
        (field (name Footprint) Package_QFP:TQFP-44_10x10mm_P0.8mm))
      (pins
        (pin (num 1) (name PB5) (type BiDi))
        (pin (num 2) (name PB6) (type BiDi))
        (pin (num 3) (name PB7) (type BiDi))
        (pin (num 4) (name ~RESET) (type input))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name XTAL2) (type BiDi))
        (pin (num 8) (name XTAL1) (type BiDi))
        (pin (num 9) (name PD0) (type BiDi))
        (pin (num 10) (name PD1) (type BiDi))
        (pin (num 11) (name PD2) (type BiDi))
        (pin (num 12) (name PD3) (type BiDi))
        (pin (num 13) (name PD4) (type BiDi))
        (pin (num 14) (name PD5) (type BiDi))
        (pin (num 15) (name PD6) (type BiDi))
        (pin (num 16) (name PD7) (type BiDi))
        (pin (num 17) (name VCC) (type passive))
        (pin (num 18) (name GND) (type passive))
        (pin (num 19) (name PC0) (type BiDi))
        (pin (num 20) (name PC1) (type BiDi))
        (pin (num 21) (name PC2) (type BiDi))
        (pin (num 22) (name PC3) (type BiDi))
        (pin (num 23) (name PC4) (type BiDi))
        (pin (num 24) (name PC5) (type BiDi))
        (pin (num 25) (name PC6) (type BiDi))
        (pin (num 26) (name PC7) (type BiDi))
        (pin (num 27) (name AVCC) (type power_in))
        (pin (num 28) (name GND) (type passive))
        (pin (num 29) (name AREF) (type input))
        (pin (num 30) (name PA7) (type BiDi))
        (pin (num 31) (name PA6) (type BiDi))
        (pin (num 32) (name PA5) (type BiDi))
        (pin (num 33) (name PA4) (type BiDi))
        (pin (num 34) (name PA3) (type BiDi))
        (pin (num 35) (name PA2) (type BiDi))
        (pin (num 36) (name PA1) (type BiDi))
        (pin (num 37) (name PA0) (type BiDi))
        (pin (num 38) (name VCC) (type passive))
        (pin (num 39) (name GND) (type passive))
        (pin (num 40) (name PB0) (type BiDi))
        (pin (num 41) (name PB1) (type BiDi))
        (pin (num 42) (name PB2) (type BiDi))
        (pin (num 43) (name PB3) (type BiDi))
        (pin (num 44) (name PB4) (type BiDi))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) MH)
        (field (name Value) MountingHole)))
    (libpart (lib NEO-6M_24P-16X12.2MM_) (part "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)")
      (fields
        (field (name Reference) U)
        (field (name Value) "MOUDLE-GPS-NEO-6M(24P-16X12.2MM)")
        (field (name Footprint) GPS24P-SMD-1.1-16X12.2MM)
        (field (name Datasheet) None)
        (field (name Field4) "SMD GPS Module;")
        (field (name Field5) NEO-6M-GPS)
        (field (name Field6) None)
        (field (name Field7) u-blox)
        (field (name Field8) Unavailable))
      (pins
        (pin (num 1) (name NC) (type BiDi))
        (pin (num 2) (name NC2) (type BiDi))
        (pin (num 3) (name TP) (type BiDi))
        (pin (num 4) (name EX) (type BiDi))
        (pin (num 5) (name UDM) (type BiDi))
        (pin (num 6) (name UDP) (type BiDi))
        (pin (num 7) (name VU) (type BiDi))
        (pin (num 8) (name NC3) (type BiDi))
        (pin (num 9) (name VRF) (type BiDi))
        (pin (num 10) (name GND) (type BiDi))
        (pin (num 11) (name RFIN) (type BiDi))
        (pin (num 12) (name GND2) (type BiDi))
        (pin (num 13) (name GND3) (type BiDi))
        (pin (num 14) (name NC4) (type BiDi))
        (pin (num 15) (name NC5) (type BiDi))
        (pin (num 16) (name NC6) (type BiDi))
        (pin (num 17) (name NC7) (type BiDi))
        (pin (num 18) (name SDA) (type BiDi))
        (pin (num 19) (name SCL) (type BiDi))
        (pin (num 20) (name TX) (type BiDi))
        (pin (num 21) (name RX) (type BiDi))
        (pin (num 22) (name VB) (type BiDi))
        (pin (num 23) (name VCC) (type BiDi))
        (pin (num 24) (name GND4) (type BiDi))))
    (libpart (lib Numitron) (part IV-9_Tube)
      (fields
        (field (name Reference) U)
        (field (name Value) IV-9_Tube))
      (pins
        (pin (num 1) (name Common_Anode) (type input))
        (pin (num 2) (name Dot) (type input))
        (pin (num 3) (name Segment_b) (type input))
        (pin (num 4) (name Segment_c) (type input))
        (pin (num 5) (name Segment_a) (type input))
        (pin (num 6) (name Segment_f) (type input))
        (pin (num 7) (name Segment_g) (type input))
        (pin (num 8) (name Segment_d) (type input))
        (pin (num 9) (name Segment_e) (type input))))
    (libpart (lib Regulator_Switching) (part MC33063AD)
      (aliases
        (alias SC33063AD)
        (alias NCV33063AVD)
        (alias MC34063AD))
      (description "1.5A, step-up/down/inverting switching regulator, 3-40V Vin, 100kHz, SO-8")
      (docs http://www.onsemi.com/pub_link/Collateral/MC34063A-D.PDF)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MC33063AD)
        (field (name Footprint) Package_SO:SOIC-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name SwC) (type openCol))
        (pin (num 2) (name SwE) (type openEm))
        (pin (num 3) (name TC) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Vfb) (type input))
        (pin (num 6) (name Vin) (type power_in))
        (pin (num 7) (name Ipk) (type input))
        (pin (num 8) (name DC) (type openCol))))
    (libpart (lib Switch) (part SW_DIP_x03)
      (description "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x3*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x03))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Timer_RTC) (part DS3231MZ)
      (description "±5ppm, I2C Real-Time Clock SOIC-8")
      (docs http://datasheets.maximintegrated.com/en/ds/DS3231M.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) DS3231MZ)
        (field (name Footprint) Package_SO:SOIC-8_3.9x4.9mm_P1.27mm))
      (pins
        (pin (num 1) (name 32KHZ) (type openCol))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name ~INT~/SQW) (type openCol))
        (pin (num 4) (name ~RST) (type BiDi))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name VBAT) (type power_in))
        (pin (num 7) (name SDA) (type BiDi))
        (pin (num 8) (name SCL) (type input))))
    (libpart (lib Transistor_BJT) (part BC817)
      (aliases
        (alias BC818)
        (alias BC847)
        (alias BC848)
        (alias BC849)
        (alias BC850)
        (alias MMBT3904)
        (alias MMBT5550L)
        (alias MMBT5551L))
      (description "0.8A Ic, 45V Vce, NPN Transistor, SOT-23")
      (docs http://www.fairchildsemi.com/ds/BC/BC817.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC817)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transistor_FET) (part BSS138)
      (aliases
        (alias 2N7002)
        (alias MMBF170))
      (description "50V Vds, 0.22A Id, N-channel MOSFET, SOT-23")
      (docs https://www.fairchildsemi.com/datasheets/BS/BSS138.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BSS138)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib device) (part Battery_Cell)
      (description "single battery cell")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part D_Zener)
      (description "Zener Diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Ferrite_Bead)
      (description "Ferrite bead")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) L)
        (field (name Value) Ferrite_Bead))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Fuse)
      (description "Fuse, generic")
      (docs ~)
      (footprints
        (fp *Fuse*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (description "LED generic")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Q_NPN_BCE)
      (description "Transistor NPN (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_BCE))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R_POT_TRIM)
      (description Trim-Potentiometer)
      (docs ~)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) R_POT_TRIM))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part Rotary_Encoder_Switch)
      (description "Rotary encoder, dual channel, incremental quadrate outputs, with switch")
      (docs ~)
      (footprints
        (fp RotaryEncoder*Switch*))
      (fields
        (field (name Reference) SW)
        (field (name Value) Rotary_Encoder_Switch))
      (pins
        (pin (num A) (name A) (type passive))
        (pin (num B) (name B) (type passive))
        (pin (num C) (name C) (type passive))
        (pin (num S1) (name S1) (type passive))
        (pin (num S2) (name S2) (type passive))))
    (libpart (lib switch) (part SW_SPDT)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_SPDT))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib voltage_ref) (part ADR292)
      (fields
        (field (name Reference) U)
        (field (name Value) ADR292))
      (pins
        (pin (num 1) (name N.C.) (type NotConnected))
        (pin (num 2) (name V_in) (type input))
        (pin (num 3) (name N.C.) (type NotConnected))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name N.C.) (type NotConnected))
        (pin (num 6) (name V_out) (type output))
        (pin (num 7) (name N.C.) (type NotConnected))
        (pin (num 8) (name N.C.) (type NotConnected)))))
  (libraries
    (library (logical 24AA32A)
      (uri /Users/max/Documents/KiCAD/library/24AA32A.lib))
    (library (logical Amplifier_Current)
      (uri "/Library/Application Support/kicad/library/Amplifier_Current.lib"))
    (library (logical Connector)
      (uri "/Library/Application Support/kicad/library/Connector.lib"))
    (library (logical Interface_Expansion)
      (uri "/Library/Application Support/kicad/library/Interface_Expansion.lib"))
    (library (logical Logic_LevelTranslator)
      (uri "/Library/Application Support/kicad/library/Logic_LevelTranslator.lib"))
    (library (logical MCU_Microchip_ATmega)
      (uri "/Library/Application Support/kicad/library/MCU_Microchip_ATmega.lib"))
    (library (logical Mechanical)
      (uri "/Library/Application Support/kicad/library/Mechanical.lib"))
    (library (logical NEO-6M_24P-16X12.2MM_)
      (uri /Users/max/Documents/KiCAD/library/GPS/NEO-6M_24P-16X12.2MM_.lib))
    (library (logical Numitron)
      (uri /Users/max/Documents/KiCAD/library/Nixies/Numitron.lib))
    (library (logical Regulator_Switching)
      (uri "/Library/Application Support/kicad/library/Regulator_Switching.lib"))
    (library (logical Switch)
      (uri "/Library/Application Support/kicad/library/Switch.lib"))
    (library (logical Timer_RTC)
      (uri "/Library/Application Support/kicad/library/Timer_RTC.lib"))
    (library (logical Transistor_BJT)
      (uri "/Library/Application Support/kicad/library/Transistor_BJT.lib"))
    (library (logical Transistor_FET)
      (uri "/Library/Application Support/kicad/library/Transistor_FET.lib"))
    (library (logical device)
      (uri "/Library/Application Support/kicad/library/device.lib"))
    (library (logical switch)
      (uri /Users/max/Documents/KiCAD/library/switch.lib))
    (library (logical voltage_ref)
      (uri /Users/max/Documents/KiCAD/library/voltage_ref.lib)))
  (nets
    (net (code 1) (name /Tubes/IV-9_Tube/Data_out)
      (node (ref U301) (pin 18)))
    (net (code 2) (name VCC)
      (node (ref U902) (pin 27))
      (node (ref U1101) (pin 2))
      (node (ref U902) (pin 17))
      (node (ref U801) (pin 2))
      (node (ref C1101) (pin 2))
      (node (ref L1201) (pin 1))
      (node (ref C1205) (pin 1))
      (node (ref D1202) (pin 1))
      (node (ref R1202) (pin 1))
      (node (ref C1204) (pin 1))
      (node (ref R1504) (pin 1))
      (node (ref R1503) (pin 1))
      (node (ref R1505) (pin 1))
      (node (ref R1506) (pin 1))
      (node (ref R1507) (pin 1))
      (node (ref R1508) (pin 1))
      (node (ref U1602) (pin 7))
      (node (ref C1605) (pin 2))
      (node (ref R926) (pin 1))
      (node (ref U301) (pin 2))
      (node (ref R925) (pin 1))
      (node (ref C301) (pin 2))
      (node (ref U303) (pin 6))
      (node (ref U303) (pin 7))
      (node (ref C303) (pin 2))
      (node (ref U401) (pin 2))
      (node (ref J901) (pin 2))
      (node (ref U902) (pin 38))
      (node (ref C401) (pin 2))
      (node (ref U902) (pin 5))
      (node (ref U403) (pin 6))
      (node (ref U403) (pin 7))
      (node (ref C403) (pin 2))
      (node (ref U503) (pin 7))
      (node (ref U503) (pin 6))
      (node (ref C501) (pin 2))
      (node (ref U501) (pin 2))
      (node (ref C503) (pin 2))
      (node (ref R917) (pin 1))
      (node (ref U601) (pin 2))
      (node (ref C601) (pin 2))
      (node (ref C902) (pin 1))
      (node (ref U603) (pin 6))
      (node (ref U603) (pin 7))
      (node (ref C903) (pin 2))
      (node (ref C603) (pin 2))
      (node (ref C701) (pin 2))
      (node (ref C801) (pin 2))
      (node (ref U803) (pin 6))
      (node (ref U803) (pin 7))
      (node (ref C803) (pin 2))
      (node (ref U701) (pin 2))
      (node (ref R204) (pin 1))
      (node (ref C703) (pin 2))
      (node (ref R202) (pin 1))
      (node (ref U703) (pin 7))
      (node (ref U703) (pin 6)))
    (net (code 3) (name +3V3)
      (node (ref R809) (pin 1))
      (node (ref U703) (pin 8))
      (node (ref U503) (pin 8))
      (node (ref R1309) (pin 2))
      (node (ref C1307) (pin 1))
      (node (ref R710) (pin 2))
      (node (ref R509) (pin 1))
      (node (ref L1202) (pin 2))
      (node (ref C1206) (pin 1))
      (node (ref R709) (pin 1))
      (node (ref R810) (pin 2))
      (node (ref R410) (pin 2))
      (node (ref R1605) (pin 1))
      (node (ref U803) (pin 8))
      (node (ref U1602) (pin 3))
      (node (ref D1602) (pin 2))
      (node (ref C1604) (pin 1))
      (node (ref R510) (pin 2))
      (node (ref R610) (pin 2))
      (node (ref C1603) (pin 1))
      (node (ref C1602) (pin 1))
      (node (ref U1601) (pin 23))
      (node (ref U603) (pin 8))
      (node (ref R309) (pin 1))
      (node (ref U303) (pin 8))
      (node (ref R310) (pin 2))
      (node (ref U403) (pin 8))
      (node (ref R609) (pin 1))
      (node (ref R409) (pin 1)))
    (net (code 4) (name Currentsensing_Tube_1)
      (node (ref R907) (pin 1))
      (node (ref R311) (pin 1))
      (node (ref C304) (pin 1)))
    (net (code 5) (name Currentsensing_Tube_2)
      (node (ref R933) (pin 1))
      (node (ref R411) (pin 1))
      (node (ref C404) (pin 1)))
    (net (code 6) (name /Tubes/sheet5BB32DC8/Data_in)
      (node (ref U501) (pin 18))
      (node (ref U401) (pin 3)))
    (net (code 7) (name Currentsensing_Tube_3)
      (node (ref R934) (pin 1))
      (node (ref C504) (pin 1))
      (node (ref R511) (pin 1)))
    (net (code 8) (name /Tubes/sheet5BB3BB93/Data_in)
      (node (ref U601) (pin 3))
      (node (ref U701) (pin 18)))
    (net (code 9) (name /Tubes/sheet5BB36ADE/Data_in)
      (node (ref U501) (pin 3))
      (node (ref U601) (pin 18)))
    (net (code 10) (name Currentsensing_Tube_4)
      (node (ref R935) (pin 1))
      (node (ref R611) (pin 1))
      (node (ref C604) (pin 1)))
    (net (code 11) (name ~enable_Shiftregister)
      (node (ref U701) (pin 13))
      (node (ref U601) (pin 13))
      (node (ref U801) (pin 13))
      (node (ref U501) (pin 13))
      (node (ref U401) (pin 13))
      (node (ref R909) (pin 1))
      (node (ref U301) (pin 13)))
    (net (code 12) (name clk)
      (node (ref R932) (pin 1))
      (node (ref U801) (pin 9))
      (node (ref U401) (pin 9))
      (node (ref U501) (pin 9))
      (node (ref U601) (pin 9))
      (node (ref U701) (pin 9))
      (node (ref U301) (pin 9)))
    (net (code 13) (name reset_Shiftregister)
      (node (ref U301) (pin 8))
      (node (ref U801) (pin 8))
      (node (ref R910) (pin 1))
      (node (ref U501) (pin 8))
      (node (ref U701) (pin 8))
      (node (ref U601) (pin 8))
      (node (ref U401) (pin 8)))
    (net (code 14) (name ~latch_Shiftregister)
      (node (ref U301) (pin 12))
      (node (ref R908) (pin 1))
      (node (ref U401) (pin 12))
      (node (ref U601) (pin 12))
      (node (ref U701) (pin 12))
      (node (ref U801) (pin 12))
      (node (ref U501) (pin 12)))
    (net (code 15) (name Currentsensing_Tube_6)
      (node (ref R937) (pin 1))
      (node (ref C704) (pin 1))
      (node (ref R711) (pin 1)))
    (net (code 16) (name /Tubes/IV-9_Tube/Data_in)
      (node (ref U301) (pin 3))
      (node (ref U401) (pin 18)))
    (net (code 17) (name /Tubes/sheet5BB3E86C/Data_in)
      (node (ref U801) (pin 18))
      (node (ref U701) (pin 3)))
    (net (code 18) (name MOSI)
      (node (ref R931) (pin 1))
      (node (ref U801) (pin 3)))
    (net (code 19) (name Currentsensing_Tube_5)
      (node (ref C804) (pin 1))
      (node (ref R811) (pin 1))
      (node (ref R936) (pin 1)))
    (net (code 20) (name "Net-(D201-Pad2)")
      (node (ref R202) (pin 2))
      (node (ref D201) (pin 2)))
    (net (code 21) (name "Net-(D201-Pad1)")
      (node (ref Q201) (pin 3))
      (node (ref D201) (pin 1)))
    (net (code 22) (name GND)
      (node (ref C802) (pin 2))
      (node (ref C1205) (pin 2))
      (node (ref BT1101) (pin 2))
      (node (ref C801) (pin 1))
      (node (ref U703) (pin 2))
      (node (ref U703) (pin 3))
      (node (ref C1201) (pin 2))
      (node (ref C1202) (pin 2))
      (node (ref C301) (pin 1))
      (node (ref U301) (pin 11))
      (node (ref U301) (pin 20))
      (node (ref C703) (pin 1))
      (node (ref Q201) (pin 2))
      (node (ref U301) (pin 10))
      (node (ref U1201) (pin 4))
      (node (ref R201) (pin 2))
      (node (ref C302) (pin 2))
      (node (ref Q701) (pin 2))
      (node (ref D1202) (pin 2))
      (node (ref D1201) (pin 2))
      (node (ref U301) (pin 1))
      (node (ref C704) (pin 2))
      (node (ref C1101) (pin 1))
      (node (ref R1203) (pin 2))
      (node (ref C1204) (pin 2))
      (node (ref Q202) (pin 2))
      (node (ref U701) (pin 1))
      (node (ref U303) (pin 2))
      (node (ref C1203) (pin 2))
      (node (ref U303) (pin 3))
      (node (ref C1401) (pin 2))
      (node (ref U701) (pin 10))
      (node (ref U701) (pin 20))
      (node (ref U701) (pin 11))
      (node (ref R203) (pin 2))
      (node (ref U701) (pin 19))
      (node (ref C1403) (pin 2))
      (node (ref C1402) (pin 2))
      (node (ref D1401) (pin 2))
      (node (ref U801) (pin 19))
      (node (ref U1101) (pin 5))
      (node (ref J1401) (pin 3))
      (node (ref J1401) (pin 2))
      (node (ref U801) (pin 11))
      (node (ref C804) (pin 2))
      (node (ref U1601) (pin 10))
      (node (ref U1601) (pin 12))
      (node (ref U1601) (pin 13))
      (node (ref R1305) (pin 2))
      (node (ref Q801) (pin 2))
      (node (ref U1601) (pin 24))
      (node (ref C1303) (pin 2))
      (node (ref C1304) (pin 2))
      (node (ref R1303) (pin 2))
      (node (ref D1301) (pin 2))
      (node (ref C803) (pin 1))
      (node (ref C303) (pin 1))
      (node (ref U801) (pin 20))
      (node (ref U801) (pin 10))
      (node (ref Q301) (pin 2))
      (node (ref U1301) (pin 4))
      (node (ref U803) (pin 3))
      (node (ref U803) (pin 2))
      (node (ref U1601) (pin 7))
      (node (ref C1302) (pin 2))
      (node (ref C1301) (pin 2))
      (node (ref C702) (pin 2))
      (node (ref C1305) (pin 2))
      (node (ref C701) (pin 1))
      (node (ref D901) (pin 2))
      (node (ref C304) (pin 2))
      (node (ref D902) (pin 2))
      (node (ref Q1301) (pin 2))
      (node (ref C604) (pin 2))
      (node (ref D903) (pin 2))
      (node (ref J901) (pin 6))
      (node (ref U401) (pin 1))
      (node (ref U401) (pin 10))
      (node (ref D1601) (pin 1))
      (node (ref Q601) (pin 2))
      (node (ref U401) (pin 20))
      (node (ref C1206) (pin 2))
      (node (ref U401) (pin 11))
      (node (ref C1306) (pin 2))
      (node (ref R205) (pin 2))
      (node (ref Q1303) (pin 2))
      (node (ref C603) (pin 1))
      (node (ref R927) (pin 2))
      (node (ref C903) (pin 1))
      (node (ref U401) (pin 19))
      (node (ref U603) (pin 3))
      (node (ref D1302) (pin 2))
      (node (ref U603) (pin 2))
      (node (ref D1304) (pin 2))
      (node (ref C902) (pin 2))
      (node (ref C901) (pin 2))
      (node (ref C602) (pin 2))
      (node (ref R1310) (pin 2))
      (node (ref C904) (pin 1))
      (node (ref C601) (pin 1))
      (node (ref C905) (pin 2))
      (node (ref U601) (pin 19))
      (node (ref C1307) (pin 2))
      (node (ref U301) (pin 19))
      (node (ref U601) (pin 11))
      (node (ref U601) (pin 20))
      (node (ref U601) (pin 10))
      (node (ref U601) (pin 1))
      (node (ref C401) (pin 1))
      (node (ref C504) (pin 2))
      (node (ref C1602) (pin 2))
      (node (ref C1603) (pin 2))
      (node (ref Q501) (pin 2))
      (node (ref C1605) (pin 1))
      (node (ref C402) (pin 2))
      (node (ref C1604) (pin 2))
      (node (ref C1502) (pin 2))
      (node (ref C1501) (pin 2))
      (node (ref C1503) (pin 2))
      (node (ref U403) (pin 2))
      (node (ref U403) (pin 3))
      (node (ref SW1501) (pin C))
      (node (ref SW1501) (pin S1))
      (node (ref C403) (pin 1))
      (node (ref SW1503) (pin 1))
      (node (ref SW1503) (pin 2))
      (node (ref SW1503) (pin 3))
      (node (ref C503) (pin 1))
      (node (ref U501) (pin 1))
      (node (ref SW901) (pin 2))
      (node (ref U501) (pin 10))
      (node (ref U501) (pin 20))
      (node (ref U501) (pin 11))
      (node (ref Q901) (pin 2))
      (node (ref U801) (pin 1))
      (node (ref U501) (pin 19))
      (node (ref C501) (pin 1))
      (node (ref Q401) (pin 2))
      (node (ref C502) (pin 2))
      (node (ref R1606) (pin 2))
      (node (ref U1603) (pin 6))
      (node (ref U1603) (pin 5))
      (node (ref U1603) (pin 4))
      (node (ref U1603) (pin 3))
      (node (ref U1603) (pin 1))
      (node (ref J1602) (pin 1))
      (node (ref J1601) (pin 1))
      (node (ref D905) (pin 2))
      (node (ref U503) (pin 2))
      (node (ref U503) (pin 3))
      (node (ref C404) (pin 2))
      (node (ref U1602) (pin 2))
      (node (ref C1601) (pin 1)))
    (net (code 23) (name "Net-(D202-Pad2)")
      (node (ref D202) (pin 2))
      (node (ref R204) (pin 2)))
    (net (code 24) (name "Net-(D202-Pad1)")
      (node (ref D202) (pin 1))
      (node (ref Q202) (pin 3)))
    (net (code 25) (name Dot)
      (node (ref R903) (pin 1))
      (node (ref Q201) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref Q202) (pin 1))
      (node (ref R203) (pin 1)))
    (net (code 26) (name Tube_LED)
      (node (ref Q401) (pin 1))
      (node (ref Q801) (pin 1))
      (node (ref Q701) (pin 1))
      (node (ref Q301) (pin 1))
      (node (ref Q501) (pin 1))
      (node (ref R902) (pin 1))
      (node (ref R205) (pin 1))
      (node (ref Q601) (pin 1)))
    (net (code 27) (name "Net-(U901-Pad2)")
      (node (ref U901) (pin 2)))
    (net (code 28) (name "Net-(C901-Pad1)")
      (node (ref C901) (pin 1))
      (node (ref U902) (pin 29)))
    (net (code 29) (name /uC/XTAL1)
      (node (ref Y901) (pin 1))
      (node (ref U902) (pin 8))
      (node (ref C904) (pin 2)))
    (net (code 30) (name /uC/XTAL2)
      (node (ref Y901) (pin 2))
      (node (ref C905) (pin 1))
      (node (ref U902) (pin 7)))
    (net (code 31) (name "Net-(R913-Pad2)")
      (node (ref R913) (pin 2))
      (node (ref U902) (pin 4)))
    (net (code 32) (name /uC/~Reset_ISP)
      (node (ref R913) (pin 1))
      (node (ref R917) (pin 2))
      (node (ref SW901) (pin 1))
      (node (ref J901) (pin 5)))
    (net (code 33) (name "Net-(R912-Pad2)")
      (node (ref R912) (pin 2))
      (node (ref U902) (pin 19)))
    (net (code 34) (name "Net-(R911-Pad2)")
      (node (ref U902) (pin 20))
      (node (ref R911) (pin 2)))
    (net (code 35) (name "Net-(R910-Pad2)")
      (node (ref U902) (pin 16))
      (node (ref R910) (pin 2)))
    (net (code 36) (name "Net-(R909-Pad2)")
      (node (ref U902) (pin 15))
      (node (ref R909) (pin 2)))
    (net (code 37) (name "Net-(R908-Pad2)")
      (node (ref U902) (pin 14))
      (node (ref R908) (pin 2)))
    (net (code 38) (name Encoder_push)
      (node (ref SW1501) (pin S2))
      (node (ref R1505) (pin 2))
      (node (ref R914) (pin 1))
      (node (ref C1503) (pin 1)))
    (net (code 39) (name "Net-(R914-Pad2)")
      (node (ref R914) (pin 2))
      (node (ref U902) (pin 11)))
    (net (code 40) (name Encoder_A)
      (node (ref R1502) (pin 2))
      (node (ref R915) (pin 1))
      (node (ref C1502) (pin 1)))
    (net (code 41) (name "Net-(R915-Pad2)")
      (node (ref R915) (pin 2))
      (node (ref U902) (pin 12)))
    (net (code 42) (name "Net-(R906-Pad2)")
      (node (ref U902) (pin 3))
      (node (ref R906) (pin 2)))
    (net (code 43) (name "Net-(R905-Pad2)")
      (node (ref U902) (pin 2))
      (node (ref R905) (pin 2)))
    (net (code 44) (name "Net-(R904-Pad2)")
      (node (ref R904) (pin 2))
      (node (ref U902) (pin 1)))
    (net (code 45) (name "Net-(R903-Pad2)")
      (node (ref U902) (pin 23))
      (node (ref R903) (pin 2)))
    (net (code 46) (name "Net-(R902-Pad2)")
      (node (ref U902) (pin 22))
      (node (ref R902) (pin 2)))
    (net (code 47) (name "Net-(R901-Pad2)")
      (node (ref R901) (pin 2)))
    (net (code 48) (name enable_2.5V_PSU)
      (node (ref R916) (pin 1)))
    (net (code 49) (name "Net-(R937-Pad2)")
      (node (ref R937) (pin 2))
      (node (ref U902) (pin 30)))
    (net (code 50) (name "Net-(R936-Pad2)")
      (node (ref R936) (pin 2))
      (node (ref U902) (pin 31)))
    (net (code 51) (name "Net-(R935-Pad2)")
      (node (ref U902) (pin 32))
      (node (ref R935) (pin 2)))
    (net (code 52) (name "Net-(R934-Pad2)")
      (node (ref U902) (pin 33))
      (node (ref R934) (pin 2)))
    (net (code 53) (name "Net-(R933-Pad2)")
      (node (ref U902) (pin 34))
      (node (ref R933) (pin 2)))
    (net (code 54) (name "Net-(R907-Pad2)")
      (node (ref U902) (pin 35))
      (node (ref R907) (pin 2)))
    (net (code 55) (name "Net-(U901-Pad8)")
      (node (ref U901) (pin 8)))
    (net (code 56) (name "Net-(U901-Pad7)")
      (node (ref U901) (pin 7)))
    (net (code 57) (name "Net-(U901-Pad6)")
      (node (ref U901) (pin 6)))
    (net (code 58) (name "Net-(U901-Pad5)")
      (node (ref U901) (pin 5)))
    (net (code 59) (name "Net-(U901-Pad4)")
      (node (ref U901) (pin 4)))
    (net (code 60) (name "Net-(U901-Pad3)")
      (node (ref U901) (pin 3)))
    (net (code 61) (name "Net-(U901-Pad1)")
      (node (ref U901) (pin 1)))
    (net (code 62) (name "Net-(R920-Pad2)")
      (node (ref R920) (pin 2))
      (node (ref U902) (pin 9)))
    (net (code 63) (name "Net-(U902-Pad18)")
      (node (ref U902) (pin 6))
      (node (ref U902) (pin 39))
      (node (ref U902) (pin 28))
      (node (ref U902) (pin 18)))
    (net (code 64) (name "Net-(U902-Pad44)")
      (node (ref U902) (pin 44)))
    (net (code 65) (name "Net-(U902-Pad43)")
      (node (ref U902) (pin 43)))
    (net (code 66) (name "Net-(U902-Pad42)")
      (node (ref U902) (pin 42)))
    (net (code 67) (name "Net-(U902-Pad41)")
      (node (ref U902) (pin 41)))
    (net (code 68) (name "Net-(U902-Pad40)")
      (node (ref U902) (pin 40)))
    (net (code 69) (name "Net-(R919-Pad2)")
      (node (ref U902) (pin 37))
      (node (ref R919) (pin 2)))
    (net (code 70) (name "Net-(R916-Pad2)")
      (node (ref R916) (pin 2))
      (node (ref U902) (pin 36)))
    (net (code 71) (name /uC/clk_ISP)
      (node (ref R906) (pin 1))
      (node (ref R932) (pin 2))
      (node (ref J901) (pin 3))
      (node (ref D903) (pin 1)))
    (net (code 72) (name /uC/MOSI_ISP)
      (node (ref D902) (pin 1))
      (node (ref J901) (pin 4))
      (node (ref R931) (pin 2))
      (node (ref R904) (pin 1)))
    (net (code 73) (name PSU_3.3V_feedback)
      (node (ref D1304) (pin 1))
      (node (ref R1309) (pin 1))
      (node (ref R919) (pin 1)))
    (net (code 74) (name "Net-(R918-Pad2)")
      (node (ref U902) (pin 13))
      (node (ref R918) (pin 2)))
    (net (code 75) (name "Net-(R922-Pad2)")
      (node (ref R922) (pin 2)))
    (net (code 76) (name "Net-(R923-Pad2)")
      (node (ref R923) (pin 2)))
    (net (code 77) (name "Net-(R924-Pad2)")
      (node (ref R924) (pin 2)))
    (net (code 78) (name Tx)
      (node (ref R921) (pin 1))
      (node (ref U1602) (pin 8)))
    (net (code 79) (name "Net-(R921-Pad2)")
      (node (ref U902) (pin 10))
      (node (ref R921) (pin 2)))
    (net (code 80) (name SCL)
      (node (ref R912) (pin 1))
      (node (ref R925) (pin 2))
      (node (ref U1101) (pin 8)))
    (net (code 81) (name SDA)
      (node (ref R911) (pin 1))
      (node (ref R926) (pin 2))
      (node (ref U1101) (pin 7)))
    (net (code 82) (name Encoder_B)
      (node (ref R1501) (pin 2))
      (node (ref R918) (pin 1))
      (node (ref C1501) (pin 1)))
    (net (code 83) (name Dip_1)
      (node (ref R1506) (pin 2))
      (node (ref SW1503) (pin 4))
      (node (ref R924) (pin 1)))
    (net (code 84) (name Dip_2)
      (node (ref R923) (pin 1))
      (node (ref SW1503) (pin 5))
      (node (ref R1507) (pin 2)))
    (net (code 85) (name Dip_3)
      (node (ref R922) (pin 1))
      (node (ref SW1503) (pin 6))
      (node (ref R1508) (pin 2)))
    (net (code 86) (name Rx)
      (node (ref R920) (pin 1))
      (node (ref U1602) (pin 1)))
    (net (code 87) (name "Net-(D904-Pad1)")
      (node (ref D904) (pin 1))
      (node (ref Q901) (pin 3)))
    (net (code 88) (name "Net-(D904-Pad2)")
      (node (ref D904) (pin 2))
      (node (ref R929) (pin 2)))
    (net (code 89) (name +12V)
      (node (ref R1301) (pin 2))
      (node (ref C1201) (pin 1))
      (node (ref C1202) (pin 1))
      (node (ref R1201) (pin 2))
      (node (ref U1301) (pin 6))
      (node (ref C1401) (pin 1))
      (node (ref C1402) (pin 1))
      (node (ref R1308) (pin 1))
      (node (ref C1403) (pin 1))
      (node (ref C1302) (pin 1))
      (node (ref U1201) (pin 6))
      (node (ref R1306) (pin 1))
      (node (ref SW1401) (pin 3))
      (node (ref C1301) (pin 1))
      (node (ref R928) (pin 1))
      (node (ref R1307) (pin 1)))
    (net (code 90) (name "Net-(D905-Pad1)")
      (node (ref R929) (pin 1))
      (node (ref D905) (pin 1))
      (node (ref R928) (pin 2)))
    (net (code 91) (name LED_Error)
      (node (ref Q901) (pin 1))
      (node (ref R901) (pin 1))
      (node (ref R927) (pin 1)))
    (net (code 92) (name /uC/MISO_ISP)
      (node (ref D901) (pin 1))
      (node (ref R930) (pin 2))
      (node (ref J901) (pin 1))
      (node (ref R905) (pin 1)))
    (net (code 93) (name MISO)
      (node (ref R930) (pin 1)))
    (net (code 94) (name "Net-(U902-Pad21)")
      (node (ref U902) (pin 21)))
    (net (code 95) (name "Net-(U902-Pad24)")
      (node (ref U902) (pin 24)))
    (net (code 96) (name "Net-(U902-Pad25)")
      (node (ref U902) (pin 25)))
    (net (code 97) (name "Net-(U902-Pad26)")
      (node (ref U902) (pin 26)))
    (net (code 98) (name "Net-(U1101-Pad1)")
      (node (ref U1101) (pin 1)))
    (net (code 99) (name "Net-(U1101-Pad3)")
      (node (ref U1101) (pin 3)))
    (net (code 100) (name "Net-(U1101-Pad4)")
      (node (ref U1101) (pin 4)))
    (net (code 101) (name V_Bat)
      (node (ref U1101) (pin 6))
      (node (ref BT1101) (pin 1)))
    (net (code 102) (name "Net-(R1202-Pad2)")
      (node (ref RV1201) (pin 1))
      (node (ref R1202) (pin 2)))
    (net (code 103) (name "Net-(R1203-Pad1)")
      (node (ref RV1201) (pin 3))
      (node (ref R1203) (pin 1)))
    (net (code 104) (name "Net-(R1201-Pad1)")
      (node (ref U1201) (pin 8))
      (node (ref U1201) (pin 1))
      (node (ref R1201) (pin 1))
      (node (ref U1201) (pin 7)))
    (net (code 105) (name "Net-(C1203-Pad1)")
      (node (ref C1203) (pin 1))
      (node (ref U1201) (pin 3)))
    (net (code 106) (name "Net-(RV1201-Pad2)")
      (node (ref U1201) (pin 5))
      (node (ref RV1201) (pin 2)))
    (net (code 107) (name "/5V PSU /SwE")
      (node (ref U1201) (pin 2))
      (node (ref L1201) (pin 2))
      (node (ref D1201) (pin 1)))
    (net (code 109) (name "Net-(D1401-Pad1)")
      (node (ref SW1401) (pin 2))
      (node (ref D1401) (pin 1))
      (node (ref F1401) (pin 1)))
    (net (code 110) (name "Net-(SW1401-Pad1)")
      (node (ref SW1401) (pin 1)))
    (net (code 111) (name "Net-(F1401-Pad2)")
      (node (ref F1401) (pin 2))
      (node (ref J1401) (pin 1)))
    (net (code 113) (name "Net-(R1303-Pad1)")
      (node (ref R1303) (pin 1))
      (node (ref RV1301) (pin 3)))
    (net (code 114) (name "Net-(C1303-Pad1)")
      (node (ref C1303) (pin 1))
      (node (ref U1301) (pin 3)))
    (net (code 115) (name "Net-(R1302-Pad2)")
      (node (ref R1302) (pin 2))
      (node (ref RV1301) (pin 1)))
    (net (code 116) (name "/3_3V PSU/MC34063_Feedback")
      (node (ref RV1301) (pin 2))
      (node (ref Q1302) (pin 2))
      (node (ref U1301) (pin 5)))
    (net (code 117) (name "Net-(Q1302-Pad3)")
      (node (ref R1307) (pin 2))
      (node (ref Q1302) (pin 3)))
    (net (code 118) (name "Net-(C1306-Pad1)")
      (node (ref R1304) (pin 1))
      (node (ref Q1301) (pin 1))
      (node (ref R1305) (pin 1))
      (node (ref C1306) (pin 1)))
    (net (code 119) (name "Net-(Q1301-Pad3)")
      (node (ref Q1301) (pin 3))
      (node (ref R1306) (pin 2))
      (node (ref Q1302) (pin 1))
      (node (ref Q1303) (pin 1)))
    (net (code 120) (name "Net-(D1303-Pad1)")
      (node (ref D1303) (pin 1))
      (node (ref Q1303) (pin 3)))
    (net (code 121) (name "Net-(D1303-Pad2)")
      (node (ref D1303) (pin 2))
      (node (ref R1308) (pin 2)))
    (net (code 122) (name enable_3.3V_PSU)
      (node (ref R1304) (pin 2)))
    (net (code 123) (name "/3_3V PSU/MC34063_HC_A")
      (node (ref L1301) (pin 1))
      (node (ref D1302) (pin 1))
      (node (ref C1305) (pin 1))
      (node (ref L1202) (pin 1))
      (node (ref C1304) (pin 1))
      (node (ref R1302) (pin 1)))
    (net (code 124) (name "Net-(Q1304-Pad1)")
      (node (ref Q1304) (pin 1))
      (node (ref R1311) (pin 1)))
    (net (code 125) (name "Net-(Q1304-Pad2)")
      (node (ref U1301) (pin 1))
      (node (ref U1301) (pin 8))
      (node (ref Q1304) (pin 2))
      (node (ref U1301) (pin 7))
      (node (ref R1301) (pin 1)))
    (net (code 126) (name "Net-(D1301-Pad1)")
      (node (ref D1301) (pin 1))
      (node (ref Q1304) (pin 3))
      (node (ref L1301) (pin 2)))
    (net (code 127) (name "/3_3V PSU/SwE")
      (node (ref R1311) (pin 2))
      (node (ref R1310) (pin 1))
      (node (ref U1301) (pin 2)))
    (net (code 128) (name "Net-(R1502-Pad1)")
      (node (ref SW1501) (pin B))
      (node (ref R1503) (pin 2))
      (node (ref R1502) (pin 1)))
    (net (code 129) (name "Net-(R1501-Pad1)")
      (node (ref R1501) (pin 1))
      (node (ref SW1501) (pin A))
      (node (ref R1504) (pin 2)))
    (net (code 130) (name "Net-(R1604-Pad2)")
      (node (ref U1601) (pin 19))
      (node (ref R1604) (pin 2)))
    (net (code 131) (name "Net-(R1608-Pad1)")
      (node (ref R1608) (pin 1)))
    (net (code 132) (name "Net-(R1603-Pad1)")
      (node (ref U1603) (pin 7))
      (node (ref R1603) (pin 1)))
    (net (code 133) (name "Net-(C1601-Pad2)")
      (node (ref R1605) (pin 2))
      (node (ref U1603) (pin 2))
      (node (ref C1601) (pin 2)))
    (net (code 134) (name "Net-(R1606-Pad1)")
      (node (ref R1606) (pin 1))
      (node (ref U1602) (pin 6)))
    (net (code 135) (name "Net-(U1601-Pad21)")
      (node (ref U1602) (pin 5))
      (node (ref U1601) (pin 21)))
    (net (code 136) (name "Net-(U1601-Pad20)")
      (node (ref U1602) (pin 4))
      (node (ref U1601) (pin 20)))
    (net (code 137) (name "Net-(R1603-Pad2)")
      (node (ref R1603) (pin 2))
      (node (ref U1601) (pin 18)))
    (net (code 138) (name "Net-(R1604-Pad1)")
      (node (ref U1603) (pin 8))
      (node (ref R1604) (pin 1)))
    (net (code 139) (name "Net-(J1602-Pad2)")
      (node (ref J1602) (pin 2))
      (node (ref R1602) (pin 2)))
    (net (code 140) (name "Net-(D1602-Pad1)")
      (node (ref D1602) (pin 1))
      (node (ref R1608) (pin 2))
      (node (ref U1601) (pin 22)))
    (net (code 141) (name "Net-(L1601-Pad1)")
      (node (ref R1602) (pin 1))
      (node (ref L1601) (pin 1))
      (node (ref U1601) (pin 11)))
    (net (code 142) (name "Net-(L1601-Pad2)")
      (node (ref R1607) (pin 2))
      (node (ref L1601) (pin 2)))
    (net (code 143) (name "Net-(R1607-Pad1)")
      (node (ref R1607) (pin 1))
      (node (ref U1601) (pin 9))
      (node (ref U1601) (pin 8)))
    (net (code 144) (name "Net-(D1601-Pad2)")
      (node (ref D1601) (pin 2))
      (node (ref R1601) (pin 2)))
    (net (code 145) (name "Net-(R1601-Pad1)")
      (node (ref R1601) (pin 1))
      (node (ref U1601) (pin 3)))
    (net (code 146) (name "Net-(U1601-Pad5)")
      (node (ref U1601) (pin 5)))
    (net (code 147) (name "Net-(U1601-Pad4)")
      (node (ref U1601) (pin 4)))
    (net (code 148) (name "Net-(U1601-Pad17)")
      (node (ref U1601) (pin 17)))
    (net (code 149) (name "Net-(U1601-Pad16)")
      (node (ref U1601) (pin 16)))
    (net (code 150) (name "Net-(U1601-Pad15)")
      (node (ref U1601) (pin 15)))
    (net (code 151) (name "Net-(U1601-Pad14)")
      (node (ref U1601) (pin 14)))
    (net (code 152) (name "Net-(U1601-Pad2)")
      (node (ref U1601) (pin 2)))
    (net (code 153) (name "Net-(U1601-Pad1)")
      (node (ref U1601) (pin 1)))
    (net (code 154) (name "Net-(U1601-Pad6)")
      (node (ref U1601) (pin 6)))
    (net (code 155) (name "Net-(R301-Pad2)")
      (node (ref R301) (pin 2))
      (node (ref U301) (pin 4)))
    (net (code 156) (name "Net-(R302-Pad2)")
      (node (ref R302) (pin 2))
      (node (ref U301) (pin 5)))
    (net (code 157) (name "Net-(R303-Pad2)")
      (node (ref R303) (pin 2))
      (node (ref U301) (pin 6)))
    (net (code 158) (name "Net-(R304-Pad2)")
      (node (ref R304) (pin 2))
      (node (ref U301) (pin 7)))
    (net (code 159) (name "Net-(R305-Pad2)")
      (node (ref R305) (pin 2))
      (node (ref U301) (pin 14)))
    (net (code 160) (name "Net-(R306-Pad2)")
      (node (ref R306) (pin 2))
      (node (ref U301) (pin 15)))
    (net (code 161) (name "Net-(R307-Pad2)")
      (node (ref R307) (pin 2))
      (node (ref U301) (pin 16)))
    (net (code 162) (name "Net-(R308-Pad2)")
      (node (ref R308) (pin 2))
      (node (ref U301) (pin 17)))
    (net (code 163) (name /Tubes/IV-9_Tube/Dot)
      (node (ref R301) (pin 1))
      (node (ref U302) (pin 2)))
    (net (code 164) (name /Tubes/IV-9_Tube/b)
      (node (ref R302) (pin 1))
      (node (ref U302) (pin 3)))
    (net (code 165) (name /Tubes/IV-9_Tube/c)
      (node (ref R303) (pin 1))
      (node (ref U302) (pin 4)))
    (net (code 166) (name /Tubes/IV-9_Tube/a)
      (node (ref R304) (pin 1))
      (node (ref U302) (pin 5)))
    (net (code 167) (name /Tubes/IV-9_Tube/f)
      (node (ref R305) (pin 1))
      (node (ref U302) (pin 6)))
    (net (code 168) (name /Tubes/IV-9_Tube/g)
      (node (ref R306) (pin 1))
      (node (ref U302) (pin 7)))
    (net (code 169) (name /Tubes/IV-9_Tube/d)
      (node (ref R307) (pin 1))
      (node (ref U302) (pin 8)))
    (net (code 170) (name /Tubes/IV-9_Tube/e)
      (node (ref R308) (pin 1))
      (node (ref U302) (pin 9)))
    (net (code 171) (name "Net-(C302-Pad1)")
      (node (ref U303) (pin 1))
      (node (ref U302) (pin 1))
      (node (ref R309) (pin 2))
      (node (ref C302) (pin 1)))
    (net (code 172) (name "Net-(U303-Pad4)")
      (node (ref U303) (pin 4)))
    (net (code 173) (name "Net-(D301-Pad1)")
      (node (ref D301) (pin 1))
      (node (ref Q301) (pin 3)))
    (net (code 174) (name "Net-(D301-Pad2)")
      (node (ref D301) (pin 2))
      (node (ref R310) (pin 1)))
    (net (code 175) (name "Net-(R311-Pad2)")
      (node (ref R311) (pin 2))
      (node (ref U303) (pin 5)))
    (net (code 176) (name "Net-(R401-Pad2)")
      (node (ref R401) (pin 2))
      (node (ref U401) (pin 4)))
    (net (code 177) (name "Net-(R402-Pad2)")
      (node (ref R402) (pin 2))
      (node (ref U401) (pin 5)))
    (net (code 178) (name "Net-(R403-Pad2)")
      (node (ref R403) (pin 2))
      (node (ref U401) (pin 6)))
    (net (code 179) (name "Net-(R404-Pad2)")
      (node (ref R404) (pin 2))
      (node (ref U401) (pin 7)))
    (net (code 180) (name "Net-(R405-Pad2)")
      (node (ref R405) (pin 2))
      (node (ref U401) (pin 14)))
    (net (code 181) (name "Net-(R406-Pad2)")
      (node (ref U401) (pin 15))
      (node (ref R406) (pin 2)))
    (net (code 182) (name "Net-(R407-Pad2)")
      (node (ref U401) (pin 16))
      (node (ref R407) (pin 2)))
    (net (code 183) (name "Net-(R408-Pad2)")
      (node (ref U401) (pin 17))
      (node (ref R408) (pin 2)))
    (net (code 184) (name /Tubes/sheet5BB32DC8/Dot)
      (node (ref R401) (pin 1))
      (node (ref U402) (pin 2)))
    (net (code 185) (name /Tubes/sheet5BB32DC8/b)
      (node (ref R402) (pin 1))
      (node (ref U402) (pin 3)))
    (net (code 186) (name /Tubes/sheet5BB32DC8/c)
      (node (ref R403) (pin 1))
      (node (ref U402) (pin 4)))
    (net (code 187) (name /Tubes/sheet5BB32DC8/a)
      (node (ref U402) (pin 5))
      (node (ref R404) (pin 1)))
    (net (code 188) (name /Tubes/sheet5BB32DC8/f)
      (node (ref U402) (pin 6))
      (node (ref R405) (pin 1)))
    (net (code 189) (name /Tubes/sheet5BB32DC8/g)
      (node (ref U402) (pin 7))
      (node (ref R406) (pin 1)))
    (net (code 190) (name /Tubes/sheet5BB32DC8/d)
      (node (ref U402) (pin 8))
      (node (ref R407) (pin 1)))
    (net (code 191) (name /Tubes/sheet5BB32DC8/e)
      (node (ref U402) (pin 9))
      (node (ref R408) (pin 1)))
    (net (code 192) (name "Net-(C402-Pad1)")
      (node (ref C402) (pin 1))
      (node (ref R409) (pin 2))
      (node (ref U403) (pin 1))
      (node (ref U402) (pin 1)))
    (net (code 193) (name "Net-(U403-Pad4)")
      (node (ref U403) (pin 4)))
    (net (code 194) (name "Net-(D401-Pad1)")
      (node (ref D401) (pin 1))
      (node (ref Q401) (pin 3)))
    (net (code 195) (name "Net-(D401-Pad2)")
      (node (ref R410) (pin 1))
      (node (ref D401) (pin 2)))
    (net (code 196) (name "Net-(R411-Pad2)")
      (node (ref R411) (pin 2))
      (node (ref U403) (pin 5)))
    (net (code 197) (name "Net-(U503-Pad4)")
      (node (ref U503) (pin 4)))
    (net (code 198) (name /Tubes/sheet5BB36ADE/e)
      (node (ref U502) (pin 9))
      (node (ref R508) (pin 1)))
    (net (code 199) (name /Tubes/sheet5BB36ADE/d)
      (node (ref U502) (pin 8))
      (node (ref R507) (pin 1)))
    (net (code 200) (name /Tubes/sheet5BB36ADE/g)
      (node (ref U502) (pin 7))
      (node (ref R506) (pin 1)))
    (net (code 201) (name /Tubes/sheet5BB36ADE/f)
      (node (ref R505) (pin 1))
      (node (ref U502) (pin 6)))
    (net (code 202) (name /Tubes/sheet5BB36ADE/a)
      (node (ref R504) (pin 1))
      (node (ref U502) (pin 5)))
    (net (code 203) (name /Tubes/sheet5BB36ADE/c)
      (node (ref R503) (pin 1))
      (node (ref U502) (pin 4)))
    (net (code 204) (name /Tubes/sheet5BB36ADE/b)
      (node (ref R502) (pin 1))
      (node (ref U502) (pin 3)))
    (net (code 205) (name /Tubes/sheet5BB36ADE/Dot)
      (node (ref R501) (pin 1))
      (node (ref U502) (pin 2)))
    (net (code 206) (name "Net-(C502-Pad1)")
      (node (ref U502) (pin 1))
      (node (ref C502) (pin 1))
      (node (ref U503) (pin 1))
      (node (ref R509) (pin 2)))
    (net (code 207) (name "Net-(R505-Pad2)")
      (node (ref U501) (pin 14))
      (node (ref R505) (pin 2)))
    (net (code 208) (name "Net-(R506-Pad2)")
      (node (ref R506) (pin 2))
      (node (ref U501) (pin 15)))
    (net (code 209) (name "Net-(R507-Pad2)")
      (node (ref U501) (pin 16))
      (node (ref R507) (pin 2)))
    (net (code 210) (name "Net-(R508-Pad2)")
      (node (ref U501) (pin 17))
      (node (ref R508) (pin 2)))
    (net (code 211) (name "Net-(R501-Pad2)")
      (node (ref R501) (pin 2))
      (node (ref U501) (pin 4)))
    (net (code 212) (name "Net-(R502-Pad2)")
      (node (ref R502) (pin 2))
      (node (ref U501) (pin 5)))
    (net (code 213) (name "Net-(R503-Pad2)")
      (node (ref R503) (pin 2))
      (node (ref U501) (pin 6)))
    (net (code 214) (name "Net-(R504-Pad2)")
      (node (ref R504) (pin 2))
      (node (ref U501) (pin 7)))
    (net (code 215) (name "Net-(D501-Pad1)")
      (node (ref Q501) (pin 3))
      (node (ref D501) (pin 1)))
    (net (code 216) (name "Net-(D501-Pad2)")
      (node (ref D501) (pin 2))
      (node (ref R510) (pin 1)))
    (net (code 217) (name "Net-(R511-Pad2)")
      (node (ref R511) (pin 2))
      (node (ref U503) (pin 5)))
    (net (code 218) (name "Net-(R601-Pad2)")
      (node (ref R601) (pin 2))
      (node (ref U601) (pin 4)))
    (net (code 219) (name "Net-(R602-Pad2)")
      (node (ref R602) (pin 2))
      (node (ref U601) (pin 5)))
    (net (code 220) (name "Net-(R603-Pad2)")
      (node (ref R603) (pin 2))
      (node (ref U601) (pin 6)))
    (net (code 221) (name "Net-(R604-Pad2)")
      (node (ref R604) (pin 2))
      (node (ref U601) (pin 7)))
    (net (code 222) (name "Net-(R605-Pad2)")
      (node (ref R605) (pin 2))
      (node (ref U601) (pin 14)))
    (net (code 223) (name "Net-(R606-Pad2)")
      (node (ref R606) (pin 2))
      (node (ref U601) (pin 15)))
    (net (code 224) (name "Net-(R607-Pad2)")
      (node (ref R607) (pin 2))
      (node (ref U601) (pin 16)))
    (net (code 225) (name "Net-(R608-Pad2)")
      (node (ref R608) (pin 2))
      (node (ref U601) (pin 17)))
    (net (code 226) (name /Tubes/sheet5BB3BB93/Dot)
      (node (ref R601) (pin 1))
      (node (ref U602) (pin 2)))
    (net (code 227) (name /Tubes/sheet5BB3BB93/b)
      (node (ref U602) (pin 3))
      (node (ref R602) (pin 1)))
    (net (code 228) (name /Tubes/sheet5BB3BB93/c)
      (node (ref U602) (pin 4))
      (node (ref R603) (pin 1)))
    (net (code 229) (name /Tubes/sheet5BB3BB93/a)
      (node (ref U602) (pin 5))
      (node (ref R604) (pin 1)))
    (net (code 230) (name /Tubes/sheet5BB3BB93/f)
      (node (ref U602) (pin 6))
      (node (ref R605) (pin 1)))
    (net (code 231) (name /Tubes/sheet5BB3BB93/g)
      (node (ref R606) (pin 1))
      (node (ref U602) (pin 7)))
    (net (code 232) (name /Tubes/sheet5BB3BB93/d)
      (node (ref U602) (pin 8))
      (node (ref R607) (pin 1)))
    (net (code 233) (name /Tubes/sheet5BB3BB93/e)
      (node (ref R608) (pin 1))
      (node (ref U602) (pin 9)))
    (net (code 234) (name "Net-(C602-Pad1)")
      (node (ref C602) (pin 1))
      (node (ref R609) (pin 2))
      (node (ref U603) (pin 1))
      (node (ref U602) (pin 1)))
    (net (code 235) (name "Net-(U603-Pad4)")
      (node (ref U603) (pin 4)))
    (net (code 236) (name "Net-(D601-Pad1)")
      (node (ref Q601) (pin 3))
      (node (ref D601) (pin 1)))
    (net (code 237) (name "Net-(D601-Pad2)")
      (node (ref D601) (pin 2))
      (node (ref R610) (pin 1)))
    (net (code 238) (name "Net-(R611-Pad2)")
      (node (ref U603) (pin 5))
      (node (ref R611) (pin 2)))
    (net (code 239) (name /Tubes/sheet5BB3E86C/Dot)
      (node (ref U702) (pin 2))
      (node (ref R701) (pin 1)))
    (net (code 240) (name /Tubes/sheet5BB3E86C/b)
      (node (ref U702) (pin 3))
      (node (ref R702) (pin 1)))
    (net (code 241) (name /Tubes/sheet5BB3E86C/c)
      (node (ref U702) (pin 4))
      (node (ref R703) (pin 1)))
    (net (code 242) (name /Tubes/sheet5BB3E86C/a)
      (node (ref R704) (pin 1))
      (node (ref U702) (pin 5)))
    (net (code 243) (name /Tubes/sheet5BB3E86C/f)
      (node (ref U702) (pin 6))
      (node (ref R705) (pin 1)))
    (net (code 244) (name /Tubes/sheet5BB3E86C/g)
      (node (ref U702) (pin 7))
      (node (ref R706) (pin 1)))
    (net (code 245) (name /Tubes/sheet5BB3E86C/d)
      (node (ref U702) (pin 8))
      (node (ref R707) (pin 1)))
    (net (code 246) (name /Tubes/sheet5BB3E86C/e)
      (node (ref R708) (pin 1))
      (node (ref U702) (pin 9)))
    (net (code 247) (name "Net-(C702-Pad1)")
      (node (ref U803) (pin 1))
      (node (ref R709) (pin 2))
      (node (ref C702) (pin 1))
      (node (ref U702) (pin 1)))
    (net (code 248) (name "Net-(U803-Pad4)")
      (node (ref U803) (pin 4)))
    (net (code 249) (name "Net-(D801-Pad1)")
      (node (ref D801) (pin 1))
      (node (ref Q801) (pin 3)))
    (net (code 250) (name "Net-(D801-Pad2)")
      (node (ref D801) (pin 2))
      (node (ref R810) (pin 1)))
    (net (code 251) (name "Net-(R811-Pad2)")
      (node (ref U803) (pin 5))
      (node (ref R811) (pin 2)))
    (net (code 252) (name "Net-(R705-Pad2)")
      (node (ref U701) (pin 14))
      (node (ref R705) (pin 2)))
    (net (code 253) (name "Net-(R706-Pad2)")
      (node (ref R706) (pin 2))
      (node (ref U701) (pin 15)))
    (net (code 254) (name "Net-(R707-Pad2)")
      (node (ref R707) (pin 2))
      (node (ref U701) (pin 16)))
    (net (code 255) (name "Net-(R708-Pad2)")
      (node (ref U701) (pin 17))
      (node (ref R708) (pin 2)))
    (net (code 256) (name "Net-(R701-Pad2)")
      (node (ref U701) (pin 4))
      (node (ref R701) (pin 2)))
    (net (code 257) (name "Net-(R702-Pad2)")
      (node (ref U701) (pin 5))
      (node (ref R702) (pin 2)))
    (net (code 258) (name "Net-(R703-Pad2)")
      (node (ref R703) (pin 2))
      (node (ref U701) (pin 6)))
    (net (code 259) (name "Net-(R704-Pad2)")
      (node (ref U701) (pin 7))
      (node (ref R704) (pin 2)))
    (net (code 260) (name "Net-(R711-Pad2)")
      (node (ref U703) (pin 5))
      (node (ref R711) (pin 2)))
    (net (code 261) (name "Net-(D701-Pad1)")
      (node (ref Q701) (pin 3))
      (node (ref D701) (pin 1)))
    (net (code 262) (name "Net-(D701-Pad2)")
      (node (ref D701) (pin 2))
      (node (ref R710) (pin 1)))
    (net (code 263) (name "Net-(C802-Pad1)")
      (node (ref C802) (pin 1))
      (node (ref R809) (pin 2))
      (node (ref U802) (pin 1))
      (node (ref U703) (pin 1)))
    (net (code 264) (name "Net-(U703-Pad4)")
      (node (ref U703) (pin 4)))
    (net (code 265) (name /Tubes/sheet5BB3E86D/e)
      (node (ref U802) (pin 9))
      (node (ref R808) (pin 1)))
    (net (code 266) (name /Tubes/sheet5BB3E86D/d)
      (node (ref U802) (pin 8))
      (node (ref R807) (pin 1)))
    (net (code 267) (name /Tubes/sheet5BB3E86D/g)
      (node (ref R806) (pin 1))
      (node (ref U802) (pin 7)))
    (net (code 268) (name /Tubes/sheet5BB3E86D/f)
      (node (ref U802) (pin 6))
      (node (ref R805) (pin 1)))
    (net (code 269) (name /Tubes/sheet5BB3E86D/a)
      (node (ref R804) (pin 1))
      (node (ref U802) (pin 5)))
    (net (code 270) (name /Tubes/sheet5BB3E86D/c)
      (node (ref R803) (pin 1))
      (node (ref U802) (pin 4)))
    (net (code 271) (name /Tubes/sheet5BB3E86D/b)
      (node (ref R802) (pin 1))
      (node (ref U802) (pin 3)))
    (net (code 272) (name /Tubes/sheet5BB3E86D/Dot)
      (node (ref U802) (pin 2))
      (node (ref R801) (pin 1)))
    (net (code 273) (name "Net-(R805-Pad2)")
      (node (ref R805) (pin 2))
      (node (ref U801) (pin 14)))
    (net (code 274) (name "Net-(R806-Pad2)")
      (node (ref R806) (pin 2))
      (node (ref U801) (pin 15)))
    (net (code 275) (name "Net-(R807-Pad2)")
      (node (ref R807) (pin 2))
      (node (ref U801) (pin 16)))
    (net (code 276) (name "Net-(R808-Pad2)")
      (node (ref R808) (pin 2))
      (node (ref U801) (pin 17)))
    (net (code 277) (name "Net-(R801-Pad2)")
      (node (ref U801) (pin 4))
      (node (ref R801) (pin 2)))
    (net (code 278) (name "Net-(R802-Pad2)")
      (node (ref U801) (pin 5))
      (node (ref R802) (pin 2)))
    (net (code 279) (name "Net-(R803-Pad2)")
      (node (ref U801) (pin 6))
      (node (ref R803) (pin 2)))
    (net (code 280) (name "Net-(R804-Pad2)")
      (node (ref U801) (pin 7))
      (node (ref R804) (pin 2)))))