163817344393194
Resistor_THT
R_Array_SIP4
4-pin Resistor SIP pack
R
0
4
4
Resistor_THT
R_Array_SIP5
5-pin Resistor SIP pack
R
0
5
5
Resistor_THT
R_Array_SIP6
6-pin Resistor SIP pack
R
0
6
6
Resistor_THT
R_Array_SIP7
7-pin Resistor SIP pack
R
0
7
7
Resistor_THT
R_Array_SIP8
8-pin Resistor SIP pack
R
0
8
8
Resistor_THT
R_Array_SIP9
9-pin Resistor SIP pack
R
0
9
9
Resistor_THT
R_Array_SIP10
10-pin Resistor SIP pack
R
0
10
10
Resistor_THT
R_Array_SIP11
11-pin Resistor SIP pack
R
0
11
11
Resistor_THT
R_Array_SIP12
12-pin Resistor SIP pack
R
0
12
12
Resistor_THT
R_Array_SIP13
13-pin Resistor SIP pack
R
0
13
13
Resistor_THT
R_Array_SIP14
14-pin Resistor SIP pack
R
0
14
14
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal
Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical
Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal
Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical
Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical
Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal
Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P2.54mm_Vertical
Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=2.54mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Vertical pin pitch 2.54mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical
Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P20.32mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=20.32mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 20.32mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0309_L9.0mm_D3.2mm_P25.40mm_Horizontal
Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=25.4mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0309 series Axial Horizontal pin pitch 25.4mm 0.5W = 1/2W length 9mm diameter 3.2mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical
Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P7.62mm_Vertical
Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=7.62mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Vertical pin pitch 7.62mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=20.32mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 20.32mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0411_L9.9mm_D3.6mm_P25.40mm_Horizontal
Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=25.4mm, 1W, length*diameter=9.9*3.6mm^2
Resistor Axial_DIN0411 series Axial Horizontal pin pitch 25.4mm 1W length 9.9mm diameter 3.6mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical
Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Vertical pin pitch 5.08mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P7.62mm_Vertical
Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Vertical pin pitch 7.62mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0414_L11.9mm_D4.5mm_P25.40mm_Horizontal
Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0414 series Axial Horizontal pin pitch 25.4mm 2W length 11.9mm diameter 4.5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P5.08mm_Vertical
Resistor, Axial_DIN0516 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Vertical pin pitch 5.08mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0516 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Vertical pin pitch 7.62mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 20.32mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 25.4mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0516_L15.5mm_D5.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=30.48mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf
Resistor Axial_DIN0516 series Axial Horizontal pin pitch 30.48mm 2W length 15.5mm diameter 5mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P5.08mm_Vertical
Resistor, Axial_DIN0614 series, Axial, Vertical, pin pitch=5.08mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Vertical pin pitch 5.08mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P7.62mm_Vertical
Resistor, Axial_DIN0614 series, Axial, Vertical, pin pitch=7.62mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Vertical pin pitch 7.62mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P15.24mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=15.24mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 15.24mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0614_L14.3mm_D5.7mm_P25.40mm_Horizontal
Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=25.4mm, 1.5W, length*diameter=14.3*5.7mm^2
Resistor Axial_DIN0614 series Axial Horizontal pin pitch 25.4mm 1.5W length 14.3mm diameter 5.7mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P5.08mm_Vertical
Resistor, Axial_DIN0617 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Vertical pin pitch 5.08mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0617 series, Axial, Vertical, pin pitch=7.62mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Vertical pin pitch 7.62mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P20.32mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 20.32mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=25.4mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 25.4mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0617_L17.0mm_D6.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=30.48mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0617 series Axial Horizontal pin pitch 30.48mm 2W length 17mm diameter 6mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0918 series, Axial, Vertical, pin pitch=7.62mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Vertical pin pitch 7.62mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=25.4mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 25.4mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0918_L18.0mm_D9.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=30.48mm, 4W, length*diameter=18*9mm^2
Resistor Axial_DIN0918 series Axial Horizontal pin pitch 30.48mm 4W length 18mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P7.62mm_Vertical
Resistor, Axial_DIN0922 series, Axial, Vertical, pin pitch=7.62mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Vertical pin pitch 7.62mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P25.40mm_Horizontal
Resistor, Axial_DIN0922 series, Axial, Horizontal, pin pitch=25.4mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Horizontal pin pitch 25.4mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_DIN0922_L20.0mm_D9.0mm_P30.48mm_Horizontal
Resistor, Axial_DIN0922 series, Axial, Horizontal, pin pitch=30.48mm, 5W, length*diameter=20*9mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf
Resistor Axial_DIN0922 series Axial Horizontal pin pitch 30.48mm 5W length 20mm diameter 9mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P5.08mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=5.08mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 5.08mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P22.40mm
Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P25.40mm
Resistor, Axial_Power series, Box, pin pitch=25.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 25.4mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L20.0mm_W6.4mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 4W length 20mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W6.4mm_P27.94mm
Resistor, Axial_Power series, Box, pin pitch=27.94mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 27.94mm 5W length 25mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W6.4mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 5W, length*width*height=25*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 5W length 25mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P27.94mm
Resistor, Axial_Power series, Box, pin pitch=27.94mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 27.94mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L25.0mm_W9.0mm_P30.48mm
Resistor, Axial_Power series, Box, pin pitch=30.48mm, 7W, length*width*height=25*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 30.48mm 7W length 25mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W6.4mm_P40.64mm
Resistor, Axial_Power series, Box, pin pitch=40.64mm, 7W, length*width*height=38*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 40.64mm 7W length 38mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W6.4mm_P45.72mm
Resistor, Axial_Power series, Box, pin pitch=45.72mm, 7W, length*width*height=38*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 45.72mm 7W length 38mm width 6.4mm height 6.4mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W9.0mm_P40.64mm
Resistor, Axial_Power series, Box, pin pitch=40.64mm, 9W, length*width*height=38*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 40.64mm 9W length 38mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L38.0mm_W9.0mm_P45.72mm
Resistor, Axial_Power series, Box, pin pitch=45.72mm, 9W, length*width*height=38*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 45.72mm 9W length 38mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P7.62mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=7.62mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 7.62mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P55.88mm
Resistor, Axial_Power series, Box, pin pitch=55.88mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 55.88mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L48.0mm_W12.5mm_P60.96mm
Resistor, Axial_Power series, Box, pin pitch=60.96mm, 15W, length*width*height=48*12.5*12.5mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 60.96mm 15W length 48mm width 12.5mm height 12.5mm
0
2
2
Resistor_THT
R_Axial_Power_L50.0mm_W9.0mm_P55.88mm
Resistor, Axial_Power series, Box, pin pitch=55.88mm, 11W, length*width*height=50*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 55.88mm 11W length 50mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L50.0mm_W9.0mm_P60.96mm
Resistor, Axial_Power series, Box, pin pitch=60.96mm, 11W, length*width*height=50*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 60.96mm 11W length 50mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P10.16mm_Vertical
Resistor, Axial_Power series, Axial, Vertical, pin pitch=10.16mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Axial Vertical pin pitch 10.16mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P66.04mm
Resistor, Axial_Power series, Box, pin pitch=66.04mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 66.04mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L60.0mm_W14.0mm_P71.12mm
Resistor, Axial_Power series, Box, pin pitch=71.12mm, 25W, length*width*height=60*14*14mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 71.12mm 25W length 60mm width 14mm height 14mm
0
2
2
Resistor_THT
R_Axial_Power_L75.0mm_W9.0mm_P81.28mm
Resistor, Axial_Power series, Box, pin pitch=81.28mm, 17W, length*width*height=75*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 81.28mm 17W length 75mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Power_L75.0mm_W9.0mm_P86.36mm
Resistor, Axial_Power series, Box, pin pitch=86.36mm, 17W, length*width*height=75*9*9mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf
Resistor Axial_Power series Box pin pitch 86.36mm 17W length 75mm width 9mm height 9mm
0
2
2
Resistor_THT
R_Axial_Shunt_L22.2mm_W8.0mm_PS14.30mm_P25.40mm
Resistor, Axial_Shunt series, Box, pin pitch=25.4mm, 3W, length*width*height=22.2*8*8mm^3, shunt pin pitch = 14.30mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 25.4mm 3W length 22.2mm width 8mm height 8mm shunt pin pitch 14.30mm
0
4
4
Resistor_THT
R_Axial_Shunt_L22.2mm_W9.5mm_PS14.30mm_P25.40mm
Resistor, Axial_Shunt series, Box, pin pitch=25.4mm, 5W, length*width*height=22.2*9.5*9.5mm^3, shunt pin pitch = 14.30mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 25.4mm 5W length 22.2mm width 9.5mm height 9.5mm shunt pin pitch 14.30mm
0
4
4
Resistor_THT
R_Axial_Shunt_L35.3mm_W9.5mm_PS25.40mm_P38.10mm
Resistor, Axial_Shunt series, Box, pin pitch=38.1mm, 7W, length*width*height=35.3*9.5*9.5mm^3, shunt pin pitch = 25.40mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 38.1mm 7W length 35.3mm width 9.5mm height 9.5mm shunt pin pitch 25.40mm
0
4
4
Resistor_THT
R_Axial_Shunt_L47.6mm_W9.5mm_PS34.93mm_P50.80mm
Resistor, Axial_Shunt series, Box, pin pitch=50.8mm, 10W, length*width*height=47.6*9.5*9.5mm^3, shunt pin pitch = 34.93mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 50.8mm 10W length 47.6mm width 9.5mm height 9.5mm shunt pin pitch 34.93mm
0
4
4
Resistor_THT
R_Axial_Shunt_L47.6mm_W12.7mm_PS34.93mm_P50.80mm
Resistor, Axial_Shunt series, Box, pin pitch=50.8mm, 15W, length*width*height=47.6*12.7*12.7mm^3, shunt pin pitch = 34.93mm, http://www.vishay.com/docs/30217/cpsl.pdf
Resistor Axial_Shunt series Box pin pitch 50.8mm 15W length 47.6mm width 12.7mm height 12.7mm shunt pin pitch 34.93mm
0
4
4
Resistor_THT
R_Bare_Metal_Element_L12.4mm_W4.8mm_P11.40mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=11.4mm, 1W, length*width=12.4*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 11.4mm 1W length 12.4mm width 4.8mm 
0
2
2
Resistor_THT
R_Bare_Metal_Element_L16.3mm_W4.8mm_P15.30mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=15.3mm, 3W, length*width=16.3*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 15.3mm 3W length 16.3mm width 4.8mm 
0
2
2
Resistor_THT
R_Bare_Metal_Element_L21.3mm_W4.8mm_P20.30mm
Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=20.3mm, 5W, length*width=21.3*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf
Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 20.3mm 5W length 21.3mm width 4.8mm 
0
2
2
Resistor_THT
R_Box_L8.4mm_W2.5mm_P5.08mm
Resistor, Box series, Radial, pin pitch=5.08mm, 0.5W = 1/2W, length*width=8.38*2.54mm^2, http://www.vishay.com/docs/60051/cns020.pdf
Resistor Box series Radial pin pitch 5.08mm 0.5W = 1/2W length 8.38mm width 2.54mm
0
2
2
Resistor_THT
R_Box_L13.0mm_W4.0mm_P9.00mm
Resistor, Box series, Radial, pin pitch=9.00mm, 2W, length*width=13.0*4.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 9.00mm 2W length 13.0mm width 4.0mm
0
2
2
Resistor_THT
R_Box_L14.0mm_W5.0mm_P9.00mm
Resistor, Box series, Radial, pin pitch=9.00mm, 5W, length*width=14.0*5.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 9.00mm 5W length 14.0mm width 5.0mm
0
2
2
Resistor_THT
R_Box_L26.0mm_W5.0mm_P20.00mm
Resistor, Box series, Radial, pin pitch=20.00mm, 10W, length*width=26.0*5.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf
Resistor Box series Radial pin pitch 20.00mm 10W length 26.0mm width 5.0mm
0
2
2
Resistor_THT
R_Radial_Power_L7.0mm_W8.0mm_Px2.40mm_Py2.30mm
Resistor, Radial_Power series, Radial, pin pitch=2.40*2.30mm^2, 7W, length*width=7*8mm^2, http://www.vitrohm.com/content/files/vitrohm_series_kv_-_201601.pdf
Resistor Radial_Power series Radial pin pitch 2.40*2.30mm^2 7W length 7mm width 8mm
0
2
2
Resistor_THT
R_Radial_Power_L9.0mm_W10.0mm_Px2.70mm_Py2.30mm
Resistor, Radial_Power series, Radial, pin pitch=2.70*2.30mm^2, 17W, length*width=9*10mm^2, http://www.vitrohm.com/content/files/vitrohm_series_kv_-_201601.pdf
Resistor Radial_Power series Radial pin pitch 2.70*2.30mm^2 17W length 9mm width 10mm
0
2
2
Resistor_THT
R_Radial_Power_L11.0mm_W7.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 2W, length*width=11.0*7.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 2W length 11.0mm width 7.0mm
0
2
2
Resistor_THT
R_Radial_Power_L12.0mm_W8.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 3W, length*width=12.0*8.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 3W length 12.0mm width 8.0mm
0
2
2
Resistor_THT
R_Radial_Power_L13.0mm_W9.0mm_P5.00mm
Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 7W, length*width=13.0*9.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 5.00mm 7W length 13.0mm width 9.0mm
0
2
2
Resistor_THT
R_Radial_Power_L16.1mm_W9.0mm_P7.37mm
Resistor, Radial_Power series, Radial, pin pitch=7.37mm, 10W, length*width=16.1*9mm^2, http://www.vishay.com/docs/30218/cpcx.pdf
Resistor Radial_Power series Radial pin pitch 7.37mm 10W length 16.1mm width 9mm
0
2
2
